(kicad_pcb (version 20171130) (host pcbnew "(5.1.10)-1")
  (general
    (thickness 1.6)
    (drawings 340)
    (tracks 802)
    (zones 0)
    (modules 44)
    (nets 79)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (1 In1.Cu signal hide)
    (2 In2.Cu signal hide)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user hide)
    (38 B.Mask user)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user)
    (47 F.CrtYd user hide)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.254)
    (trace_clearance 0.2032)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.7 2.7)
    (pad_drill 2.7)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +5V)
  (net 3 /A15)
  (net 4 /A14)
  (net 5 /A13)
  (net 6 /A12)
  (net 7 /A11)
  (net 8 /A10)
  (net 9 /A9)
  (net 10 /A8)
  (net 11 /A7)
  (net 12 /A6)
  (net 13 /A5)
  (net 14 /A4)
  (net 15 /A3)
  (net 16 /A2)
  (net 17 /A1)
  (net 18 /A0)
  (net 19 /D7)
  (net 20 /D6)
  (net 21 /D5)
  (net 22 /D4)
  (net 23 /D3)
  (net 24 /D2)
  (net 25 /D1)
  (net 26 /D0)
  (net 27 /VPB)
  (net 28 /RWB)
  (net 29 /~SYNC)
  (net 30 /~RCMEN)
  (net 31 /PH0)
  (net 32 /~RES)
  (net 33 /~IRQ)
  (net 34 /~NMI)
  (net 35 /RDY)
  (net 36 /SOB)
  (net 37 /MLB)
  (net 38 /PHI2O)
  (net 39 /PHI1O)
  (net 40 /ROMDIR)
  (net 41 /ROMG)
  (net 42 /PH0_ALT)
  (net 43 /DMA)
  (net 44 /4Y)
  (net 45 /4B)
  (net 46 /4A)
  (net 47 /3Y)
  (net 48 /3B)
  (net 49 /3A)
  (net 50 "Net-(JP1-Pad2)")
  (net 51 "Net-(JP2-Pad1)")
  (net 52 /BA1)
  (net 53 /BA0)
  (net 54 /BA2)
  (net 55 /BA3)
  (net 56 /BA5)
  (net 57 /BA4)
  (net 58 /BA6)
  (net 59 /BA7)
  (net 60 /BA9)
  (net 61 /BA8)
  (net 62 /BA10)
  (net 63 /BA11)
  (net 64 /BA13)
  (net 65 /BA12)
  (net 66 /~DMA)
  (net 67 "Net-(U2-Pad33)")
  (net 68 "Net-(U2-Pad6)")
  (net 69 /PH1)
  (net 70 "Net-(D1-Pad2)")
  (net 71 "Net-(U5-Pad18)")
  (net 72 "Net-(U5-Pad17)")
  (net 73 "Net-(U5-Pad3)")
  (net 74 "Net-(U5-Pad2)")
  (net 75 "Net-(RN4-Pad3)")
  (net 76 "Net-(RN4-Pad4)")
  (net 77 "Net-(RN4-Pad6)")
  (net 78 "Net-(RN4-Pad5)")
  (net_class Default "This is the default net class."
    (clearance 0.2032)
    (trace_width 0.254)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net /3A)
    (add_net /3B)
    (add_net /3Y)
    (add_net /4A)
    (add_net /4B)
    (add_net /4Y)
    (add_net /A0)
    (add_net /A1)
    (add_net /A10)
    (add_net /A11)
    (add_net /A12)
    (add_net /A13)
    (add_net /A14)
    (add_net /A15)
    (add_net /A2)
    (add_net /A3)
    (add_net /A4)
    (add_net /A5)
    (add_net /A6)
    (add_net /A7)
    (add_net /A8)
    (add_net /A9)
    (add_net /BA0)
    (add_net /BA1)
    (add_net /BA10)
    (add_net /BA11)
    (add_net /BA12)
    (add_net /BA13)
    (add_net /BA2)
    (add_net /BA3)
    (add_net /BA4)
    (add_net /BA5)
    (add_net /BA6)
    (add_net /BA7)
    (add_net /BA8)
    (add_net /BA9)
    (add_net /D0)
    (add_net /D1)
    (add_net /D2)
    (add_net /D3)
    (add_net /D4)
    (add_net /D5)
    (add_net /D6)
    (add_net /D7)
    (add_net /DMA)
    (add_net /MLB)
    (add_net /PH0)
    (add_net /PH0_ALT)
    (add_net /PH1)
    (add_net /PHI1O)
    (add_net /PHI2O)
    (add_net /RDY)
    (add_net /ROMDIR)
    (add_net /ROMG)
    (add_net /RWB)
    (add_net /SOB)
    (add_net /VPB)
    (add_net /~DMA)
    (add_net /~IRQ)
    (add_net /~NMI)
    (add_net /~RCMEN)
    (add_net /~RES)
    (add_net /~SYNC)
    (add_net GND)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(JP1-Pad2)")
    (add_net "Net-(JP2-Pad1)")
    (add_net "Net-(RN4-Pad3)")
    (add_net "Net-(RN4-Pad4)")
    (add_net "Net-(RN4-Pad5)")
    (add_net "Net-(RN4-Pad6)")
    (add_net "Net-(U2-Pad33)")
    (add_net "Net-(U2-Pad6)")
    (add_net "Net-(U5-Pad17)")
    (add_net "Net-(U5-Pad18)")
    (add_net "Net-(U5-Pad2)")
    (add_net "Net-(U5-Pad3)")
  )
  (module Symbol:OSHW-Symbol_6.7x6mm_SilkScreen (layer F.Cu) (tedit 0)
    (at 220.472 96.647 270)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference REF** (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value OSHW-Symbol_6.7x6mm_SilkScreen (at 0.75 0 90) (layer F.Fab) hide)
  )
  (module Symbol:KiCad-Logo_5mm_SilkScreen (layer B.Cu) (tedit 0)
    (at 192.532 90.17 180)
    (descr "KiCad Logo")
    (tags "Logo KiCad")
    (attr virtual)
    (fp_text reference REF** (at 0 5.08) (layer B.SilkS) hide)
    (fp_text value KiCad-Logo_5mm_SilkScreen (at 0 -3.81) (layer B.Fab) hide)
  )
  (module "My Libraries:BE5v2" (layer F.Cu) (tedit 5FBC48F5)
    (at 183.134 108.204)
    (descr "Imported from BE5.svg")
    (tags svg2mod)
    (attr virtual)
    (fp_text reference svg2mod (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value G*** (at 0 8.048) (layer F.SilkS) hide)
  )
  (module MountingHole:MountingHole_2.7mm_M2.5 (layer F.Cu) (tedit 56D1B4CB)
    (at 220.853 111.7346)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (attr virtual)
    (fp_text reference H4 (at 0 -3.7) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 3.7) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.7mm_M2.5 (layer F.Cu) (tedit 56D1B4CB)
    (at 136.05 111.76)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (attr virtual)
    (fp_text reference H3 (at 0 -3.7) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 3.7) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.7mm_M2.5 (layer F.Cu) (tedit 56D1B4CB)
    (at 220.853 64.897)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (attr virtual)
    (fp_text reference He (at 0 -3.7) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 3.7) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.7mm_M2.5 (layer F.Cu) (tedit 56D1B4CB)
    (at 136.05 64.93)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (attr virtual)
    (fp_text reference H1 (at 0 -3.7) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 3.7) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 144.9705 110.4265 90)
    (descr "Through hole straight pin header, 2x02, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x02 2.54mm double row")
    (fp_text reference J1 (at 1.27 -2.33 90) (layer F.SilkS) hide)
    (fp_text value POWER (at 1.27 4.87 90) (layer F.Fab))
    (fp_text user %R (at 1.27 1.27) (layer F.Fab))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x07_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 213.36 89.154)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (fp_text reference J10 (at 0 -2.33) (layer F.SilkS))
    (fp_text value NOR-Extra (at 0 17.57) (layer F.Fab))
    (fp_text user %R (at 0 7.62 90) (layer F.Fab))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 /3A))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 /3B))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 /3Y))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 /4A))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 /4B))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 /4Y))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 69 /PH1))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x07_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x11_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 176.403 73.406)
    (descr "Through hole straight pin header, 1x11, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x11 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value ADDR_BUS (at 0 27.73) (layer F.Fab))
    (fp_text user %R (at 0 12.7 90) (layer F.Fab))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /A6))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /A5))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /A4))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /A3))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /A2))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /A1))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /A0))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /~SYNC))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 /~NMI))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x11_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm (layer F.Cu) (tedit 5D9F72B1)
    (at 164.089 95.123 180)
    (descr "SOIC, 20 Pin (JEDEC MS-013AC, https://www.analog.com/media/en/package-pcb-resources/package/233848rw_20.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference U5 (at 0 -7.35) (layer F.SilkS))
    (fp_text value 74HCT245 (at 0 7.35) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 20 smd roundrect (at 4.65 -5.715 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 19 smd roundrect (at 4.65 -4.445 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 41 /ROMG))
    (pad 18 smd roundrect (at 4.65 -3.175 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 71 "Net-(U5-Pad18)"))
    (pad 17 smd roundrect (at 4.65 -1.905 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 72 "Net-(U5-Pad17)"))
    (pad 16 smd roundrect (at 4.65 -0.635 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 /BA13))
    (pad 15 smd roundrect (at 4.65 0.635 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 /BA12))
    (pad 14 smd roundrect (at 4.65 1.905 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 63 /BA11))
    (pad 13 smd roundrect (at 4.65 3.175 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 62 /BA10))
    (pad 12 smd roundrect (at 4.65 4.445 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 60 /BA9))
    (pad 11 smd roundrect (at 4.65 5.715 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 61 /BA8))
    (pad 10 smd roundrect (at -4.65 5.715 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 9 smd roundrect (at -4.65 4.445 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 /A8))
    (pad 8 smd roundrect (at -4.65 3.175 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 /A9))
    (pad 7 smd roundrect (at -4.65 1.905 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 /A10))
    (pad 6 smd roundrect (at -4.65 0.635 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 /A11))
    (pad 5 smd roundrect (at -4.65 -0.635 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 /A12))
    (pad 4 smd roundrect (at -4.65 -1.905 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /A13))
    (pad 3 smd roundrect (at -4.65 -3.175 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 73 "Net-(U5-Pad3)"))
    (pad 2 smd roundrect (at -4.65 -4.445 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 74 "Net-(U5-Pad2)"))
    (pad 1 smd roundrect (at -4.65 -5.715 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 40 /ROMDIR))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-20W_7.5x12.8mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x11_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 179.959 102.616 90)
    (descr "Through hole straight pin header, 1x11, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x11 2.54mm single row")
    (fp_text reference J11 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value ADDR_BUS (at 0 27.73 90) (layer F.Fab))
    (fp_text user %R (at 0 12.7) (layer F.Fab))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /A15))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /A14))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /A13))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /A12))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /A11))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /A10))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /A9))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /A8))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /A7))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x11_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x11_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 179.959 69.596 90)
    (descr "Through hole straight pin header, 1x11, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x11 2.54mm single row")
    (fp_text reference J4 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value "Bus Signals" (at 0 27.73 90) (layer F.Fab))
    (fp_text user %R (at 0 12.7) (layer F.Fab))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 /PH0))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 /SOB))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 /PHI2O))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 /~RES))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 /VPB))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 /RDY))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 /PHI1O))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 /~IRQ))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 /MLB))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x11_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x11_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 208.915 98.806 180)
    (descr "Through hole straight pin header, 1x11, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x11 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value "Main Data" (at 0 27.73) (layer F.Fab))
    (fp_text user %R (at 0 12.7 90) (layer F.Fab))
    (pad 11 thru_hole oval (at 0 25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /RWB))
    (pad 10 thru_hole oval (at 0 22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /D0))
    (pad 9 thru_hole oval (at 0 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /D1))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 /D2))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /D3))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /D4))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /D5))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /D6))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /D7))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x11_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 143.764 66.294 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J12 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value ROMEN (at 0 4.87 90) (layer F.Fab))
    (fp_text user %R (at 0 1.27) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 /~RCMEN))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 158.5595 105.918)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 1K (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2439014634146341)
      (net 70 "Net-(D1-Pad2)"))
    (pad 1 smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2439014634146341)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_1206_3216Metric (layer F.Cu) (tedit 5F68FEF0)
    (at 158.6865 110.0455 90)
    (descr "Diode SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D1 (at -1.5875 -1.8415 90) (layer F.SilkS))
    (fp_text value PWR (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 70 "Net-(D1-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 1 GND))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm (layer F.Cu) (tedit 5D9F72B1)
    (at 164.089 77.343 180)
    (descr "SOIC, 20 Pin (JEDEC MS-013AC, https://www.analog.com/media/en/package-pcb-resources/package/233848rw_20.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference U4 (at 0 -7.35 180) (layer F.SilkS))
    (fp_text value 74HCT245 (at 0 7.35 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 20 smd roundrect (at 4.65 -5.715 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 19 smd roundrect (at 4.65 -4.445 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 41 /ROMG))
    (pad 18 smd roundrect (at 4.65 -3.175 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 59 /BA7))
    (pad 17 smd roundrect (at 4.65 -1.905 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 58 /BA6))
    (pad 16 smd roundrect (at 4.65 -0.635 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 56 /BA5))
    (pad 15 smd roundrect (at 4.65 0.635 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 57 /BA4))
    (pad 14 smd roundrect (at 4.65 1.905 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 55 /BA3))
    (pad 13 smd roundrect (at 4.65 3.175 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 54 /BA2))
    (pad 12 smd roundrect (at 4.65 4.445 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 52 /BA1))
    (pad 11 smd roundrect (at 4.65 5.715 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 53 /BA0))
    (pad 10 smd roundrect (at -4.65 5.715 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 9 smd roundrect (at -4.65 4.445 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /A0))
    (pad 8 smd roundrect (at -4.65 3.175 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 /A1))
    (pad 7 smd roundrect (at -4.65 1.905 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 /A2))
    (pad 6 smd roundrect (at -4.65 0.635 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 /A3))
    (pad 5 smd roundrect (at -4.65 -0.635 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 /A4))
    (pad 4 smd roundrect (at -4.65 -1.905 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 /A5))
    (pad 3 smd roundrect (at -4.65 -3.175 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 /A6))
    (pad 2 smd roundrect (at -4.65 -4.445 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 /A7))
    (pad 1 smd roundrect (at -4.65 -5.715 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 40 /ROMDIR))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-20W_7.5x12.8mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-14_3.9x8.7mm_P1.27mm (layer F.Cu) (tedit 5D9F72B1)
    (at 215.2015 82.169)
    (descr "SOIC, 14 Pin (JEDEC MS-012AB, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_14.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference U3 (at 2.8575 5.207 90) (layer F.SilkS))
    (fp_text value 74HCT02 (at 0 5.28) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 14 smd roundrect (at 2.475 -3.81) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 13 smd roundrect (at 2.475 -2.54) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 44 /4Y))
    (pad 12 smd roundrect (at 2.475 -1.27) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 45 /4B))
    (pad 11 smd roundrect (at 2.475 0) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 46 /4A))
    (pad 10 smd roundrect (at 2.475 1.27) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 /3Y))
    (pad 9 smd roundrect (at 2.475 2.54) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 48 /3B))
    (pad 8 smd roundrect (at 2.475 3.81) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 49 /3A))
    (pad 7 smd roundrect (at -2.475 3.81) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 6 smd roundrect (at -2.475 2.54) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 69 /PH1))
    (pad 5 smd roundrect (at -2.475 1.27) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 51 "Net-(JP2-Pad1)"))
    (pad 4 smd roundrect (at -2.475 0) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 42 /PH0_ALT))
    (pad 3 smd roundrect (at -2.475 -1.27) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at -2.475 -2.54) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 66 /~DMA))
    (pad 1 smd roundrect (at -2.475 -3.81) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 43 /DMA))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-14_3.9x8.7mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_QFP:PQFP-44_10x10mm_P0.8mm (layer F.Cu) (tedit 5A02F146)
    (at 192.659 86.106)
    (descr "44-Lead Plastic Quad Flatpack - 10x10x2.5mm Body (http://www.onsemi.com/pub/Collateral/122BK.PDF)")
    (tags "PQFP 0.8")
    (attr smd)
    (fp_text reference U2 (at 5.969 -5.461) (layer F.SilkS))
    (fp_text value w65c02s-QFP (at 0 7.8) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 44 smd rect (at -4 -6.05) (size 0.52 1.5) (layers F.Cu F.Paste F.Mask)
      (net 37 /MLB))
    (pad 43 smd rect (at -3.2 -6.05) (size 0.52 1.5) (layers F.Cu F.Paste F.Mask)
      (net 33 /~IRQ))
    (pad 42 smd rect (at -2.4 -6.05) (size 0.52 1.5) (layers F.Cu F.Paste F.Mask)
      (net 39 /PHI1O))
    (pad 41 smd rect (at -1.6 -6.05) (size 0.52 1.5) (layers F.Cu F.Paste F.Mask)
      (net 35 /RDY))
    (pad 40 smd rect (at -0.8 -6.05) (size 0.52 1.5) (layers F.Cu F.Paste F.Mask)
      (net 27 /VPB))
    (pad 39 smd rect (at 0 -6.05) (size 0.52 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 38 smd rect (at 0.8 -6.05) (size 0.52 1.5) (layers F.Cu F.Paste F.Mask)
      (net 32 /~RES))
    (pad 37 smd rect (at 1.6 -6.05) (size 0.52 1.5) (layers F.Cu F.Paste F.Mask)
      (net 38 /PHI2O))
    (pad 36 smd rect (at 2.4 -6.05) (size 0.52 1.5) (layers F.Cu F.Paste F.Mask)
      (net 36 /SOB))
    (pad 35 smd rect (at 3.2 -6.05) (size 0.52 1.5) (layers F.Cu F.Paste F.Mask)
      (net 31 /PH0))
    (pad 34 smd rect (at 4 -6.05) (size 0.52 1.5) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(JP1-Pad2)"))
    (pad 33 smd rect (at 6.05 -4) (size 1.5 0.52) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(U2-Pad33)"))
    (pad 32 smd rect (at 6.05 -3.2) (size 1.5 0.52) (layers F.Cu F.Paste F.Mask)
      (net 28 /RWB))
    (pad 31 smd rect (at 6.05 -2.4) (size 1.5 0.52) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 30 smd rect (at 6.05 -1.6) (size 1.5 0.52) (layers F.Cu F.Paste F.Mask)
      (net 26 /D0))
    (pad 29 smd rect (at 6.05 -0.8) (size 1.5 0.52) (layers F.Cu F.Paste F.Mask)
      (net 25 /D1))
    (pad 28 smd rect (at 6.05 0) (size 1.5 0.52) (layers F.Cu F.Paste F.Mask)
      (net 24 /D2))
    (pad 27 smd rect (at 6.05 0.8) (size 1.5 0.52) (layers F.Cu F.Paste F.Mask)
      (net 23 /D3))
    (pad 26 smd rect (at 6.05 1.6) (size 1.5 0.52) (layers F.Cu F.Paste F.Mask)
      (net 22 /D4))
    (pad 25 smd rect (at 6.05 2.4) (size 1.5 0.52) (layers F.Cu F.Paste F.Mask)
      (net 21 /D5))
    (pad 24 smd rect (at 6.05 3.2) (size 1.5 0.52) (layers F.Cu F.Paste F.Mask)
      (net 20 /D6))
    (pad 23 smd rect (at 6.05 4) (size 1.5 0.52) (layers F.Cu F.Paste F.Mask)
      (net 19 /D7))
    (pad 22 smd rect (at 4 6.05) (size 0.52 1.5) (layers F.Cu F.Paste F.Mask)
      (net 3 /A15))
    (pad 21 smd rect (at 3.2 6.05) (size 0.52 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 /A14))
    (pad 20 smd rect (at 2.4 6.05) (size 0.52 1.5) (layers F.Cu F.Paste F.Mask)
      (net 5 /A13))
    (pad 19 smd rect (at 1.6 6.05) (size 0.52 1.5) (layers F.Cu F.Paste F.Mask)
      (net 6 /A12))
    (pad 18 smd rect (at 0.8 6.05) (size 0.52 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 17 smd rect (at 0 6.05) (size 0.52 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 16 smd rect (at -0.8 6.05) (size 0.52 1.5) (layers F.Cu F.Paste F.Mask)
      (net 7 /A11))
    (pad 15 smd rect (at -1.6 6.05) (size 0.52 1.5) (layers F.Cu F.Paste F.Mask)
      (net 8 /A10))
    (pad 14 smd rect (at -2.4 6.05) (size 0.52 1.5) (layers F.Cu F.Paste F.Mask)
      (net 9 /A9))
    (pad 13 smd rect (at -3.2 6.05) (size 0.52 1.5) (layers F.Cu F.Paste F.Mask)
      (net 10 /A8))
    (pad 12 smd rect (at -4 6.05) (size 0.52 1.5) (layers F.Cu F.Paste F.Mask)
      (net 11 /A7))
    (pad 11 smd rect (at -6.05 4) (size 1.5 0.52) (layers F.Cu F.Paste F.Mask)
      (net 12 /A6))
    (pad 10 smd rect (at -6.05 3.2) (size 1.5 0.52) (layers F.Cu F.Paste F.Mask)
      (net 13 /A5))
    (pad 9 smd rect (at -6.05 2.4) (size 1.5 0.52) (layers F.Cu F.Paste F.Mask)
      (net 14 /A4))
    (pad 8 smd rect (at -6.05 1.6) (size 1.5 0.52) (layers F.Cu F.Paste F.Mask)
      (net 15 /A3))
    (pad 7 smd rect (at -6.05 0.8) (size 1.5 0.52) (layers F.Cu F.Paste F.Mask)
      (net 16 /A2))
    (pad 6 smd rect (at -6.05 0) (size 1.5 0.52) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(U2-Pad6)"))
    (pad 5 smd rect (at -6.05 -0.8) (size 1.5 0.52) (layers F.Cu F.Paste F.Mask)
      (net 17 /A1))
    (pad 4 smd rect (at -6.05 -1.6) (size 1.5 0.52) (layers F.Cu F.Paste F.Mask)
      (net 18 /A0))
    (pad 3 smd rect (at -6.05 -2.4) (size 1.5 0.52) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at -6.05 -3.2) (size 1.5 0.52) (layers F.Cu F.Paste F.Mask)
      (net 29 /~SYNC))
    (pad 1 smd rect (at -6.05 -4) (size 1.5 0.52) (layers F.Cu F.Paste F.Mask)
      (net 34 /~NMI))
    (model ${KISYS3DMOD}/Package_QFP.3dshapes/PQFP-44_10x10mm_P0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-28_W15.24mm_Socket_LongPads locked (layer F.Cu) (tedit 5A02E8C5)
    (at 152.654 102.997 180)
    (descr "28-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils), Socket, LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 15.24mm 600mil Socket LongPads")
    (fp_text reference U1 (at 7.62 -2.33) (layer F.SilkS))
    (fp_text value 27C512 (at 7.62 35.35) (layer F.Fab))
    (fp_text user %R (at 7.62 16.51) (layer F.Fab))
    (pad 28 thru_hole oval (at 15.24 0 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 14 thru_hole oval (at 0 33.02 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 27 thru_hole oval (at 15.24 2.54 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 13 thru_hole oval (at 0 30.48 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 /D2))
    (pad 26 thru_hole oval (at 15.24 5.08 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 64 /BA13))
    (pad 12 thru_hole oval (at 0 27.94 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 /D1))
    (pad 25 thru_hole oval (at 15.24 7.62 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 61 /BA8))
    (pad 11 thru_hole oval (at 0 25.4 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 /D0))
    (pad 24 thru_hole oval (at 15.24 10.16 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 60 /BA9))
    (pad 10 thru_hole oval (at 0 22.86 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 /BA0))
    (pad 23 thru_hole oval (at 15.24 12.7 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 63 /BA11))
    (pad 9 thru_hole oval (at 0 20.32 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 52 /BA1))
    (pad 22 thru_hole oval (at 15.24 15.24 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 /~RCMEN))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 /BA2))
    (pad 21 thru_hole oval (at 15.24 17.78 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 62 /BA10))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 55 /BA3))
    (pad 20 thru_hole oval (at 15.24 20.32 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 57 /BA4))
    (pad 19 thru_hole oval (at 15.24 22.86 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 /D7))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 56 /BA5))
    (pad 18 thru_hole oval (at 15.24 25.4 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 /D6))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 58 /BA6))
    (pad 17 thru_hole oval (at 15.24 27.94 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 /D5))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 59 /BA7))
    (pad 16 thru_hole oval (at 15.24 30.48 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 /D4))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 65 /BA12))
    (pad 15 thru_hole oval (at 15.24 33.02 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 /D3))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-28_W15.24mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 213.106 75.3745)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference RNP1 (at -2.159 0.0635 90) (layer F.SilkS))
    (fp_text value 3k3 (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2439014634146341)
      (net 66 /~DMA))
    (pad 1 smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2439014634146341)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_Array_Convex_4x0612 (layer F.Cu) (tedit 5B82E1AD)
    (at 164.0855 97.1995)
    (descr "Precision Thin Film Chip Resistor Array, VISHAY (see http://www.vishay.com/docs/28770/acasat.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN4 (at 0 -2.3305 180) (layer F.SilkS))
    (fp_text value 0 (at 0 2.8 180) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.7 -1.27) (size 0.7 0.64) (layers F.Cu F.Paste F.Mask)
      (net 65 /BA12))
    (pad 3 smd rect (at -0.7 0.4) (size 0.7 0.5) (layers F.Cu F.Paste F.Mask)
      (net 75 "Net-(RN4-Pad3)"))
    (pad 2 smd rect (at -0.7 -0.4) (size 0.7 0.5) (layers F.Cu F.Paste F.Mask)
      (net 64 /BA13))
    (pad 4 smd rect (at -0.7 1.27) (size 0.7 0.64) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(RN4-Pad4)"))
    (pad 7 smd rect (at 0.7 -0.4) (size 0.7 0.5) (layers F.Cu F.Paste F.Mask)
      (net 5 /A13))
    (pad 8 smd rect (at 0.7 -1.27) (size 0.7 0.64) (layers F.Cu F.Paste F.Mask)
      (net 6 /A12))
    (pad 6 smd rect (at 0.7 0.4) (size 0.7 0.5) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(RN4-Pad6)"))
    (pad 5 smd rect (at 0.7 1.27) (size 0.7 0.64) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(RN4-Pad5)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Convex_4x0612.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_Array_Convex_4x0612 (layer F.Cu) (tedit 5B82E1AD)
    (at 164.0205 91.821)
    (descr "Precision Thin Film Chip Resistor Array, VISHAY (see http://www.vishay.com/docs/28770/acasat.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN3 (at -0.0635 -2.413 180) (layer F.SilkS))
    (fp_text value 0 (at 0 2.8 180) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.7 -1.27) (size 0.7 0.64) (layers F.Cu F.Paste F.Mask)
      (net 61 /BA8))
    (pad 3 smd rect (at -0.7 0.4) (size 0.7 0.5) (layers F.Cu F.Paste F.Mask)
      (net 62 /BA10))
    (pad 2 smd rect (at -0.7 -0.4) (size 0.7 0.5) (layers F.Cu F.Paste F.Mask)
      (net 60 /BA9))
    (pad 4 smd rect (at -0.7 1.27) (size 0.7 0.64) (layers F.Cu F.Paste F.Mask)
      (net 63 /BA11))
    (pad 7 smd rect (at 0.7 -0.4) (size 0.7 0.5) (layers F.Cu F.Paste F.Mask)
      (net 9 /A9))
    (pad 8 smd rect (at 0.7 -1.27) (size 0.7 0.64) (layers F.Cu F.Paste F.Mask)
      (net 10 /A8))
    (pad 6 smd rect (at 0.7 0.4) (size 0.7 0.5) (layers F.Cu F.Paste F.Mask)
      (net 8 /A10))
    (pad 5 smd rect (at 0.7 1.27) (size 0.7 0.64) (layers F.Cu F.Paste F.Mask)
      (net 7 /A11))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Convex_4x0612.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_Array_Convex_4x0612 (layer F.Cu) (tedit 5B82E1AD)
    (at 164.1475 80.264)
    (descr "Precision Thin Film Chip Resistor Array, VISHAY (see http://www.vishay.com/docs/28770/acasat.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN2 (at 0 -2.413 180) (layer F.SilkS))
    (fp_text value 0 (at 0 2.8 180) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.7 -1.27) (size 0.7 0.64) (layers F.Cu F.Paste F.Mask)
      (net 57 /BA4))
    (pad 3 smd rect (at -0.7 0.4) (size 0.7 0.5) (layers F.Cu F.Paste F.Mask)
      (net 58 /BA6))
    (pad 2 smd rect (at -0.7 -0.4) (size 0.7 0.5) (layers F.Cu F.Paste F.Mask)
      (net 56 /BA5))
    (pad 4 smd rect (at -0.7 1.27) (size 0.7 0.64) (layers F.Cu F.Paste F.Mask)
      (net 59 /BA7))
    (pad 7 smd rect (at 0.7 -0.4) (size 0.7 0.5) (layers F.Cu F.Paste F.Mask)
      (net 13 /A5))
    (pad 8 smd rect (at 0.7 -1.27) (size 0.7 0.64) (layers F.Cu F.Paste F.Mask)
      (net 14 /A4))
    (pad 6 smd rect (at 0.7 0.4) (size 0.7 0.5) (layers F.Cu F.Paste F.Mask)
      (net 12 /A6))
    (pad 5 smd rect (at 0.7 1.27) (size 0.7 0.64) (layers F.Cu F.Paste F.Mask)
      (net 11 /A7))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Convex_4x0612.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_Array_Convex_4x0612 (layer F.Cu) (tedit 5B82E1AD)
    (at 164.0825 73.9775)
    (descr "Precision Thin Film Chip Resistor Array, VISHAY (see http://www.vishay.com/docs/28770/acasat.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN1 (at 0.0015 -2.3495 180) (layer F.SilkS))
    (fp_text value 0 (at 0 2.8 180) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.7 -1.27) (size 0.7 0.64) (layers F.Cu F.Paste F.Mask)
      (net 53 /BA0))
    (pad 3 smd rect (at -0.7 0.4) (size 0.7 0.5) (layers F.Cu F.Paste F.Mask)
      (net 54 /BA2))
    (pad 2 smd rect (at -0.7 -0.4) (size 0.7 0.5) (layers F.Cu F.Paste F.Mask)
      (net 52 /BA1))
    (pad 4 smd rect (at -0.7 1.27) (size 0.7 0.64) (layers F.Cu F.Paste F.Mask)
      (net 55 /BA3))
    (pad 7 smd rect (at 0.7 -0.4) (size 0.7 0.5) (layers F.Cu F.Paste F.Mask)
      (net 17 /A1))
    (pad 8 smd rect (at 0.7 -1.27) (size 0.7 0.64) (layers F.Cu F.Paste F.Mask)
      (net 18 /A0))
    (pad 6 smd rect (at 0.7 0.4) (size 0.7 0.5) (layers F.Cu F.Paste F.Mask)
      (net 16 /A2))
    (pad 5 smd rect (at 0.7 1.27) (size 0.7 0.64) (layers F.Cu F.Paste F.Mask)
      (net 15 /A3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Convex_4x0612.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 187.833 77.851)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at 0 1.65) (layer B.SilkS))
    (fp_text value 3k3 (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2439014634146341)
      (net 33 /~IRQ))
    (pad 1 smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2439014634146341)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 184.277 80.645 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at 0 1.65 90) (layer B.SilkS))
    (fp_text value 3k3 (at 0 -1.65 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2439014634146341)
      (net 34 /~NMI))
    (pad 1 smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2439014634146341)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 192.405 77.851 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 0 1.65) (layer B.SilkS))
    (fp_text value 3k3 (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2439014634146341)
      (net 35 /RDY))
    (pad 1 smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2439014634146341)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm locked (layer F.Cu) (tedit 5B391E66)
    (at 216.7255 72.898)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP3 (at 0 -1.8) (layer F.SilkS) hide)
    (fp_text value X4 (at 0.0635 -1.524) (layer F.SilkS))
    (pad 2 smd custom (at 0.65 0) (size 1 0.5) (layers F.Cu F.Mask)
      (net 1 GND) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy -0.5 -0.75) (xy -0.5 0.75) (xy 0 0.75)) (width 0))
      ))
    (pad 1 smd custom (at -0.65 0) (size 1 0.5) (layers F.Cu F.Mask)
      (net 51 "Net-(JP2-Pad1)") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy 0.5 -0.75) (xy 0.5 0.75) (xy 0 0.75)) (width 0))
      ))
  )
  (module Jumper:SolderJumper-2_P1.3mm_Bridged_Pad1.0x1.5mm locked (layer F.Cu) (tedit 5C756AB2)
    (at 213.106 72.898 180)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, bridged with 1 copper strip")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP2 (at 0 1.651) (layer F.SilkS) hide)
    (fp_text value X5 (at -0.127 1.524) (layer F.SilkS))
    (pad 2 smd rect (at 0.65 0 180) (size 1 1.5) (layers F.Cu F.Mask)
      (net 43 /DMA))
    (pad 1 smd rect (at -0.65 0 180) (size 1 1.5) (layers F.Cu F.Mask)
      (net 51 "Net-(JP2-Pad1)"))
  )
  (module Jumper:SolderJumper-2_P1.3mm_Bridged_Pad1.0x1.5mm (layer B.Cu) (tedit 5C756AB2)
    (at 198.247 77.851 180)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, bridged with 1 copper strip")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP1 (at 0 1.8) (layer B.SilkS) hide)
    (fp_text value BE_VDD (at 0.254 1.778) (layer B.SilkS))
    (pad 2 smd rect (at 0.65 0 180) (size 1 1.5) (layers B.Cu B.Mask)
      (net 50 "Net-(JP1-Pad2)"))
    (pad 1 smd rect (at -0.65 0 180) (size 1 1.5) (layers B.Cu B.Mask)
      (net 2 +5V))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 212.344 69.596 270)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J9 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value CLK_ALT (at 0 4.87 90) (layer F.Fab))
    (fp_text user %R (at 0 1.27) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 /PH0_ALT))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 /DMA))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 161.9885 68.326 270)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J8 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value ROMG_SEL (at 0 7.41 90) (layer F.Fab))
    (fp_text user %R (at 0 2.54) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 /ROMG))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 171.2595 68.326 270)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J7 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value ROMDIR_SEL (at 0 7.41 90) (layer F.Fab))
    (fp_text user %R (at 0 2.54) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 /ROMDIR))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x05_P2.54mm_Vertical locked (layer F.Cu) (tedit 59FED5CC)
    (at 163.3855 110.871 90)
    (descr "Through hole straight pin header, 2x05, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x05 2.54mm double row")
    (fp_text reference J6 (at 1.27 -2.33 90) (layer F.SilkS) hide)
    (fp_text value Data (at 1.143 13.1445 90) (layer F.SilkS))
    (fp_text user %R (at 1.27 5.08) (layer F.Fab))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /D7))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /D6))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /D4))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /D5))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /D3))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 /D2))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /D1))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /D0))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x10_P2.54mm_Vertical locked (layer F.Cu) (tedit 59FED5CC)
    (at 193.1035 110.9345 90)
    (descr "Through hole straight pin header, 2x10, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x10 2.54mm double row")
    (fp_text reference J5 (at 1.27 -2.33 90) (layer F.SilkS) hide)
    (fp_text value Address (at 1.0795 -2.8575 90) (layer F.SilkS))
    (fp_text user %R (at 1.27 11.43) (layer F.Fab))
    (pad 20 thru_hole oval (at 2.54 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /A15))
    (pad 19 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /A14))
    (pad 18 thru_hole oval (at 2.54 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /A13))
    (pad 17 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /A12))
    (pad 16 thru_hole oval (at 2.54 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /A11))
    (pad 15 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 14 thru_hole oval (at 2.54 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /A9))
    (pad 13 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /A10))
    (pad 12 thru_hole oval (at 2.54 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 11 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /A8))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /A7))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /A6))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /A5))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /A3))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /A4))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /A2))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /A1))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /A0))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x10_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 216.789 75.3745 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C7 (at -2.413 -0.0635 90) (layer F.SilkS))
    (fp_text value 1u (at 0 1.68 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.95 0 180) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.95 0 180) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 184.277 85.217 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C6 (at 0 1.68 270) (layer B.SilkS))
    (fp_text value 1u (at 0 -1.68 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.95 0 270) (size 1 1.45) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.95 0 270) (size 1 1.45) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 153.289 105.918)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C5 (at 1.7272 -1.5494 180) (layer B.SilkS))
    (fp_text value 1u (at 0 -1.68) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.95 0) (size 1 1.45) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.95 0) (size 1 1.45) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 164.084 85.09)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at 0 1.68) (layer B.SilkS))
    (fp_text value 1u (at 0 -1.68) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.95 0) (size 1 1.45) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.95 0) (size 1 1.45) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 200.787 85.217 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at 0 1.68 270) (layer B.SilkS))
    (fp_text value 10uF (at 0 -1.68 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.95 0 270) (size 1 1.45) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.95 0 270) (size 1 1.45) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Radial_D6.3mm_H5.0mm_P2.50mm (layer F.Cu) (tedit 5BC5C9B9)
    (at 152.273 108.839)
    (descr "C, Radial series, Radial, pin pitch=2.50mm, diameter=6.3mm, height=5mm, Non-Polar Electrolytic Capacitor")
    (tags "C Radial series Radial pin pitch 2.50mm diameter 6.3mm height 5mm Non-Polar Electrolytic Capacitor")
    (fp_text reference C2 (at -1.016 3.81) (layer F.SilkS))
    (fp_text value 10uF (at 1.25 4.4) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Radial_D6.3mm_H5.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 163.449 101.219)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 0 1.68) (layer B.SilkS))
    (fp_text value 1u (at 0 -1.68) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.95 0) (size 1 1.45) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.95 0) (size 1 1.45) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Thanks Chat!\nYou Look Great Today!" (at 221.234 85.09 -90) (layer B.SilkS))
  (gr_text "GD 65c02\n@baldengineer\nrev1" (at 142.727562 79.9084 90) (layer B.SilkS))
  (gr_text 5V (at 147.447 112.4712 180) (layer B.SilkS))
  (gr_text 5V (at 144.907 112.4712 180) (layer B.SilkS))
  (gr_text A3 (at 155.448 87.884 270) (layer B.SilkS))
  (gr_text A1 (at 155.448 82.677 270) (layer B.SilkS))
  (gr_text A5 (at 155.448 92.837 270) (layer B.SilkS))
  (gr_text A12 (at 155.448 100.457 270) (layer B.SilkS))
  (gr_text D0 (at 155.448 77.724 270) (layer B.SilkS))
  (gr_text A0 (at 155.448 80.264 270) (layer B.SilkS))
  (gr_text D2 (at 155.448 72.771 270) (layer B.SilkS))
  (gr_text A7 (at 155.448 97.917 270) (layer B.SilkS))
  (gr_text A4 (at 155.448 90.297 270) (layer B.SilkS))
  (gr_text D1 (at 155.448 75.184 270) (layer B.SilkS))
  (gr_text A2 (at 155.448 85.217 270) (layer B.SilkS))
  (gr_text A6 (at 155.448 95.377 270) (layer B.SilkS))
  (gr_text A0 (at 173.729667 81.153) (layer B.SilkS))
  (gr_text A4 (at 173.729667 93.98) (layer B.SilkS))
  (gr_text ~SYNC (at 172.91062 76.073) (layer B.SilkS))
  (gr_text A1 (at 173.729667 83.947) (layer B.SilkS))
  (gr_text "A5\n" (at 173.729667 96.52) (layer B.SilkS))
  (gr_text ~NMI (at 173.38681 73.787) (layer B.SilkS))
  (gr_text A6 (at 173.729667 99.187) (layer B.SilkS))
  (gr_text A2 (at 173.729667 86.36) (layer B.SilkS))
  (gr_text "5V\n" (at 173.729667 78.613) (layer B.SilkS))
  (gr_text A3 (at 173.729667 88.9) (layer B.SilkS))
  (gr_text ~SYNC (at 179.946096 76.073) (layer B.SilkS))
  (gr_text A4 (at 179.127048 93.98) (layer B.SilkS))
  (gr_text A1 (at 179.127048 83.947) (layer B.SilkS))
  (gr_text A0 (at 179.127048 81.153) (layer B.SilkS))
  (gr_text "A5\n" (at 179.127048 96.52) (layer B.SilkS))
  (gr_text "5V\n" (at 179.127048 78.613) (layer B.SilkS))
  (gr_text ~NMI (at 179.469905 73.787) (layer B.SilkS))
  (gr_text A3 (at 179.127048 88.9) (layer B.SilkS))
  (gr_text A6 (at 179.127048 99.187) (layer B.SilkS))
  (gr_text A2 (at 179.127048 86.36) (layer B.SilkS))
  (gr_text 5V (at 156.845 66.294) (layer B.SilkS))
  (gr_text ~G (at 159.385 66.294) (layer B.SilkS))
  (gr_text DIR (at 168.656 66.294) (layer B.SilkS))
  (gr_text 5V (at 165.989 66.294) (layer B.SilkS))
  (gr_text ~ROMEN (at 141.224 65.659 270) (layer B.SilkS))
  (gr_text D3 (at 134.747 69.977 90) (layer B.SilkS))
  (gr_text D5 (at 134.747 75.184 90) (layer B.SilkS))
  (gr_text D6 (at 134.747 77.724 90) (layer B.SilkS))
  (gr_text D7 (at 134.747 80.264 90) (layer B.SilkS))
  (gr_text D4 (at 134.747 72.517 90) (layer B.SilkS))
  (gr_text A9 (at 134.62 92.964 90) (layer B.SilkS))
  (gr_text A11 (at 134.62 90.297 90) (layer B.SilkS))
  (gr_text A10 (at 134.62 85.344 90) (layer B.SilkS))
  (gr_text A13 (at 134.62 98.171 90) (layer B.SilkS))
  (gr_text "A9\n" (at 134.62 95.504 90) (layer B.SilkS))
  (gr_text ~EN (at 134.62 87.757 90) (layer B.SilkS))
  (gr_text D1 (at 163.322 106.299) (layer B.SilkS))
  (gr_text D7 (at 173.609 106.299) (layer B.SilkS))
  (gr_text D5 (at 168.402 106.299) (layer B.SilkS))
  (gr_text D3 (at 165.989 106.299) (layer B.SilkS))
  (gr_text D0 (at 163.449 113.03 180) (layer B.SilkS))
  (gr_text D6 (at 173.609 113.03 180) (layer B.SilkS))
  (gr_text D4 (at 171.196 113.03 180) (layer B.SilkS))
  (gr_text D2 (at 165.989 113.03 180) (layer B.SilkS))
  (gr_text Address (at 190.246 109.728 -90) (layer B.SilkS))
  (gr_text Data (at 176.657 109.601 270) (layer B.SilkS))
  (gr_text PH1 (at 216.248 89.2175) (layer B.SilkS))
  (gr_text 4A (at 215.7095 96.7105 270) (layer B.SilkS))
  (gr_text 3B (at 215.7095 101.7905 270) (layer B.SilkS))
  (gr_text 3A (at 215.7095 104.4575 270) (layer B.SilkS))
  (gr_text 3Y (at 215.7095 99.2505 270) (layer B.SilkS))
  (gr_text 4B (at 215.7095 94.1705 270) (layer B.SilkS))
  (gr_text 4Y (at 215.7095 91.694 270) (layer B.SilkS))
  (gr_text A10 (at 208.407 113.157 180) (layer B.SilkS))
  (gr_text A0 (at 193.04 113.157 180) (layer B.SilkS))
  (gr_text A14 (at 216.154 113.157 180) (layer B.SilkS))
  (gr_text A12 (at 213.36 113.157 180) (layer B.SilkS))
  (gr_text A4 (at 198.12 113.157 180) (layer B.SilkS))
  (gr_text A8 (at 205.74 113.157 180) (layer B.SilkS))
  (gr_text A2 (at 195.58 113.157 180) (layer B.SilkS))
  (gr_text A6 (at 203.2 113.157 180) (layer B.SilkS))
  (gr_text A3 (at 198.12 106.426) (layer B.SilkS))
  (gr_text A11 (at 210.82 106.426) (layer B.SilkS))
  (gr_text A9 (at 208.28 106.426) (layer B.SilkS))
  (gr_text A7 (at 203.2 106.426) (layer B.SilkS))
  (gr_text A5 (at 200.533 106.426) (layer B.SilkS))
  (gr_text A1 (at 193.04 106.426) (layer B.SilkS))
  (gr_text A15 (at 216.027 106.426) (layer B.SilkS))
  (gr_text A13 (at 213.233 106.426) (layer B.SilkS))
  (gr_text A14 (at 202.692 104.775) (layer B.SilkS))
  (gr_text A15 (at 205.486 104.775) (layer B.SilkS))
  (gr_text A13 (at 200.152 104.775) (layer B.SilkS))
  (gr_text A10 (at 189.611 104.775) (layer B.SilkS))
  (gr_text A9 (at 184.785 104.775) (layer B.SilkS))
  (gr_text A7 (at 179.705 104.775) (layer B.SilkS))
  (gr_text A11 (at 192.405 104.775) (layer B.SilkS))
  (gr_text A12 (at 195.199 104.775) (layer B.SilkS))
  (gr_text A8 (at 182.372 104.775) (layer B.SilkS))
  (gr_text A14 (at 202.692 104.648 180) (layer F.SilkS))
  (gr_text A15 (at 205.486 104.648 180) (layer F.SilkS))
  (gr_text A13 (at 200.152 104.648 180) (layer F.SilkS))
  (gr_text A10 (at 189.611 104.648 180) (layer F.SilkS))
  (gr_text A9 (at 184.785 104.648 180) (layer F.SilkS))
  (gr_text A7 (at 179.705 104.648 180) (layer F.SilkS))
  (gr_text A11 (at 192.405 104.648 180) (layer F.SilkS))
  (gr_text A12 (at 195.199 104.648 180) (layer F.SilkS))
  (gr_text A8 (at 182.372 104.648 180) (layer F.SilkS))
  (gr_text A14 (at 202.946 100.33) (layer B.SilkS))
  (gr_text A15 (at 205.74 100.33) (layer B.SilkS))
  (gr_text A13 (at 200.406 100.33) (layer B.SilkS))
  (gr_text A10 (at 189.865 100.33) (layer B.SilkS))
  (gr_text A9 (at 185.039 100.33) (layer B.SilkS))
  (gr_text A7 (at 179.959 100.33) (layer B.SilkS))
  (gr_text A11 (at 192.659 100.33) (layer B.SilkS))
  (gr_text A12 (at 195.453 100.33) (layer B.SilkS))
  (gr_text A8 (at 182.626 100.33) (layer B.SilkS))
  (gr_text D1 (at 206.34319 78.5495) (layer B.SilkS))
  (gr_text RWB (at 205.867 73.5965) (layer B.SilkS))
  (gr_text D2 (at 206.34319 83.566) (layer B.SilkS))
  (gr_text D0 (at 206.34319 76.0095) (layer B.SilkS))
  (gr_text D3 (at 206.34319 86.1695) (layer B.SilkS))
  (gr_text D5 (at 206.34319 93.7895) (layer B.SilkS))
  (gr_text D6 (at 206.34319 96.266) (layer B.SilkS))
  (gr_text D7 (at 206.34319 98.806) (layer B.SilkS))
  (gr_text D4 (at 206.34319 88.5825) (layer B.SilkS))
  (gr_text SOB (at 203.0095 72.50438 270) (layer B.SilkS))
  (gr_text PHI10 (at 185.166 73.075808 270) (layer B.SilkS))
  (gr_text RDY (at 190.246 72.447237 270) (layer B.SilkS))
  (gr_text ~RES (at 195.3895 72.447237 270) (layer B.SilkS))
  (gr_text ~IRQ (at 182.626 72.313904 270) (layer B.SilkS))
  (gr_text VPB (at 192.786 72.447237 270) (layer B.SilkS))
  (gr_text PHI2O (at 200.3425 73.113904 270) (layer B.SilkS))
  (gr_text RDY (at 189.992 66.465523 270) (layer B.SilkS))
  (gr_text VPB (at 192.532 66.465523 270) (layer B.SilkS))
  (gr_text PHI2O (at 200.0885 65.798856 270) (layer B.SilkS))
  (gr_text PH0 (at 205.232 66.40838 270) (layer B.SilkS))
  (gr_text ~RES (at 195.1355 66.465523 270) (layer B.SilkS))
  (gr_text DMA (at 212.5345 66.40838 270) (layer B.SilkS))
  (gr_text SOB (at 202.7555 66.40838 270) (layer B.SilkS))
  (gr_text ~IRQ (at 182.372 66.598856 270) (layer B.SilkS))
  (gr_text MLB (at 179.705 66.427427 270) (layer B.SilkS))
  (gr_text PH0_ALT (at 209.7405 65.132189 270) (layer B.SilkS))
  (gr_text PHI10 (at 184.912 65.836951 270) (layer B.SilkS))
  (gr_text A13 (at 166.37 96.901) (layer F.SilkS))
  (gr_text A12 (at 166.37 95.885) (layer F.SilkS))
  (gr_text A13 (at 161.798 97.028) (layer F.SilkS))
  (gr_text A12 (at 161.798 95.885) (layer F.SilkS))
  (gr_text A9 (at 166.243 91.44) (layer F.SilkS))
  (gr_text A11 (at 166.243 93.218) (layer F.SilkS))
  (gr_text A11 (at 161.925 93.091) (layer F.SilkS))
  (gr_text A8 (at 161.925 90.551) (layer F.SilkS))
  (gr_text A7 (at 166.243 81.534) (layer F.SilkS))
  (gr_text A5 (at 166.243 79.883) (layer F.SilkS))
  (gr_text A6 (at 162.052 80.772) (layer F.SilkS))
  (gr_text A4 (at 162.052 78.994) (layer F.SilkS))
  (gr_text A3 (at 166.243 75.311) (layer F.SilkS))
  (gr_text A2 (at 161.925 74.422) (layer F.SilkS))
  (gr_text A1 (at 166.243 73.66) (layer F.SilkS))
  (gr_text A0 (at 161.925 72.771) (layer F.SilkS))
  (gr_text A12 (at 155.448 100.33 90) (layer F.SilkS))
  (gr_text A7 (at 155.448 97.79 90) (layer F.SilkS))
  (gr_text A6 (at 155.448 95.25 90) (layer F.SilkS))
  (gr_text A5 (at 155.448 92.71 90) (layer F.SilkS))
  (gr_text A4 (at 155.448 90.17 90) (layer F.SilkS))
  (gr_text A3 (at 155.448 87.757 90) (layer F.SilkS))
  (gr_text A2 (at 155.448 85.09 90) (layer F.SilkS))
  (gr_text A1 (at 155.448 82.55 90) (layer F.SilkS))
  (gr_text A0 (at 155.448 80.137 90) (layer F.SilkS))
  (gr_text D0 (at 155.448 77.597 90) (layer F.SilkS))
  (gr_text D1 (at 155.448 75.057 90) (layer F.SilkS))
  (gr_text D2 (at 155.448 72.644 90) (layer F.SilkS))
  (gr_text A13 (at 134.62 98.171 -90) (layer F.SilkS))
  (gr_text "A9\n" (at 134.62 95.504 -90) (layer F.SilkS))
  (gr_text A9 (at 134.62 92.964 -90) (layer F.SilkS))
  (gr_text A11 (at 134.62 90.297 -90) (layer F.SilkS))
  (gr_text D3 (at 134.62 69.977 -90) (layer F.SilkS))
  (gr_text D4 (at 134.62 72.517 -90) (layer F.SilkS))
  (gr_text D5 (at 134.62 75.184 -90) (layer F.SilkS))
  (gr_text D6 (at 134.62 77.724 -90) (layer F.SilkS))
  (gr_text D7 (at 134.62 80.264 -90) (layer F.SilkS))
  (gr_text A10 (at 134.62 85.344 -90) (layer F.SilkS))
  (gr_text ~EN (at 134.62 87.757 270) (layer F.SilkS))
  (gr_text RDY (at 190.246 72.472477 -90) (layer F.SilkS))
  (gr_text VPB (at 192.786 72.472477 -90) (layer F.SilkS))
  (gr_text PHI2O (at 200.3425 73.139144 -90) (layer F.SilkS))
  (gr_text ~RES (at 195.3895 72.472477 -90) (layer F.SilkS))
  (gr_text SOB (at 203.0095 72.52962 -90) (layer F.SilkS))
  (gr_text ~IRQ (at 182.626 72.339144 270) (layer F.SilkS))
  (gr_text PHI10 (at 185.166 73.101048 -90) (layer F.SilkS))
  (gr_text ~SYNC (at 172.847 76.073) (layer F.SilkS))
  (gr_text A4 (at 173.666047 93.98) (layer F.SilkS))
  (gr_text A1 (at 173.666047 83.947) (layer F.SilkS))
  (gr_text A0 (at 173.666047 81.153) (layer F.SilkS))
  (gr_text "A5\n" (at 173.666047 96.52) (layer F.SilkS))
  (gr_text "5V\n" (at 173.666047 78.613) (layer F.SilkS))
  (gr_text ~NMI (at 173.32319 73.787) (layer F.SilkS))
  (gr_text A3 (at 173.666047 88.9) (layer F.SilkS))
  (gr_text A6 (at 173.666047 99.187) (layer F.SilkS))
  (gr_text A2 (at 173.666047 86.36) (layer F.SilkS))
  (gr_text ~NMI (at 179.482809 73.787) (layer F.SilkS))
  (gr_text ~SYNC (at 179.959 76.073) (layer F.SilkS))
  (gr_text "5V\n" (at 179.139952 78.613) (layer F.SilkS))
  (gr_text A0 (at 179.139952 81.153) (layer F.SilkS))
  (gr_text A1 (at 179.139952 83.947) (layer F.SilkS))
  (gr_text A2 (at 179.139952 86.36) (layer F.SilkS))
  (gr_text A3 (at 179.139952 88.9) (layer F.SilkS))
  (gr_text A4 (at 179.139952 93.98) (layer F.SilkS))
  (gr_text "A5\n" (at 179.139952 96.52) (layer F.SilkS))
  (gr_text A6 (at 179.139952 99.187) (layer F.SilkS))
  (gr_text A7 (at 179.959 100.33 180) (layer F.SilkS))
  (gr_text A8 (at 182.626 100.33 180) (layer F.SilkS))
  (gr_text A9 (at 185.039 100.33 180) (layer F.SilkS))
  (gr_text A10 (at 189.865 100.33 180) (layer F.SilkS))
  (gr_text A11 (at 192.659 100.33 180) (layer F.SilkS))
  (gr_text A12 (at 195.453 100.33 180) (layer F.SilkS))
  (gr_text A13 (at 200.406 100.33 180) (layer F.SilkS))
  (gr_text A14 (at 202.946 100.33 180) (layer F.SilkS))
  (gr_text A15 (at 205.74 100.33 180) (layer F.SilkS))
  (gr_text PH0_ALT (at 209.7405 65.157429 -90) (layer F.SilkS))
  (gr_text DMA (at 212.5345 66.43362 -90) (layer F.SilkS))
  (gr_text GND (at 219.075 72.771 90) (layer F.SilkS))
  (gr_text PH1 (at 216.498 89.0905) (layer F.SilkS))
  (gr_text 3A (at 215.8365 104.3305 90) (layer F.SilkS))
  (gr_text 3B (at 215.779357 101.6635 90) (layer F.SilkS))
  (gr_text 3Y (at 215.8365 99.1235 90) (layer F.SilkS))
  (gr_text 4A (at 215.8365 96.5835 90) (layer F.SilkS))
  (gr_text 4B (at 215.779357 94.0435 90) (layer F.SilkS))
  (gr_text 4Y (at 215.8365 91.567 90) (layer F.SilkS))
  (gr_text D7 (at 206.34319 98.806) (layer F.SilkS))
  (gr_text D6 (at 206.34319 96.266) (layer F.SilkS))
  (gr_text D5 (at 206.34319 93.7895) (layer F.SilkS))
  (gr_text D4 (at 206.34319 88.5825) (layer F.SilkS))
  (gr_text D3 (at 206.34319 86.1695) (layer F.SilkS))
  (gr_text D2 (at 206.34319 83.566) (layer F.SilkS))
  (gr_text D1 (at 206.34319 78.5495) (layer F.SilkS))
  (gr_text D0 (at 206.34319 76.0095) (layer F.SilkS))
  (gr_text RWB (at 205.867 73.5965) (layer F.SilkS))
  (gr_text PH0 (at 205.232 66.43362 -90) (layer F.SilkS))
  (gr_text SOB (at 202.7555 66.43362 -90) (layer F.SilkS))
  (gr_text PHI2O (at 200.0885 65.824096 -90) (layer F.SilkS))
  (gr_text ~RES (at 195.1355 66.490763 -90) (layer F.SilkS))
  (gr_text VPB (at 192.532 66.490763 -90) (layer F.SilkS))
  (gr_text RDY (at 189.992 66.490763 -90) (layer F.SilkS))
  (gr_text PHI10 (at 184.912 65.862191 -90) (layer F.SilkS))
  (gr_text ~IRQ (at 182.372 66.624096 270) (layer F.SilkS))
  (gr_text MLB (at 179.705 66.452667 270) (layer F.SilkS))
  (gr_text DIR (at 168.656 66.167 180) (layer F.SilkS))
  (gr_text 5V (at 165.989 66.167 180) (layer F.SilkS))
  (gr_text ~G (at 159.385 66.167 180) (layer F.SilkS))
  (gr_text 5V (at 156.845 66.167 180) (layer F.SilkS))
  (gr_text ~ROMEN (at 141.351 65.659 90) (layer F.SilkS))
  (gr_text 5V (at 147.447 112.522) (layer F.SilkS))
  (gr_text 5V (at 144.907 112.522) (layer F.SilkS))
  (gr_text D7 (at 173.609 106.172 180) (layer F.SilkS))
  (gr_text D5 (at 168.402 106.172 180) (layer F.SilkS))
  (gr_text D3 (at 165.989 106.172 180) (layer F.SilkS))
  (gr_text D1 (at 163.322 106.172 180) (layer F.SilkS))
  (gr_text D6 (at 173.609 113.157) (layer F.SilkS))
  (gr_text D4 (at 171.196 113.157) (layer F.SilkS))
  (gr_text D2 (at 165.989 113.157) (layer F.SilkS))
  (gr_text D0 (at 163.449 113.157) (layer F.SilkS))
  (gr_text A15 (at 216.027 106.299 180) (layer F.SilkS))
  (gr_text A13 (at 213.233 106.299 180) (layer F.SilkS))
  (gr_text A11 (at 210.82 106.299 180) (layer F.SilkS))
  (gr_text A9 (at 208.28 106.299 180) (layer F.SilkS))
  (gr_text A7 (at 203.2 106.299 180) (layer F.SilkS))
  (gr_text A3 (at 198.12 106.299 180) (layer F.SilkS))
  (gr_text A5 (at 200.533 106.299 180) (layer F.SilkS))
  (gr_text A1 (at 193.04 106.299 180) (layer F.SilkS))
  (gr_text A14 (at 216.154 113.157) (layer F.SilkS))
  (gr_text A12 (at 213.36 113.157) (layer F.SilkS))
  (gr_text A10 (at 208.407 113.157) (layer F.SilkS))
  (gr_text A8 (at 205.74 113.157) (layer F.SilkS))
  (gr_text A6 (at 203.2 113.157) (layer F.SilkS))
  (gr_text A4 (at 198.12 113.157) (layer F.SilkS))
  (gr_text A2 (at 195.58 113.157) (layer F.SilkS))
  (gr_text A0 (at 193.04 113.157) (layer F.SilkS))
  (gr_arc (start 221.234 64.77) (end 223.774 64.77) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 221.234 111.887) (end 221.234 114.427) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 135.89 111.9124) (end 133.35 111.9124) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 135.89 64.77) (end 135.89 62.23) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 135.89 62.23) (end 221.234 62.23) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 133.35 111.9124) (end 133.35 64.77) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 221.234 114.427) (end 135.89 114.4524) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 223.774 64.77) (end 223.774 111.887) (layer Edge.Cuts) (width 0.05))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.381))
    (polygon
      (pts
        (xy 226.06 119.38) (xy 127 119.38) (xy 127 60.96) (xy 226.06 60.96)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.381))
    (polygon
      (pts
        (xy 226.06 119.38) (xy 127 119.38) (xy 127 60.96) (xy 226.06 60.96)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.381))
    (polygon
      (pts
        (xy 226.06 119.38) (xy 127 119.38) (xy 127 60.96) (xy 226.06 60.96)
      )
    )
  )
  (zone (net 2) (net_name +5V) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.381))
    (polygon
      (pts
        (xy 226.06 119.38) (xy 127 119.38) (xy 127 60.96) (xy 226.06 60.96)
      )
    )
  )
)
