(kicad_pcb (version 20171130) (host pcbnew "(5.1.6)-1")
  (general
    (thickness 1.6)
    (drawings 34)
    (tracks 134)
    (zones 0)
    (modules 13)
    (nets 6)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user hide)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.5)
    (user_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 1 0.5)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 13 15)
    (pad_drill 0)
    (pad_to_mask_clearance 0.05)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "LCR_Meter_Gerbers"))
  )
  (net 0 "")
  (net 1 /Hpot)
  (net 2 /Lpot)
  (net 3 /Hcur)
  (net 4 /Lcur)
  (net 5 GND)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /Hcur)
    (add_net /Hpot)
    (add_net /Lcur)
    (add_net /Lpot)
    (add_net GND)
  )
  (module Multicomp_LCR_4Wire:Guard_Pad (layer B.Cu) (tedit 600E650D)
    (at 149.95 107.5 180)
    (fp_text reference J5 (at 0.15 16.4) (layer B.SilkS) hide)
    (fp_text value Conn_01x01 (at -0.95 -16.6) (layer B.Fab))
    (pad 1 smd trapezoid (at 0 0 180) (size 12 15) (rect_delta 0 -1 ) (layers B.Cu B.Paste B.Mask)
      (net 5 GND))
  )
  (module Multicomp_LCR_4Wire:Guard_Pad (layer F.Cu) (tedit 600E650D)
    (at 149.95 107.5)
    (fp_text reference J6 (at -0.5 -14.15) (layer F.SilkS) hide)
    (fp_text value Conn_01x01 (at -1.55 -18.55) (layer F.Fab))
    (pad 1 smd trapezoid (at 0 0) (size 12 15) (rect_delta 0 1 ) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
  )
  (module Multicomp_LCR_4Wire:Finger_Pad (layer B.Cu) (tedit 600E64EE)
    (at 130 107.5 180)
    (fp_text reference J4 (at 0.65 -14.35) (layer B.SilkS) hide)
    (fp_text value Conn_01x01 (at -0.4 -12.05) (layer B.Fab))
    (pad 1 smd trapezoid (at 0 0 180) (size 14 15) (rect_delta 0 -1 ) (layers B.Cu B.Paste B.Mask)
      (net 4 /Lcur))
  )
  (module Multicomp_LCR_4Wire:Finger_Pad (layer F.Cu) (tedit 600E64EE)
    (at 130 107.5)
    (fp_text reference J3 (at 0.8 -15.75) (layer F.SilkS) hide)
    (fp_text value Conn_01x01 (at 1.4 -19.35) (layer F.Fab))
    (pad 1 smd trapezoid (at 0 0) (size 14 15) (rect_delta 0 1 ) (layers F.Cu F.Paste F.Mask)
      (net 2 /Lpot))
  )
  (module Multicomp_LCR_4Wire:Finger_Pad (layer B.Cu) (tedit 600E64EE)
    (at 111 107.5 180)
    (fp_text reference J2 (at -0.2 -18.55) (layer B.SilkS) hide)
    (fp_text value Conn_01x01 (at 0.1 -12.6) (layer B.Fab))
    (pad 1 smd trapezoid (at 0 0 180) (size 14 15) (rect_delta 0 -1 ) (layers B.Cu B.Paste B.Mask)
      (net 3 /Hcur))
  )
  (module Multicomp_LCR_4Wire:Finger_Pad (layer F.Cu) (tedit 600E64EE)
    (at 111 107.5)
    (fp_text reference J1 (at -0.25 -16.4) (layer F.SilkS) hide)
    (fp_text value Conn_01x01 (at 0.55 -21.6) (layer F.Fab))
    (pad 1 smd trapezoid (at 0 0) (size 14 15) (rect_delta 0 1 ) (layers F.Cu F.Paste F.Mask)
      (net 1 /Hpot))
  )
  (module Multicomp_LCR_4Wire:Secure (layer F.Cu) (tedit 600BA81F)
    (at 145 128.5)
    (fp_text reference H1 (at -6 12.5) (layer F.SilkS) hide)
    (fp_text value Secure (at -5.7 15.5) (layer F.Fab))
    (pad "" np_thru_hole oval (at 0 0) (size 6 3) (drill oval 6 3) (layers *.Cu *.Mask))
  )
  (module Multicomp_LCR_4Wire:Secure (layer F.Cu) (tedit 600BA81F)
    (at 145 119.5)
    (fp_text reference H2 (at 0.5 21) (layer F.SilkS) hide)
    (fp_text value Secure (at 1 23.4) (layer F.Fab) hide)
    (pad "" np_thru_hole oval (at 0 0) (size 6 3) (drill oval 6 3) (layers *.Cu *.Mask))
  )
  (module Multicomp_LCR_4Wire:Shield_Pad (layer B.Cu) (tedit 600BA5B3)
    (at 132.5 120)
    (fp_text reference J7 (at 0.5 24.5) (layer B.SilkS) hide)
    (fp_text value Guard (at 0.5 20.5) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 8 4) (layers B.Cu B.Paste B.Mask)
      (net 5 GND))
  )
  (module Multicomp_LCR_4Wire:Shield_Pad (layer B.Cu) (tedit 600BA5B3)
    (at 132.5 130.5)
    (fp_text reference J8 (at 0.5 12.5) (layer B.SilkS) hide)
    (fp_text value Guard (at 0.5 9) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 8 4) (layers B.Cu B.Paste B.Mask)
      (net 5 GND))
  )
  (module Multicomp_LCR_4Wire:3mm (layer F.Cu) (tedit 600BA713)
    (at 105 120)
    (fp_text reference J9 (at -0.5 19.5) (layer F.SilkS) hide)
    (fp_text value Mount (at -2 24.2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 5 GND))
  )
  (module Multicomp_LCR_4Wire:3mm (layer F.Cu) (tedit 600BA713)
    (at 155 130)
    (fp_text reference J10 (at 0.1 9) (layer F.SilkS) hide)
    (fp_text value Mount (at 0.5 14) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 5 GND))
  )
  (module Multicomp_LCR_4Wire:DUT (layer B.Cu) (tedit 600BA3DE)
    (at 118 126)
    (fp_text reference J11 (at 0.3 -5.6) (layer B.SilkS) hide)
    (fp_text value Conn_01x04 (at -0.1 3.4) (layer B.Fab) hide)
    (pad 1 smd rect (at -2.7 0.1) (size 4.6 1.8) (layers B.Cu B.Paste B.Mask)
      (net 1 /Hpot))
    (pad 2 smd rect (at -2.7 -2.1) (size 4.6 1.8) (layers B.Cu B.Paste B.Mask)
      (net 3 /Hcur))
    (pad 3 smd rect (at 2.7 0.1) (size 4.6 1.8) (layers B.Cu B.Paste B.Mask)
      (net 2 /Lpot))
    (pad 4 smd rect (at 2.7 -2.1) (size 4.6 1.8) (layers B.Cu B.Paste B.Mask)
      (net 4 /Lcur))
  )
  (gr_line (start 155.47 99.98) (end 156.48 115) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 144.43 99.98) (end 155.47 99.98) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 143.43 115) (end 144.43 99.98) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 136.52 99.98) (end 137.53 115) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 123.48 99.98) (end 136.52 99.98) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 122.47 115) (end 123.48 99.98) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 117.52 99.98) (end 118.53 115) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 104.48 99.98) (end 117.52 99.98) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 103.47 115) (end 104.48 99.98) (layer Edge.Cuts) (width 0.05))
  (gr_text Hcur (at 114 116.5 180) (layer B.SilkS))
  (gr_text Lcur (at 130.2 116.5 180) (layer B.SilkS))
  (gr_text "FHM Jan 2021" (at 107.4 133.8 180) (layer B.SilkS))
  (gr_text "Multicomp Pro\nLCR" (at 122.5 124.5) (layer F.SilkS))
  (gr_text Hpot (at 114 116.5) (layer F.SilkS))
  (gr_text Lpot (at 130.2 116.5) (layer F.SilkS))
  (gr_text Guard (at 147 116.5) (layer F.SilkS))
  (gr_text Guard (at 147 116.5 180) (layer B.SilkS))
  (gr_text "Hpot\n" (at 114.7 128.7 180) (layer B.SilkS))
  (gr_text Lpot (at 120.9 128.7 180) (layer B.SilkS))
  (gr_text "Lcur\n" (at 120.9 121.4 180) (layer B.SilkS))
  (gr_text Hcur (at 114.7 121.4 180) (layer B.SilkS))
  (gr_text Guard (at 132.6 126.8 180) (layer B.SilkS))
  (gr_text Guard (at 132.6 123.7 180) (layer B.SilkS))
  (gr_line (start 118.53 115) (end 122.47 115) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 158 115) (end 156.48 115) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 160 133) (end 160 117) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 102 135) (end 158 135) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 100 117) (end 100 133) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 103.47 115) (end 102 115) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 102 133) (end 100 133) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 158 133) (end 158 135) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 158 117) (end 160 117) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 102 117) (end 102 115) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 137.53 115) (end 143.43 115) (layer Edge.Cuts) (width 0.05))
  (zone (net 5) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 160 117) (xy 160 133) (xy 158 135) (xy 102 135) (xy 100 133)
        (xy 100 117) (xy 102 115) (xy 158 115)
      )
    )
  )
  (zone (net 5) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 160 117) (xy 160 133) (xy 158 135) (xy 102 135) (xy 100 133)
        (xy 100 117) (xy 102 115) (xy 158 115)
      )
    )
  )
)
