(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 33)
    (no_connects 0)
    (area 109.981429 102.788999 156.539001 129.615001)
    (thickness 1.6)
    (drawings 8)
    (tracks 62)
    (zones 0)
    (modules 14)
    (nets 8)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.254)
    (user_trace_width 0.381)
    (user_trace_width 0.635)
    (user_trace_width 1.27)
    (user_trace_width 1.905)
    (user_trace_width 2.54)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 4.5 3.3)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (grid_origin 120.904 108.712)
    (visible_elements 7FFEFDFF)
    (pcbplotparams
      (layerselection 0x01030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 "Net-(C1-Pad2)")
  (net 3 "Net-(D1-Pad2)")
  (net 4 "Net-(D1-Pad3)")
  (net 5 "Net-(D1-Pad1)")
  (net 6 "Net-(F1-Pad2)")
  (net 7 "Net-(Q1-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D1-Pad3)")
    (add_net "Net-(F1-Pad2)")
    (add_net "Net-(Q1-Pad3)")
  )
  (module Fuse_Holders_and_Fuses:Fuseholder5x20_horiz_open_universal_Type-III (layer F.Cu) (tedit 5A949FE3)
    (at 129.286 126.492 90)
    (descr "Fuseholder, 5x20, open, horizontal, Type-III, universal, inline, lateral,")
    (tags "Fuseholder 5x20 open horizontal Type-III universal inline lateral Sicherungshalter offen ")
    (fp_text reference F1 (at 10.16 -1.27 90) (layer F.SilkS) hide)
    (fp_text value Fuse (at 9.738 -2.762 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 15.32 0 90) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 6 "Net-(F1-Pad2)"))
    (pad 2 thru_hole circle (at 20.4 0 90) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 6 "Net-(F1-Pad2)"))
    (pad 1 thru_hole circle (at 5.08 0 90) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 17.86 -2.54 90) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 6 "Net-(F1-Pad2)"))
    (pad 2 thru_hole circle (at 17.86 2.54 90) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 6 "Net-(F1-Pad2)"))
    (pad 1 thru_hole circle (at 2.54 -2.54 90) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 1 thru_hole circle (at 2.54 2.54 90) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
  )
  (module modules:JST_W_WIRE_PADS (layer F.Cu) (tedit 5A94A2AF)
    (at 120.904 108.712 90)
    (descr "JST EH series connector, S02B-EH, 2.50mm pitch, side entry")
    (tags "connector jst eh side horizontal angled")
    (fp_text reference J1 (at 1.25 3 90) (layer F.SilkS))
    (fp_text value JST2.54 (at 1.25 -8 90) (layer F.Fab))
    (fp_text user %R (at 1.25 -2 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask)
      (net 6 "Net-(F1-Pad2)"))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 "Net-(D1-Pad3)") (zone_connect 2))
    (pad 1 smd rect (at -0.7112 -2.8702 90) (size 3.302 7.62) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(F1-Pad2)"))
    (pad 2 smd rect (at 3.2258 -2.8956 90) (size 3.302 7.62) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad3)"))
    (model Connectors_JST.3dshapes/JST_EH_S02B-EH_02x2.50mm_Angled.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5A948574)
    (at 135.636 109.474 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at -2.54 0 270) (layer F.SilkS))
    (fp_text value .01 (at 0.254 1.524 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.524 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5A94857F)
    (at 140.462 115.062 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at -2.286 0 270) (layer F.SilkS))
    (fp_text value 470 (at 0 1.524 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5A948571)
    (at 135.636 106.934)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 2.286 0 90) (layer F.SilkS))
    (fp_text value 4K7 (at 0 1.524) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5A94857D)
    (at 140.462 117.348 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at -2.286 0 270) (layer F.SilkS))
    (fp_text value 2K2 (at 2.032 0 270) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D1-Pad2)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad3)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5A948589)
    (at 136.398 117.348 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 2.286 0 270) (layer F.SilkS))
    (fp_text value 1K0 (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad3)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(Q1-Pad3)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 5A98FEBE)
    (at 135.636 112.776)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 2.54 0 270) (layer F.SilkS))
    (fp_text value MMBT3906 (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(Q1-Pad3)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 5A948583)
    (at 145.542 115.824)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference D1 (at 1.778 -1.524 90) (layer F.SilkS))
    (fp_text value TL431DBZ (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D1-Pad2)"))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad3)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-220-3_Vertical (layer F.Cu) (tedit 5A94A2DB)
    (at 136.398 121.412 270)
    (descr "TO-220-3, Vertical, RM 2.54mm")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference Q2 (at 2.54 -3.556 270) (layer F.SilkS))
    (fp_text value BT151 (at 2.54 3.92 270) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.62 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(D1-Pad3)") (zone_connect 2))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(Q1-Pad3)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometers:Potentiometer_Trimmer_Suntan_TSR-3386C_Vertical (layer F.Cu) (tedit 5A94859D)
    (at 142.748 105.664)
    (descr "Potentiometer, vertically mounted, Omeg PC16PU, Omeg PC16PU, Omeg PC16PU, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GH/249GH Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148A/149A Single with mounting plates, Vishay/Spectrol 148/149 Double, Vishay/Spectrol 148A/149A Double with mounting plates, Piher PC-16 Single, Piher PC-16 Single, Piher PC-16 Single, Piher PC-16SV Single, Piher PC-16 Double, Piher PC-16 Triple, Piher T16H Single, Piher T16L Single, Piher T16H Double, Alps RK163 Single, Alps RK163 Double, Alps RK097 Single, Alps RK097 Double, Bourns PTV09A-2 Single with mounting sleve Single, Bourns PTV09A-1 with mounting sleve Single, Bourns PRS11S Single, Alps RK09K Single with mounting sleve Single, Alps RK09K with mounting sleve Single, Alps RK09L Single, Alps RK09L Single, Alps RK09L Double, Alps RK09L Double, Alps RK09Y Single, Bourns 3339S Single, Bourns 3339S Single, Bourns 3339P Single, Bourns 3339H Single, Vishay T7YA Single, Suntan TSR-3386H Single, Suntan TSR-3386H Single, http://www.Suntan.com/docs/51016/TSR-3386.pdf")
    (tags "Potentiometer vertical  Omeg PC16PU  Omeg PC16PU  Omeg PC16PU  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GH/249GH Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148A/149A Single with mounting plates  Vishay/Spectrol 148/149 Double  Vishay/Spectrol 148A/149A Double with mounting plates  Piher PC-16 Single  Piher PC-16 Single  Piher PC-16 Single  Piher PC-16SV Single  Piher PC-16 Double  Piher PC-16 Triple  Piher T16H Single  Piher T16L Single  Piher T16H Double  Alps RK163 Single  Alps RK163 Double  Alps RK097 Single  Alps RK097 Double  Bourns PTV09A-2 Single with mounting sleve Single  Bourns PTV09A-1 with mounting sleve Single  Bourns PRS11S Single  Alps RK09K Single with mounting sleve Single  Alps RK09K with mounting sleve Single  Alps RK09L Single  Alps RK09L Single  Alps RK09L Double  Alps RK09L Double  Alps RK09Y Single  Bourns 3339S Single  Bourns 3339S Single  Bourns 3339P Single  Bourns 3339H Single  Vishay T7YA Single  Suntan TSR-3386H Single  Suntan TSR-3386H Single")
    (fp_text reference RV1 (at 1.778 2.54 90) (layer F.SilkS))
    (fp_text value 5K (at 0 8.705) (layer F.Fab))
    (pad 3 thru_hole circle (at 0 5.08) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(D1-Pad2)"))
    (pad 2 thru_hole circle (at 0 2.54) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(D1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model Potentiometers.3dshapes/Potentiometer_Trimmer_Suntan_TSR-3386C_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:JST_W_WIRE_PADS (layer F.Cu) (tedit 5A94A2CC)
    (at 120.904 126.238 90)
    (descr "JST EH series connector, S02B-EH, 2.50mm pitch, side entry")
    (tags "connector jst eh side horizontal angled")
    (fp_text reference J2 (at 1.25 3 90) (layer F.SilkS))
    (fp_text value JST2.54 (at 1.25 -8 90) (layer F.Fab))
    (fp_text user %R (at 1.25 -2 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 "Net-(D1-Pad3)") (zone_connect 2))
    (pad 1 smd rect (at -0.7112 -2.8702 90) (size 3.302 7.62) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 3.2258 -2.8956 90) (size 3.302 7.62) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad3)"))
    (model Connectors_JST.3dshapes/JST_EH_S02B-EH_02x2.50mm_Angled.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SMC-RM10_Universal_Handsoldering (layer B.Cu) (tedit 5A94B35D)
    (at 141.986 119.888 90)
    (descr "Diode, Universal, SMC (DO-214AB), RM10, Handsoldering, SMD, Thruhole")
    (tags "Diode Universal SMC (DO-214AB) RM10 Handsoldering SMD Thruhole")
    (fp_text reference D2 (at 0 4.1 90) (layer B.SilkS))
    (fp_text value SS34 (at 0 -4.3 90) (layer B.Fab))
    (fp_text user %R (at 0 1.7 90) (layer B.Fab))
    (pad 1 smd rect (at -5 0 90) (size 4.5 3.3) (drill (offset 0.6 0)) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 5 0 270) (size 4.5 3.3) (drill (offset 0.6 0)) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(D1-Pad3)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SMC.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_2.7mm (layer F.Cu) (tedit 5A98FECC)
    (at 118.11 115.824)
    (descr "Mounting Hole 2.7mm, no annular")
    (tags "mounting hole 2.7mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.7) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.7mm (at 0 3.7) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (gr_text "OVP CROWBAR" (at 151.3332 108.204 90) (layer B.SilkS))
  (gr_text "H226     RSP" (at 153.924 108.2294 90) (layer B.SilkS))
  (gr_text OUT (at 116.332 124.968 270) (layer B.SilkS))
  (gr_text IN (at 116.332 107.696 270) (layer B.SilkS))
  (gr_line (start 156.464 103.124) (end 156.464 129.54) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 114.046 129.54) (end 114.046 103.124) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 156.464 129.54) (end 114.046 129.54) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 156.464 103.124) (end 114.046 103.124) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 4) (net_name "Net-(D1-Pad3)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.3 103.378) (xy 114.3 129.286) (xy 155.956 129.286) (xy 155.956 103.378)
      )
    )
  )
)
