<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<board>
<plain>
<wire x1="43.18" y1="58.4105" x2="43.18" y2="32.385" width="0.2032" layer="20"/>
<wire x1="43.18" y1="32.385" x2="45.72" y2="29.845" width="0.2032" layer="20" curve="90"/>
<wire x1="45.72" y1="29.845" x2="91.44" y2="29.845" width="0.2032" layer="20"/>
<wire x1="91.44" y1="29.845" x2="93.98" y2="32.385" width="0.2032" layer="20" curve="90"/>
<wire x1="93.98" y1="32.385" x2="93.98" y2="58.4195" width="0.2032" layer="20"/>
<wire x1="93.98" y1="58.4195" x2="91.4395" y2="60.9595" width="0.2032" layer="20" curve="90.011279"/>
<wire x1="91.4395" y1="60.9595" x2="45.7195" y2="60.9505" width="0.2032" layer="20"/>
<wire x1="45.7195" y1="60.9505" x2="43.18" y2="58.4105" width="0.2032" layer="20" curve="89.988721"/>
<text>IAFF</text>
<text>IAFF</text>
<text>LUKE 10:2</text>
<text>The harvest 
is plentiful!</text>
</plain>
<libraries>
<library name="caps-elec">
<packages>
<package name="0502">
<description>0.1" (2.54mm) spacing</description>
</package>
<package name="0632">
<description>0.1" (2.54mm) spacing</description>
</package>
</packages>
</library>
<library name="gm-caps-film-box">
<description>&lt;b&gt;Capacitors, Film, Box&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;1000pF - 2.2uF  (uF = µF = mF)
&lt;li&gt;popular nonpolarized capacitors because they are small
&lt;li&gt;these have short leads so that pad spacing equals lead spacing
&lt;li&gt;e.g., WIMA capacitors
&lt;/ul&gt;</description>
<packages>
<package name="072X035">
<description>&lt;b&gt;7.2mm x 3.5mm&lt;/b&gt;
&lt;p&gt;WIMA MKP2, MKS2</description>
</package>
</packages>
</library>
<library name="potentiometers">
<packages>
<package name="16MM_C.MOUNT">
<description>&lt;b&gt;16mm / Right-Angle /  PC Mount / Short Pin&lt;/b&gt;
&lt;p&gt;
For aligning the center of the pot shaft to a specific drill location
&lt;p&gt;
&lt;a href="http://smallbear-electronics.mybigcommerce.com/alpha-single-gang-16mm-right-angle-pc-mount/"&gt;http://smallbear-electronics.mybigcommerce.com/alpha-single-gang-16mm-right-angle-pc-mount/&lt;/a&gt;</description>
</package>
</packages>
</library>
<library name="diodes">
<packages>
<package name="DO41-3">
<description>&lt;b&gt;DO-41 0.3" pad spacing&lt;/b&gt;</description>
</package>
<package name="3MM_IO">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
</packages>
</library>
<library name="supply pins">
<packages>
<package name="IN">
<description>&lt;b&gt;Square Pad (w/label) - 80mil Diameter, 47mil Drill&lt;b&gt;</description>
</package>
<package name="OUT">
<description>&lt;b&gt;Square Pad (w/label) - 80mil Diameter, 47mil Drill&lt;b&gt;</description>
</package>
<package name="PAD3">
<description>&lt;b&gt;Square Pad (w/label) - 80mil Diameter, 47mil Drill&lt;b&gt;</description>
</package>
</packages>
</library>
<library name="jacks">
<packages>
<package name="DC_TS">
</package>
</packages>
</library>
<library name="transistors-BJT">
<packages>
<package name="TO92">
</package>
</packages>
</library>
<library name="transistors-GERM">
<packages>
<package name="TO-5">
<description>&lt;b&gt;TO-5&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="resistors">
<packages>
<package name="0.3&quot;.B">
<description>0.3"  (7.62mm) lead spacing, 1/4W (flat)</description>
</package>
</packages>
</library>
<library name="enclosures">
<packages>
<package name="1590B">
</package>
<package name="DC_TOP">
</package>
<package name="DC_DRILL">
</package>
<package name="3PDT">
</package>
<package name="LUMBURG_SIDE">
</package>
</packages>
</library>
<library name="switches">
<packages>
<package name="SPST.WIRE">
<description>Wire to switch</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C3" library="caps-elec" package="0502" value="10uF"/>
<element name="C5" library="gm-caps-film-box" package="072X035" value="100n"/>
<element name="C7" library="caps-elec" package="0502" value="10uF"/>
<element name="C6" library="caps-elec" package="0502" value="10uF"/>
<element name="C1" library="caps-elec" package="0632" value="100uF"/>
<element name="C2" library="gm-caps-film-box" package="072X035" value="100n"/>
<element name="COMP" library="potentiometers" package="16MM_C.MOUNT" value="B10k">
<attribute name="NAME"/>
<attribute name="NAME"/>
</element>
<element name="D1" library="diodes" package="DO41-3" value="1N4001"/>
<element name="DRIVE" library="potentiometers" package="16MM_C.MOUNT" value="B10k">
<attribute name="NAME"/>
<attribute name="NAME"/>
</element>
<element name="GATE" library="potentiometers" package="16MM_C.MOUNT" value="B10k">
<attribute name="NAME"/>
<attribute name="NAME"/>
</element>
<element name="IN1" library="supply pins" package="IN" value="IN"/>
<element name="9V" library="jacks" package="DC_TS" value="DC_TS"/>
<element name="LED" library="diodes" package="3MM_IO" value="LED.1"/>
<element name="OUT1" library="supply pins" package="OUT" value="OUT"/>
<element name="Q1" library="transistors-BJT" package="TO92" value="2n3904"/>
<element name="Q2" library="transistors-GERM" package="TO-5" value="AC125">
<attribute name="NAME"/>
</element>
<element name="Q3" library="transistors-GERM" package="TO-5" value="AC125">
<attribute name="NAME"/>
</element>
<element name="R2" library="resistors" package="0.3&quot;.B" value="220k"/>
<element name="R3" library="resistors" package="0.3&quot;.B" value="10k"/>
<element name="R6" library="resistors" package="0.3&quot;.B" value="47k"/>
<element name="R5" library="resistors" package="0.3&quot;.B" value="470R"/>
<element name="R7" library="resistors" package="0.3&quot;.B" value="5.1k"/>
<element name="R8" library="resistors" package="0.3&quot;.B" value="220k"/>
<element name="R1" library="resistors" package="0.3&quot;.B" value="4.7k"/>
<element name="STAB" library="potentiometers" package="16MM_C.MOUNT" value="B5k">
<attribute name="NAME"/>
<attribute name="NAME"/>
</element>
<element name="VOL" library="potentiometers" package="16MM_C.MOUNT" value="B5k">
<attribute name="NAME"/>
<attribute name="NAME"/>
</element>
<element name="SW" library="supply pins" package="PAD3" value="PADS.SQR_LBL"/>
<element name="G" library="supply pins" package="PAD3" value="PADS.SQR_LBL"/>
<element name="U$1" library="enclosures" package="1590B" value=""/>
<element name="U$2" library="enclosures" package="DC_TOP" value=""/>
<element name="U$3" library="enclosures" package="DC_DRILL" value=""/>
<element name="U$4" library="enclosures" package="3PDT" value=""/>
<element name="U$5" library="enclosures" package="LUMBURG_SIDE" value=""/>
<element name="U$6" library="enclosures" package="LUMBURG_SIDE" value=""/>
<element name="C4" library="caps-elec" package="0502" value="10uF"/>
<element name="R4" library="resistors" package="0.3&quot;.B" value="1M"/>
<element name="FAT" library="switches" package="SPST.WIRE" value=""/>
</elements>
<signals>
<signal name="Q1_P">
<contactref element="C5" pad="1"/>
<contactref element="Q1" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="R2" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="FAT" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="C5" pad="2"/>
<contactref element="Q2" pad="2"/>
<contactref element="R6" pad="1"/>
<contactref element="C4" pad="-"/>
</signal>
<signal name="GND">
<contactref element="Q1" pad="3"/>
<contactref element="GATE" pad="1"/>
<contactref element="GATE" pad="2"/>
<contactref element="VOL" pad="1"/>
<contactref element="R8" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="9V" pad="GND"/>
<contactref element="G" pad="1"/>
<contactref element="D1" pad="A"/>
<contactref element="C1" pad="-"/>
</signal>
<signal name="N$4">
<contactref element="C3" pad="+"/>
<contactref element="Q1" pad="2"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="Q3_P">
<contactref element="R6" pad="2"/>
<contactref element="DRIVE" pad="3"/>
<contactref element="COMP" pad="1"/>
<contactref element="COMP" pad="2"/>
<contactref element="Q3" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="DRIVE" pad="2"/>
<contactref element="C7" pad="-"/>
</signal>
<signal name="Q2_P">
<contactref element="R3" pad="2"/>
<contactref element="STAB" pad="3"/>
<contactref element="C7" pad="+"/>
<contactref element="COMP" pad="3"/>
<contactref element="DRIVE" pad="1"/>
<contactref element="Q2" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="R5" pad="2"/>
<contactref element="Q2" pad="3"/>
<contactref element="Q3" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="GATE" pad="3"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="VOL" pad="3"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="R7" pad="2"/>
<contactref element="Q3" pad="3"/>
</signal>
<signal name="N$13">
<contactref element="C6" pad="+"/>
<contactref element="VOL" pad="2"/>
</signal>
<signal name="VB">
<contactref element="D1" pad="C"/>
<contactref element="STAB" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="9V" pad="PWR"/>
<contactref element="C1" pad="+"/>
</signal>
<signal name="N$16">
<contactref element="LED" pad="A"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="IN">
<contactref element="C3" pad="-"/>
<contactref element="IN1" pad="1"/>
</signal>
<signal name="OUT">
<contactref element="C6" pad="-"/>
<contactref element="R8" pad="2"/>
<contactref element="OUT1" pad="1"/>
</signal>
<signal name="SW">
<contactref element="LED" pad="K"/>
<contactref element="SW" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="R4" pad="1"/>
<contactref element="FAT" pad="2"/>
<contactref element="C4" pad="+"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
