(kicad_pcb (version 20171130) (host pcbnew 5.0.2+dfsg1-1~bpo9+1)
  (general
    (thickness 1.6)
    (drawings 30)
    (tracks 484)
    (zones 0)
    (modules 61)
    (nets 49)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 VCC)
  (net 3 VDD)
  (net 4 "Net-(D1-Pad1)")
  (net 5 RXD)
  (net 6 "Net-(D2-Pad1)")
  (net 7 "Net-(D3-Pad2)")
  (net 8 "Net-(D4-Pad2)")
  (net 9 "Net-(D5-Pad2)")
  (net 10 "Net-(D6-Pad2)")
  (net 11 "Net-(D7-Pad2)")
  (net 12 "Net-(D8-Pad2)")
  (net 13 "Net-(D9-Pad2)")
  (net 14 "Net-(D10-Pad2)")
  (net 15 "Net-(D11-Pad2)")
  (net 16 LED1)
  (net 17 LED2)
  (net 18 LED3)
  (net 19 LED4)
  (net 20 LED5)
  (net 21 "Net-(R1-Pad2)")
  (net 22 "Net-(R2-Pad1)")
  (net 23 "Net-(R3-Pad2)")
  (net 24 "Net-(R4-Pad2)")
  (net 25 "Net-(R5-Pad1)")
  (net 26 "Net-(R6-Pad2)")
  (net 27 "Net-(R7-Pad1)")
  (net 28 SCL)
  (net 29 SDA)
  (net 30 "Net-(R10-Pad1)")
  (net 31 ~PWM_EN)
  (net 32 "Net-(R13-Pad1)")
  (net 33 "Net-(R18-Pad1)")
  (net 34 PWM1)
  (net 35 TXD)
  (net 36 PWM2)
  (net 37 PWM3)
  (net 38 PWM4)
  (net 39 PWM5)
  (net 40 /PWRin)
  (net 41 DispACT)
  (net 42 DispWiFi)
  (net 43 DispERR)
  (net 44 DispL1)
  (net 45 DispL2)
  (net 46 DispL3)
  (net 47 DispL4)
  (net 48 DispL5)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net DispACT)
    (add_net DispERR)
    (add_net DispL1)
    (add_net DispL2)
    (add_net DispL3)
    (add_net DispL4)
    (add_net DispL5)
    (add_net DispWiFi)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D10-Pad2)")
    (add_net "Net-(D11-Pad2)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(D6-Pad2)")
    (add_net "Net-(D7-Pad2)")
    (add_net "Net-(D8-Pad2)")
    (add_net "Net-(D9-Pad2)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R10-Pad1)")
    (add_net "Net-(R13-Pad1)")
    (add_net "Net-(R18-Pad1)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R4-Pad2)")
    (add_net "Net-(R5-Pad1)")
    (add_net "Net-(R6-Pad2)")
    (add_net "Net-(R7-Pad1)")
    (add_net PWM1)
    (add_net PWM2)
    (add_net PWM3)
    (add_net PWM4)
    (add_net PWM5)
    (add_net RXD)
    (add_net SCL)
    (add_net SDA)
    (add_net TXD)
    (add_net ~PWM_EN)
  )
  (net_class ICPWR ""
    (clearance 0.1524)
    (trace_width 0.3048)
    (via_dia 0.8128)
    (via_drill 0.3302)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net VCC)
  )
  (net_class LEDPWR ""
    (clearance 0.1524)
    (trace_width 1.2192)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /PWRin)
    (add_net LED1)
    (add_net LED2)
    (add_net LED3)
    (add_net LED4)
    (add_net LED5)
    (add_net VDD)
  )
  (module n39-kicad:AKL_101-02 (layer F.Cu) (tedit 5CA2751C)
    (at 101.6 58.42 180)
    (descr "ALK 101-02")
    (fp_text reference J7 (at -0.635 -5.08 180) (layer F.SilkS))
    (fp_text value LED5 (at 2.286 -4.826 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 20 LED5))
    (pad 1 thru_hole circle (at 0 0 180) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 3 VDD))
  )
  (module n39-kicad:AKL_101-02 (layer F.Cu) (tedit 5CA27506)
    (at 63.5 58.42 180)
    (descr "ALK 101-02")
    (fp_text reference J4 (at -1.27 -5.08 180) (layer F.SilkS))
    (fp_text value LED2 (at 2.286 -4.826 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 3 VDD))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 17 LED2))
  )
  (module RF_Module:ESP-12E (layer F.Cu) (tedit 5CA26E95)
    (at 59.69 80.645 180)
    (descr "Wi-Fi Module, http://wiki.ai-thinker.com/_media/esp8266/docs/aithinker_esp_12f_datasheet_en.pdf")
    (tags "Wi-Fi Module")
    (attr smd)
    (fp_text reference U2 (at -7.62 13.335 180) (layer F.SilkS))
    (fp_text value ESP-12E (at -0.06 -12.78 180) (layer F.Fab))
    (fp_text user Antenna (at -0.06 -7) (layer Cmts.User))
    (fp_text user "KEEP-OUT ZONE" (at 0.03 -9.55) (layer Cmts.User))
    (fp_text user %R (at 0.49 -0.8 180) (layer F.Fab))
    (pad 1 smd rect (at -7.6 -3.5 180) (size 2.5 1) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(R3-Pad2)"))
    (pad 2 smd rect (at -7.6 -1.5 180) (size 2.5 1) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at -7.6 0.5 180) (size 2.5 1) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(R1-Pad2)"))
    (pad 4 smd rect (at -7.6 2.5 180) (size 2.5 1) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at -7.6 4.5 180) (size 2.5 1) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at -7.6 6.5 180) (size 2.5 1) (layers F.Cu F.Paste F.Mask)
      (net 31 ~PWM_EN))
    (pad 7 smd rect (at -7.6 8.5 180) (size 2.5 1) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at -7.6 10.5 180) (size 2.5 1) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 9 smd rect (at -5 12 180) (size 1 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 10 smd rect (at -3 12 180) (size 1 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd rect (at -1 12 180) (size 1 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 12 smd rect (at 1 12 180) (size 1 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at 3 12 180) (size 1 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at 5 12 180) (size 1 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 15 smd rect (at 7.6 10.5 180) (size 2.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 16 smd rect (at 7.6 8.5 180) (size 2.5 1) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(R5-Pad1)"))
    (pad 17 smd rect (at 7.6 6.5 180) (size 2.5 1) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(R4-Pad2)"))
    (pad 18 smd rect (at 7.6 4.5 180) (size 2.5 1) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(R6-Pad2)"))
    (pad 19 smd rect (at 7.6 2.5 180) (size 2.5 1) (layers F.Cu F.Paste F.Mask)
      (net 28 SCL))
    (pad 20 smd rect (at 7.6 0.5 180) (size 2.5 1) (layers F.Cu F.Paste F.Mask)
      (net 29 SDA))
    (pad 21 smd rect (at 7.6 -1.5 180) (size 2.5 1) (layers F.Cu F.Paste F.Mask)
      (net 5 RXD))
    (pad 22 smd rect (at 7.6 -3.5 180) (size 2.5 1) (layers F.Cu F.Paste F.Mask)
      (net 35 TXD))
    (model ${KISYS3DMOD}/RF_Module.3dshapes/ESP-12E.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_SMD:Panasonic_EVQPUJ_EVQPUA (layer F.Cu) (tedit 5CA26DF6)
    (at 45.085 69.215 270)
    (descr http://industrial.panasonic.com/cdbs/www-data/pdf/ATV0000/ATV0000CE5.pdf)
    (tags "SMD SMT SPST EVQPUJ EVQPUA")
    (attr smd)
    (fp_text reference SW2 (at -5.08 1.905 90) (layer F.SilkS))
    (fp_text value SW_PROG (at 0 3.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 2.625 0.85 90) (size 1.55 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -2.625 0.85 90) (size 1.55 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -2.625 -0.85 90) (size 1.55 1) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(R6-Pad2)"))
    (pad 1 smd rect (at 2.625 -0.85 90) (size 1.55 1) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(R6-Pad2)"))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/Panasonic_EVQPUJ_EVQPUA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:TO-263-5_TabPin3 (layer B.Cu) (tedit 5CA2960D)
    (at 60.96 45.72 90)
    (descr "TO-263 / D2PAK / DDPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO263/PG-TO263-5-1/")
    (tags "D2PAK DDPAK TO-263 D2PAK-5 TO-263-5 SOT-426")
    (attr smd)
    (fp_text reference U3 (at -3.81 5.08 90) (layer B.SilkS))
    (fp_text value CAT4101 (at 0 -6.65 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad "" smd rect (at 0.95 -2.775 90) (size 4.55 5.25) (layers B.Paste))
    (pad "" smd rect (at 5.8 2.775 90) (size 4.55 5.25) (layers B.Paste))
    (pad "" smd rect (at 0.95 2.775 90) (size 4.55 5.25) (layers B.Paste))
    (pad "" smd rect (at 5.8 -2.775 90) (size 4.55 5.25) (layers B.Paste))
    (pad 3 smd rect (at 3.375 0 90) (size 9.4 10.8) (layers B.Cu B.Mask)
      (net 1 GND))
    (pad 5 smd rect (at -5.775 -3.4 90) (size 4.6 1.1) (layers B.Cu B.Paste B.Mask)
      (net 17 LED2))
    (pad 4 smd rect (at -5.775 -1.7 90) (size 4.6 1.1) (layers B.Cu B.Paste B.Mask)
      (net 27 "Net-(R7-Pad1)"))
    (pad 3 smd rect (at -5.775 0 90) (size 4.6 1.1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -5.775 1.7 90) (size 4.6 1.1) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (pad 1 smd rect (at -5.775 3.4 90) (size 4.6 1.1) (layers B.Cu B.Paste B.Mask)
      (net 36 PWM2))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/TO-263-5_TabPin3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5CA61FBD)
    (at 71.755 52.07)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (attr smd)
    (fp_text reference D9 (at -2.9 0) (layer F.SilkS))
    (fp_text value gn (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(D9-Pad2)"))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 46 DispL3))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5CA2696B)
    (at 50.165 50.165 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C1 (at -2.54 0 180) (layer F.SilkS))
    (fp_text value 100n (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5CA26898)
    (at 62.865 50.165 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C3 (at -2.54 0 180) (layer F.SilkS))
    (fp_text value 100n (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 VCC))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5CA26539)
    (at 75.565 50.165 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C6 (at -2.54 0 180) (layer F.SilkS))
    (fp_text value 100n (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 VCC))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5CA26FB9)
    (at 83.82 81.28)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C7 (at 2.54 0) (layer F.SilkS))
    (fp_text value 100n (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5CA26712)
    (at 88.265 50.165 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C8 (at -2.54 0 180) (layer F.SilkS))
    (fp_text value 100n (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 VCC))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5CA26755)
    (at 100.965 50.165 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C9 (at -2.54 0 180) (layer F.SilkS))
    (fp_text value 100n (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5CA27699)
    (at 52.705 66.04)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (attr smd)
    (fp_text reference D2 (at 2.54 0) (layer F.SilkS))
    (fp_text value rt (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 VCC))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5CA2830B)
    (at 94.615 89.535 270)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (attr smd)
    (fp_text reference D3 (at -2.75 0 270) (layer F.SilkS))
    (fp_text value gn (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(D3-Pad2)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5CA2704A)
    (at 88.9 89.535 90)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (attr smd)
    (fp_text reference D4 (at 0 -4.445 90) (layer F.SilkS))
    (fp_text value or (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 41 DispACT))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5CA27057)
    (at 86.995 89.535 90)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (attr smd)
    (fp_text reference D5 (at 0 -3.81 90) (layer F.SilkS))
    (fp_text value rt (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 "Net-(D5-Pad2)"))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 42 DispWiFi))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5CA2704D)
    (at 90.805 89.535 90)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (attr smd)
    (fp_text reference D6 (at 0 -5.08 90) (layer F.SilkS))
    (fp_text value bl (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 43 DispERR))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(D6-Pad2)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5CA26970)
    (at 46.355 52.07)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (attr smd)
    (fp_text reference D7 (at -2.935 0) (layer F.SilkS))
    (fp_text value gn (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 44 DispL1))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(D7-Pad2)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5CA61FB0)
    (at 59.055 52.07)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (attr smd)
    (fp_text reference D8 (at -2.9 0) (layer F.SilkS))
    (fp_text value gn (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(D8-Pad2)"))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 45 DispL2))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5CA61FEC)
    (at 84.455 52.07)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (attr smd)
    (fp_text reference D10 (at -3.175 0) (layer F.SilkS))
    (fp_text value gn (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(D10-Pad2)"))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 DispL4))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5CA2675B)
    (at 97.155 52.07)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (attr smd)
    (fp_text reference D11 (at -3.175 0) (layer F.SilkS))
    (fp_text value gn (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 48 DispL5))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 "Net-(D11-Pad2)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5CA26C39)
    (at 73.025 81.915 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 2.54 0 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 VCC))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 "Net-(R1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5CA61F83)
    (at 46.355 50.165)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at -2.9 0) (layer F.SilkS))
    (fp_text value 549R (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 "Net-(R2-Pad1)"))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5CA26C21)
    (at 73.025 83.82 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R3 (at 2.54 0 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 VCC))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 "Net-(R3-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5CA26B14)
    (at 73.025 76.2 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R4 (at 2.54 0 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 "Net-(R4-Pad2)"))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 VCC))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5CA26B07)
    (at 49.53 71.12 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R5 (at 0 -1.27 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 "Net-(R5-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5CA27696)
    (at 49.53 67.31 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R6 (at 0 1.27 270) (layer F.SilkS))
    (fp_text value 1k (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(D2-Pad1)"))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 "Net-(R6-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5CA61FAC)
    (at 59.055 50.165)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R7 (at -2.9 0) (layer F.SilkS))
    (fp_text value 549R (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 "Net-(R7-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5CA26B43)
    (at 73.025 78.105 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R8 (at 2.54 0 180) (layer F.SilkS))
    (fp_text value 4k7 (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 SCL))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 VCC))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5CA26B48)
    (at 73.025 80.01 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R9 (at 2.54 0 180) (layer F.SilkS))
    (fp_text value 4k7 (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 VCC))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 SDA))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5CA61FD2)
    (at 71.755 50.165)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R10 (at -3.3 0) (layer F.SilkS))
    (fp_text value 549R (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 "Net-(R10-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5CA2705F)
    (at 92.71 89.535 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R11 (at -3.175 0 270) (layer F.SilkS))
    (fp_text value 330R (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(D3-Pad2)"))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 VCC))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5CA2851F)
    (at 73.025 74.295 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R12 (at 2.9 0) (layer F.SilkS))
    (fp_text value 4k7 (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 ~PWM_EN))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 VCC))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5CA2657A)
    (at 84.455 50.165)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R13 (at -3.175 0) (layer F.SilkS))
    (fp_text value 549R (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 "Net-(R13-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5CA27046)
    (at 88.9 85.725 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R14 (at 0 4.445 270) (layer F.SilkS))
    (fp_text value 330R (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 VCC))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5CA2705B)
    (at 86.995 85.725 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R15 (at 0 3.81 270) (layer F.SilkS))
    (fp_text value 330R (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 VCC))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 "Net-(D5-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5CA27050)
    (at 90.805 85.725 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R16 (at 0 5.08 270) (layer F.SilkS))
    (fp_text value 330R (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 VCC))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(D6-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5CA6201B)
    (at 50.165 52.07 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R17 (at -2.94 0 180) (layer F.SilkS))
    (fp_text value 330R (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 VCC))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(D7-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5CA26758)
    (at 97.155 50.165)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R18 (at -3.175 0) (layer F.SilkS))
    (fp_text value 549R (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 "Net-(R18-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5CA62022)
    (at 62.865 52.07 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R19 (at -2.94 0 180) (layer F.SilkS))
    (fp_text value 330R (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 VCC))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(D8-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5CA6204B)
    (at 75.565 52.07 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R20 (at -2.95 0) (layer F.SilkS))
    (fp_text value 330R (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(D9-Pad2)"))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 VCC))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5CA6202D)
    (at 88.265 52.07 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R21 (at -2.94 0 180) (layer F.SilkS))
    (fp_text value 330R (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 VCC))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(D10-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5CA62034)
    (at 100.965 52.07 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R22 (at -2.94 0 180) (layer F.SilkS))
    (fp_text value 330R (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 "Net-(D11-Pad2)"))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 VCC))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_SMD:Panasonic_EVQPUJ_EVQPUA (layer F.Cu) (tedit 5CA26DF3)
    (at 45.085 89.535 270)
    (descr http://industrial.panasonic.com/cdbs/www-data/pdf/ATV0000/ATV0000CE5.pdf)
    (tags "SMD SMT SPST EVQPUJ EVQPUA")
    (attr smd)
    (fp_text reference SW1 (at 2.54 -3.81 270) (layer F.SilkS))
    (fp_text value SW_RST (at 0 3.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at 2.625 -0.85 90) (size 1.55 1) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(R3-Pad2)"))
    (pad 1 smd rect (at -2.625 -0.85 90) (size 1.55 1) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(R3-Pad2)"))
    (pad 2 smd rect (at -2.625 0.85 90) (size 1.55 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.625 0.85 90) (size 1.55 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/Panasonic_EVQPUJ_EVQPUA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:TO-263-5_TabPin3 (layer B.Cu) (tedit 5CA29609)
    (at 48.26 45.72 90)
    (descr "TO-263 / D2PAK / DDPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO263/PG-TO263-5-1/")
    (tags "D2PAK DDPAK TO-263 D2PAK-5 TO-263-5 SOT-426")
    (attr smd)
    (fp_text reference U1 (at -3.81 5.08 90) (layer B.SilkS))
    (fp_text value CAT4101 (at 0 -6.65 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -5.775 3.4 90) (size 4.6 1.1) (layers B.Cu B.Paste B.Mask)
      (net 34 PWM1))
    (pad 2 smd rect (at -5.775 1.7 90) (size 4.6 1.1) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (pad 3 smd rect (at -5.775 0 90) (size 4.6 1.1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -5.775 -1.7 90) (size 4.6 1.1) (layers B.Cu B.Paste B.Mask)
      (net 22 "Net-(R2-Pad1)"))
    (pad 5 smd rect (at -5.775 -3.4 90) (size 4.6 1.1) (layers B.Cu B.Paste B.Mask)
      (net 16 LED1))
    (pad 3 smd rect (at 3.375 0 90) (size 9.4 10.8) (layers B.Cu B.Mask)
      (net 1 GND))
    (pad "" smd rect (at 5.8 -2.775 90) (size 4.55 5.25) (layers B.Paste))
    (pad "" smd rect (at 0.95 2.775 90) (size 4.55 5.25) (layers B.Paste))
    (pad "" smd rect (at 5.8 2.775 90) (size 4.55 5.25) (layers B.Paste))
    (pad "" smd rect (at 0.95 -2.775 90) (size 4.55 5.25) (layers B.Paste))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/TO-263-5_TabPin3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-223-3_TabPin2 (layer F.Cu) (tedit 5CA27062)
    (at 99.06 69.215 180)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U4 (at 1.27 4.445 180) (layer F.SilkS))
    (fp_text value LM1117-3.3 (at 0 4.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 3.15 0 180) (size 2 3.8) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 2 smd rect (at -3.15 0 180) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 3 smd rect (at -3.15 2.3 180) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 3 VDD))
    (pad 1 smd rect (at -3.15 -2.3 180) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:TO-263-5_TabPin3 (layer B.Cu) (tedit 5CA29611)
    (at 73.66 45.72 90)
    (descr "TO-263 / D2PAK / DDPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO263/PG-TO263-5-1/")
    (tags "D2PAK DDPAK TO-263 D2PAK-5 TO-263-5 SOT-426")
    (attr smd)
    (fp_text reference U5 (at -3.81 5.08 90) (layer B.SilkS))
    (fp_text value CAT4101 (at 0 -6.65 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -5.775 3.4 90) (size 4.6 1.1) (layers B.Cu B.Paste B.Mask)
      (net 37 PWM3))
    (pad 2 smd rect (at -5.775 1.7 90) (size 4.6 1.1) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (pad 3 smd rect (at -5.775 0 90) (size 4.6 1.1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -5.775 -1.7 90) (size 4.6 1.1) (layers B.Cu B.Paste B.Mask)
      (net 30 "Net-(R10-Pad1)"))
    (pad 5 smd rect (at -5.775 -3.4 90) (size 4.6 1.1) (layers B.Cu B.Paste B.Mask)
      (net 18 LED3))
    (pad 3 smd rect (at 3.375 0 90) (size 9.4 10.8) (layers B.Cu B.Mask)
      (net 1 GND))
    (pad "" smd rect (at 5.8 -2.775 90) (size 4.55 5.25) (layers B.Paste))
    (pad "" smd rect (at 0.95 2.775 90) (size 4.55 5.25) (layers B.Paste))
    (pad "" smd rect (at 5.8 2.775 90) (size 4.55 5.25) (layers B.Paste))
    (pad "" smd rect (at 0.95 -2.775 90) (size 4.55 5.25) (layers B.Paste))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/TO-263-5_TabPin3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:TSSOP-28_4.4x9.7mm_P0.65mm (layer F.Cu) (tedit 5CA26FB0)
    (at 83.82 74.93 180)
    (descr "TSSOP28: plastic thin shrink small outline package; 28 leads; body width 4.4 mm; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot361-1_po.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U6 (at 0 5.715 180) (layer F.SilkS))
    (fp_text value PCA9685PW (at 0 5.9 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -2.85 -4.225 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -2.85 -3.575 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -2.85 -2.925 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -2.85 -2.275 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at -2.85 -1.625 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -2.85 -0.975 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at -2.85 -0.325 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 42 DispWiFi))
    (pad 8 smd rect (at -2.85 0.325 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 41 DispACT))
    (pad 9 smd rect (at -2.85 0.975 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 43 DispERR))
    (pad 10 smd rect (at -2.85 1.625 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 47 DispL4))
    (pad 11 smd rect (at -2.85 2.275 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 38 PWM4))
    (pad 12 smd rect (at -2.85 2.925 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 48 DispL5))
    (pad 13 smd rect (at -2.85 3.575 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 39 PWM5))
    (pad 14 smd rect (at -2.85 4.225 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 15 smd rect (at 2.85 4.225 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 16 smd rect (at 2.85 3.575 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 37 PWM3))
    (pad 17 smd rect (at 2.85 2.925 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 46 DispL3))
    (pad 18 smd rect (at 2.85 2.275 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 36 PWM2))
    (pad 19 smd rect (at 2.85 1.625 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 45 DispL2))
    (pad 20 smd rect (at 2.85 0.975 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 34 PWM1))
    (pad 21 smd rect (at 2.85 0.325 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 44 DispL1))
    (pad 22 smd rect (at 2.85 -0.325 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 23 smd rect (at 2.85 -0.975 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 31 ~PWM_EN))
    (pad 24 smd rect (at 2.85 -1.625 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 25 smd rect (at 2.85 -2.275 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 26 smd rect (at 2.85 -2.925 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 28 SCL))
    (pad 27 smd rect (at 2.85 -3.575 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 29 SDA))
    (pad 28 smd rect (at 2.85 -4.225 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TSSOP-28_4.4x9.7mm_P0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:TO-263-5_TabPin3 (layer B.Cu) (tedit 5CA29618)
    (at 86.36 45.72 90)
    (descr "TO-263 / D2PAK / DDPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO263/PG-TO263-5-1/")
    (tags "D2PAK DDPAK TO-263 D2PAK-5 TO-263-5 SOT-426")
    (attr smd)
    (fp_text reference U7 (at -3.81 5.08 90) (layer B.SilkS))
    (fp_text value CAT4101 (at 0 -6.65 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad "" smd rect (at 0.95 -2.775 90) (size 4.55 5.25) (layers B.Paste))
    (pad "" smd rect (at 5.8 2.775 90) (size 4.55 5.25) (layers B.Paste))
    (pad "" smd rect (at 0.95 2.775 90) (size 4.55 5.25) (layers B.Paste))
    (pad "" smd rect (at 5.8 -2.775 90) (size 4.55 5.25) (layers B.Paste))
    (pad 3 smd rect (at 3.375 0 90) (size 9.4 10.8) (layers B.Cu B.Mask)
      (net 1 GND))
    (pad 5 smd rect (at -5.775 -3.4 90) (size 4.6 1.1) (layers B.Cu B.Paste B.Mask)
      (net 19 LED4))
    (pad 4 smd rect (at -5.775 -1.7 90) (size 4.6 1.1) (layers B.Cu B.Paste B.Mask)
      (net 32 "Net-(R13-Pad1)"))
    (pad 3 smd rect (at -5.775 0 90) (size 4.6 1.1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -5.775 1.7 90) (size 4.6 1.1) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (pad 1 smd rect (at -5.775 3.4 90) (size 4.6 1.1) (layers B.Cu B.Paste B.Mask)
      (net 38 PWM4))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/TO-263-5_TabPin3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:TO-263-5_TabPin3 (layer B.Cu) (tedit 5CA2961C)
    (at 99.06 45.72 90)
    (descr "TO-263 / D2PAK / DDPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO263/PG-TO263-5-1/")
    (tags "D2PAK DDPAK TO-263 D2PAK-5 TO-263-5 SOT-426")
    (attr smd)
    (fp_text reference U8 (at -3.81 5.08 90) (layer B.SilkS))
    (fp_text value CAT4101 (at 0 -6.65 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -5.775 3.4 90) (size 4.6 1.1) (layers B.Cu B.Paste B.Mask)
      (net 39 PWM5))
    (pad 2 smd rect (at -5.775 1.7 90) (size 4.6 1.1) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (pad 3 smd rect (at -5.775 0 90) (size 4.6 1.1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -5.775 -1.7 90) (size 4.6 1.1) (layers B.Cu B.Paste B.Mask)
      (net 33 "Net-(R18-Pad1)"))
    (pad 5 smd rect (at -5.775 -3.4 90) (size 4.6 1.1) (layers B.Cu B.Paste B.Mask)
      (net 20 LED5))
    (pad 3 smd rect (at 3.375 0 90) (size 9.4 10.8) (layers B.Cu B.Mask)
      (net 1 GND))
    (pad "" smd rect (at 5.8 -2.775 90) (size 4.55 5.25) (layers B.Paste))
    (pad "" smd rect (at 0.95 2.775 90) (size 4.55 5.25) (layers B.Paste))
    (pad "" smd rect (at 5.8 2.775 90) (size 4.55 5.25) (layers B.Paste))
    (pad "" smd rect (at 0.95 -2.775 90) (size 4.55 5.25) (layers B.Paste))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/TO-263-5_TabPin3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_MiniMELF (layer F.Cu) (tedit 5CA26DFE)
    (at 48.895 80.01 270)
    (descr "Diode Mini-MELF")
    (tags "Diode Mini-MELF")
    (attr smd)
    (fp_text reference D1 (at 3.81 0 270) (layer F.SilkS))
    (fp_text value 1N4148 (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -2 270) (layer F.Fab))
    (pad 1 smd rect (at -1.75 0 270) (size 1.3 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 1.75 0 270) (size 1.3 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 RXD))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_MiniMELF.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 5CA26DFA)
    (at 45.085 83.185 180)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J1 (at -2.54 8.89 270) (layer F.SilkS))
    (fp_text value UART (at 0 9.95 180) (layer F.Fab))
    (fp_text user %R (at 0 3.81 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 TXD))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(D1-Pad1)"))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 VDD))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5CA276DF)
    (at 72.39 70.485)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C2 (at 1.27 -1.905) (layer F.SilkS))
    (fp_text value 10u (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 2 VCC))
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5CA27BEA)
    (at 104.775 69.215 270)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C4 (at 3.175 0 270) (layer F.SilkS))
    (fp_text value 10u (at 0 1.82 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 3 VDD))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5CA27BE3)
    (at 97.155 74.295 180)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C5 (at -3.175 0 180) (layer F.SilkS))
    (fp_text value 10u (at 0 1.82 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 2 VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module n39-kicad:AKL_101-02 (layer F.Cu) (tedit 5CA27BC8)
    (at 105.41 90.17 180)
    (descr "ALK 101-02")
    (fp_text reference J2 (at 8.255 3.175 270) (layer F.SilkS))
    (fp_text value PWR (at 2.286 -4.826 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 40 /PWRin))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module n39-kicad:AKL_101-02 (layer F.Cu) (tedit 5CA27502)
    (at 50.8 58.42 180)
    (descr "ALK 101-02")
    (fp_text reference J3 (at -1.27 -5.08 180) (layer F.SilkS))
    (fp_text value LED1 (at 2.286 -4.826 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 16 LED1))
    (pad 1 thru_hole circle (at 0 0 180) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 3 VDD))
  )
  (module n39-kicad:AKL_101-02 (layer F.Cu) (tedit 5CA2750E)
    (at 76.2 58.42 180)
    (descr "ALK 101-02")
    (fp_text reference J5 (at -1.27 -5.08 180) (layer F.SilkS))
    (fp_text value LED3 (at 2.286 -4.826 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 18 LED3))
    (pad 1 thru_hole circle (at 0 0 180) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 3 VDD))
  )
  (module n39-kicad:AKL_101-02 (layer F.Cu) (tedit 5CA27517)
    (at 88.9 58.42 180)
    (descr "ALK 101-02")
    (fp_text reference J6 (at -1.27 -5.08 180) (layer F.SilkS))
    (fp_text value LED4 (at 2.286 -4.826 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 3 VDD))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 19 LED4))
  )
  (module Fuse:Fuseholder_TR5_Littelfuse_No560_No460 (layer F.Cu) (tedit 5CA27BBD)
    (at 102.87 78.105 270)
    (descr "Fuse, Fuseholder, TR5, Littelfuse/Wickmann, No. 460, No560,")
    (tags "Fuse Fuseholder TR5 Littelfuse/Wickmann No. 460 No560 ")
    (fp_text reference F1 (at 6.35 5.715 270) (layer F.SilkS))
    (fp_text value Fuse (at 2.39 7.43 270) (layer F.Fab))
    (fp_text user %R (at 2.75 -2.75 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 3 VDD))
    (pad 2 thru_hole circle (at 5.08 0.01 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 40 /PWRin))
    (model ${KISYS3DMOD}/Fuse.3dshapes/Fuseholder_TR5_Littelfuse_No560_No460.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 5CA61919)
    (at 71.755 91.44 90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J8 (at 0 -2.33 270) (layer F.SilkS))
    (fp_text value UART (at 0 9.95 90) (layer F.Fab))
    (fp_text user %R (at 0 3.81 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 SDA))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 SCL))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 VCC))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text VCC (at 79.375 86.995 90) (layer F.SilkS))
  (gr_text SCL (at 76.835 86.995 90) (layer F.SilkS))
  (gr_text SDA (at 74.295 86.995 90) (layer F.SilkS))
  (gr_text GND (at 71.755 86.995 90) (layer F.SilkS))
  (gr_text "Iout 1A" (at 106.045 57.785 90) (layer F.SilkS))
  (gr_text "Spotty \n5-channel LED controller" (at 70.485 64.77) (layer F.SilkS))
  (gr_text Program (at 41.91 69.215 270) (layer F.SilkS))
  (gr_text Reset (at 41.91 89.535 270) (layer F.SilkS))
  (gr_text "Fuse:\n6.3A fast" (at 96.52 83.185 90) (layer F.SilkS))
  (gr_text "Vmax 15V\nImax 6.3A" (at 91.44 71.12 90) (layer F.SilkS))
  (gr_text GND (at 97.155 92.71 90) (layer F.SilkS))
  (gr_text PWR (at 94.615 92.71 90) (layer F.SilkS))
  (gr_text VDD (at 43.18 75.565) (layer F.SilkS))
  (gr_text RX (at 43.18 78.105) (layer F.SilkS))
  (gr_text GND (at 43.18 80.645) (layer F.SilkS))
  (gr_text TX (at 43.18 83.185) (layer F.SilkS))
  (gr_text ACT (at 88.9 91.44 90) (layer F.SilkS))
  (gr_text ERR (at 90.805 91.44 90) (layer F.SilkS))
  (gr_text WiFi (at 86.995 91.44 90) (layer F.SilkS))
  (gr_line (start 39.37 94.615) (end 39.37 46.99) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 107.95 94.615) (end 39.37 94.615) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 107.95 46.99) (end 107.95 94.615) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 39.37 46.99) (end 107.95 46.99) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 39.37 46.99) (xy 107.95 46.99) (xy 107.95 94.615) (xy 39.37 94.615)
      )
    )
  )
  (zone (net 0) (net_name "") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 82.55 47.625) (xy 90.17 47.625) (xy 90.17 53.34) (xy 82.55 53.34)
      )
    )
  )
  (zone (net 0) (net_name "") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 69.85 47.625) (xy 77.47 47.625) (xy 77.47 53.34) (xy 69.85 53.34)
      )
    )
  )
  (zone (net 0) (net_name "") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 95.25 47.625) (xy 102.87 47.625) (xy 102.87 53.34) (xy 95.25 53.34)
      )
    )
  )
  (zone (net 0) (net_name "") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 57.15 47.625) (xy 64.77 47.625) (xy 64.77 53.34) (xy 57.15 53.34)
      )
    )
  )
  (zone (net 0) (net_name "") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 44.45 47.625) (xy 52.07 47.625) (xy 52.07 53.34) (xy 44.45 53.34)
      )
    )
  )
  (zone (net 0) (net_name "") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 50.8 93.345) (xy 50.8 85.09) (xy 68.58 85.09) (xy 68.58 93.345)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 107.95 94.615) (xy 39.37 94.615) (xy 39.37 46.99) (xy 107.95 46.99)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 82.55 81.915) (xy 81.915 81.28) (xy 81.915 80.01) (xy 80.01 80.01) (xy 80.01 78.74)
        (xy 87.63 78.74) (xy 87.63 80.01) (xy 85.725 80.01) (xy 85.725 81.28) (xy 85.09 81.915)
      )
    )
  )
)
