(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 54)
    (no_connects 0)
    (area 134.719889 94.5766 164.586734 113.1684)
    (thickness 1.6)
    (drawings 18)
    (tracks 556)
    (zones 0)
    (modules 13)
    (nets 31)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.2032)
    (trace_clearance 0.1524)
    (zone_clearance 0.2032)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.0254)
    (via_size 0.6604)
    (via_drill 0.3302)
    (via_min_size 0.6096)
    (via_min_drill 0.3302)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.2 0.75)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 138.049 111.379)
    (grid_origin 138.049 111.379)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 GND)
  (net 3 +5V)
  (net 4 /REED_SW)
  (net 5 /BUTTON_1)
  (net 6 /ICSP_MOSI)
  (net 7 /ICSP_RST)
  (net 8 /LED_DIG_1)
  (net 9 /TRIAC_DRIVE)
  (net 10 /LED_SEG_G)
  (net 11 /LED_SEG_D)
  (net 12 /BUTTON_2)
  (net 13 /FAN_DRIVE)
  (net 14 /LED_SEG_DP)
  (net 15 /LED_SEG_E)
  (net 16 /LED_SEG_F)
  (net 17 /LED_SEG_A)
  (net 18 /TEMP_ADC)
  (net 19 /LED_SEG_B)
  (net 20 /LED_DIG_2)
  (net 21 /LED_DIG_3)
  (net 22 /LED_SEG_C)
  (net 23 "Net-(U1-Pad19)")
  (net 24 "Net-(U1-Pad22)")
  (net 25 "Net-(U1-Pad24)")
  (net 26 "Net-(U1-Pad25)")
  (net 27 /FAN_CURR)
  (net 28 /FAN_VOLT)
  (net 29 "Net-(R3-Pad2)")
  (net 30 /FAN_CURR_ADC)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.2032)
    (via_dia 0.6604)
    (via_drill 0.3302)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net /BUTTON_1)
    (add_net /BUTTON_2)
    (add_net /FAN_CURR)
    (add_net /FAN_CURR_ADC)
    (add_net /FAN_DRIVE)
    (add_net /FAN_VOLT)
    (add_net /ICSP_MOSI)
    (add_net /ICSP_RST)
    (add_net /LED_DIG_1)
    (add_net /LED_DIG_2)
    (add_net /LED_DIG_3)
    (add_net /LED_SEG_A)
    (add_net /LED_SEG_B)
    (add_net /LED_SEG_C)
    (add_net /LED_SEG_D)
    (add_net /LED_SEG_DP)
    (add_net /LED_SEG_E)
    (add_net /LED_SEG_F)
    (add_net /LED_SEG_G)
    (add_net /REED_SW)
    (add_net /TEMP_ADC)
    (add_net /TRIAC_DRIVE)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(U1-Pad19)")
    (add_net "Net-(U1-Pad22)")
    (add_net "Net-(U1-Pad24)")
    (add_net "Net-(U1-Pad25)")
  )
  (module TO_SOT_Packages_SMD:SOT-89-3 (layer F.Cu) (tedit 59F71926)
    (at 152.527 103.759)
    (descr SOT-89-3)
    (tags SOT-89-3)
    (attr smd)
    (fp_text reference D1 (at 0.45 -3.2) (layer F.SilkS) hide)
    (fp_text value TL431PK (at 0.45 3.25) (layer F.Fab))
    (fp_text user %R (at 0.38 0 90) (layer F.Fab))
    (pad 2 smd trapezoid (at 2.667 0 270) (size 1.6 0.85) (rect_delta 0 0.6 ) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.48 -1.5 270) (size 1 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at -1.3335 0 270) (size 1 1.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.48 1.5 270) (size 1 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.3335 0 270) (size 2.2 1.84) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd trapezoid (at -0.0762 0 90) (size 1.5 1) (rect_delta 0 0.7 ) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-89-3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module AC_Custom:TSM-110-XX-XXX-SV (layer B.Cu) (tedit 59F6F05F)
    (at 152.04 100)
    (fp_text reference J3 (at -1.27 -4.445) (layer B.SilkS) hide)
    (fp_text value CONN_01X10 (at 5.194 -4.496) (layer B.Fab) hide)
    (pad 1 smd rect (at 10.16 -1.46) (size 1.27 3.43) (layers B.Cu B.Paste B.Mask)
      (net 14 /LED_SEG_DP))
    (pad 2 smd rect (at 7.62 1.46) (size 1.27 3.43) (layers B.Cu B.Paste B.Mask)
      (net 15 /LED_SEG_E))
    (pad 3 smd rect (at 5.08 -1.46) (size 1.27 3.43) (layers B.Cu B.Paste B.Mask)
      (net 16 /LED_SEG_F))
    (pad 4 smd rect (at 2.54 1.46) (size 1.27 3.43) (layers B.Cu B.Paste B.Mask)
      (net 17 /LED_SEG_A))
    (pad 5 smd rect (at 0 -1.46) (size 1.27 3.43) (layers B.Cu B.Paste B.Mask)
      (net 18 /TEMP_ADC))
    (pad 6 smd rect (at -2.54 1.46) (size 1.27 3.43) (layers B.Cu B.Paste B.Mask)
      (net 19 /LED_SEG_B))
    (pad 7 smd rect (at -5.08 -1.46) (size 1.27 3.43) (layers B.Cu B.Paste B.Mask)
      (net 20 /LED_DIG_2))
    (pad 8 smd rect (at -7.62 1.46) (size 1.27 3.43) (layers B.Cu B.Paste B.Mask)
      (net 21 /LED_DIG_3))
    (pad 9 smd rect (at -10.16 -1.46) (size 1.27 3.43) (layers B.Cu B.Paste B.Mask)
      (net 22 /LED_SEG_C))
    (pad 10 smd rect (at -12.7 1.46) (size 1.27 3.43) (layers B.Cu B.Paste B.Mask)
      (net 3 +5V))
    (model "C:/Users/andrew.cowan/Dropbox/Backup/Projects/2017.10.29   858D+ Hot Air Upgrade/Adapter PCB/3D models/TSM-110-01-S-SV.wrl"
      (at (xyz -0.05 0 0.048))
      (scale (xyz 0.393 0.393 0.393))
      (rotate (xyz 270 0 0))
    )
  )
  (module Housings_DFN_QFN:QFN-32-1EP_5x5mm_Pitch0.5mm (layer F.Cu) (tedit 59F6F04E)
    (at 142.621 103.807381 315)
    (descr "UH Package; 32-Lead Plastic QFN (5mm x 5mm); (see Linear Technology QFN_32_05-08-1693.pdf)")
    (tags "QFN 0.5")
    (attr smd)
    (fp_text reference U1 (at 0 -3.75 315) (layer F.SilkS) hide)
    (fp_text value ATMEGA328A-MU (at 0 3.75 315) (layer F.Fab))
    (pad 1 smd rect (at -2.4 -1.75 315) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 16 /LED_SEG_F))
    (pad 2 smd rect (at -2.4 -1.25 315) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 14 /LED_SEG_DP))
    (pad 3 smd rect (at -2.4 -0.75 315) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -2.4 -0.25 315) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 5 smd rect (at -2.4 0.25 315) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at -2.4 0.75 315) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 7 smd rect (at -2.4 1.25 315) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 21 /LED_DIG_3))
    (pad 8 smd rect (at -2.4 1.75 315) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 20 /LED_DIG_2))
    (pad 9 smd rect (at -1.75 2.4 45) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 22 /LED_SEG_C))
    (pad 10 smd rect (at -1.25 2.4 45) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 10 /LED_SEG_G))
    (pad 11 smd rect (at -0.75 2.4 45) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 19 /LED_SEG_B))
    (pad 12 smd rect (at -0.25 2.4 45) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 8 /LED_DIG_1))
    (pad 13 smd rect (at 0.25 2.4 45) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 9 /TRIAC_DRIVE))
    (pad 14 smd rect (at 0.75 2.4 45) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 12 /BUTTON_2))
    (pad 15 smd rect (at 1.25 2.4 45) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 6 /ICSP_MOSI))
    (pad 16 smd rect (at 1.75 2.4 45) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 /REED_SW))
    (pad 17 smd rect (at 2.4 1.75 315) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 /BUTTON_1))
    (pad 18 smd rect (at 2.4 1.25 315) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 19 smd rect (at 2.4 0.75 315) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(U1-Pad19)"))
    (pad 20 smd rect (at 2.4 0.25 315) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 21 smd rect (at 2.4 -0.25 315) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 22 smd rect (at 2.4 -0.75 315) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(U1-Pad22)"))
    (pad 23 smd rect (at 2.4 -1.25 315) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 18 /TEMP_ADC))
    (pad 24 smd rect (at 2.4 -1.75 315) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(U1-Pad24)"))
    (pad 25 smd rect (at 1.75 -2.4 45) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(U1-Pad25)"))
    (pad 26 smd rect (at 1.25 -2.4 45) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 13 /FAN_DRIVE))
    (pad 27 smd rect (at 0.75 -2.4 45) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 30 /FAN_CURR_ADC))
    (pad 28 smd rect (at 0.25 -2.4 45) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 28 /FAN_VOLT))
    (pad 29 smd rect (at -0.25 -2.4 45) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 7 /ICSP_RST))
    (pad 30 smd rect (at -0.75 -2.4 45) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 17 /LED_SEG_A))
    (pad 31 smd rect (at -1.25 -2.4 45) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 15 /LED_SEG_E))
    (pad 32 smd rect (at -1.75 -2.4 45) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 11 /LED_SEG_D))
    (pad 33 smd rect (at 0.8625 0.8625 315) (size 1.725 1.725) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 33 smd rect (at 0.8625 -0.8625 315) (size 1.725 1.725) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 33 smd rect (at -0.8625 0.8625 315) (size 1.725 1.725) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 33 smd rect (at -0.8625 -0.8625 315) (size 1.725 1.725) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (model ${KISYS3DMOD}/Housings_DFN_QFN.3dshapes/QFN-32-1EP_5x5mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 59F719A0)
    (at 142.433 108.712 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 0 -1.3335 180) (layer F.SilkS))
    (fp_text value C_Small (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 59F719BE)
    (at 152.928 107.188)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at -0.02 1.7145) (layer F.SilkS))
    (fp_text value C_Small (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 59F719B0)
    (at 142.433 98.679)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at -2.987 0.0635) (layer F.SilkS))
    (fp_text value C_Small (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 -1.25) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module AC_Custom:TSM-110-XX-XXX-SV (layer B.Cu) (tedit 59F6F057)
    (at 149.5 107.62 180)
    (fp_text reference J2 (at -1.27 -4.445 180) (layer B.SilkS) hide)
    (fp_text value CONN_01X10 (at -8.75 -4.521 180) (layer B.Fab) hide)
    (pad 1 smd rect (at 10.16 -1.46 180) (size 1.27 3.43) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 7.62 1.46 180) (size 1.27 3.43) (layers B.Cu B.Paste B.Mask)
      (net 8 /LED_DIG_1))
    (pad 3 smd rect (at 5.08 -1.46 180) (size 1.27 3.43) (layers B.Cu B.Paste B.Mask)
      (net 9 /TRIAC_DRIVE))
    (pad 4 smd rect (at 2.54 1.46 180) (size 1.27 3.43) (layers B.Cu B.Paste B.Mask)
      (net 4 /REED_SW))
    (pad 5 smd rect (at 0 -1.46 180) (size 1.27 3.43) (layers B.Cu B.Paste B.Mask)
      (net 10 /LED_SEG_G))
    (pad 6 smd rect (at -2.54 1.46 180) (size 1.27 3.43) (layers B.Cu B.Paste B.Mask)
      (net 11 /LED_SEG_D))
    (pad 7 smd rect (at -5.08 -1.46 180) (size 1.27 3.43) (layers B.Cu B.Paste B.Mask)
      (net 5 /BUTTON_1))
    (pad 8 smd rect (at -7.62 1.46 180) (size 1.27 3.43) (layers B.Cu B.Paste B.Mask)
      (net 12 /BUTTON_2))
    (pad 9 smd rect (at -10.16 -1.46 180) (size 1.27 3.43) (layers B.Cu B.Paste B.Mask)
      (net 13 /FAN_DRIVE))
    (pad 10 smd rect (at -12.7 1.46 180) (size 1.27 3.43) (layers B.Cu B.Paste B.Mask)
      (net 27 /FAN_CURR))
    (model "C:/Users/andrew.cowan/Dropbox/Backup/Projects/2017.10.29   858D+ Hot Air Upgrade/Adapter PCB/3D models/TSM-110-01-S-SV.wrl"
      (at (xyz -0.05 0 0.048))
      (scale (xyz 0.393 0.393 0.393))
      (rotate (xyz 270 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 59F71997)
    (at 148.082 107.569)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 0.0635 1.4605) (layer F.SilkS))
    (fp_text value R (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 59F719CD)
    (at 160.528 110.236)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at -2.9845 0.0635) (layer F.SilkS))
    (fp_text value C_Small (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 -1.25) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 30 /FAN_CURR_ADC))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 59F719C8)
    (at 160.528 108.966 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 2.921 0 180) (layer F.SilkS))
    (fp_text value R (at 0 1.55 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 27 /FAN_CURR))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 30 /FAN_CURR_ADC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module AC_Custom:TSM-103-XX-XXXX-DV (layer F.Cu) (tedit 59F6F047)
    (at 159.347 103.816 180)
    (fp_text reference J1 (at -0.762 5.588 180) (layer F.SilkS) hide)
    (fp_text value CONN_02X03 (at -0.254 -6.35 180) (layer F.Fab))
    (pad 1 smd rect (at 2.54 -2.47 180) (size 1.27 3.68) (layers F.Cu F.Paste F.Mask)
      (net 4 /REED_SW))
    (pad 2 smd rect (at 2.54 2.47 180) (size 1.27 3.68) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 3 smd rect (at 0 -2.47 180) (size 1.27 3.68) (layers F.Cu F.Paste F.Mask)
      (net 5 /BUTTON_1))
    (pad 4 smd rect (at 0 2.47 180) (size 1.27 3.68) (layers F.Cu F.Paste F.Mask)
      (net 6 /ICSP_MOSI))
    (pad 5 smd rect (at -2.54 -2.47 180) (size 1.27 3.68) (layers F.Cu F.Paste F.Mask)
      (net 7 /ICSP_RST))
    (pad 6 smd rect (at -2.54 2.47 180) (size 1.27 3.68) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model "C:/Users/andrew.cowan/Dropbox/Backup/Projects/2017.10.29   858D+ Hot Air Upgrade/Adapter PCB/3D models/TSM-103-01-S-DV.wrl"
      (at (xyz 0 0 0.1))
      (scale (xyz 0.393 0.393 0.393))
      (rotate (xyz 270 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 59F7193E)
    (at 148.082 106.172)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at -0.0635 -1.27) (layer F.SilkS))
    (fp_text value R (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 28 /FAN_VOLT))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(R3-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 59F71937)
    (at 148.039 101.473 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 0 -1.45 180) (layer F.SilkS))
    (fp_text value R (at 0 1.55 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 28 /FAN_VOLT))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "858D+ Mod" (at 149.987 99.695) (layer F.SilkS))
  (gr_text "Cowan, Oct 17" (at 150.1775 97.3455) (layer F.SilkS))
  (gr_arc (start 162.814 110.744) (end 163.449 110.744) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_arc (start 162.814 96.901) (end 162.814 96.266) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_arc (start 138.684 96.901) (end 138.049 96.901) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_arc (start 138.684 110.744) (end 138.684 111.379) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_text ICSP (at 159.766 98.3615) (layer F.SilkS))
  (gr_line (start 162.814 96.266) (end 138.684 96.266) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 163.449 110.744) (end 163.449 96.901) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 138.684 111.379) (end 162.814 111.379) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 138.049 96.901) (end 138.049 110.744) (layer Edge.Cuts) (width 0.0254))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2032))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 138.684 96.901) (xy 162.814 96.901) (xy 162.814 110.744) (xy 138.684 110.744)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2032))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 138.684 96.901) (xy 162.814 96.901) (xy 162.814 110.744) (xy 138.684 110.744)
      )
    )
  )
)
