(kicad_pcb (version 20171130) (host pcbnew "(5.1.6)-1")
  (general
    (thickness 1.6)
    (drawings 24)
    (tracks 160)
    (zones 0)
    (modules 18)
    (nets 67)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.1524)
    (user_trace_width 0.3048)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.508)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +12V)
  (net 3 +3.3V)
  (net 4 "Net-(F1-Pad1)")
  (net 5 "Net-(J1-Pad3)")
  (net 6 LED_B)
  (net 7 LED_G)
  (net 8 LED_R)
  (net 9 RX)
  (net 10 TX)
  (net 11 GPIO_R)
  (net 12 GPIO_G)
  (net 13 GPIO_B)
  (net 14 RST)
  (net 15 "Net-(SW2-Pad2)")
  (net 16 "Net-(SW2-Pad1)")
  (net 17 "Net-(U1-Pad37)")
  (net 18 "Net-(U1-Pad36)")
  (net 19 "Net-(U1-Pad33)")
  (net 20 "Net-(U1-Pad32)")
  (net 21 "Net-(U1-Pad31)")
  (net 22 "Net-(U1-Pad30)")
  (net 23 "Net-(U1-Pad29)")
  (net 24 "Net-(U1-Pad28)")
  (net 25 "Net-(U1-Pad27)")
  (net 26 "Net-(U1-Pad26)")
  (net 27 "Net-(U1-Pad24)")
  (net 28 "Net-(U1-Pad23)")
  (net 29 "Net-(U1-Pad22)")
  (net 30 "Net-(U1-Pad21)")
  (net 31 "Net-(U1-Pad20)")
  (net 32 "Net-(U1-Pad19)")
  (net 33 "Net-(U1-Pad18)")
  (net 34 "Net-(U1-Pad17)")
  (net 35 "Net-(U1-Pad12)")
  (net 36 "Net-(U1-Pad11)")
  (net 37 "Net-(U1-Pad10)")
  (net 38 "Net-(U1-Pad9)")
  (net 39 "Net-(U1-Pad8)")
  (net 40 "Net-(U1-Pad7)")
  (net 41 "Net-(U1-Pad6)")
  (net 42 "Net-(U1-Pad5)")
  (net 43 "Net-(U1-Pad4)")
  (net 44 VCC_USB)
  (net 45 "Net-(FB1-Pad1)")
  (net 46 "Net-(J3-Pad6)")
  (net 47 "Net-(J3-Pad4)")
  (net 48 D+)
  (net 49 D-)
  (net 50 "Net-(SW1-Pad4)")
  (net 51 "Net-(SW1-Pad2)")
  (net 52 "Net-(U3-Pad28)")
  (net 53 "Net-(U3-Pad27)")
  (net 54 "Net-(U3-Pad23)")
  (net 55 "Net-(U3-Pad22)")
  (net 56 "Net-(U3-Pad19)")
  (net 57 "Net-(U3-Pad14)")
  (net 58 "Net-(U3-Pad13)")
  (net 59 "Net-(U3-Pad12)")
  (net 60 "Net-(U3-Pad11)")
  (net 61 "Net-(U3-Pad10)")
  (net 62 "Net-(U3-Pad9)")
  (net 63 "Net-(U3-Pad6)")
  (net 64 "Net-(U3-Pad3)")
  (net 65 "Net-(U3-Pad2)")
  (net 66 "Net-(C4-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
    (diff_pair_width 0.1778)
    (diff_pair_gap 0.254)
    (add_net +12V)
    (add_net +3.3V)
    (add_net D+)
    (add_net D-)
    (add_net GND)
    (add_net GPIO_B)
    (add_net GPIO_G)
    (add_net GPIO_R)
    (add_net LED_B)
    (add_net LED_G)
    (add_net LED_R)
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(F1-Pad1)")
    (add_net "Net-(FB1-Pad1)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J3-Pad4)")
    (add_net "Net-(J3-Pad6)")
    (add_net "Net-(SW1-Pad2)")
    (add_net "Net-(SW1-Pad4)")
    (add_net "Net-(SW2-Pad1)")
    (add_net "Net-(SW2-Pad2)")
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad11)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U1-Pad17)")
    (add_net "Net-(U1-Pad18)")
    (add_net "Net-(U1-Pad19)")
    (add_net "Net-(U1-Pad20)")
    (add_net "Net-(U1-Pad21)")
    (add_net "Net-(U1-Pad22)")
    (add_net "Net-(U1-Pad23)")
    (add_net "Net-(U1-Pad24)")
    (add_net "Net-(U1-Pad26)")
    (add_net "Net-(U1-Pad27)")
    (add_net "Net-(U1-Pad28)")
    (add_net "Net-(U1-Pad29)")
    (add_net "Net-(U1-Pad30)")
    (add_net "Net-(U1-Pad31)")
    (add_net "Net-(U1-Pad32)")
    (add_net "Net-(U1-Pad33)")
    (add_net "Net-(U1-Pad36)")
    (add_net "Net-(U1-Pad37)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(U1-Pad8)")
    (add_net "Net-(U1-Pad9)")
    (add_net "Net-(U3-Pad10)")
    (add_net "Net-(U3-Pad11)")
    (add_net "Net-(U3-Pad12)")
    (add_net "Net-(U3-Pad13)")
    (add_net "Net-(U3-Pad14)")
    (add_net "Net-(U3-Pad19)")
    (add_net "Net-(U3-Pad2)")
    (add_net "Net-(U3-Pad22)")
    (add_net "Net-(U3-Pad23)")
    (add_net "Net-(U3-Pad27)")
    (add_net "Net-(U3-Pad28)")
    (add_net "Net-(U3-Pad3)")
    (add_net "Net-(U3-Pad6)")
    (add_net "Net-(U3-Pad9)")
    (add_net RST)
    (add_net RX)
    (add_net TX)
    (add_net VCC_USB)
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 102.4105 110.363)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at 2.6185 0 90) (layer F.SilkS))
    (fp_text value 10nF (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 66 "Net-(C4-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module led_strip_controller:F0603E2R00FSTR (layer F.Cu) (tedit 0)
    (at 55.245 118.618 90)
    (fp_text reference F1 (at -2.5019 0 180) (layer F.SilkS))
    (fp_text value "Fuse (2A)" (at 0.8001 -0.889 90) (layer F.SilkS) hide)
    (fp_text user 0.029in/0.737mm (at 0 3.5306 90) (layer Dwgs.User))
    (fp_text user 0.097in/2.464mm (at 0 -3.5306 90) (layer Dwgs.User))
    (fp_text user 0.038in/0.965mm (at 3.9243 0 90) (layer Dwgs.User))
    (fp_text user * (at 0 0 90) (layer F.Fab))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0 90) (layer Cmts.User))
    (pad 2 smd rect (at 0.8001 0 90) (size 0.8636 0.9652) (layers F.Cu F.Paste F.Mask)
      (net 2 +12V))
    (pad 1 smd rect (at -0.8001 0 90) (size 0.8636 0.9652) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(F1-Pad1)"))
  )
  (module Package_SO:SSOP-28_5.3x10.2mm_P0.65mm (layer F.Cu) (tedit 5A02F25C)
    (at 94.996 116.078)
    (descr "28-Lead Plastic Shrink Small Outline (SS)-5.30 mm Body [SSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U3 (at -0.381 6.477) (layer F.SilkS))
    (fp_text value FT232RL (at 0 6.25) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 28 smd rect (at 3.6 -4.225) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(U3-Pad28)"))
    (pad 27 smd rect (at 3.6 -3.575) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(U3-Pad27)"))
    (pad 26 smd rect (at 3.6 -2.925) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 25 smd rect (at 3.6 -2.275) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 24 smd rect (at 3.6 -1.625) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask))
    (pad 23 smd rect (at 3.6 -0.975) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(U3-Pad23)"))
    (pad 22 smd rect (at 3.6 -0.325) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(U3-Pad22)"))
    (pad 21 smd rect (at 3.6 0.325) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 20 smd rect (at 3.6 0.975) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(FB1-Pad1)"))
    (pad 19 smd rect (at 3.6 1.625) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(U3-Pad19)"))
    (pad 18 smd rect (at 3.6 2.275) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 17 smd rect (at 3.6 2.925) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(C4-Pad1)"))
    (pad 16 smd rect (at 3.6 3.575) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 49 D-))
    (pad 15 smd rect (at 3.6 4.225) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 48 D+))
    (pad 14 smd rect (at -3.6 4.225) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(U3-Pad14)"))
    (pad 13 smd rect (at -3.6 3.575) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(U3-Pad13)"))
    (pad 12 smd rect (at -3.6 2.925) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(U3-Pad12)"))
    (pad 11 smd rect (at -3.6 2.275) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(U3-Pad11)"))
    (pad 10 smd rect (at -3.6 1.625) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(U3-Pad10)"))
    (pad 9 smd rect (at -3.6 0.975) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(U3-Pad9)"))
    (pad 8 smd rect (at -3.6 0.325) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at -3.6 -0.325) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -3.6 -0.975) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(U3-Pad6)"))
    (pad 5 smd rect (at -3.6 -1.625) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 10 TX))
    (pad 4 smd rect (at -3.6 -2.275) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(C4-Pad1)"))
    (pad 3 smd rect (at -3.6 -2.925) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(U3-Pad3)"))
    (pad 2 smd rect (at -3.6 -3.575) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(U3-Pad2)"))
    (pad 1 smd rect (at -3.6 -4.225) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 9 RX))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SSOP-28_5.3x10.2mm_P0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module led_strip_controller:10118192-0002LF (layer F.Cu) (tedit 0)
    (at 103.378 104.902 180)
    (fp_text reference J3 (at 5.969 -4.191) (layer F.SilkS) hide)
    (fp_text value USB_B_Micro (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text user * (at 0 0) (layer F.Fab))
    (fp_text user * (at 6.096 -2.667) (layer F.SilkS) hide)
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
    (pad 11 smd rect (at 1.2 0.471101 270) (size 1.905 1.905) (layers F.Cu F.Paste F.Mask))
    (pad 10 smd rect (at -1.2 0.471101 270) (size 1.905 1.905) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at 3.8 0.471101 270) (size 1.8034 1.905) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at -3.8 0.471101 270) (size 1.8034 1.905) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at 3.099999 -2.078899 270) (size 2.1082 1.6002) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at -3.099999 -2.078899 270) (size 2.1082 1.6002) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(J3-Pad6)"))
    (pad 5 smd rect (at 1.3 -2.2039 180) (size 0.4064 1.3462) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0.649999 -2.2039 180) (size 0.4064 1.3462) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(J3-Pad4)"))
    (pad 3 smd rect (at 0 -2.2039 180) (size 0.4064 1.3462) (layers F.Cu F.Paste F.Mask)
      (net 48 D+))
    (pad 2 smd rect (at -0.649999 -2.2039 180) (size 0.4064 1.3462) (layers F.Cu F.Paste F.Mask)
      (net 49 D-))
    (pad 1 smd rect (at -1.3 -2.2039 180) (size 0.4064 1.3462) (layers F.Cu F.Paste F.Mask)
      (net 44 VCC_USB))
  )
  (module led_strip_controller:MH2029-400Y (layer F.Cu) (tedit 0)
    (at 91.44 108.331)
    (fp_text reference FB1 (at 2.667 -0.127 90) (layer F.SilkS))
    (fp_text value Ferrite_Bead (at 7.874 -11.049) (layer F.SilkS) hide)
    (fp_text user 0.04in/1.016mm (at 0 -3.7465) (layer Dwgs.User))
    (fp_text user 0.12in/3.048mm (at 0 3.7465) (layer Dwgs.User))
    (fp_text user 0.04in/1.016mm (at 3.556 0) (layer Dwgs.User))
    (fp_text user * (at 0 0) (layer F.Fab))
    (fp_text user * (at 0 0) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
    (pad 2 smd rect (at 1.016 0) (size 1.016 1.016) (layers F.Cu F.Paste F.Mask)
      (net 44 VCC_USB))
    (pad 1 smd rect (at -1.016 0) (size 1.016 1.016) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(FB1-Pad1)"))
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 91.44 105.791 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at -2.667 -0.127 270) (layer F.SilkS))
    (fp_text value 10nF (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 44 VCC_USB))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RF_Module:ESP32-WROOM-32 (layer F.Cu) (tedit 5B5B4654)
    (at 79.232 113.785)
    (descr "Single 2.4 GHz Wi-Fi and Bluetooth combo chip https://www.espressif.com/sites/default/files/documentation/esp32-wroom-32_datasheet_en.pdf")
    (tags "Single 2.4 GHz Wi-Fi and Bluetooth combo  chip")
    (attr smd)
    (fp_text reference U1 (at 7.89 11.183 180) (layer F.SilkS))
    (fp_text value ESP32-WROOM-32D (at 0 11.5) (layer F.Fab))
    (fp_text user "5 mm" (at 7.8 -19.075 90) (layer Cmts.User))
    (fp_text user "5 mm" (at -11.2 -14.375) (layer Cmts.User))
    (fp_text user "5 mm" (at 11.8 -14.375) (layer Cmts.User))
    (fp_text user Antenna (at 0 -13) (layer Cmts.User))
    (fp_text user "KEEP-OUT ZONE" (at 0 -19) (layer Cmts.User))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 38 smd rect (at 8.5 -8.255) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 37 smd rect (at 8.5 -6.985) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(U1-Pad37)"))
    (pad 36 smd rect (at 8.5 -5.715) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(U1-Pad36)"))
    (pad 35 smd rect (at 8.5 -4.445) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 TX))
    (pad 34 smd rect (at 8.5 -3.175) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 RX))
    (pad 33 smd rect (at 8.5 -1.905) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(U1-Pad33)"))
    (pad 32 smd rect (at 8.5 -0.635) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(U1-Pad32)"))
    (pad 31 smd rect (at 8.5 0.635) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(U1-Pad31)"))
    (pad 30 smd rect (at 8.5 1.905) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(U1-Pad30)"))
    (pad 29 smd rect (at 8.5 3.175) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(U1-Pad29)"))
    (pad 28 smd rect (at 8.5 4.445) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(U1-Pad28)"))
    (pad 27 smd rect (at 8.5 5.715) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(U1-Pad27)"))
    (pad 26 smd rect (at 8.5 6.985) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(U1-Pad26)"))
    (pad 25 smd rect (at 8.5 8.255) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(SW2-Pad2)"))
    (pad 24 smd rect (at 5.715 9.255 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(U1-Pad24)"))
    (pad 23 smd rect (at 4.445 9.255 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(U1-Pad23)"))
    (pad 22 smd rect (at 3.175 9.255 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(U1-Pad22)"))
    (pad 21 smd rect (at 1.905 9.255 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(U1-Pad21)"))
    (pad 20 smd rect (at 0.635 9.255 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(U1-Pad20)"))
    (pad 19 smd rect (at -0.635 9.255 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(U1-Pad19)"))
    (pad 18 smd rect (at -1.905 9.255 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(U1-Pad18)"))
    (pad 17 smd rect (at -3.175 9.255 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(U1-Pad17)"))
    (pad 16 smd rect (at -4.445 9.255 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 12 GPIO_G))
    (pad 15 smd rect (at -5.715 9.255 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 14 smd rect (at -8.5 8.255) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 GPIO_R))
    (pad 13 smd rect (at -8.5 6.985) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 GPIO_B))
    (pad 12 smd rect (at -8.5 5.715) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(U1-Pad12)"))
    (pad 11 smd rect (at -8.5 4.445) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(U1-Pad11)"))
    (pad 10 smd rect (at -8.5 3.175) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(U1-Pad10)"))
    (pad 9 smd rect (at -8.5 1.905) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(U1-Pad9)"))
    (pad 8 smd rect (at -8.5 0.635) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(U1-Pad8)"))
    (pad 7 smd rect (at -8.5 -0.635) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(U1-Pad7)"))
    (pad 6 smd rect (at -8.5 -1.905) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(U1-Pad6)"))
    (pad 5 smd rect (at -8.5 -3.175) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(U1-Pad5)"))
    (pad 4 smd rect (at -8.5 -4.445) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(U1-Pad4)"))
    (pad 3 smd rect (at -8.5 -5.715) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 RST))
    (pad 2 smd rect (at -8.5 -6.985) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 +3.3V))
    (pad 1 smd rect (at -8.5 -8.255) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 39 smd rect (at -1 -0.755) (size 5 5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/RF_Module.3dshapes/ESP32-WROOM-32.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 5A19A429)
    (at 107.315 131.826 180)
    (descr "Through hole straight socket strip, 1x04, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x04 2.54mm single row")
    (fp_text reference J2 (at 0.127 -2.286) (layer F.SilkS))
    (fp_text value Conn_01x04_Female (at 0 10.39) (layer F.Fab))
    (fp_text user %R (at 0 3.81 90) (layer F.Fab))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 LED_B))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 LED_R))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 LED_G))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +12V))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:TO-252-3_TabPin2 (layer F.Cu) (tedit 5A70F30B)
    (at 62.611 118.745 180)
    (descr "TO-252 / DPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO252/PG-TO252-3-1/")
    (tags "DPAK TO-252 DPAK-3 TO-252-3 SOT-428")
    (attr smd)
    (fp_text reference U2 (at 0.508 4.191) (layer F.SilkS))
    (fp_text value IFX27001TFV33 (at 0 4.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad "" smd rect (at 0.425 1.525 180) (size 3.05 2.75) (layers F.Paste))
    (pad "" smd rect (at 3.775 -1.525 180) (size 3.05 2.75) (layers F.Paste))
    (pad "" smd rect (at 0.425 -1.525 180) (size 3.05 2.75) (layers F.Paste))
    (pad "" smd rect (at 3.775 1.525 180) (size 3.05 2.75) (layers F.Paste))
    (pad 2 smd rect (at 2.1 0 180) (size 6.4 5.8) (layers F.Cu F.Mask)
      (net 3 +3.3V))
    (pad 3 smd rect (at -4.2 2.28 180) (size 2.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 +12V))
    (pad 2 smd rect (at -4.2 0 180) (size 2.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 3 +3.3V))
    (pad 1 smd rect (at -4.2 -2.28 180) (size 2.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/TO-252-3_TabPin2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module led_strip_controller:SW_DPDT_CK_JS202011SCQN (layer F.Cu) (tedit 5ED9E74F)
    (at 105.537 116.586 90)
    (descr "Sub-miniature slide switch, vertical, SMT J bend https://dznh3ojzb2azq.cloudfront.net/products/Slide/JS/documents/datasheet.pdf")
    (tags "switch DPDT SMT")
    (attr smd)
    (fp_text reference SW2 (at -5.588 -0.889 180) (layer F.SilkS))
    (fp_text value SW_PROG (at 0 5.08 90) (layer F.Fab))
    (fp_text user %R (at 0 -7.62 90) (layer F.Fab))
    (pad 3 smd rect (at 2.5 -2.75 90) (size 1.2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0 -2.75 90) (size 1.2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(SW2-Pad2)"))
    (pad 1 smd rect (at -2.5 -2.75 90) (size 1.2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(SW2-Pad1)"))
    (pad 6 smd rect (at 2.5 2.75 90) (size 1.2 2.5) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 0 2.75 90) (size 1.2 2.5) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at -2.5 2.75 90) (size 1.2 2.5) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_DPDT_CK_JS202011JCQN.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_SMD:SW_SPST_Omron_B3FS-101xP (layer F.Cu) (tedit 5E6E8E39)
    (at 57.15 108.712 270)
    (descr "Surface Mount Tactile Switch for High-Density Mounting, 4.3mm height, https://omronfs.omron.com/en_US/ecb/products/pdf/en-b3fs.pdf")
    (tags "Tactile Switch")
    (attr smd)
    (fp_text reference SW1 (at 0 -4.3 90) (layer F.SilkS))
    (fp_text value SW_RST (at 0 4.2 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.2 90) (layer F.Fab))
    (pad 3 smd rect (at -4 2.25 90) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 4 2.25 90) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(SW1-Pad4)"))
    (pad 1 smd rect (at -4 -2.25 90) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 14 RST))
    (pad 2 smd rect (at 4 -2.25 90) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(SW1-Pad2)"))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_Omron_B3FS-101xP.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 64.389 106.934 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at -2.286 0.127 90) (layer F.SilkS))
    (fp_text value 10K (at 0 1.905) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 RST))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3.3V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module led_strip_controller:TO-252-2 (layer F.Cu) (tedit 5ED9EF67)
    (at 75.219 129.539)
    (descr "TO-252 / DPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO252/PG-TO252-3-1/")
    (tags "DPAK TO-252 DPAK-3 TO-252-3 SOT-428")
    (attr smd)
    (fp_text reference Q3 (at -0.035 4.827) (layer F.SilkS))
    (fp_text value Q_NPN_BCE (at 0 4.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad "" smd rect (at 0.425 1.525) (size 3.05 2.75) (layers F.Paste))
    (pad "" smd rect (at 3.775 -1.525) (size 3.05 2.75) (layers F.Paste))
    (pad "" smd rect (at 0.425 -1.525) (size 3.05 2.75) (layers F.Paste))
    (pad "" smd rect (at 3.775 1.525) (size 3.05 2.75) (layers F.Paste))
    (pad 2 smd rect (at 2.1 0) (size 6.4 5.8) (layers F.Cu F.Mask)
      (net 6 LED_B))
    (pad 3 smd rect (at -4.2 2.286) (size 2.6 1.06) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -4.2 -2.286) (size 2.6 1.06) (layers F.Cu F.Paste F.Mask)
      (net 13 GPIO_B))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/TO-252-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module led_strip_controller:TO-252-2 (layer F.Cu) (tedit 5ED9EF67)
    (at 99.095 129.541)
    (descr "TO-252 / DPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO252/PG-TO252-3-1/")
    (tags "DPAK TO-252 DPAK-3 TO-252-3 SOT-428")
    (attr smd)
    (fp_text reference Q2 (at 0.219 4.444) (layer F.SilkS))
    (fp_text value Q_NPN_BCE (at 0 4.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad "" smd rect (at 0.425 1.525) (size 3.05 2.75) (layers F.Paste))
    (pad "" smd rect (at 3.775 -1.525) (size 3.05 2.75) (layers F.Paste))
    (pad "" smd rect (at 0.425 -1.525) (size 3.05 2.75) (layers F.Paste))
    (pad "" smd rect (at 3.775 1.525) (size 3.05 2.75) (layers F.Paste))
    (pad 2 smd rect (at 2.1 0) (size 6.4 5.8) (layers F.Cu F.Mask)
      (net 7 LED_G))
    (pad 3 smd rect (at -4.2 2.286) (size 2.6 1.06) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -4.2 -2.286) (size 2.6 1.06) (layers F.Cu F.Paste F.Mask)
      (net 12 GPIO_G))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/TO-252-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module led_strip_controller:TO-252-2 (layer F.Cu) (tedit 5ED9EF67)
    (at 87.157 129.541)
    (descr "TO-252 / DPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO252/PG-TO252-3-1/")
    (tags "DPAK TO-252 DPAK-3 TO-252-3 SOT-428")
    (attr smd)
    (fp_text reference Q1 (at 0.092 4.698) (layer F.SilkS))
    (fp_text value Q_NPN_BCE (at 0 4.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad "" smd rect (at 0.425 1.525) (size 3.05 2.75) (layers F.Paste))
    (pad "" smd rect (at 3.775 -1.525) (size 3.05 2.75) (layers F.Paste))
    (pad "" smd rect (at 0.425 -1.525) (size 3.05 2.75) (layers F.Paste))
    (pad "" smd rect (at 3.775 1.525) (size 3.05 2.75) (layers F.Paste))
    (pad 2 smd rect (at 2.1 0) (size 6.4 5.8) (layers F.Cu F.Mask)
      (net 8 LED_R))
    (pad 3 smd rect (at -4.2 2.286) (size 2.6 1.06) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -4.2 -2.286) (size 2.6 1.06) (layers F.Cu F.Paste F.Mask)
      (net 11 GPIO_R))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/TO-252-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module led_strip_controller:BarrelJack_CUI-PJ002AH (layer F.Cu) (tedit 5ED9FF1E)
    (at 67.31 129.54 270)
    (descr "Wuerth electronics barrel jack connector (5.5mm outher diameter, inner diameter 2.05mm or 2.55mm depending on exact order number), See: http://katalog.we-online.de/em/datasheet/6941xx301002.pdf")
    (tags "connector barrel jack")
    (fp_text reference J1 (at 5.08 -2.54 180) (layer F.SilkS))
    (fp_text value Barrel_Jack_Switch (at 0 15.24 90) (layer F.Fab))
    (fp_text user %R (at 0 7.5 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 3.5 1) (drill oval 3.1 0.37) (layers *.Cu *.Mask)
      (net 4 "Net-(F1-Pad1)"))
    (pad 2 thru_hole oval (at 0 6 270) (size 3.5 1) (drill oval 3.1 0.26) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 4.7 3) (size 4 1.8) (drill oval 3 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad3)"))
    (model ${KISYS3DMOD}/Connector_BarrelJack.3dshapes/BarrelJack_Wuerth_6941xx301002.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 64.389 108.966 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at -2.413 -0.127 90) (layer F.SilkS))
    (fp_text value 22uF (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3.3V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 64.389 111.252 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at -2.4615 0 90) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 +12V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Instructions:\n\n1. Attach a 12V, center-positive power supply with at\n   least 600mA (1A preferred)\n2. Switch up the PROG switch (to programming mode)\n3. Attach a Micro USB cable to a computer\n4. Write code to control the LEDs:\n\n      R - GPIO12\n      G - GPIO13\n      B - GPIO14\n\n5. Flash the ESP32 and turn off the PROG switch\n6. Attach the LED strip.\n7. Rejoice!" (at 102.87 118.745) (layer B.SilkS))
  (gr_text "LED Controller v1.2\ngithub.com/roytu" (at 61.849 123.317) (layer F.SilkS))
  (gr_text "2 Amps" (at 55.372 116.459) (layer F.SilkS))
  (gr_text PROG (at 108.839 111.125) (layer F.SilkS))
  (gr_text +12V (at 101.346 124.46) (layer F.SilkS))
  (gr_text LED_G (at 101.346 123.317) (layer F.SilkS))
  (gr_text LED_R (at 101.346 122.174) (layer F.SilkS))
  (gr_text LED_B (at 101.346 121.031) (layer F.SilkS))
  (dimension 58.42 (width 0.15) (layer Dwgs.User)
    (gr_text "2.3000 in" (at 82.55 144.81) (layer Dwgs.User))
    (feature1 (pts (xy 111.76 143.51) (xy 111.76 144.096421)))
    (feature2 (pts (xy 53.34 143.51) (xy 53.34 144.096421)))
    (crossbar (pts (xy 53.34 143.51) (xy 111.76 143.51)))
    (arrow1a (pts (xy 111.76 143.51) (xy 110.633496 144.096421)))
    (arrow1b (pts (xy 111.76 143.51) (xy 110.633496 142.923579)))
    (arrow2a (pts (xy 53.34 143.51) (xy 54.466504 144.096421)))
    (arrow2b (pts (xy 53.34 143.51) (xy 54.466504 142.923579)))
  )
  (dimension 33.02 (width 0.15) (layer Dwgs.User)
    (gr_text "1.3 in" (at 43.21 119.38 90) (layer Dwgs.User))
    (feature1 (pts (xy 41.91 102.87) (xy 42.496421 102.87)))
    (feature2 (pts (xy 41.91 135.89) (xy 42.496421 135.89)))
    (crossbar (pts (xy 41.91 135.89) (xy 41.91 102.87)))
    (arrow1a (pts (xy 41.91 102.87) (xy 42.496421 103.996504)))
    (arrow1b (pts (xy 41.91 102.87) (xy 41.323579 103.996504)))
    (arrow2a (pts (xy 41.91 135.89) (xy 42.496421 134.763496)))
    (arrow2b (pts (xy 41.91 135.89) (xy 41.323579 134.763496)))
  )
  (dimension 35.56 (width 0.15) (layer Dwgs.User)
    (gr_text "1.4 in" (at 45.69 120.65 270) (layer Dwgs.User))
    (feature1 (pts (xy 46.99 138.43) (xy 46.403579 138.43)))
    (feature2 (pts (xy 46.99 102.87) (xy 46.403579 102.87)))
    (crossbar (pts (xy 46.99 102.87) (xy 46.99 138.43)))
    (arrow1a (pts (xy 46.99 138.43) (xy 46.403579 137.303496)))
    (arrow1b (pts (xy 46.99 138.43) (xy 47.576421 137.303496)))
    (arrow2a (pts (xy 46.99 102.87) (xy 46.403579 103.996504)))
    (arrow2b (pts (xy 46.99 102.87) (xy 47.576421 103.996504)))
  )
  (dimension 59.69 (width 0.15) (layer Dwgs.User)
    (gr_text "2.35 in" (at 81.915 139.67) (layer Dwgs.User))
    (feature1 (pts (xy 52.07 140.97) (xy 52.07 140.383579)))
    (feature2 (pts (xy 111.76 140.97) (xy 111.76 140.383579)))
    (crossbar (pts (xy 111.76 140.97) (xy 52.07 140.97)))
    (arrow1a (pts (xy 52.07 140.97) (xy 53.196504 140.383579)))
    (arrow1b (pts (xy 52.07 140.97) (xy 53.196504 141.556421)))
    (arrow2a (pts (xy 111.76 140.97) (xy 110.633496 140.383579)))
    (arrow2b (pts (xy 111.76 140.97) (xy 110.633496 141.556421)))
  )
  (gr_line (start 53.34 135.89) (end 53.34 102.87) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 110.49 135.89) (end 53.34 135.89) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 110.49 102.87) (end 110.49 135.89) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 53.34 102.87) (end 110.49 102.87) (layer Edge.Cuts) (width 0.05))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 110.500573 135.89) (xy 53.350573 135.89) (xy 53.350573 102.87) (xy 110.500573 102.87)
      )
    )
  )
)
