(kicad_pcb (version 20171130) (host pcbnew "(5.0.0)")
  (general
    (thickness 1.6)
    (drawings 26)
    (tracks 84)
    (zones 0)
    (modules 19)
    (nets 7)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.5)
    (user_trace_width 0.5)
    (user_trace_width 0.75)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 "Net-(C2-Pad1)")
  (net 3 "Net-(C3-Pad1)")
  (net 4 "Net-(C4-Pad1)")
  (net 5 "Net-(C5-Pad1)")
  (net 6 "Net-(C6-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C6-Pad1)")
  )
  (module azure-test:Mill-Max_1.83_D0.74 (layer F.Cu) (tedit 5B9C837A)
    (at 120.2 102.7)
    (descr "wire loop with bead as test point, loop diameter 1.8mm, hole diameter 1.0mm")
    (tags "test point wire loop bead")
    (fp_text reference C5 (at -0.5 2) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 -2.25) (layer F.Fab))
    (fp_text user %R (at 0 2.25) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 0.74) (layers *.Cu *.Mask)
      (net 5 "Net-(C5-Pad1)"))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Loop_D1.80mm_Drill1.0mm_Beaded.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module azure-test:Mill-Max_1.83_D0.74 (layer F.Cu) (tedit 5B9C85CB)
    (at 130.5 106)
    (descr "wire loop with bead as test point, loop diameter 1.8mm, hole diameter 1.0mm")
    (tags "test point wire loop bead")
    (fp_text reference C1 (at -2.3 1.1) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 -2.25) (layer F.Fab))
    (fp_text user %R (at 0 2.25) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 0.74) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Loop_D1.80mm_Drill1.0mm_Beaded.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module azure-test:Mill-Max_1.83_D0.74 (layer F.Cu) (tedit 5B9C86AE)
    (at 130.5 119.5)
    (descr "wire loop with bead as test point, loop diameter 1.8mm, hole diameter 1.0mm")
    (tags "test point wire loop bead")
    (fp_text reference C6 (at 2.2 0) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 -2.25) (layer F.Fab))
    (fp_text user %R (at 0 2.25) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 0.74) (layers *.Cu *.Mask)
      (net 6 "Net-(C6-Pad1)"))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Loop_D1.80mm_Drill1.0mm_Beaded.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module azure-test:Mill-Max_1.83_D0.74 (layer F.Cu) (tedit 5B9C85C1)
    (at 132.1 108.16)
    (descr "wire loop with bead as test point, loop diameter 1.8mm, hole diameter 1.0mm")
    (tags "test point wire loop bead")
    (fp_text reference C2 (at -1.8 0.84) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 -2.25) (layer F.Fab))
    (fp_text user %R (at 0 2.25) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 0.74) (layers *.Cu *.Mask)
      (net 2 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Loop_D1.80mm_Drill1.0mm_Beaded.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module azure-test:Mill-Max_1.83_D0.74 (layer F.Cu) (tedit 5B9C8389)
    (at 122.8 108.6)
    (descr "wire loop with bead as test point, loop diameter 1.8mm, hole diameter 1.0mm")
    (tags "test point wire loop bead")
    (fp_text reference C4 (at 1 1.8) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 -2.25) (layer F.Fab))
    (fp_text user %R (at 0 2.25) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 0.74) (layers *.Cu *.Mask)
      (net 4 "Net-(C4-Pad1)"))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Loop_D1.80mm_Drill1.0mm_Beaded.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module azure-test:Mill-Max_1.83_D0.74 (layer F.Cu) (tedit 5B9C839B)
    (at 127.4 110.4)
    (descr "wire loop with bead as test point, loop diameter 1.8mm, hole diameter 1.0mm")
    (tags "test point wire loop bead")
    (fp_text reference C3 (at 1.9 1) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 -2.25) (layer F.Fab))
    (fp_text user %R (at 0 2.25) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 0.74) (layers *.Cu *.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Loop_D1.80mm_Drill1.0mm_Beaded.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical_SMD_Pin1Left (layer B.Cu) (tedit 59FED5CC)
    (at 129.79 97.755 90)
    (descr "surface-mounted straight pin header, 1x06, 2.54mm pitch, single row, style 1 (pin 1 left)")
    (tags "Surface mounted pin header SMD 1x06 2.54mm single row style1 pin1 left")
    (attr smd)
    (fp_text reference J7 (at 0 -8.5 -90) (layer B.SilkS))
    (fp_text value Conn_01x06_Male (at 0 -8.68 90) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 6 smd rect (at 1.655 -6.35 90) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(C6-Pad1)"))
    (pad 4 smd rect (at 1.655 -1.27 90) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 1.655 3.81 90) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C2-Pad1)"))
    (pad 5 smd rect (at -1.655 -3.81 90) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(C5-Pad1)"))
    (pad 3 smd rect (at -1.655 1.27 90) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (pad 1 smd rect (at -1.655 6.35 90) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical_SMD_Pin1Left.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Pad_1.5x1.5mm (layer B.Cu) (tedit 5A0F774F)
    (at 136.105 114.15 270)
    (descr "SMD rectangular pad as test Point, square 1.5mm side length")
    (tags "test point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference J1 (at 2 0 180) (layer B.SilkS))
    (fp_text value Conn_01x01 (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 1.65 270) (layer B.Fab))
    (pad 1 smd rect (at 0 0 270) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 1 "Net-(C1-Pad1)"))
  )
  (module TestPoint:TestPoint_Pad_1.5x1.5mm (layer B.Cu) (tedit 5A0F774F)
    (at 133.565 114.15 270)
    (descr "SMD rectangular pad as test Point, square 1.5mm side length")
    (tags "test point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference J2 (at 2 0 180) (layer B.SilkS))
    (fp_text value Conn_01x01 (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 1.65 270) (layer B.Fab))
    (pad 1 smd rect (at 0 0 270) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 2 "Net-(C2-Pad1)"))
  )
  (module TestPoint:TestPoint_Pad_1.5x1.5mm (layer B.Cu) (tedit 5A0F774F)
    (at 131.025 114.15 270)
    (descr "SMD rectangular pad as test Point, square 1.5mm side length")
    (tags "test point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference J3 (at 2 0 180) (layer B.SilkS))
    (fp_text value Conn_01x01 (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 1.65 270) (layer B.Fab))
    (pad 1 smd rect (at 0 0 270) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 3 "Net-(C3-Pad1)"))
  )
  (module TestPoint:TestPoint_Pad_1.5x1.5mm (layer B.Cu) (tedit 5A0F774F)
    (at 128.485 114.15 270)
    (descr "SMD rectangular pad as test Point, square 1.5mm side length")
    (tags "test point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference J4 (at 2 0 180) (layer B.SilkS))
    (fp_text value Conn_01x01 (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 1.65 270) (layer B.Fab))
    (pad 1 smd rect (at 0 0 270) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 4 "Net-(C4-Pad1)"))
  )
  (module TestPoint:TestPoint_Pad_1.5x1.5mm (layer B.Cu) (tedit 5A0F774F)
    (at 125.945 114.15 270)
    (descr "SMD rectangular pad as test Point, square 1.5mm side length")
    (tags "test point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference J5 (at 2 0 180) (layer B.SilkS))
    (fp_text value Conn_01x01 (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 1.65 270) (layer B.Fab))
    (pad 1 smd rect (at 0 0 270) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 5 "Net-(C5-Pad1)"))
  )
  (module TestPoint:TestPoint_Pad_1.5x1.5mm (layer B.Cu) (tedit 5A0F774F)
    (at 123.405 114.15 270)
    (descr "SMD rectangular pad as test Point, square 1.5mm side length")
    (tags "test point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference J6 (at 1.924999 -0.074999 180) (layer B.SilkS))
    (fp_text value Conn_01x01 (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 1.65 270) (layer B.Fab))
    (pad 1 smd rect (at 0 0 270) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 6 "Net-(C6-Pad1)"))
  )
  (module azure-test:Mill-Max_1.83_D0.74 (layer F.Cu) (tedit 5B9C859D)
    (at 130.5 106)
    (descr "wire loop with bead as test point, loop diameter 1.8mm, hole diameter 1.0mm")
    (tags "test point wire loop bead")
    (fp_text reference . (at 0 1) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 -2.25) (layer F.Fab))
    (fp_text user %R (at 0 2.25) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 0.74) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Loop_D1.80mm_Drill1.0mm_Beaded.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module azure-test:Mill-Max_1.83_D0.74 (layer F.Cu) (tedit 5B9C8580)
    (at 128.91 103.82)
    (descr "wire loop with bead as test point, loop diameter 1.8mm, hole diameter 1.0mm")
    (tags "test point wire loop bead")
    (fp_text reference C2a1 (at 2.69 -0.12 180) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 -2.25) (layer F.Fab))
    (fp_text user %R (at 0 2.25) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 0.74) (layers *.Cu *.Mask)
      (net 2 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Loop_D1.80mm_Drill1.0mm_Beaded.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module azure-test:Mill-Max_1.83_D0.74 (layer F.Cu) (tedit 5B9C867E)
    (at 133.7 101.6)
    (descr "wire loop with bead as test point, loop diameter 1.8mm, hole diameter 1.0mm")
    (tags "test point wire loop bead")
    (fp_text reference C3a1 (at -2.6 -0.8) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 -2.25) (layer F.Fab))
    (fp_text user %R (at 0 2.25) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 0.74) (layers *.Cu *.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Loop_D1.80mm_Drill1.0mm_Beaded.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module azure-test:Mill-Max_1.83_D0.74 (layer F.Cu) (tedit 5B9C868B)
    (at 138.24 103.56)
    (descr "wire loop with bead as test point, loop diameter 1.8mm, hole diameter 1.0mm")
    (tags "test point wire loop bead")
    (fp_text reference C4a1 (at 0.26 2.64 270) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 -2.25) (layer F.Fab))
    (fp_text user %R (at 0 2.25) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 0.74) (layers *.Cu *.Mask)
      (net 4 "Net-(C4-Pad1)"))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Loop_D1.80mm_Drill1.0mm_Beaded.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module azure-test:Mill-Max_1.83_D0.74 (layer F.Cu) (tedit 5B9C869B)
    (at 140.8 109.3)
    (descr "wire loop with bead as test point, loop diameter 1.8mm, hole diameter 1.0mm")
    (tags "test point wire loop bead")
    (fp_text reference C5a1 (at 0.3 -2.7 90) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 -2.25) (layer F.Fab))
    (fp_text user %R (at 0 2.25) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 0.74) (layers *.Cu *.Mask)
      (net 5 "Net-(C5-Pad1)"))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Loop_D1.80mm_Drill1.0mm_Beaded.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module azure-test:Mill-Max_1.83_D0.74 (layer F.Cu) (tedit 5B9C836F)
    (at 130.5 92.5)
    (descr "wire loop with bead as test point, loop diameter 1.8mm, hole diameter 1.0mm")
    (tags "test point wire loop bead")
    (fp_text reference C6a1 (at 2.8 0.4) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 -2.25) (layer F.Fab))
    (fp_text user %R (at 0 2.25) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 0.74) (layers *.Cu *.Mask)
      (net 6 "Net-(C6-Pad1)"))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Loop_D1.80mm_Drill1.0mm_Beaded.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_arc (start 130.5 106) (end 132.499999 120.999999) (angle -74.81071326) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 130.5 106) (end 115.500001 107.999999) (angle -74.81071326) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 130.5 106) (end 128.500001 91.000001) (angle -74.81071326) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 130.5 106) (end 145.499999 104.000001) (angle -74.81071326) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 130.5 105.952459) (end 146.5 105.952459) (angle 7.351663208) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 130.5 106) (end 114.5 106) (angle 7.182773574) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 130.5 106) (end 130.5 122) (angle 7.178298149) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 130.452459 106) (end 130.452459 90) (angle 7.37003809) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 130.452459 106) (end 130.452459 122) (angle -7.356248823) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 130.5 106) (end 130.5 90) (angle -7.182773574) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 130.5 106) (end 146.5 106) (angle -7.182773574) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 130.5 106) (end 114.5 106) (angle -7.182773574) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 132.5 121.87) (end 132.5 121) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 128.5 121) (end 128.5 121.87) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 146.37 108) (end 145.5 108) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 145.5 104) (end 146.38 104) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 132.5 90.13) (end 132.5 91) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 128.5 91) (end 128.5 90.12) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 115.5 104) (end 114.63 104) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 114.63 108) (end 115.5 108) (layer Edge.Cuts) (width 0.2))
)
