(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 233)
    (no_connects 0)
    (area 184.884287 37.94 261.695001 256.065001)
    (thickness 1.6)
    (drawings 82)
    (tracks 450)
    (zones 0)
    (modules 96)
    (nets 48)
  )
  (page A3)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.3)
    (trace_clearance 0.25)
    (zone_clearance 0.3)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3.1 3.1)
    (pad_drill 3)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (grid_origin 203.2 248.92)
    (visible_elements 7FFEFFFF)
    (pcbplotparams
      (layerselection 0x010e0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference false)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +12V)
  (net 2 GND)
  (net 3 +5V)
  (net 4 +3V3)
  (net 5 BCM2)
  (net 6 BCM3)
  (net 7 BCM4)
  (net 8 BCM14)
  (net 9 BCM15)
  (net 10 BCM17)
  (net 11 BCM18)
  (net 12 BCM27)
  (net 13 BCM22)
  (net 14 BCM23)
  (net 15 BCM24)
  (net 16 BCM10)
  (net 17 BCM9)
  (net 18 BCM25)
  (net 19 BCM11)
  (net 20 BCM8)
  (net 21 BCM7)
  (net 22 "Net-(J2-Pad27)")
  (net 23 "Net-(J2-Pad28)")
  (net 24 BCM5)
  (net 25 BCM6)
  (net 26 BCM12)
  (net 27 BCM13)
  (net 28 BCM19)
  (net 29 BCM16)
  (net 30 BCM26)
  (net 31 BCM20)
  (net 32 BCM21)
  (net 33 V1)
  (net 34 V2)
  (net 35 V3)
  (net 36 V4)
  (net 37 V5)
  (net 38 V6)
  (net 39 V7)
  (net 40 V8)
  (net 41 V9)
  (net 42 V10)
  (net 43 V11)
  (net 44 V12)
  (net 45 V13)
  (net 46 V14)
  (net 47 "Net-(J2-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.25)
    (trace_width 0.3)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net BCM10)
    (add_net BCM11)
    (add_net BCM12)
    (add_net BCM13)
    (add_net BCM14)
    (add_net BCM15)
    (add_net BCM16)
    (add_net BCM17)
    (add_net BCM18)
    (add_net BCM19)
    (add_net BCM2)
    (add_net BCM20)
    (add_net BCM21)
    (add_net BCM22)
    (add_net BCM23)
    (add_net BCM24)
    (add_net BCM25)
    (add_net BCM26)
    (add_net BCM27)
    (add_net BCM3)
    (add_net BCM4)
    (add_net BCM5)
    (add_net BCM6)
    (add_net BCM7)
    (add_net BCM8)
    (add_net BCM9)
    (add_net "Net-(J2-Pad27)")
    (add_net "Net-(J2-Pad28)")
  )
  (net_class Power ""
    (clearance 0.25)
    (trace_width 1)
    (via_dia 1)
    (via_drill 0.5)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net +3V3)
    (add_net +5V)
    (add_net GND)
    (add_net "Net-(J2-Pad2)")
    (add_net V1)
    (add_net V10)
    (add_net V11)
    (add_net V12)
    (add_net V13)
    (add_net V14)
    (add_net V2)
    (add_net V3)
    (add_net V4)
    (add_net V5)
    (add_net V6)
    (add_net V7)
    (add_net V8)
    (add_net V9)
  )
  (module Connectors:1pin (layer F.Cu) (tedit 5ABA5A8B)
    (at 257.81 245.11)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 1.27 -3.81) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 3) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3.2) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Connectors:1pin (layer F.Cu) (tedit 5ABA535F)
    (at 257.81 189.23)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at -0.635 -4.445) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 3) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3.2) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Connectors:1pin (layer F.Cu) (tedit 5ABA534B)
    (at 257.81 105.41)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at -0.635 -4.445) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 3) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3.2) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Connectors:1pin (layer F.Cu) (tedit 5ABA532D)
    (at 257.81 49.53)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 4.445) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 3) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3.2) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Connectors:1pin (layer F.Cu) (tedit 5ABA5319)
    (at 207.01 49.53)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 4.445) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 3) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3.2) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Connectors:1pin (layer F.Cu) (tedit 5ABA533F)
    (at 207.01 105.41)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at -0.635 -4.445) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 3) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3.2) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Connectors:1pin (layer F.Cu) (tedit 5ABA5357)
    (at 207.01 189.23)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at -0.635 -4.445) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 3) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3.2) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Pin_Headers:Pin_Header_Straight_2x20_Pitch2.54mm (layer F.Cu) (tedit 5AB9F4D2)
    (at 207.645 119.38)
    (descr "Through hole straight pin header, 2x20, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x20 2.54mm double row")
    (fp_text reference J2 (at 5.715 -1.27) (layer F.SilkS))
    (fp_text value Conn_02x20_Odd_Even (at 1.27 50.59) (layer F.Fab))
    (fp_text user %R (at 1.27 24.13 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 "Net-(J2-Pad2)"))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 BCM2))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 "Net-(J2-Pad2)"))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 BCM3))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 BCM4))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 BCM14))
    (pad 9 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 10 thru_hole oval (at 2.54 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 BCM15))
    (pad 11 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 BCM17))
    (pad 12 thru_hole oval (at 2.54 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 BCM18))
    (pad 13 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 BCM27))
    (pad 14 thru_hole oval (at 2.54 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 15 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 BCM22))
    (pad 16 thru_hole oval (at 2.54 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 BCM23))
    (pad 17 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad 18 thru_hole oval (at 2.54 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 BCM24))
    (pad 19 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 BCM10))
    (pad 20 thru_hole oval (at 2.54 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 21 thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 BCM9))
    (pad 22 thru_hole oval (at 2.54 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 BCM25))
    (pad 23 thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 BCM11))
    (pad 24 thru_hole oval (at 2.54 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 BCM8))
    (pad 25 thru_hole oval (at 0 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 26 thru_hole oval (at 2.54 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 BCM7))
    (pad 27 thru_hole oval (at 0 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(J2-Pad27)"))
    (pad 28 thru_hole oval (at 2.54 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(J2-Pad28)"))
    (pad 29 thru_hole oval (at 0 35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 BCM5))
    (pad 30 thru_hole oval (at 2.54 35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 31 thru_hole oval (at 0 38.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 BCM6))
    (pad 32 thru_hole oval (at 2.54 38.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 BCM12))
    (pad 33 thru_hole oval (at 0 40.64) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 BCM13))
    (pad 34 thru_hole oval (at 2.54 40.64) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 35 thru_hole oval (at 0 43.18) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 BCM19))
    (pad 36 thru_hole oval (at 2.54 43.18) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 BCM16))
    (pad 37 thru_hole oval (at 0 45.72) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 BCM26))
    (pad 38 thru_hole oval (at 2.54 45.72) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 BCM20))
    (pad 39 thru_hole oval (at 0 48.26) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 40 thru_hole oval (at 2.54 48.26) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 BCM21))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x20_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:CP_Radial_D6.3mm_P2.50mm (layer F.Cu) (tedit 5ABA49BA)
    (at 213.36 50.165)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (fp_text reference C1 (at 5.08 -2.54) (layer F.SilkS))
    (fp_text value 100u (at 1.25 4.46) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:CP_Radial_D6.3mm_P2.50mm (layer F.Cu) (tedit 5ABA49BE)
    (at 219.075 62.23 90)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (fp_text reference C2 (at 4.445 3.175 180) (layer F.SilkS))
    (fp_text value 100u (at 1.25 4.46 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:CP_Radial_D4.0mm_P1.50mm (layer F.Cu) (tedit 597BC7C2)
    (at 210.7 112.42 90)
    (descr "CP, Radial series, Radial, pin pitch=1.50mm, , diameter=4mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 1.50mm  diameter 4mm Electrolytic Capacitor")
    (fp_text reference C3 (at 0.75 -3.31 90) (layer F.SilkS))
    (fp_text value 10u (at 0.75 3.31 90) (layer F.Fab))
    (fp_text user %R (at 0.75 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad 2 thru_hole circle (at 1.5 0 90) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D4.0mm_P1.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3.8mm_W2.6mm_P2.50mm (layer F.Cu) (tedit 5AB9E9F0)
    (at 224.155 53.34 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.8*2.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.8mm width 2.6mm Capacitor")
    (fp_text reference C4 (at 4.445 0 180) (layer F.SilkS))
    (fp_text value 0u1 (at 1.25 2.61 180) (layer F.Fab))
    (fp_text user %R (at 1.25 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.8mm_W2.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3.8mm_W2.6mm_P2.50mm (layer F.Cu) (tedit 597BC7C2)
    (at 224.155 68.58 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.8*2.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.8mm width 2.6mm Capacitor")
    (fp_text reference C5 (at 1.25 -2.61 180) (layer F.SilkS))
    (fp_text value 0u1 (at 1.25 2.61 180) (layer F.Fab))
    (fp_text user %R (at 1.25 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.8mm_W2.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3.8mm_W2.6mm_P2.50mm (layer F.Cu) (tedit 597BC7C2)
    (at 224.155 83.82 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.8*2.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.8mm width 2.6mm Capacitor")
    (fp_text reference C6 (at 1.25 -2.61 180) (layer F.SilkS))
    (fp_text value 0u1 (at 1.25 2.61 180) (layer F.Fab))
    (fp_text user %R (at 1.25 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.8mm_W2.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3.8mm_W2.6mm_P2.50mm (layer F.Cu) (tedit 597BC7C2)
    (at 224.155 99.06 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.8*2.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.8mm width 2.6mm Capacitor")
    (fp_text reference C7 (at 1.25 -2.61 180) (layer F.SilkS))
    (fp_text value 0u1 (at 1.25 2.61 180) (layer F.Fab))
    (fp_text user %R (at 1.25 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.8mm_W2.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3.8mm_W2.6mm_P2.50mm (layer F.Cu) (tedit 597BC7C2)
    (at 224.155 114.3 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.8*2.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.8mm width 2.6mm Capacitor")
    (fp_text reference C8 (at 1.25 -2.61 180) (layer F.SilkS))
    (fp_text value 0u1 (at 1.25 2.61 180) (layer F.Fab))
    (fp_text user %R (at 1.25 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.8mm_W2.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3.8mm_W2.6mm_P2.50mm (layer F.Cu) (tedit 597BC7C2)
    (at 224.155 129.54 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.8*2.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.8mm width 2.6mm Capacitor")
    (fp_text reference C9 (at 1.25 -2.61 180) (layer F.SilkS))
    (fp_text value 0u1 (at 1.25 2.61 180) (layer F.Fab))
    (fp_text user %R (at 1.25 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.8mm_W2.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3.8mm_W2.6mm_P2.50mm (layer F.Cu) (tedit 597BC7C2)
    (at 224.155 144.78 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.8*2.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.8mm width 2.6mm Capacitor")
    (fp_text reference C10 (at 1.25 -2.61 180) (layer F.SilkS))
    (fp_text value 0u1 (at 1.25 2.61 180) (layer F.Fab))
    (fp_text user %R (at 1.25 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.8mm_W2.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3.8mm_W2.6mm_P2.50mm (layer F.Cu) (tedit 597BC7C2)
    (at 224.155 160.02 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.8*2.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.8mm width 2.6mm Capacitor")
    (fp_text reference C11 (at 1.25 -2.61 180) (layer F.SilkS))
    (fp_text value 0u1 (at 1.25 2.61 180) (layer F.Fab))
    (fp_text user %R (at 1.25 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.8mm_W2.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3.8mm_W2.6mm_P2.50mm (layer F.Cu) (tedit 597BC7C2)
    (at 224.155 175.26 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.8*2.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.8mm width 2.6mm Capacitor")
    (fp_text reference C12 (at 1.25 -2.61 180) (layer F.SilkS))
    (fp_text value 0u1 (at 1.25 2.61 180) (layer F.Fab))
    (fp_text user %R (at 1.25 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.8mm_W2.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3.8mm_W2.6mm_P2.50mm (layer F.Cu) (tedit 597BC7C2)
    (at 224.155 190.5 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.8*2.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.8mm width 2.6mm Capacitor")
    (fp_text reference C13 (at 1.25 -2.61 180) (layer F.SilkS))
    (fp_text value 0u1 (at 1.25 2.61 180) (layer F.Fab))
    (fp_text user %R (at 1.25 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.8mm_W2.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3.8mm_W2.6mm_P2.50mm (layer F.Cu) (tedit 597BC7C2)
    (at 224.155 205.74 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.8*2.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.8mm width 2.6mm Capacitor")
    (fp_text reference C14 (at 1.25 -2.61 180) (layer F.SilkS))
    (fp_text value 0u1 (at 1.25 2.61 180) (layer F.Fab))
    (fp_text user %R (at 1.25 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.8mm_W2.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3.8mm_W2.6mm_P2.50mm (layer F.Cu) (tedit 597BC7C2)
    (at 224.155 220.98 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.8*2.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.8mm width 2.6mm Capacitor")
    (fp_text reference C15 (at 1.25 -2.61 180) (layer F.SilkS))
    (fp_text value 0u1 (at 1.25 2.61 180) (layer F.Fab))
    (fp_text user %R (at 1.25 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.8mm_W2.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3.8mm_W2.6mm_P2.50mm (layer F.Cu) (tedit 597BC7C2)
    (at 224.155 236.22 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.8*2.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.8mm width 2.6mm Capacitor")
    (fp_text reference C16 (at 1.25 -2.61 180) (layer F.SilkS))
    (fp_text value 0u1 (at 1.25 2.61 180) (layer F.Fab))
    (fp_text user %R (at 1.25 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.8mm_W2.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3.8mm_W2.6mm_P2.50mm (layer F.Cu) (tedit 5AB9FB99)
    (at 227.33 246.38 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.8*2.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.8mm width 2.6mm Capacitor")
    (fp_text reference C17 (at 1.27 2.54 180) (layer F.SilkS))
    (fp_text value 0u1 (at 1.25 2.61 180) (layer F.Fab))
    (fp_text user %R (at 1.25 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.8mm_W2.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3.8mm_W2.6mm_P2.50mm (layer F.Cu) (tedit 5ABA49B4)
    (at 224.155 49.53 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.8*2.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.8mm width 2.6mm Capacitor")
    (fp_text reference C18 (at 1.905 2.54 180) (layer F.SilkS))
    (fp_text value 0u1 (at 1.25 2.61 180) (layer F.Fab))
    (fp_text user %R (at 1.25 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.8mm_W2.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3.8mm_W2.6mm_P2.50mm (layer F.Cu) (tedit 597BC7C2)
    (at 219.075 67.31 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.8*2.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.8mm width 2.6mm Capacitor")
    (fp_text reference C19 (at 1.25 -2.61 180) (layer F.SilkS))
    (fp_text value 0u1 (at 1.25 2.61 180) (layer F.Fab))
    (fp_text user %R (at 1.25 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.8mm_W2.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3.8mm_W2.6mm_P2.50mm (layer F.Cu) (tedit 5AB9FC47)
    (at 222.25 80.01 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.8*2.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.8mm width 2.6mm Capacitor")
    (fp_text reference C20 (at 1.905 2.54 180) (layer F.SilkS))
    (fp_text value 0u1 (at 1.25 2.61 180) (layer F.Fab))
    (fp_text user %R (at 1.25 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.8mm_W2.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3.8mm_W2.6mm_P2.50mm (layer F.Cu) (tedit 5AB9FC40)
    (at 222.25 95.25 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.8*2.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.8mm width 2.6mm Capacitor")
    (fp_text reference C21 (at 2.54 2.54 180) (layer F.SilkS))
    (fp_text value 0u1 (at 1.25 2.61 180) (layer F.Fab))
    (fp_text user %R (at 1.25 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.8mm_W2.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3.8mm_W2.6mm_P2.50mm (layer F.Cu) (tedit 5ABCE05E)
    (at 222.25 110.49 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.8*2.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.8mm width 2.6mm Capacitor")
    (fp_text reference C22 (at 2.05 2.57 180) (layer F.SilkS))
    (fp_text value 0u1 (at 1.25 2.61 180) (layer F.Fab))
    (fp_text user %R (at 1.25 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.8mm_W2.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3.8mm_W2.6mm_P2.50mm (layer F.Cu) (tedit 5ABCE050)
    (at 222.25 125.73 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.8*2.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.8mm width 2.6mm Capacitor")
    (fp_text reference C23 (at 3.05 -2.19 180) (layer F.SilkS))
    (fp_text value 0u1 (at 1.25 2.61 180) (layer F.Fab))
    (fp_text user %R (at 1.25 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.8mm_W2.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3.8mm_W2.6mm_P2.50mm (layer F.Cu) (tedit 597BC7C2)
    (at 222.25 140.97 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.8*2.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.8mm width 2.6mm Capacitor")
    (fp_text reference C24 (at 1.25 -2.61 180) (layer F.SilkS))
    (fp_text value 0u1 (at 1.25 2.61 180) (layer F.Fab))
    (fp_text user %R (at 1.25 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.8mm_W2.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3.8mm_W2.6mm_P2.50mm (layer F.Cu) (tedit 5AB9FBDB)
    (at 222.25 156.21 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.8*2.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.8mm width 2.6mm Capacitor")
    (fp_text reference C25 (at 1.905 2.54 180) (layer F.SilkS))
    (fp_text value 0u1 (at 1.25 2.61 180) (layer F.Fab))
    (fp_text user %R (at 1.25 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.8mm_W2.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3.8mm_W2.6mm_P2.50mm (layer F.Cu) (tedit 5AB9FBC7)
    (at 222.25 171.45 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.8*2.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.8mm width 2.6mm Capacitor")
    (fp_text reference C26 (at 5.08 0 180) (layer F.SilkS))
    (fp_text value 0u1 (at 1.25 2.61 180) (layer F.Fab))
    (fp_text user %R (at 1.25 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.8mm_W2.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3.8mm_W2.6mm_P2.50mm (layer F.Cu) (tedit 5AB9FBBF)
    (at 222.25 186.69 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.8*2.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.8mm width 2.6mm Capacitor")
    (fp_text reference C27 (at 5.08 0 180) (layer F.SilkS))
    (fp_text value 0u1 (at 1.25 2.61 180) (layer F.Fab))
    (fp_text user %R (at 1.25 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.8mm_W2.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3.8mm_W2.6mm_P2.50mm (layer F.Cu) (tedit 5AB9FBEA)
    (at 222.25 201.93 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.8*2.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.8mm width 2.6mm Capacitor")
    (fp_text reference C28 (at 1.905 2.54 180) (layer F.SilkS))
    (fp_text value 0u1 (at 1.25 2.61 180) (layer F.Fab))
    (fp_text user %R (at 1.25 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.8mm_W2.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3.8mm_W2.6mm_P2.50mm (layer F.Cu) (tedit 5AB9FBEE)
    (at 222.25 217.17 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.8*2.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.8mm width 2.6mm Capacitor")
    (fp_text reference C29 (at 1.905 2.54 180) (layer F.SilkS))
    (fp_text value 0u1 (at 1.25 2.61 180) (layer F.Fab))
    (fp_text user %R (at 1.25 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.8mm_W2.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3.8mm_W2.6mm_P2.50mm (layer F.Cu) (tedit 5AB9FBF4)
    (at 222.25 232.41 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.8*2.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.8mm width 2.6mm Capacitor")
    (fp_text reference C30 (at 1.905 2.54 180) (layer F.SilkS))
    (fp_text value 0u1 (at 1.25 2.61 180) (layer F.Fab))
    (fp_text user %R (at 1.25 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.8mm_W2.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3.8mm_W2.6mm_P2.50mm (layer F.Cu) (tedit 597BC7C2)
    (at 222.25 245.11 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.8*2.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.8mm width 2.6mm Capacitor")
    (fp_text reference C31 (at 1.25 -2.61 180) (layer F.SilkS))
    (fp_text value 0u1 (at 1.25 2.61 180) (layer F.Fab))
    (fp_text user %R (at 1.25 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.8mm_W2.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3.8mm_W2.6mm_P2.50mm (layer F.Cu) (tedit 5ABA49AA)
    (at 229.235 48.26 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.8*2.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.8mm width 2.6mm Capacitor")
    (fp_text reference C32 (at 0.635 -2.54 180) (layer F.SilkS))
    (fp_text value 0u1 (at 1.25 2.61 180) (layer F.Fab))
    (fp_text user %R (at 1.25 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.8mm_W2.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3.8mm_W2.6mm_P2.50mm (layer F.Cu) (tedit 597BC7C2)
    (at 229.235 59.69)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.8*2.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.8mm width 2.6mm Capacitor")
    (fp_text reference C33 (at 1.25 -2.61) (layer F.SilkS))
    (fp_text value 0u1 (at 1.25 2.61) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.8mm_W2.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3.8mm_W2.6mm_P2.50mm (layer F.Cu) (tedit 597BC7C2)
    (at 229.235 74.93)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.8*2.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.8mm width 2.6mm Capacitor")
    (fp_text reference C34 (at 1.25 -2.61) (layer F.SilkS))
    (fp_text value 0u1 (at 1.25 2.61) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.8mm_W2.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3.8mm_W2.6mm_P2.50mm (layer F.Cu) (tedit 597BC7C2)
    (at 229.235 90.17)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.8*2.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.8mm width 2.6mm Capacitor")
    (fp_text reference C35 (at 1.25 -2.61) (layer F.SilkS))
    (fp_text value 0u1 (at 1.25 2.61) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.8mm_W2.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3.8mm_W2.6mm_P2.50mm (layer F.Cu) (tedit 597BC7C2)
    (at 229.235 105.41)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.8*2.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.8mm width 2.6mm Capacitor")
    (fp_text reference C36 (at 1.25 -2.61) (layer F.SilkS))
    (fp_text value 0u1 (at 1.25 2.61) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.8mm_W2.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3.8mm_W2.6mm_P2.50mm (layer F.Cu) (tedit 597BC7C2)
    (at 229.235 120.65)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.8*2.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.8mm width 2.6mm Capacitor")
    (fp_text reference C37 (at 1.25 -2.61) (layer F.SilkS))
    (fp_text value 0u1 (at 1.25 2.61) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.8mm_W2.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3.8mm_W2.6mm_P2.50mm (layer F.Cu) (tedit 597BC7C2)
    (at 229.235 135.89)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.8*2.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.8mm width 2.6mm Capacitor")
    (fp_text reference C38 (at 1.25 -2.61) (layer F.SilkS))
    (fp_text value 0u1 (at 1.25 2.61) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.8mm_W2.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3.8mm_W2.6mm_P2.50mm (layer F.Cu) (tedit 597BC7C2)
    (at 229.235 151.13)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.8*2.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.8mm width 2.6mm Capacitor")
    (fp_text reference C39 (at 1.25 -2.61) (layer F.SilkS))
    (fp_text value 0u1 (at 1.25 2.61) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.8mm_W2.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3.8mm_W2.6mm_P2.50mm (layer F.Cu) (tedit 597BC7C2)
    (at 229.235 166.37)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.8*2.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.8mm width 2.6mm Capacitor")
    (fp_text reference C40 (at 1.25 -2.61) (layer F.SilkS))
    (fp_text value 0u1 (at 1.25 2.61) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.8mm_W2.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3.8mm_W2.6mm_P2.50mm (layer F.Cu) (tedit 597BC7C2)
    (at 229.235 181.61)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.8*2.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.8mm width 2.6mm Capacitor")
    (fp_text reference C41 (at 1.25 -2.61) (layer F.SilkS))
    (fp_text value 0u1 (at 1.25 2.61) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.8mm_W2.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3.8mm_W2.6mm_P2.50mm (layer F.Cu) (tedit 597BC7C2)
    (at 229.235 196.85)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.8*2.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.8mm width 2.6mm Capacitor")
    (fp_text reference C42 (at 1.25 -2.61) (layer F.SilkS))
    (fp_text value 0u1 (at 1.25 2.61) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.8mm_W2.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3.8mm_W2.6mm_P2.50mm (layer F.Cu) (tedit 597BC7C2)
    (at 229.235 212.09)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.8*2.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.8mm width 2.6mm Capacitor")
    (fp_text reference C43 (at 1.25 -2.61) (layer F.SilkS))
    (fp_text value 0u1 (at 1.25 2.61) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.8mm_W2.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3.8mm_W2.6mm_P2.50mm (layer F.Cu) (tedit 597BC7C2)
    (at 229.235 227.33)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.8*2.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.8mm width 2.6mm Capacitor")
    (fp_text reference C44 (at 1.25 -2.61) (layer F.SilkS))
    (fp_text value 0u1 (at 1.25 2.61) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.8mm_W2.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3.8mm_W2.6mm_P2.50mm (layer F.Cu) (tedit 5AB9FBFB)
    (at 222.25 241.3 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.8*2.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.8mm width 2.6mm Capacitor")
    (fp_text reference C45 (at 5.08 0 180) (layer F.SilkS))
    (fp_text value 0u1 (at 1.25 2.61 180) (layer F.Fab))
    (fp_text user %R (at 1.25 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.8mm_W2.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLibrary:CTB0308-2 (layer F.Cu) (tedit 5AB9E1DB)
    (at 241.935 50.165 90)
    (fp_text reference J3 (at -2.54 -4.445 90) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 1.905 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 1.905 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 33 V1))
    (pad 2 thru_hole circle (at -1.905 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 7 BCM4))
  )
  (module MyLibrary:CTB0308-2 (layer F.Cu) (tedit 5AB9E1DB)
    (at 241.935 57.785 90)
    (fp_text reference J4 (at -2.54 -4.445 90) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 1.905 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 1.905 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -1.905 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 BCM2))
  )
  (module MyLibrary:CTB0308-2 (layer F.Cu) (tedit 5AB9E1DB)
    (at 241.935 65.405 90)
    (fp_text reference J5 (at -2.54 -4.445 90) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 1.905 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 1.905 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 34 V2))
    (pad 2 thru_hole circle (at -1.905 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 6 BCM3))
  )
  (module MyLibrary:CTB0308-2 (layer F.Cu) (tedit 5AB9E1DB)
    (at 241.935 73.025 90)
    (fp_text reference J6 (at -2.54 -4.445 90) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 1.905 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 1.905 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -1.905 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 8 BCM14))
  )
  (module MyLibrary:CTB0308-2 (layer F.Cu) (tedit 5AB9E1DB)
    (at 241.935 80.645 90)
    (fp_text reference J7 (at -2.54 -4.445 90) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 1.905 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 1.905 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 35 V3))
    (pad 2 thru_hole circle (at -1.905 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 9 BCM15))
  )
  (module MyLibrary:CTB0308-2 (layer F.Cu) (tedit 5AB9E1DB)
    (at 241.935 88.265 90)
    (fp_text reference J8 (at -2.54 -4.445 90) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 1.905 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 1.905 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -1.905 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 10 BCM17))
  )
  (module MyLibrary:CTB0308-2 (layer F.Cu) (tedit 5AB9E1DB)
    (at 241.935 95.885 90)
    (fp_text reference J9 (at -2.54 -4.445 90) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 1.905 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 1.905 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 36 V4))
    (pad 2 thru_hole circle (at -1.905 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 11 BCM18))
  )
  (module MyLibrary:CTB0308-2 (layer F.Cu) (tedit 5AB9E1DB)
    (at 241.935 103.505 90)
    (fp_text reference J10 (at -2.54 -4.445 90) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 1.905 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 1.905 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -1.905 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 12 BCM27))
  )
  (module MyLibrary:CTB0308-2 (layer F.Cu) (tedit 5AB9E1DB)
    (at 241.935 111.125 90)
    (fp_text reference J11 (at -2.54 -4.445 90) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 1.905 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 1.905 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 37 V5))
    (pad 2 thru_hole circle (at -1.905 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 13 BCM22))
  )
  (module MyLibrary:CTB0308-2 (layer F.Cu) (tedit 5AB9E1DB)
    (at 241.935 118.745 90)
    (fp_text reference J12 (at -2.54 -4.445 90) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 1.905 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 1.905 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -1.905 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 14 BCM23))
  )
  (module MyLibrary:CTB0308-2 (layer F.Cu) (tedit 5AB9E1DB)
    (at 241.935 126.365 90)
    (fp_text reference J13 (at -2.54 -4.445 90) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 1.905 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 1.905 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 38 V6))
    (pad 2 thru_hole circle (at -1.905 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 15 BCM24))
  )
  (module MyLibrary:CTB0308-2 (layer F.Cu) (tedit 5AB9E1DB)
    (at 241.935 133.985 90)
    (fp_text reference J14 (at -2.54 -4.445 90) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 1.905 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 1.905 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -1.905 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 16 BCM10))
  )
  (module MyLibrary:CTB0308-2 (layer F.Cu) (tedit 5AB9E1DB)
    (at 241.935 141.605 90)
    (fp_text reference J15 (at -2.54 -4.445 90) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 1.905 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 1.905 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 39 V7))
    (pad 2 thru_hole circle (at -1.905 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 17 BCM9))
  )
  (module MyLibrary:CTB0308-2 (layer F.Cu) (tedit 5AB9E1DB)
    (at 241.935 149.225 90)
    (fp_text reference J16 (at -2.54 -4.445 90) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 1.905 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 1.905 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -1.905 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 18 BCM25))
  )
  (module MyLibrary:CTB0308-2 (layer F.Cu) (tedit 5AB9E1DB)
    (at 241.935 156.845 90)
    (fp_text reference J17 (at -2.54 -4.445 90) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 1.905 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 1.905 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 40 V8))
    (pad 2 thru_hole circle (at -1.905 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 19 BCM11))
  )
  (module MyLibrary:CTB0308-2 (layer F.Cu) (tedit 5AB9E1DB)
    (at 241.935 164.465 90)
    (fp_text reference J18 (at -2.54 -4.445 90) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 1.905 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 1.905 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -1.905 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 20 BCM8))
  )
  (module MyLibrary:CTB0308-2 (layer F.Cu) (tedit 5AB9E1DB)
    (at 241.935 172.085 90)
    (fp_text reference J19 (at -2.54 -4.445 90) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 1.905 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 1.905 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 41 V9))
    (pad 2 thru_hole circle (at -1.905 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 21 BCM7))
  )
  (module MyLibrary:CTB0308-2 (layer F.Cu) (tedit 5AB9E1DB)
    (at 241.935 179.705 90)
    (fp_text reference J20 (at -2.54 -4.445 90) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 1.905 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 1.905 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -1.905 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 24 BCM5))
  )
  (module MyLibrary:CTB0308-2 (layer F.Cu) (tedit 5AB9E1DB)
    (at 241.935 187.325 90)
    (fp_text reference J21 (at -2.54 -4.445 90) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 1.905 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 1.905 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 42 V10))
    (pad 2 thru_hole circle (at -1.905 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 25 BCM6))
  )
  (module MyLibrary:CTB0308-2 (layer F.Cu) (tedit 5AB9E1DB)
    (at 241.935 194.945 90)
    (fp_text reference J22 (at -2.54 -4.445 90) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 1.905 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 1.905 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -1.905 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 26 BCM12))
  )
  (module MyLibrary:CTB0308-2 (layer F.Cu) (tedit 5AB9E1DB)
    (at 241.935 202.565 90)
    (fp_text reference J23 (at -2.54 -4.445 90) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 1.905 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 1.905 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 43 V11))
    (pad 2 thru_hole circle (at -1.905 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 27 BCM13))
  )
  (module MyLibrary:CTB0308-2 (layer F.Cu) (tedit 5AB9E1DB)
    (at 241.935 210.185 90)
    (fp_text reference J24 (at -2.54 -4.445 90) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 1.905 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 1.905 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -1.905 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 28 BCM19))
  )
  (module MyLibrary:CTB0308-2 (layer F.Cu) (tedit 5AB9E1DB)
    (at 241.935 217.805 90)
    (fp_text reference J25 (at -2.54 -4.445 90) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 1.905 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 1.905 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 44 V12))
    (pad 2 thru_hole circle (at -1.905 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 29 BCM16))
  )
  (module MyLibrary:CTB0308-2 (layer F.Cu) (tedit 5AB9E1DB)
    (at 241.935 225.425 90)
    (fp_text reference J26 (at -2.54 -4.445 90) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 1.905 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 1.905 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -1.905 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 30 BCM26))
  )
  (module MyLibrary:CTB0308-2 (layer F.Cu) (tedit 5AB9E1DB)
    (at 241.935 233.045 90)
    (fp_text reference J27 (at -2.54 -4.445 90) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 1.905 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 1.905 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 45 V13))
    (pad 2 thru_hole circle (at -1.905 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 31 BCM20))
  )
  (module MyLibrary:CTB0308-3 (layer F.Cu) (tedit 5AB9E1C8)
    (at 241.935 242.57 90)
    (fp_text reference J28 (at -4.445 -4.445 90) (layer F.SilkS))
    (fp_text value Conn_01x03 (at -0.635 -2.54 90) (layer F.Fab) hide)
    (pad 2 thru_hole circle (at 0 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 32 BCM21))
    (pad 1 thru_hole circle (at 3.81 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole circle (at -3.81 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 46 V14))
  )
  (module Pin_Headers:Pin_Header_Straight_2x03_Pitch2.54mm (layer F.Cu) (tedit 5AB9EE9D)
    (at 232.41 48.26)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference V1 (at 1.27 7.62) (layer F.SilkS))
    (fp_text value Conn_02x03_Odd_Even (at 1.27 7.41) (layer F.Fab))
    (fp_text user %R (at 1.27 2.54 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 V1))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 V1))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 V1))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03_Pitch2.54mm (layer F.Cu) (tedit 5AB9EEAB)
    (at 232.41 63.5)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference V2 (at 1.27 7.62) (layer F.SilkS))
    (fp_text value Conn_02x03_Odd_Even (at 1.27 7.41) (layer F.Fab))
    (fp_text user %R (at 1.27 2.54 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 V2))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 V2))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 V2))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03_Pitch2.54mm (layer F.Cu) (tedit 5AB9EEAE)
    (at 232.41 78.74)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference V3 (at 1.27 7.62) (layer F.SilkS))
    (fp_text value Conn_02x03_Odd_Even (at 1.27 7.41) (layer F.Fab))
    (fp_text user %R (at 1.27 2.54 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 V3))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 V3))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 V3))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03_Pitch2.54mm (layer F.Cu) (tedit 5AB9F469)
    (at 232.41 93.98)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference V4 (at 1.27 7.62) (layer F.SilkS))
    (fp_text value Conn_02x03_Odd_Even (at 1.27 7.41) (layer F.Fab))
    (fp_text user %R (at 1.27 2.54 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 V4))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 V4))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 V4))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03_Pitch2.54mm (layer F.Cu) (tedit 5AB9F472)
    (at 232.41 109.22)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference V5 (at 1.27 7.62) (layer F.SilkS))
    (fp_text value Conn_02x03_Odd_Even (at 1.27 7.41) (layer F.Fab))
    (fp_text user %R (at 1.27 2.54 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 V5))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 V5))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 V5))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03_Pitch2.54mm (layer F.Cu) (tedit 5AB9F482)
    (at 232.41 124.46)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference V6 (at 1.27 7.62) (layer F.SilkS))
    (fp_text value Conn_02x03_Odd_Even (at 1.27 7.41) (layer F.Fab))
    (fp_text user %R (at 1.27 2.54 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 V6))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 V6))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 V6))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03_Pitch2.54mm (layer F.Cu) (tedit 5AB9F489)
    (at 232.41 139.7)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference V7 (at 1.27 7.62) (layer F.SilkS))
    (fp_text value Conn_02x03_Odd_Even (at 1.27 7.41) (layer F.Fab))
    (fp_text user %R (at 1.27 2.54 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 V7))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 V7))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 V7))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03_Pitch2.54mm (layer F.Cu) (tedit 5AB9F48D)
    (at 232.41 154.94)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference V8 (at 1.27 7.62) (layer F.SilkS))
    (fp_text value Conn_02x03_Odd_Even (at 1.27 7.41) (layer F.Fab))
    (fp_text user %R (at 1.27 2.54 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 V8))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 V8))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 V8))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03_Pitch2.54mm (layer F.Cu) (tedit 5AB9F493)
    (at 232.41 170.18)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference V9 (at 1.27 7.62) (layer F.SilkS))
    (fp_text value Conn_02x03_Odd_Even (at 1.27 7.41) (layer F.Fab))
    (fp_text user %R (at 1.27 2.54 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 V9))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 V9))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 V9))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03_Pitch2.54mm (layer F.Cu) (tedit 5AB9F498)
    (at 232.41 185.42)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference V10 (at 1.27 7.62) (layer F.SilkS))
    (fp_text value Conn_02x03_Odd_Even (at 1.27 7.41) (layer F.Fab))
    (fp_text user %R (at 1.27 2.54 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 V10))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 V10))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 V10))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03_Pitch2.54mm (layer F.Cu) (tedit 5AB9F49E)
    (at 232.41 200.66)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference V11 (at 1.27 7.62) (layer F.SilkS))
    (fp_text value Conn_02x03_Odd_Even (at 1.27 7.41) (layer F.Fab))
    (fp_text user %R (at 1.27 2.54 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 V11))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 V11))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 V11))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03_Pitch2.54mm (layer F.Cu) (tedit 5AB9F4A7)
    (at 232.41 215.9)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference V12 (at 1.27 7.62) (layer F.SilkS))
    (fp_text value Conn_02x03_Odd_Even (at 1.27 7.41) (layer F.Fab))
    (fp_text user %R (at 1.27 2.54 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 V12))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 V12))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 V12))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03_Pitch2.54mm (layer F.Cu) (tedit 5AB9FB88)
    (at 232.41 231.14)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference V13 (at 2.54 -2.54) (layer F.SilkS))
    (fp_text value Conn_02x03_Odd_Even (at 1.27 7.41) (layer F.Fab))
    (fp_text user %R (at 1.27 2.54 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 V13))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 V13))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 V13))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03_Pitch2.54mm (layer F.Cu) (tedit 5AB9FB8C)
    (at 232.41 241.3)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference V14 (at 1.27 -2.54) (layer F.SilkS))
    (fp_text value Conn_02x03_Odd_Even (at 1.27 7.41) (layer F.Fab))
    (fp_text user %R (at 1.27 2.54 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 V14))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 V14))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 V14))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLibrary:CTB0708-3 (layer F.Cu) (tedit 5AB9E29E)
    (at 208.915 61.595 270)
    (fp_text reference J1 (at -5.715 -6.35 270) (layer F.SilkS))
    (fp_text value Conn_01x03 (at 0 -4.445 270) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 5.08 0 270) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 0 0 270) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 3 thru_hole circle (at -4.445 0 270) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 1 +12V))
  )
  (module Connectors:1pin (layer F.Cu) (tedit 5ABA536C)
    (at 207.01 245.11)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -4.445) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 3) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3.2) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5ABCE102)
    (at 221.615 122.555 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J29 (at 3.175 3.81 180) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 4.87 180) (layer F.Fab))
    (fp_text user %R (at 0 1.27 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 "Net-(J2-Pad2)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Pi PWR" (at 215.9 120.65) (layer F.SilkS))
  (gr_text "RasPi Home Assistant GPIO Breakout Board\nHA_IO_V2.kicad_pcb 2019-01-05" (at 210.185 193.04 270) (layer F.SilkS))
  (gr_line (start 261.62 248.92) (end 203.2 248.92) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 261.62 45.72) (end 261.62 248.92) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 203.2 45.72) (end 261.62 45.72) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 203.2 248.92) (end 203.2 45.72) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "J1:\n   12V\n   5V\n   GND" (at 203.835 74.93) (layer F.SilkS))
  (gr_text BCM21 (at 246.38 242.57) (layer F.SilkS))
  (gr_text V14 (at 246.38 246.38) (layer F.SilkS))
  (gr_text GND (at 246.38 238.76) (layer F.SilkS))
  (gr_text BCM20 (at 246.38 234.95) (layer F.SilkS))
  (gr_text V13 (at 246.38 231.14) (layer F.SilkS))
  (gr_text BCM26 (at 246.38 227.33) (layer F.SilkS))
  (gr_text GND (at 246.38 208.28) (layer F.SilkS))
  (gr_text BCM13 (at 246.38 204.47) (layer F.SilkS))
  (gr_text V11 (at 246.38 200.66) (layer F.SilkS))
  (gr_text BCM12 (at 246.38 196.85) (layer F.SilkS))
  (gr_text BCM19 (at 246.38 212.09) (layer F.SilkS))
  (gr_text V12 (at 246.38 215.9) (layer F.SilkS))
  (gr_text BCM16 (at 246.38 219.71) (layer F.SilkS))
  (gr_text GND (at 246.38 223.52) (layer F.SilkS))
  (gr_text BCM5 (at 246.38 181.61) (layer F.SilkS))
  (gr_text V10 (at 246.38 185.42) (layer F.SilkS))
  (gr_text BCM6 (at 246.38 189.23) (layer F.SilkS))
  (gr_text GND (at 246.38 193.04) (layer F.SilkS))
  (gr_text GND (at 246.38 177.8) (layer F.SilkS))
  (gr_text BCM7 (at 246.38 173.99) (layer F.SilkS))
  (gr_text V9 (at 246.38 170.18) (layer F.SilkS))
  (gr_text BCM8 (at 246.38 166.37) (layer F.SilkS))
  (gr_text BCM25 (at 246.38 151.13) (layer F.SilkS))
  (gr_text V8 (at 246.38 154.94) (layer F.SilkS))
  (gr_text BCM11 (at 246.38 158.75) (layer F.SilkS))
  (gr_text GND (at 246.38 162.56) (layer F.SilkS))
  (gr_text GND (at 246.38 147.32) (layer F.SilkS))
  (gr_text BCM9 (at 246.38 143.51) (layer F.SilkS))
  (gr_text V7 (at 246.38 139.7) (layer F.SilkS))
  (gr_text BCM10 (at 246.38 135.89) (layer F.SilkS))
  (gr_text BCM23 (at 246.38 120.65) (layer F.SilkS))
  (gr_text V6 (at 246.38 124.46) (layer F.SilkS))
  (gr_text BCM24 (at 246.38 128.27) (layer F.SilkS))
  (gr_text GND (at 246.38 132.08) (layer F.SilkS))
  (gr_text BCM27 (at 246.38 105.41) (layer F.SilkS))
  (gr_text V5 (at 246.38 109.22) (layer F.SilkS))
  (gr_text BCM22 (at 246.38 113.03) (layer F.SilkS))
  (gr_text GND (at 246.38 116.84) (layer F.SilkS))
  (gr_text BCM17 (at 246.38 90.17) (layer F.SilkS))
  (gr_text V4 (at 246.38 93.98) (layer F.SilkS))
  (gr_text BCM18 (at 246.38 97.79) (layer F.SilkS))
  (gr_text GND (at 246.38 101.6) (layer F.SilkS))
  (gr_text GND (at 246.38 86.36) (layer F.SilkS))
  (dimension 203.2 (width 0.3) (layer Cmts.User)
    (gr_text "8.0000 in" (at 190.42 147.32 270) (layer Cmts.User))
    (feature1 (pts (xy 203.2 248.92) (xy 189.07 248.92)))
    (feature2 (pts (xy 203.2 45.72) (xy 189.07 45.72)))
    (crossbar (pts (xy 191.77 45.72) (xy 191.77 248.92)))
    (arrow1a (pts (xy 191.77 248.92) (xy 191.183579 247.793496)))
    (arrow1b (pts (xy 191.77 248.92) (xy 192.356421 247.793496)))
    (arrow2a (pts (xy 191.77 45.72) (xy 191.183579 46.846504)))
    (arrow2b (pts (xy 191.77 45.72) (xy 192.356421 46.846504)))
  )
  (dimension 58.42 (width 0.3) (layer Cmts.User)
    (gr_text "2.3000 in" (at 232.41 39.29) (layer Cmts.User))
    (feature1 (pts (xy 203.2 45.72) (xy 203.2 37.94)))
    (feature2 (pts (xy 261.62 45.72) (xy 261.62 37.94)))
    (crossbar (pts (xy 261.62 40.64) (xy 203.2 40.64)))
    (arrow1a (pts (xy 203.2 40.64) (xy 204.326504 40.053579)))
    (arrow1b (pts (xy 203.2 40.64) (xy 204.326504 41.226421)))
    (arrow2a (pts (xy 261.62 40.64) (xy 260.493496 40.053579)))
    (arrow2b (pts (xy 261.62 40.64) (xy 260.493496 41.226421)))
  )
  (gr_text BCM15 (at 246.38 82.55) (layer F.SilkS))
  (gr_text V3 (at 246.38 78.74) (layer F.SilkS))
  (gr_text BCM14 (at 246.38 74.93) (layer F.SilkS))
  (gr_text GND (at 246.38 71.12) (layer F.SilkS))
  (gr_text BCM3 (at 246.38 67.31) (layer F.SilkS))
  (gr_text V2 (at 246.38 63.5) (layer F.SilkS))
  (gr_text BCM2 (at 246.38 59.69) (layer F.SilkS))
  (gr_text GND (at 246.38 55.88) (layer F.SilkS))
  (gr_text BCM4 (at 246.38 52.07) (layer F.SilkS))
  (gr_text V1 (at 246.38 48.26) (layer F.SilkS))
  (dimension 55.88 (width 0.3) (layer Cmts.User)
    (gr_text "2.2000 in" (at 197.405 77.47 90) (layer Cmts.User))
    (feature1 (pts (xy 207.01 49.53) (xy 196.055 49.53)))
    (feature2 (pts (xy 207.01 105.41) (xy 196.055 105.41)))
    (crossbar (pts (xy 198.755 105.41) (xy 198.755 49.53)))
    (arrow1a (pts (xy 198.755 49.53) (xy 199.341421 50.656504)))
    (arrow1b (pts (xy 198.755 49.53) (xy 198.168579 50.656504)))
    (arrow2a (pts (xy 198.755 105.41) (xy 199.341421 104.283496)))
    (arrow2b (pts (xy 198.755 105.41) (xy 198.168579 104.283496)))
  )
  (dimension 83.82 (width 0.3) (layer Cmts.User)
    (gr_text "3.3000 in" (at 197.405 147.32 90) (layer Cmts.User))
    (feature1 (pts (xy 207.01 105.41) (xy 196.055 105.41)))
    (feature2 (pts (xy 207.01 189.23) (xy 196.055 189.23)))
    (crossbar (pts (xy 198.755 189.23) (xy 198.755 105.41)))
    (arrow1a (pts (xy 198.755 105.41) (xy 199.341421 106.536504)))
    (arrow1b (pts (xy 198.755 105.41) (xy 198.168579 106.536504)))
    (arrow2a (pts (xy 198.755 189.23) (xy 199.341421 188.103496)))
    (arrow2b (pts (xy 198.755 189.23) (xy 198.168579 188.103496)))
  )
  (dimension 55.88 (width 0.3) (layer Cmts.User)
    (gr_text "2.2000 in" (at 197.405 217.17 90) (layer Cmts.User))
    (feature1 (pts (xy 207.01 189.23) (xy 196.055 189.23)))
    (feature2 (pts (xy 207.01 245.11) (xy 196.055 245.11)))
    (crossbar (pts (xy 198.755 245.11) (xy 198.755 189.23)))
    (arrow1a (pts (xy 198.755 189.23) (xy 199.341421 190.356504)))
    (arrow1b (pts (xy 198.755 189.23) (xy 198.168579 190.356504)))
    (arrow2a (pts (xy 198.755 245.11) (xy 199.341421 243.983496)))
    (arrow2b (pts (xy 198.755 245.11) (xy 198.168579 243.983496)))
  )
  (dimension 50.8 (width 0.3) (layer Cmts.User)
    (gr_text "2.0000 in" (at 232.41 254.715) (layer Cmts.User))
    (feature1 (pts (xy 257.81 245.11) (xy 257.81 256.065)))
    (feature2 (pts (xy 207.01 245.11) (xy 207.01 256.065)))
    (crossbar (pts (xy 207.01 253.365) (xy 257.81 253.365)))
    (arrow1a (pts (xy 257.81 253.365) (xy 256.683496 253.951421)))
    (arrow1b (pts (xy 257.81 253.365) (xy 256.683496 252.778579)))
    (arrow2a (pts (xy 207.01 253.365) (xy 208.136504 253.951421)))
    (arrow2b (pts (xy 207.01 253.365) (xy 208.136504 252.778579)))
  )
  (gr_text "12V\n5V\n3V3" (at 230.632 218.44) (layer F.SilkS))
  (gr_text "12V\n5V\n3V3" (at 230.505 203.2) (layer F.SilkS))
  (gr_text "12V\n5V\n3V3" (at 230.505 187.96) (layer F.SilkS))
  (gr_text "12V\n5V\n3V3" (at 230.505 172.72) (layer F.SilkS))
  (gr_text "12V\n5V\n3V3" (at 230.505 157.48) (layer F.SilkS))
  (gr_text "12V\n5V\n3V3" (at 230.505 142.24) (layer F.SilkS))
  (gr_text "12V\n5V\n3V3" (at 230.505 81.28) (layer F.SilkS))
  (gr_text "12V\n5V\n3V3" (at 230.505 127) (layer F.SilkS))
  (gr_text "12V\n5V\n3V3" (at 230.505 111.76) (layer F.SilkS))
  (gr_text "12V\n5V\n3V3" (at 230.505 96.52) (layer F.SilkS))
  (gr_text "12V\n5V\n3V3" (at 230.505 66.04) (layer F.SilkS))
  (gr_text "12V\n5V\n3V3" (at 230.632 233.934) (layer F.SilkS))
  (target plus (at 215.265 245.745) (size 5) (width 0.15) (layer Edge.Cuts))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 261.62 248.92) (xy 203.2 248.92) (xy 203.2 45.72) (xy 261.62 45.72)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 261.62 248.92) (xy 203.2 248.92) (xy 203.2 45.72) (xy 261.62 45.72)
      )
    )
  )
)
