<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.2.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="107.95" y2="0" width="0" layer="20"/>
<wire x1="107.95" y1="0" x2="107.95" y2="39.37" width="0" layer="20"/>
<wire x1="107.95" y1="39.37" x2="0" y2="39.37" width="0" layer="20"/>
<wire x1="0" y1="39.37" x2="0" y2="0" width="0" layer="20"/>
<text>Klair de Klune</text>
</plain>
<libraries>
<library name="zth_eteknet">
<packages>
<package name="PAD-LARGE-N">
<description>Through-hole pad, large size, "narrow"</description>
</package>
<package name="POT16RAR">
<description>16mm single-gang potentiometer, right-angle PCB mount, smaller trace</description>
</package>
<package name="RESISTOR-0.25W">
<description>Resistor - 1/4 Watt</description>
</package>
<package name="E2-5-6">
<description>Capacitor - polar electrolytic</description>
</package>
<package name="CMX-L01">
<description>Capacitor - electrolytic, polar, large</description>
</package>
<package name="CMX-M01">
<description>Capacitor - electrolytic, polar, medium</description>
</package>
<package name="DIODE-L">
<description>Diode</description>
</package>
<package name="DIODE-1N40XX">
<description>1N400X diode</description>
</package>
<package name="LED-RL-N">
<description>LED (remote), Large, smaller hole size</description>
</package>
<package name="DIL08">
<description>Dual In Line Package - 8-pin</description>
</package>
<package name="C050-025X075WW-S">
<description>Capacitor - grid 5 mm (2x wide)</description>
</package>
<package name="SPDTR-L">
<description>SPDT switch, remote connection, larger size</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="V" library="zth_eteknet" package="PAD-LARGE-N" value=" ">
<attribute name="NAME"/>
</element>
<element name="G" library="zth_eteknet" package="PAD-LARGE-N" value=" ">
<attribute name="NAME"/>
</element>
<element name="GAIN-A" library="zth_eteknet" package="POT16RAR" value="B100k"/>
<element name="R29" library="zth_eteknet" package="RESISTOR-0.25W" value="6k8">
<attribute name="NAME"/>
</element>
<element name="X" library="zth_eteknet" package="PAD-LARGE-N" value=" ">
<attribute name="NAME"/>
</element>
<element name="C19" library="zth_eteknet" package="CMX-M01" value="1u">
<attribute name="NAME"/>
</element>
<element name="C17" library="zth_eteknet" package="CMX-L01" value="47u">
<attribute name="NAME"/>
</element>
<element name="D4" library="zth_eteknet" package="DIODE-1N40XX" value="1N4742">
<attribute name="NAME"/>
</element>
<element name="R14" library="zth_eteknet" package="RESISTOR-0.25W" value="18k">
<attribute name="NAME"/>
</element>
<element name="D1" library="zth_eteknet" package="LED-RL-N" value="red">
<attribute name="NAME"/>
</element>
<element name="R30" library="zth_eteknet" package="RESISTOR-0.25W" value="6k8">
<attribute name="NAME"/>
</element>
<element name="Y" library="zth_eteknet" package="PAD-LARGE-N" value=" ">
<attribute name="NAME"/>
</element>
<element name="IC1" library="zth_eteknet" package="DIL08" value="MAX1044">
<attribute name="NAME"/>
</element>
<element name="D6" library="zth_eteknet" package="DIODE-1N40XX" value="4001">
<attribute name="NAME"/>
</element>
<element name="D5" library="zth_eteknet" package="DIODE-1N40XX" value="4001">
<attribute name="NAME"/>
</element>
<element name="C20" library="zth_eteknet" package="CMX-M01" value="1u">
<attribute name="NAME"/>
</element>
<element name="C22" library="zth_eteknet" package="CMX-M01" value="1u">
<attribute name="NAME"/>
</element>
<element name="C21" library="zth_eteknet" package="CMX-M01" value="1u">
<attribute name="NAME"/>
</element>
<element name="C18" library="zth_eteknet" package="CMX-M01" value="47u">
<attribute name="NAME"/>
</element>
<element name="IC2" library="zth_eteknet" package="DIL08" value="TL072">
<attribute name="NAME"/>
</element>
<element name="R1" library="zth_eteknet" package="RESISTOR-0.25W" value="10k">
<attribute name="NAME"/>
</element>
<element name="C1" library="zth_eteknet" package="C050-025X075WW-S" value="100n">
<attribute name="NAME"/>
</element>
<element name="R2" library="zth_eteknet" package="RESISTOR-0.25W" value="1M">
<attribute name="NAME"/>
</element>
<element name="R7" library="zth_eteknet" package="RESISTOR-0.25W" value="1k5">
<attribute name="NAME"/>
</element>
<element name="R19" library="zth_eteknet" package="RESISTOR-0.25W" value="15k">
<attribute name="NAME"/>
</element>
<element name="C3" library="zth_eteknet" package="C050-025X075WW-S" value="100n">
<attribute name="NAME"/>
</element>
<element name="C4" library="zth_eteknet" package="C050-025X075WW-S" value="68n">
<attribute name="NAME"/>
</element>
<element name="R5" library="zth_eteknet" package="RESISTOR-0.25W" value="5k1">
<attribute name="NAME"/>
</element>
<element name="R6" library="zth_eteknet" package="RESISTOR-0.25W" value="10k">
<attribute name="NAME"/>
</element>
<element name="C5" library="zth_eteknet" package="C050-025X075WW-S" value="68n">
<attribute name="NAME"/>
</element>
<element name="GAIN-B" library="zth_eteknet" package="POT16RAR" value="B100k"/>
<element name="R8" library="zth_eteknet" package="RESISTOR-0.25W" value="1k5">
<attribute name="NAME"/>
</element>
<element name="C6" library="zth_eteknet" package="C050-025X075WW-S" value="390n">
<attribute name="NAME"/>
</element>
<element name="R9" library="zth_eteknet" package="RESISTOR-0.25W" value="1k">
<attribute name="NAME"/>
</element>
<element name="R10" library="zth_eteknet" package="RESISTOR-0.25W" value="2k">
<attribute name="NAME"/>
</element>
<element name="C16" library="zth_eteknet" package="E2-5-6" value="1u">
<attribute name="NAME"/>
</element>
<element name="R11" library="zth_eteknet" package="RESISTOR-0.25W" value="15k">
<attribute name="NAME"/>
</element>
<element name="R12" library="zth_eteknet" package="RESISTOR-0.25W" value="422k">
<attribute name="NAME"/>
</element>
<element name="C7" library="zth_eteknet" package="C050-025X075WW-S" value="82n">
<attribute name="NAME"/>
</element>
<element name="C8" library="zth_eteknet" package="C050-025X075WW-S" value="390p">
<attribute name="NAME"/>
</element>
<element name="C9" library="zth_eteknet" package="CMX-M01" value="1u">
<attribute name="NAME"/>
</element>
<element name="R13" library="zth_eteknet" package="RESISTOR-0.25W" value="1k">
<attribute name="NAME"/>
</element>
<element name="D2" library="zth_eteknet" package="DIODE-L" value="1N34A">
<attribute name="NAME"/>
</element>
<element name="D3" library="zth_eteknet" package="DIODE-L" value="1N34A">
<attribute name="NAME"/>
</element>
<element name="C10" library="zth_eteknet" package="CMX-M01" value="1u">
<attribute name="NAME"/>
</element>
<element name="C11" library="zth_eteknet" package="C050-025X075WW-S" value="2n2">
<attribute name="NAME"/>
</element>
<element name="R16" library="zth_eteknet" package="RESISTOR-0.25W" value="47k">
<attribute name="NAME"/>
</element>
<element name="R15" library="zth_eteknet" package="RESISTOR-0.25W" value="22k">
<attribute name="NAME"/>
</element>
<element name="R17" library="zth_eteknet" package="RESISTOR-0.25W" value="27k">
<attribute name="NAME"/>
</element>
<element name="R18" library="zth_eteknet" package="RESISTOR-0.25W" value="12k">
<attribute name="NAME"/>
</element>
<element name="C12" library="zth_eteknet" package="C050-025X075WW-S" value="27n">
<attribute name="NAME"/>
</element>
<element name="R20" library="zth_eteknet" package="RESISTOR-0.25W" value="392k">
<attribute name="NAME"/>
</element>
<element name="IC3" library="zth_eteknet" package="DIL08" value="TL072">
<attribute name="NAME"/>
</element>
<element name="C13" library="zth_eteknet" package="C050-025X075WW-S" value="820p">
<attribute name="NAME"/>
</element>
<element name="R21" library="zth_eteknet" package="RESISTOR-0.25W" value="1k8">
<attribute name="NAME"/>
</element>
<element name="R23" library="zth_eteknet" package="RESISTOR-0.25W" value="4k7">
<attribute name="NAME"/>
</element>
<element name="R22" library="zth_eteknet" package="RESISTOR-0.25W" value="100k">
<attribute name="NAME"/>
</element>
<element name="R24" library="zth_eteknet" package="RESISTOR-0.25W" value="100k">
<attribute name="NAME"/>
</element>
<element name="TREBLE" library="zth_eteknet" package="POT16RAR" value="B10k"/>
<element name="C14" library="zth_eteknet" package="C050-025X075WW-S" value="3n9">
<attribute name="NAME"/>
</element>
<element name="R25" library="zth_eteknet" package="RESISTOR-0.25W" value="560">
<attribute name="NAME"/>
</element>
<element name="OUTPUT" library="zth_eteknet" package="POT16RAR" value="B10k"/>
<element name="R26" library="zth_eteknet" package="RESISTOR-0.25W" value="68k">
<attribute name="NAME"/>
</element>
<element name="R27" library="zth_eteknet" package="RESISTOR-0.25W" value="68k">
<attribute name="NAME"/>
</element>
<element name="R28" library="zth_eteknet" package="RESISTOR-0.25W" value="100k">
<attribute name="NAME"/>
<attribute name="SPICEPREFIX" value="R"/>
</element>
<element name="SW" library="zth_eteknet" package="SPDTR-L" value="SPDT-RL">
<attribute name="NAME"/>
</element>
<element name="R3" library="zth_eteknet" package="RESISTOR-0.25W" value="100k">
<attribute name="NAME"/>
</element>
<element name="R4" library="zth_eteknet" package="RESISTOR-0.25W" value="560">
<attribute name="NAME"/>
</element>
<element name="YG" library="zth_eteknet" package="PAD-LARGE-N" value=" ">
<attribute name="NAME"/>
</element>
<element name="C2" library="zth_eteknet" package="CMX-M01" value="4u7">
<attribute name="NAME"/>
</element>
<element name="C15" library="zth_eteknet" package="CMX-M01" value="4u7">
<attribute name="NAME"/>
</element>
<element name="LGS" library="zth_eteknet" package="PAD-LARGE-N" value=" ">
<attribute name="NAME"/>
</element>
<element name="LG" library="zth_eteknet" package="PAD-LARGE-N" value=" ">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="C17" pad="-"/>
<contactref element="D4" pad="A"/>
<contactref element="G" pad="1"/>
<contactref element="IC1" pad="3"/>
<contactref element="C22" pad="-"/>
<contactref element="R30" pad="1"/>
<contactref element="C18" pad="-"/>
<contactref element="IC2" pad="4"/>
<contactref element="C16" pad="-"/>
<contactref element="D3" pad="C"/>
<contactref element="D2" pad="A"/>
<contactref element="OUTPUT" pad="P0"/>
<contactref element="R3" pad="1"/>
<contactref element="R28" pad="1"/>
<contactref element="YG" pad="1"/>
<contactref element="C19" pad="+"/>
<contactref element="LG" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="R14" pad="1"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="V+">
<contactref element="C17" pad="+"/>
<contactref element="D4" pad="C"/>
<contactref element="V" pad="1"/>
<contactref element="IC1" pad="1"/>
<contactref element="IC1" pad="8"/>
<contactref element="R29" pad="2"/>
<contactref element="IC2" pad="8"/>
<contactref element="D5" pad="A"/>
<contactref element="R14" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="C20" pad="+"/>
<contactref element="D6" pad="A"/>
<contactref element="D5" pad="C"/>
</signal>
<signal name="N$5">
<contactref element="IC1" pad="4"/>
<contactref element="C21" pad="-"/>
</signal>
<signal name="N$6">
<contactref element="IC1" pad="2"/>
<contactref element="C21" pad="+"/>
<contactref element="C20" pad="-"/>
</signal>
<signal name="VSS">
<contactref element="R29" pad="1"/>
<contactref element="R30" pad="2"/>
<contactref element="C18" pad="+"/>
<contactref element="R2" pad="2"/>
<contactref element="IC3" pad="3"/>
<contactref element="IC3" pad="5"/>
<contactref element="R8" pad="1"/>
<contactref element="R9" pad="1"/>
<contactref element="GAIN-B" pad="W"/>
<contactref element="GAIN-A" pad="P1"/>
</signal>
<signal name="VEE">
<contactref element="IC1" pad="5"/>
<contactref element="IC3" pad="4"/>
<contactref element="C19" pad="-"/>
</signal>
<signal name="VCC">
<contactref element="C22" pad="+"/>
<contactref element="IC3" pad="8"/>
<contactref element="D6" pad="C"/>
</signal>
<signal name="N$2">
<contactref element="X" pad="1"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="IC2" pad="3"/>
<contactref element="R2" pad="1"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="IC2" pad="1"/>
<contactref element="IC2" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="R5" pad="2"/>
<contactref element="C4" pad="1"/>
<contactref element="C2" pad="+"/>
</signal>
<signal name="N$3">
<contactref element="R1" pad="2"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="C3" pad="2"/>
<contactref element="C5" pad="1"/>
<contactref element="R6" pad="1"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="R5" pad="1"/>
<contactref element="C4" pad="2"/>
<contactref element="R8" pad="2"/>
<contactref element="C6" pad="1"/>
<contactref element="GAIN-A" pad="P0"/>
</signal>
<signal name="N$13">
<contactref element="C5" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="IC2" pad="5"/>
<contactref element="GAIN-B" pad="P0"/>
</signal>
<signal name="N$12">
<contactref element="C6" pad="2"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="C16" pad="+"/>
<contactref element="R7" pad="2"/>
<contactref element="R19" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="R10" pad="1"/>
<contactref element="R11" pad="1"/>
<contactref element="C7" pad="1"/>
</signal>
<signal name="N$17">
<contactref element="C8" pad="1"/>
<contactref element="R12" pad="1"/>
<contactref element="R11" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="IC2" pad="6"/>
</signal>
<signal name="N$18">
<contactref element="R12" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="IC2" pad="7"/>
<contactref element="C9" pad="+"/>
</signal>
<signal name="N$20">
<contactref element="R16" pad="1"/>
<contactref element="C11" pad="1"/>
<contactref element="C10" pad="+"/>
</signal>
<signal name="N$21">
<contactref element="C11" pad="2"/>
<contactref element="R15" pad="2"/>
</signal>
<signal name="N$24">
<contactref element="R17" pad="1"/>
<contactref element="R18" pad="1"/>
<contactref element="R15" pad="1"/>
<contactref element="GAIN-A" pad="W"/>
</signal>
<signal name="N$25">
<contactref element="R18" pad="2"/>
<contactref element="C12" pad="2"/>
</signal>
<signal name="N$23">
<contactref element="R20" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="R22" pad="1"/>
<contactref element="R21" pad="1"/>
<contactref element="IC3" pad="7"/>
</signal>
<signal name="N$28">
<contactref element="R20" pad="1"/>
<contactref element="C13" pad="1"/>
<contactref element="R16" pad="2"/>
<contactref element="C12" pad="1"/>
<contactref element="R17" pad="2"/>
<contactref element="R19" pad="2"/>
<contactref element="IC3" pad="6"/>
</signal>
<signal name="N$22">
<contactref element="R22" pad="2"/>
<contactref element="C14" pad="2"/>
<contactref element="R24" pad="1"/>
<contactref element="IC3" pad="2"/>
</signal>
<signal name="N$29">
<contactref element="R23" pad="1"/>
<contactref element="TREBLE" pad="P0"/>
</signal>
<signal name="N$30">
<contactref element="R24" pad="2"/>
<contactref element="R23" pad="2"/>
<contactref element="IC3" pad="1"/>
<contactref element="C15" pad="+"/>
</signal>
<signal name="N$33">
<contactref element="OUTPUT" pad="W"/>
<contactref element="SW" pad="T1"/>
<contactref element="R27" pad="1"/>
</signal>
<signal name="N$34">
<contactref element="R26" pad="1"/>
<contactref element="SW" pad="T2"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$35">
<contactref element="SW" pad="C"/>
<contactref element="R26" pad="2"/>
<contactref element="R27" pad="2"/>
<contactref element="R28" pad="2"/>
<contactref element="Y" pad="1"/>
</signal>
<signal name="N$36">
<contactref element="R4" pad="1"/>
<contactref element="R3" pad="2"/>
<contactref element="C2" pad="-"/>
</signal>
<signal name="N$31">
<contactref element="OUTPUT" pad="P1"/>
<contactref element="R25" pad="1"/>
</signal>
<signal name="N$32">
<contactref element="R25" pad="2"/>
<contactref element="C15" pad="-"/>
</signal>
<signal name="N$14">
<contactref element="GAIN-B" pad="P1"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="N$26">
<contactref element="R21" pad="2"/>
<contactref element="TREBLE" pad="P1"/>
</signal>
<signal name="N$27">
<contactref element="C14" pad="1"/>
<contactref element="TREBLE" pad="W"/>
</signal>
<signal name="N$37">
<contactref element="R13" pad="2"/>
<contactref element="D2" pad="C"/>
<contactref element="D3" pad="A"/>
<contactref element="C10" pad="-"/>
</signal>
<signal name="N$19">
<contactref element="D1" pad="C"/>
<contactref element="LGS" pad="1"/>
</signal>
<signal name="N$16">
<contactref element="C9" pad="-"/>
<contactref element="R13" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
