<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="72.39" y2="0" width="0" layer="20"/>
<wire x1="72.39" y1="0" x2="72.39" y2="72.39" width="0" layer="20"/>
<wire x1="72.39" y1="72.39" x2="0" y2="72.39" width="0" layer="20"/>
<wire x1="0" y1="72.39" x2="0" y2="0" width="0" layer="20"/>
<text>TRIG TIT</text>
<text>TRIG RING</text>
<text>15KV IN</text>
<text>GND</text>
<text>SCR</text>
</plain>
<libraries>
<library name="CONRADS">
<packages>
<package name="SLIMMOX101">
</package>
<package name="SLIMMOX108">
</package>
<package name="105MWR400K">
</package>
<package name="615R150GAST50">
</package>
<package name="CONRADSNEW_TR-180">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R3" library="CONRADS" package="SLIMMOX101" value="1M"/>
<element name="R2" library="CONRADS" package="SLIMMOX108" value="150M"/>
<element name="R1" library="CONRADS" package="SLIMMOX108" value="150M"/>
<element name="C1" library="CONRADS" package="105MWR400K" value="1uF"/>
<element name="C2" library="CONRADS" package="615R150GAST50" value="500pF"/>
<element name="R4" library="CONRADS" package="SLIMMOX108" value="1M"/>
<element name="U$1" library="CONRADS" package="CONRADSNEW_TR-180" value="TR-180B"/>
</elements>
<signals>
<signal name="15KV">
<contactref element="R2" pad="P$1"/>
<contactref element="R1" pad="P$1"/>
</signal>
<signal name="SCR_IN">
<contactref element="R2" pad="P$2"/>
<contactref element="R3" pad="P$1"/>
<contactref element="R1" pad="P$2"/>
<contactref element="C1" pad="P$1"/>
</signal>
<signal name="PS">
<contactref element="C1" pad="P$2"/>
<contactref element="U$1" pad="PS"/>
</signal>
<signal name="ANODE">
<contactref element="R4" pad="P$1"/>
</signal>
<signal name="TRIG">
<contactref element="R4" pad="P$2"/>
<contactref element="C2" pad="P$1"/>
</signal>
<signal name="SF">
<contactref element="C2" pad="P$2"/>
<contactref element="U$1" pad="SF"/>
</signal>
<signal name="GND">
<contactref element="R3" pad="P$2"/>
<contactref element="U$1" pad="SS"/>
<contactref element="U$1" pad="PF"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
