<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="4.4" y1="1.8" x2="33.07" y2="1.9" width="0" layer="20"/>
<wire x1="33.07" y1="1.9" x2="33.2" y2="1.9" width="0" layer="20"/>
<wire x1="33.2" y1="1.9" x2="33.1" y2="45.8" width="0" layer="20"/>
<wire x1="33.1" y1="45.8" x2="4.4" y2="45.9" width="0" layer="20"/>
<wire x1="4.4" y1="45.9" x2="4.4" y2="1.8" width="0" layer="20"/>
</plain>
<libraries>
<library name="JST">
<packages>
<package name="JST-XH-11PIN-2.5MM">
<description>JST-XH-11Pin-2.5mm</description>
</package>
<package name="JST-9PIN-2MM">
<description>JST-PH-9Pin-2mm</description>
</package>
<package name="JST-9PIN-2MM-10,18">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JSTXH11PIN2.5MM1" library="JST" package="JST-XH-11PIN-2.5MM" value="JST-XH-11PIN-2.5MM"/>
<element name="JST-PH-9PIN-2MM1" library="JST" package="JST-9PIN-2MM" value="JST-PH-9PIN-2MM"/>
<element name="JST-9PIN-2MM-10,1" library="JST" package="JST-9PIN-2MM-10,18" value=""/>
</elements>
<signals>
<signal name="PIN1POSTIVE">
<contactref element="JSTXH11PIN2.5MM1" pad="PIN1POSITIVE"/>
<contactref element="JST-PH-9PIN-2MM1" pad="P$1"/>
</signal>
<signal name="PIN2">
<contactref element="JSTXH11PIN2.5MM1" pad="PIN2"/>
<contactref element="JST-PH-9PIN-2MM1" pad="P$2"/>
</signal>
<signal name="PIN3">
<contactref element="JSTXH11PIN2.5MM1" pad="PIN3"/>
<contactref element="JST-PH-9PIN-2MM1" pad="P$3"/>
</signal>
<signal name="PIN4">
<contactref element="JSTXH11PIN2.5MM1" pad="PIN4"/>
<contactref element="JST-PH-9PIN-2MM1" pad="P$4"/>
</signal>
<signal name="PIN5">
<contactref element="JSTXH11PIN2.5MM1" pad="PIN5"/>
<contactref element="JST-PH-9PIN-2MM1" pad="P$5"/>
</signal>
<signal name="PIN6">
<contactref element="JSTXH11PIN2.5MM1" pad="PIN6"/>
<contactref element="JST-PH-9PIN-2MM1" pad="P$6"/>
</signal>
<signal name="PIN7">
<contactref element="JSTXH11PIN2.5MM1" pad="PIN7"/>
<contactref element="JST-PH-9PIN-2MM1" pad="P$7"/>
</signal>
<signal name="PIN8">
<contactref element="JSTXH11PIN2.5MM1" pad="PIN8"/>
<contactref element="JST-PH-9PIN-2MM1" pad="P$8"/>
</signal>
<signal name="PIN9">
<contactref element="JSTXH11PIN2.5MM1" pad="PIN9"/>
<contactref element="JST-PH-9PIN-2MM1" pad="P$9"/>
</signal>
<signal name="PIN10">
<contactref element="JSTXH11PIN2.5MM1" pad="PIN10"/>
<contactref element="JST-9PIN-2MM-10,1" pad="P$10"/>
</signal>
<signal name="PIN11">
<contactref element="JSTXH11PIN2.5MM1" pad="PIN11"/>
<contactref element="JST-9PIN-2MM-10,1" pad="P$11"/>
</signal>
<signal name="PIN12">
<contactref element="JST-9PIN-2MM-10,1" pad="P$12"/>
</signal>
<signal name="PIN13">
<contactref element="JST-9PIN-2MM-10,1" pad="P$13"/>
</signal>
<signal name="PIN14">
<contactref element="JST-9PIN-2MM-10,1" pad="P$14"/>
</signal>
<signal name="PIN15">
<contactref element="JST-9PIN-2MM-10,1" pad="P$15"/>
</signal>
<signal name="PIN16">
<contactref element="JST-9PIN-2MM-10,1" pad="P$16"/>
</signal>
<signal name="PIN17">
<contactref element="JST-9PIN-2MM-10,1" pad="P$17"/>
</signal>
<signal name="PIN18">
<contactref element="JST-9PIN-2MM-10,1" pad="P$18"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
