(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 82)
    (no_connects 0)
    (area 92.424999 89.924999 172.575001 110.075001)
    (thickness 1.6)
    (drawings 5)
    (tracks 202)
    (zones 0)
    (modules 36)
    (nets 25)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (trace_clearance 0.1524)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 4.4 4.4)
    (pad_drill 2.2)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 92.5 110)
    (grid_origin 92.5 110)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C6-Pad1)")
  (net 2 "Net-(C7-Pad1)")
  (net 3 "Net-(C7-Pad2)")
  (net 4 "Net-(C8-Pad1)")
  (net 5 "Net-(D1-Pad2)")
  (net 6 "Net-(P2-Pad3)")
  (net 7 "Net-(P2-Pad2)")
  (net 8 "Net-(P2-Pad1)")
  (net 9 "Net-(R2-Pad2)")
  (net 10 "Net-(R3-Pad2)")
  (net 11 "Net-(R5-Pad1)")
  (net 12 "Net-(R9-Pad2)")
  (net 13 "Net-(R10-Pad1)")
  (net 14 "Net-(U1-Pad1)")
  (net 15 "Net-(U1-Pad2)")
  (net 16 "Net-(U2-Pad6)")
  (net 17 "Net-(U3-Pad8)")
  (net 18 "Net-(U3-Pad14)")
  (net 19 "Net-(U4-Pad4)")
  (net 20 /GND)
  (net 21 /VINP)
  (net 22 /5V0)
  (net 23 /VIN)
  (net 24 /VINF)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.254)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net /5V0)
    (add_net /GND)
    (add_net /VIN)
    (add_net /VINF)
    (add_net /VINP)
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(C7-Pad2)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(P2-Pad1)")
    (add_net "Net-(P2-Pad2)")
    (add_net "Net-(P2-Pad3)")
    (add_net "Net-(R10-Pad1)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R5-Pad1)")
    (add_net "Net-(R9-Pad2)")
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U2-Pad6)")
    (add_net "Net-(U3-Pad14)")
    (add_net "Net-(U3-Pad8)")
    (add_net "Net-(U4-Pad4)")
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2_Pad (layer F.Cu) (tedit 58C0B60E)
    (at 156.5 93)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2_Pad (at 0 3.2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask)
      (net 20 /GND))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2_Pad (layer F.Cu) (tedit 58C0B608)
    (at 156.5 107)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2_Pad (at 0 3.2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask)
      (net 20 /GND))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2_Pad (layer F.Cu) (tedit 58C0B602)
    (at 95.5 107)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2_Pad (at 0 3.2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask)
      (net 20 /GND))
  )
  (module Capacitors_SMD:C_1210 (layer F.Cu) (tedit 58C0A812)
    (at 117.4 102.6 270)
    (descr "Capacitor SMD 1210, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C1 (at 0 -2.25 270) (layer F.SilkS) hide)
    (fp_text value "0.22uF 250V" (at 0 2.5 270) (layer F.Fab))
    (fp_text user %R (at 0 -2.25 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.5 0 270) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 24 /VINF))
    (pad 2 smd rect (at 1.5 0 270) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 20 /GND))
    (model Capacitors_SMD.3dshapes/C_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1210 (layer F.Cu) (tedit 58C0A824)
    (at 129.55 102 180)
    (descr "Capacitor SMD 1210, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C2 (at 0 -2.25 180) (layer F.SilkS) hide)
    (fp_text value "10uF 50V" (at 0 2.5 180) (layer F.Fab))
    (fp_text user %R (at 0 -2.25 180) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 180) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 21 /VINP))
    (pad 2 smd rect (at 1.5 0 180) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 20 /GND))
    (model Capacitors_SMD.3dshapes/C_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1210 (layer F.Cu) (tedit 58C0A827)
    (at 129.55 98.8 180)
    (descr "Capacitor SMD 1210, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C3 (at 0 -2.25 180) (layer F.SilkS) hide)
    (fp_text value "10uF 50V" (at 0 2.5 180) (layer F.Fab))
    (fp_text user %R (at 0 -2.25 180) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 180) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 21 /VINP))
    (pad 2 smd rect (at 1.5 0 180) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 20 /GND))
    (model Capacitors_SMD.3dshapes/C_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1210 (layer F.Cu) (tedit 58C0A82A)
    (at 129.55 95.6 180)
    (descr "Capacitor SMD 1210, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C4 (at 0 -2.25 180) (layer F.SilkS) hide)
    (fp_text value "10uF 50V" (at 0 2.5 180) (layer F.Fab))
    (fp_text user %R (at 0 -2.25 180) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 180) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 21 /VINP))
    (pad 2 smd rect (at 1.5 0 180) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 20 /GND))
    (model Capacitors_SMD.3dshapes/C_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58C0A822)
    (at 130.05 104.6 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at 0 -1.5 180) (layer F.SilkS) hide)
    (fp_text value "10nF 50V" (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 21 /VINP))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 20 /GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58C0A845)
    (at 143.65 97.3)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C6 (at 0 -1.5) (layer F.SilkS) hide)
    (fp_text value "3.3uF 10V" (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.5) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 20 /GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58C0A842)
    (at 143.65 99.2)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C7 (at 0 -1.5) (layer F.SilkS) hide)
    (fp_text value "0.47uF 50V" (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.5) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C7-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58C0A84E)
    (at 143.65 95.4)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C8 (at 0 -1.5) (layer F.SilkS) hide)
    (fp_text value "0.1uF 10V" (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.5) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 20 /GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1210 (layer F.Cu) (tedit 58C0A83A)
    (at 148.15 103.3 270)
    (descr "Capacitor SMD 1210, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C9 (at 0 -2.25 270) (layer F.SilkS) hide)
    (fp_text value "22uF 10V" (at 0 2.5 270) (layer F.Fab))
    (fp_text user %R (at 0 -2.25 270) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 22 /5V0))
    (pad 2 smd rect (at 1.5 0 270) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 20 /GND))
    (model Capacitors_SMD.3dshapes/C_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1210 (layer F.Cu) (tedit 58C0A838)
    (at 144.75 103.3 270)
    (descr "Capacitor SMD 1210, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C10 (at 0 -2.25 270) (layer F.SilkS) hide)
    (fp_text value "22uF 10V" (at 0 2.5 270) (layer F.Fab))
    (fp_text user %R (at 0 -2.25 270) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 22 /5V0))
    (pad 2 smd rect (at 1.5 0 270) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 20 /GND))
    (model Capacitors_SMD.3dshapes/C_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1210 (layer F.Cu) (tedit 58C0A835)
    (at 141.35 103.3 270)
    (descr "Capacitor SMD 1210, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C11 (at 0 -2.25 270) (layer F.SilkS) hide)
    (fp_text value "22uF 10V" (at 0 2.5 270) (layer F.Fab))
    (fp_text user %R (at 0 -2.25 270) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 22 /5V0))
    (pad 2 smd rect (at 1.5 0 270) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 20 /GND))
    (model Capacitors_SMD.3dshapes/C_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58C0A83F)
    (at 146.65 98.2 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C12 (at 0 -1.5 90) (layer F.SilkS) hide)
    (fp_text value "0.1uF 10V" (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 22 /5V0))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 20 /GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SMA_Standard (layer F.Cu) (tedit 58C0A809)
    (at 114 103.9 270)
    (descr "Diode SMA")
    (tags "Diode SMA")
    (attr smd)
    (fp_text reference D1 (at 0 -3.81 270) (layer F.SilkS) hide)
    (fp_text value 30V (at 0 4.3 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0 270) (size 2.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 24 /VINF))
    (pad 2 smd rect (at 2 0 270) (size 2.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D1-Pad2)"))
    (model Diodes_SMD.3dshapes/D_SMA_Standard.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 180))
    )
  )
  (module Diodes_SMD:D_SMA_Standard (layer F.Cu) (tedit 58C0AC87)
    (at 110.3 103.9 270)
    (descr "Diode SMA")
    (tags "Diode SMA")
    (attr smd)
    (fp_text reference D2 (at 0 -3.81 270) (layer F.SilkS) hide)
    (fp_text value 15V (at 0 4.3 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0 270) (size 2.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 20 /GND))
    (pad 2 smd rect (at 2 0 270) (size 2.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D1-Pad2)"))
    (model Diodes_SMD.3dshapes/D_SMA_Standard.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 180))
    )
  )
  (module Fuse_Holders_and_Fuses:Fuse_SMD2920 (layer F.Cu) (tedit 58C0A804)
    (at 113.7 96.3 180)
    (descr "Fuse, 2920 chip size")
    (tags "Fuse SMD2920")
    (attr smd)
    (fp_text reference F1 (at 0 -4.13 180) (layer F.SilkS) hide)
    (fp_text value 2A (at 0 4.38 180) (layer F.Fab))
    (pad 1 smd rect (at -3.7 0 270) (size 5.6 2.3) (layers F.Cu F.Paste F.Mask)
      (net 24 /VINF))
    (pad 2 smd rect (at 3.7 0 270) (size 5.6 2.3) (layers F.Cu F.Paste F.Mask)
      (net 23 /VIN))
  )
  (module aiber:VISHAY-2525 (layer F.Cu) (tedit 58C0A832)
    (at 136.35 103.2 90)
    (fp_text reference L1 (at 0 4.318 90) (layer F.SilkS) hide)
    (fp_text value 2.2uH (at 0.254 -4.064 90) (layer F.Fab))
    (pad 1 smd rect (at -2.921 0 90) (size 2.413 3.429) (layers F.Cu F.Paste F.Mask)
      (net 22 /5V0))
    (pad 2 smd rect (at 2.921 0 90) (size 2.413 3.429) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C7-Pad1)"))
  )
  (module aiber:Molex-1723101102 (layer F.Cu) (tedit 58C0A862)
    (at 92.25 100 270)
    (fp_text reference P1 (at 0 1.3 270) (layer F.SilkS) hide)
    (fp_text value CONN_01X02 (at 0 -17 270) (layer F.Fab))
    (pad 1 thru_hole circle (at -1.75 -13.16 270) (size 2.5 2.5) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 /VIN))
    (pad 2 thru_hole circle (at 1.75 -13.16 270) (size 2.5 2.5) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 /GND))
    (pad "" np_thru_hole circle (at 0 -5.25 270) (size 3.048 3.048) (drill 3.048) (layers *.Cu *.Mask))
  )
  (module aiber:Amphenol-87520-0010BLF (layer F.Cu) (tedit 58C0A85B)
    (at 163.5 100 90)
    (fp_text reference P2 (at 0 12 90) (layer F.SilkS) hide)
    (fp_text value USB_A (at 0 -5 90) (layer F.Fab))
    (pad 3 thru_hole circle (at 1 -2.71 90) (size 1.4 1.4) (drill 0.92) (layers *.Cu *.Mask)
      (net 6 "Net-(P2-Pad3)"))
    (pad 2 thru_hole circle (at -1 -2.71 90) (size 1.4 1.4) (drill 0.92) (layers *.Cu *.Mask)
      (net 7 "Net-(P2-Pad2)"))
    (pad 1 thru_hole circle (at -3.5 -2.71 90) (size 2 2) (drill 0.92) (layers *.Cu *.Mask)
      (net 8 "Net-(P2-Pad1)"))
    (pad 4 thru_hole circle (at 3.5 -2.71 90) (size 2 2) (drill 0.92) (layers *.Cu *.Mask)
      (net 20 /GND))
    (pad 5 thru_hole circle (at -6.57 0 90) (size 3.4 3.4) (drill 2.3) (layers *.Cu *.Mask)
      (net 20 /GND))
    (pad 5 thru_hole circle (at 6.57 0 90) (size 3.4 3.4) (drill 2.3) (layers *.Cu *.Mask)
      (net 20 /GND))
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58C0A807)
    (at 117.4 106.2)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 -1.65) (layer F.SilkS) hide)
    (fp_text value 10k (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.65) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 24 /VINF))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 20 /GND))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58C0A816)
    (at 121.55 102.7)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0 -1.65) (layer F.SilkS) hide)
    (fp_text value 3.9M (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.65) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 24 /VINF))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(R2-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58C0A80E)
    (at 121.55 104.6 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 0 -1.65 180) (layer F.SilkS) hide)
    (fp_text value 220k (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.65 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(R2-Pad2)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(R3-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58C0A80C)
    (at 121.55 106.5 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 0 -1.65 180) (layer F.SilkS) hide)
    (fp_text value 68k (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.65 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(R3-Pad2)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 20 /GND))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58C0A810)
    (at 121.55 100.8 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at 0 -1.65 180) (layer F.SilkS) hide)
    (fp_text value 510k (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.65 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(R5-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 24 /VINF))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58C0A820)
    (at 130.05 106.6 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at 0 -1.65 180) (layer F.SilkS) hide)
    (fp_text value 10k (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.65 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 21 /VINP))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 20 /GND))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58C0A84B)
    (at 143.65 93.5 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R7 (at 0 -1.65 180) (layer F.SilkS) hide)
    (fp_text value 3 (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.65 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 22 /5V0))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C8-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58C0A850)
    (at 146.65 94.5 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R8 (at 0 -1.65 270) (layer F.SilkS) hide)
    (fp_text value 10k (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.65 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 22 /5V0))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 20 /GND))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58C0A857)
    (at 154.6 102.9)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R9 (at 0 -1.65) (layer F.SilkS) hide)
    (fp_text value 10k (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.65) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 22 /5V0))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(R9-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58C0A854)
    (at 150.2 98.2 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R10 (at 0 -1.65 90) (layer F.SilkS) hide)
    (fp_text value 22k (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.65 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R10-Pad1)"))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 20 /GND))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module aiber:SO-8 (layer F.Cu) (tedit 58C0A819)
    (at 122.45 96.3)
    (fp_text reference U1 (at 0 5.08) (layer F.SilkS) hide)
    (fp_text value SI4946BEY (at 0 -5.08) (layer F.Fab))
    (pad 3 smd rect (at 0.635 2.5273) (size 0.5588 1.1938) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(U1-Pad1)"))
    (pad 2 smd rect (at -0.635 2.5273) (size 0.5588 1.1938) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(U1-Pad2)"))
    (pad 1 smd rect (at -1.905 2.5273) (size 0.5588 1.1938) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(U1-Pad1)"))
    (pad 4 smd rect (at 1.905 2.5273) (size 0.5588 1.1938) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(U1-Pad2)"))
    (pad 8 smd rect (at -1.905 -2.5273) (size 0.5588 1.1938) (layers F.Cu F.Paste F.Mask)
      (net 24 /VINF))
    (pad 7 smd rect (at -0.635 -2.5273) (size 0.5588 1.1938) (layers F.Cu F.Paste F.Mask)
      (net 24 /VINF))
    (pad 6 smd rect (at 0.635 -2.5273) (size 0.5588 1.1938) (layers F.Cu F.Paste F.Mask)
      (net 21 /VINP))
    (pad 5 smd rect (at 1.905 -2.5273) (size 0.5588 1.1938) (layers F.Cu F.Paste F.Mask)
      (net 21 /VINP))
  )
  (module TO_SOT_Packages_SMD:TSOT-23-8 (layer F.Cu) (tedit 58C0A81B)
    (at 125.65 105.7)
    (descr "8-pin TSOT23 package, http://cds.linear.com/docs/en/packaging/SOT_8_05-08-1637.pdf")
    (tags TSOT-23-8)
    (attr smd)
    (fp_text reference U2 (at 0 -2.45) (layer F.SilkS) hide)
    (fp_text value LTC4365 (at 0 2.5) (layer F.Fab))
    (pad 1 smd rect (at -1.31 -0.97) (size 1.22 0.4) (layers F.Cu F.Paste F.Mask)
      (net 24 /VINF))
    (pad 2 smd rect (at -1.31 -0.33) (size 1.22 0.4) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(R2-Pad2)"))
    (pad 3 smd rect (at -1.31 0.33) (size 1.22 0.4) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(R3-Pad2)"))
    (pad 4 smd rect (at -1.31 0.97) (size 1.22 0.4) (layers F.Cu F.Paste F.Mask)
      (net 20 /GND))
    (pad 5 smd rect (at 1.31 0.97) (size 1.22 0.4) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(R5-Pad1)"))
    (pad 6 smd rect (at 1.31 0.33) (size 1.22 0.4) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(U2-Pad6)"))
    (pad 7 smd rect (at 1.31 -0.33) (size 1.22 0.4) (layers F.Cu F.Paste F.Mask)
      (net 21 /VINP))
    (pad 8 smd rect (at 1.31 -0.97) (size 1.22 0.4) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(U1-Pad2)"))
  )
  (module aiber:LM53603 (layer F.Cu) (tedit 58C0A830)
    (at 136.65 97.575 180)
    (fp_text reference U3 (at 0 7 180) (layer F.SilkS) hide)
    (fp_text value LM53603-Q1 (at 0 -2 180) (layer F.Fab))
    (pad 2 smd rect (at -2.9 0.65 180) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C7-Pad1)"))
    (pad 1 smd rect (at -2.9 0 180) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C7-Pad1)"))
    (pad 3 smd rect (at -2.9 1.3 180) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C7-Pad2)"))
    (pad 4 smd rect (at -2.9 1.95 180) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C6-Pad1)"))
    (pad 6 smd rect (at -2.9 3.25 180) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 20 /GND))
    (pad 5 smd rect (at -2.9 2.6 180) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C8-Pad1)"))
    (pad 7 smd rect (at -2.9 3.9 180) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 20 /GND))
    (pad 8 smd rect (at -2.9 4.55 180) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(U3-Pad8)"))
    (pad 16 smd rect (at 2.9 0 180) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 20 /GND))
    (pad 15 smd rect (at 2.9 0.65 180) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 20 /GND))
    (pad 14 smd rect (at 2.9 1.3 180) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(U3-Pad14)"))
    (pad 13 smd rect (at 2.9 1.95 180) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 21 /VINP))
    (pad 12 smd rect (at 2.9 2.6 180) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 21 /VINP))
    (pad 11 smd rect (at 2.9 3.25 180) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 21 /VINP))
    (pad 10 smd rect (at 2.9 3.9 180) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 20 /GND))
    (pad 9 smd rect (at 2.9 4.55 180) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 22 /5V0))
    (pad 17 smd rect (at 0 2.275 180) (size 3 5) (layers F.Cu F.Paste F.Mask)
      (net 20 /GND) (solder_mask_margin -0.01))
  )
  (module aiber:TPS2511 (layer F.Cu) (tedit 58C0A83C)
    (at 154.6 100 270)
    (fp_text reference U4 (at 0 4.1 270) (layer F.SilkS) hide)
    (fp_text value TPS2511 (at 0 -3.1 270) (layer F.Fab))
    (pad 9 smd rect (at 0 0 270) (size 1.5 1.65) (layers F.Cu F.Paste F.Mask)
      (net 20 /GND) (solder_mask_margin -0.01))
    (pad 7 smd rect (at -0.325 -2.1 270) (size 0.35 1.55) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(P2-Pad2)"))
    (pad 8 smd rect (at -0.975 -2.1 270) (size 0.35 1.55) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(P2-Pad1)"))
    (pad 6 smd rect (at 0.325 -2.1 270) (size 0.35 1.55) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(P2-Pad3)"))
    (pad 5 smd rect (at 0.975 -2.1 270) (size 0.35 1.55) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(R9-Pad2)"))
    (pad 1 smd rect (at -0.975 2.1 270) (size 0.35 1.55) (layers F.Cu F.Paste F.Mask)
      (net 20 /GND))
    (pad 2 smd rect (at -0.325 2.1 270) (size 0.35 1.55) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R10-Pad1)"))
    (pad 3 smd rect (at 0.325 2.1 270) (size 0.35 1.55) (layers F.Cu F.Paste F.Mask)
      (net 22 /5V0))
    (pad 4 smd rect (at 0.975 2.1 270) (size 0.35 1.55) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(U4-Pad4)"))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2_Pad (layer F.Cu) (tedit 58C0B5FB)
    (at 95.5 93)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2_Pad (at 0 3.2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask)
      (net 20 /GND))
  )
  (gr_text "12V USB Power Rev A\nJustin Gatzen 2017\n\nInput: 8-30V 2A\nOutput: 5V 2A" (at 132.5 100 360) (layer B.SilkS))
  (gr_line (start 172.5 110) (end 92.5 110) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 172.5 90) (end 172.5 110) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 92.5 90) (end 172.5 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 92.5 110) (end 92.5 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 20) (net_name /GND) (layer F.Cu) (hatch edge 0.508)
    (priority 10)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.1524)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 2.032) (smoothing chamfer))
    (polygon
      (pts
        (xy 92.5 90) (xy 92.5 110) (xy 172.5 110) (xy 172.5 90)
      )
    )
  )
  (zone (net 20) (net_name /GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 92.5 90) (xy 92.5 110) (xy 172.5 110) (xy 172.5 90)
      )
    )
  )
  (zone (net 23) (net_name /VIN) (layer F.Cu) (hatch edge 0.508)
    (priority 20)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet))
    (polygon
      (pts
        (xy 103.9 99.8) (xy 111.6 99.8) (xy 111.6 93) (xy 108.6 93) (xy 103.9 97)
      )
    )
  )
  (zone (net 24) (net_name /VINF) (layer F.Cu) (hatch edge 0.508)
    (priority 20)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet))
    (polygon
      (pts
        (xy 112.8 103.45) (xy 114.9 103.45) (xy 115.9 102.5) (xy 119.1 102.5) (xy 120 103.35)
        (xy 120.95 103.35) (xy 120.95 100.15) (xy 119.1 100.15) (xy 118.95 100) (xy 118.95 94.95)
        (xy 119.25 94.65) (xy 122.1 94.65) (xy 122.1 92.9) (xy 115.7 92.9) (xy 115.7 99.35)
        (xy 114.65 100.3) (xy 112.8 100.3)
      )
    )
  )
  (zone (net 5) (net_name "Net-(D1-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (priority 20)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet))
    (polygon
      (pts
        (xy 109.4 104.65) (xy 114.9 104.65) (xy 114.9 107.15) (xy 109.4 107.15)
      )
    )
  )
  (zone (net 21) (net_name /VINP) (layer F.Cu) (hatch edge 0.508)
    (priority 20)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet))
    (polygon
      (pts
        (xy 122.8 92.9) (xy 122.8 94.65) (xy 126.65 94.65) (xy 127.35 93.95) (xy 128.8 93.95)
        (xy 130.3 95.35) (xy 130.25 107.55) (xy 131.9 107.55) (xy 131.875 96.25) (xy 132.25 95.85)
        (xy 134.5 95.85) (xy 134.5 94.1) (xy 131.85 94.1) (xy 130.5 92.9)
      )
    )
  )
  (zone (net 14) (net_name "Net-(U1-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 20)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet))
    (polygon
      (pts
        (xy 120.275 99.4) (xy 120.275 95.5) (xy 123.35 95.5) (xy 123.35 99.4) (xy 122.825 99.4)
        (xy 122.825 97.95) (xy 122.675 97.8) (xy 121 97.8) (xy 120.8 98) (xy 120.8 99.4)
      )
    )
  )
  (zone (net 2) (net_name "Net-(C7-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 20)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet))
    (polygon
      (pts
        (xy 138.8 96.7) (xy 138.8 97.8) (xy 137.7 99.05) (xy 134.65 99.05) (xy 134.65 101.45)
        (xy 138.05 101.45) (xy 140.4 99.8) (xy 143.15 99.8) (xy 143.15 98.55) (xy 140.8 98.55)
        (xy 140.3 98) (xy 140.3 96.7)
      )
    )
  )
  (zone (net 22) (net_name /5V0) (layer F.Cu) (hatch edge 0.508)
    (priority 20)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet))
    (polygon
      (pts
        (xy 134.65 107.3) (xy 134.65 104.9) (xy 135.15 104.9) (xy 140.1 101.3) (xy 146.05 101.3)
        (xy 146.05 98.7) (xy 147.25 98.7) (xy 147.25 101.3) (xy 149.4 101.3) (xy 150.55 100.15)
        (xy 153.25 100.15) (xy 153.25 100.5) (xy 151.4 100.5) (xy 151.4 101.5) (xy 153.3 102.25)
        (xy 154 102.25) (xy 154 103.55) (xy 153.3 103.55) (xy 153 103.25) (xy 140.35 103.25)
        (xy 138.05 104.95) (xy 138.05 107.3)
      )
    )
  )
  (zone (net 8) (net_name "Net-(P2-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 20)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.1524)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 2.032) (smoothing chamfer))
    (polygon
      (pts
        (xy 155.95 98.85) (xy 159.1 98.85) (xy 159.7 99.45) (xy 159.7 102.5) (xy 160.8 102.5)
        (xy 160.8 104.5) (xy 158.75 104.5) (xy 158.75 99.75) (xy 158.2 99.2) (xy 155.95 99.2)
      )
    )
  )
)
