<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<wire x1="18.69953125" y1="20.660409375" x2="16.02286875" y2="16.18488125" width="0.025" layer="20" curve="61.764424"/>
<wire x1="18.69953125" y1="20.660409375" x2="1.83468125" y2="24.487840625" width="0.025" layer="20" curve="277.955739"/>
<wire x1="2.81486875" y1="21.48818125" x2="1.83468125" y2="24.487840625" width="0.025" layer="20" curve="36.191356"/>
<wire x1="2.81486875" y1="6.16221875" x2="7.89486875" y2="1.08221875" width="0.025" layer="20" curve="90"/>
<wire x1="10.94286875" y1="1.08221875" x2="16.02286875" y2="6.16221875" width="0.025" layer="20" curve="90"/>
<wire x1="9.40401875" y1="43.07301875" x2="10.42001875" y2="42.05701875" width="0.025" layer="20" curve="90"/>
<wire x1="10.42001875" y1="44.4479" x2="9.40401875" y2="43.4319" width="0.025" layer="20" curve="90"/>
<wire x1="15.52971875" y1="43.4319" x2="14.51371875" y2="44.4479" width="0.025" layer="20" curve="90"/>
<wire x1="14.51371875" y1="42.05701875" x2="15.52971875" y2="43.07301875" width="0.025" layer="20" curve="90"/>
<circle x="12.46686875" y="32.266959375" radius="5.2" width="0.025" layer="20"/>
<wire x1="10.42001875" y1="22.57386875" x2="9.40401875" y2="21.55786875" width="0.025" layer="20" curve="90"/>
<wire x1="9.40401875" y1="21.00505" x2="10.42001875" y2="19.98905" width="0.025" layer="20" curve="90"/>
<wire x1="14.51371875" y1="19.98905" x2="15.52971875" y2="21.00505" width="0.025" layer="20" curve="90"/>
<wire x1="15.52971875" y1="21.55786875" x2="14.51371875" y2="22.57386875" width="0.025" layer="20" curve="90"/>
<wire x1="16.02286875" y1="6.16221875" x2="16.02286875" y2="16.18488125" width="0.025" layer="20"/>
<wire x1="2.81486875" y1="21.48818125" x2="2.81486875" y2="6.16221875" width="0.025" layer="20"/>
<wire x1="7.89486875" y1="1.08221875" x2="10.94286875" y2="1.08221875" width="0.025" layer="20"/>
<wire x1="9.40401875" y1="43.4319" x2="9.40401875" y2="43.07301875" width="0.025" layer="20"/>
<wire x1="10.42001875" y1="44.4479" x2="14.51371875" y2="44.4479" width="0.025" layer="20"/>
<wire x1="15.52971875" y1="43.4319" x2="15.52971875" y2="43.07301875" width="0.025" layer="20"/>
<wire x1="14.51371875" y1="42.05701875" x2="10.42001875" y2="42.05701875" width="0.025" layer="20"/>
<wire x1="9.40401875" y1="21.55786875" x2="9.40401875" y2="21.00505" width="0.025" layer="20"/>
<wire x1="14.51371875" y1="19.98905" x2="10.42001875" y2="19.98905" width="0.025" layer="20"/>
<wire x1="15.52971875" y1="21.55786875" x2="15.52971875" y2="21.00505" width="0.025" layer="20"/>
<wire x1="10.42001875" y1="22.57386875" x2="14.51371875" y2="22.57386875" width="0.025" layer="20"/>
<text>MotorPCB V2 </text>
<text>KRA 2018</text>
</plain>
<libraries>
<library name="testpad">
<description>&lt;b&gt;Test Pins/Pads&lt;/b&gt;&lt;p&gt;
Cream on SMD OFF.&lt;br&gt;
new: Attribute TP_SIGNAL_NAME&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="KEVINDC">
</package>
</packages>
</library>
<library name="con-cui_custom">
<packages>
<package name="CUI_PJ006A">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="con-cui_custom" package="CUI_PJ006A" value=""/>
<element name="U$1" library="testpad" package="KEVINDC" value="MOTOR"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="U$1" pad="P$3"/>
<contactref element="J1" pad="P$1"/>
</signal>
<signal name="N$2">
<contactref element="U$1" pad="MOTOR+"/>
<contactref element="J1" pad="P$2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
