(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 18)
    (no_connects 0)
    (area 129.972999 84.120919 159.333001 121.873333)
    (thickness 1.6)
    (drawings 25)
    (tracks 80)
    (zones 0)
    (modules 7)
    (nets 12)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.45)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.6 1.6)
    (pad_drill 1)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFEF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VCC)
  (net 2 GND)
  (net 3 "Net-(J1-Pad2)")
  (net 4 "Net-(J1-Pad3)")
  (net 5 "Net-(J1-Pad4)")
  (net 6 "Net-(J1-Pad5)")
  (net 7 "Net-(LED1-Pad4)")
  (net 8 "Net-(LED1-Pad2)")
  (net 9 "Net-(LED2-Pad3)")
  (net 10 "Net-(LED2-Pad4)")
  (net 11 "Net-(U1-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.45)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(LED1-Pad2)")
    (add_net "Net-(LED1-Pad4)")
    (add_net "Net-(LED2-Pad3)")
    (add_net "Net-(LED2-Pad4)")
    (add_net "Net-(U1-Pad3)")
    (add_net VCC)
  )
  (module defcon:CR2025 (layer F.Cu) (tedit 595984C1)
    (at 144.78 93.98)
    (fp_text reference BT1 (at 0 3) (layer F.SilkS))
    (fp_text value Battery_Cell (at 0.2 5.2) (layer F.Fab))
    (pad 1 smd rect (at 11.45 0) (size 2.5 5.1) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd circle (at 0 0.1) (size 17.8 17.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -11.45 0) (size 2.5 5.1) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5959926C)
    (at 151.40686 107.03814 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference 10uF (at -0.1397 1.31318 90) (layer F.SilkS))
    (fp_text value CP1 (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x06_Pitch2.54mm (layer F.Cu) (tedit 58CD4EC1)
    (at 138.43 116.84 90)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value CONN_01X06 (at 0 15.03 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 VCC))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x06_Pitch2.54mm.wrl
      (at (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED_WS2812B-PLCC4 (layer B.Cu) (tedit 587A6D9E)
    (at 140.97 93.98 180)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference LED1 (at 0 3.5 180) (layer B.SilkS))
    (fp_text value WS2812B (at 0 -4 180) (layer B.Fab))
    (pad 3 smd rect (at 2.5 -1.6 180) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 2.5 1.6 180) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(LED1-Pad4)"))
    (pad 2 smd rect (at -2.5 -1.6 180) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(LED1-Pad2)"))
    (pad 1 smd rect (at -2.5 1.6 180) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_WS2812B-PLCC4 (layer B.Cu) (tedit 587A6D9E)
    (at 148.59 93.98 180)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference LED2 (at 0 3.5 180) (layer B.SilkS))
    (fp_text value WS2812B (at 0 -4 180) (layer B.Fab))
    (pad 3 smd rect (at 2.5 -1.6 180) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(LED2-Pad3)"))
    (pad 4 smd rect (at 2.5 1.6 180) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(LED2-Pad4)"))
    (pad 2 smd rect (at -2.5 -1.6 180) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(LED1-Pad4)"))
    (pad 1 smd rect (at -2.5 1.6 180) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 59599261)
    (at 138.43 109.22 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference 47R (at 0.03048 -1.524 90) (layer F.SilkS))
    (fp_text value 47R (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(LED2-Pad3)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-8_W7.62mm (layer F.Cu) (tedit 595A0283)
    (at 140.97 105.41)
    (descr "8-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "DIL DIP PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U1 (at 3.81 -2.39) (layer F.SilkS))
    (fp_text value ATTINY85-20PU (at 3.81 10.01) (layer F.Fab))
    (fp_text user %R (at 3.81 3.81) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (pad 5 thru_hole circle (at 7.62 7.62) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad3)"))
    (pad 2 thru_hole circle (at 0 2.54) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(LED2-Pad4)"))
    (pad 6 thru_hole circle (at 7.62 5.08) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad4)"))
    (pad 3 thru_hole circle (at 0 5.08) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(U1-Pad3)"))
    (pad 7 thru_hole circle (at 7.62 2.54) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad5)"))
    (pad 4 thru_hole circle (at 0 7.62) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 8 thru_hole circle (at 7.62 0) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 1 VCC))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-8_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text nekosurf (at 155.00604 87.91194 315) (layer F.SilkS))
  (gr_text "\n" (at 155.6639 94.6785 45) (layer B.Mask))
  (gr_text "6C 65 76 \n69 73 69 \n6F 6E 2C\n20 74 75 \n6E 65 64 \n20 74 6F \n20 61 20 \n64 65 61 \n64 20 63 \n68 61 6E \n6E 65 6C \n2E 57 47" (at 153.543 109.86008) (layer B.SilkS))
  (gr_text "54 68 65 \n20 73 6B \n79 20 61 \n62 6F 76\n65 20 74 \n68 65 20\n70 6F 72 \n74 20 77 \n61 73 20 \n74 68 65\n20 63 6F \n6C 6F 72 \n20 6F 66 " (at 139.94892 109.61116) (layer B.SilkS))
  (gr_text kyeho (at 152.3492 87.23376 315) (layer F.SilkS))
  (gr_text Metal (at 134.61746 98.66122 315) (layer F.SilkS))
  (gr_text defcon25 (at 134.30758 88.34374 45) (layer F.SilkS))
  (gr_text dash (at 156.1846 98.3488 45) (layer F.SilkS))
  (gr_text v0.0000001 (at 132.9944 98.9076 315) (layer F.SilkS))
  (gr_text "PIN7\n" (at 148.6281 118.6815) (layer F.SilkS))
  (gr_text PIN6 (at 146.0373 118.9863) (layer F.SilkS))
  (gr_text PIN5 (at 143.4465 118.7196) (layer F.SilkS))
  (gr_text ~RST (at 140.97 119.0244) (layer F.SilkS))
  (gr_text VCC (at 151.1427 119.0244) (layer F.SilkS))
  (gr_text GND (at 138.44016 118.64848) (layer F.SilkS))
  (gr_line (start 159.258 97.917) (end 153.924 103.251) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 159.258 90.043) (end 159.258 97.917) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 153.71318 84.19592) (end 159.25 90) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 136.017 84.201) (end 153.67 84.201) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 130.048 90.17) (end 136.017 84.201) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 130.048 98.044) (end 130.048 90.17) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 135.382 103.378) (end 130.048 98.044) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 135.382 120.015) (end 135.382 103.378) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 153.924 120.015) (end 135.382 120.015) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 153.924 103.124) (end 153.924 120.015) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 135.4328 103.22052) (xy 135.6868 120.11152) (xy 154.2288 119.98452) (xy 154.2288 103.22052) (xy 159.3088 98.01352)
        (xy 159.3088 90.26652) (xy 153.7208 84.29752) (xy 136.1948 84.17052) (xy 130.2258 90.26652) (xy 130.2258 98.26752)
        (xy 135.6868 103.22052)
      )
    )
  )
)
