(kicad_pcb (version 20171130) (host pcbnew 5.1.10-88a1d61d58~88~ubuntu20.10.1)
  (general
    (thickness 1.6)
    (drawings 15)
    (tracks 110)
    (zones 0)
    (modules 6)
    (nets 29)
  )
  (page A4)
  (title_block
    (title "28C64 to Molex 78805 socket with 2732 pinout")
    (date 2021-05-30)
    (rev 001)
    (company b.kenyon.w@gmail.com)
  )
  (layers
    (0 Top signal)
    (31 Bottom signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.2)
    (user_trace_width 0.4)
    (trace_clearance 0.2)
    (zone_clearance 0.1524)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.5)
    (via_drill 0.3)
    (via_min_size 0.5)
    (via_min_drill 0.3)
    (uvia_size 0.5)
    (uvia_drill 0.3)
    (uvias_allowed no)
    (uvia_min_size 0.5)
    (uvia_min_drill 0.3)
    (edge_width 0.01)
    (segment_width 0.2032)
    (pcb_text_width 0.254)
    (pcb_text_size 1.2192 1.2192)
    (mod_edge_width 0.0254)
    (mod_text_size 0.4572 0.4572)
    (mod_text_width 0.0254)
    (pad_size 1 0.8)
    (pad_drill 0)
    (pad_to_mask_clearance 0)
    (solder_mask_min_width 0.22)
    (aux_axis_origin 0 0)
    (grid_origin 147.2184 99.187)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "GERBER_Meeprom_004"))
  )
  (net 0 "")
  (net 1 /D3)
  (net 2 /A10)
  (net 3 /D4)
  (net 4 /A7)
  (net 5 /D5)
  (net 6 /A6)
  (net 7 /D6)
  (net 8 /A5)
  (net 9 /D7)
  (net 10 /A4)
  (net 11 /A11)
  (net 12 /A3)
  (net 13 /~OE)
  (net 14 /A2)
  (net 15 /A1)
  (net 16 /A0)
  (net 17 /A12)
  (net 18 /D0)
  (net 19 /A9)
  (net 20 /D1)
  (net 21 /A8)
  (net 22 /D2)
  (net 23 /~CE)
  (net 24 /~WE)
  (net 25 VCC)
  (net 26 GND)
  (net 27 "Net-(R2-Pad1)")
  (net 28 "Net-(R3-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.5)
    (via_drill 0.3)
    (uvia_dia 0.5)
    (uvia_drill 0.3)
    (diff_pair_width 0.2)
    (diff_pair_gap 0.3)
    (add_net /A0)
    (add_net /A1)
    (add_net /A10)
    (add_net /A11)
    (add_net /A12)
    (add_net /A2)
    (add_net /A3)
    (add_net /A4)
    (add_net /A5)
    (add_net /A6)
    (add_net /A7)
    (add_net /A8)
    (add_net /A9)
    (add_net /D0)
    (add_net /D1)
    (add_net /D2)
    (add_net /D3)
    (add_net /D4)
    (add_net /D5)
    (add_net /D6)
    (add_net /D7)
    (add_net /~CE)
    (add_net /~OE)
    (add_net /~WE)
    (add_net GND)
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad26)")
    (add_net VCC)
  )
  (module 000_LOCAL:CL-SB-12C-0x (layer Top) (tedit 60B3899A)
    (at 147.2184 110.937 180)
    (fp_text reference SW1 (at 0 0) (layer F.SilkS))
    (fp_text value SW_SPDT (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 2.5 -1.65 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 27 "Net-(R2-Pad1)"))
    (pad 2 thru_hole circle (at 0 1.65 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 17 /A12))
    (pad 3 thru_hole circle (at -2.5 -1.65 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 28 "Net-(R3-Pad1)"))
    (model ${KIPRJMOD}/000_LOCAL.pretty/3d/CL-SB-12C-01.stp
      (offset (xyz 0 0 3.5))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 180))
    )
  )
  (module 000_LOCAL:R_0805 (layer Top) (tedit 60997F9A)
    (at 150.9684 86.187)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at -0.05 0 -90 unlocked) (layer F.SilkS))
    (fp_text value 100k (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.95 0) (size 0.7 1.3) (layers Top F.Paste F.Mask) (roundrect_rratio 0.1)
      (net 28 "Net-(R3-Pad1)"))
    (pad 2 smd roundrect (at 0.95 0) (size 0.7 1.3) (layers Top F.Paste F.Mask) (roundrect_rratio 0.1)
      (net 25 VCC))
    (model ${KIPRJMOD}/000_LOCAL.pretty/3d/R_0805.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000_LOCAL:Molex78802_PCB_24 (layer Top) (tedit 60A90175)
    (at 147.2184 99.187)
    (descr "Castellated edge contacts to fit Molex 78805 Socket")
    (solder_mask_margin 0.0508)
    (attr virtual)
    (fp_text reference J1 (at -1.905 0 -90) (layer Dwgs.User) hide)
    (fp_text value "Molex 78805 socket 27C32 pinout" (at 1.27 0 -90) (layer F.Fab) hide)
    (fp_text user "0.7 border on bottom - 31.52 x 15 x 1.5 usable bottom" (at -5.5 -14.46) (layer Dwgs.User))
    (fp_text user "10.0 x 1.0 retainer wedges on top" (at -3.5 -14.96) (layer Dwgs.User))
    (fp_text user "Castellation depth 0.5mm min" (at 6.35 0 -90) (layer Dwgs.User))
    (fp_text user "Board outline: 0.01mm grid, copy Eco2.User" (at -6 0 -90) (layer Eco2.User))
    (fp_text user "Eco1.User is Edge.Cuts for use without carrier." (at -4.445 0 -90) (layer Eco1.User))
    (pad 24 thru_hole circle (at 8.5552 -13.97 180) (size 1.6002 1.6002) (drill 1.59766) (layers *.Cu *.Mask)
      (net 25 VCC))
    (pad 12 thru_hole circle (at -8.5552 13.97) (size 1.6002 1.6002) (drill 1.59766) (layers *.Cu *.Mask)
      (net 26 GND) (zone_connect 0))
    (pad 23 thru_hole circle (at 8.5552 -11.43 180) (size 1.6002 1.6002) (drill 1.59766) (layers *.Cu *.Mask)
      (net 21 /A8))
    (pad 11 thru_hole circle (at -8.5552 11.43) (size 1.6002 1.6002) (drill 1.59766) (layers *.Cu *.Mask)
      (net 22 /D2) (zone_connect 0))
    (pad 22 thru_hole circle (at 8.5552 -8.89 180) (size 1.6002 1.6002) (drill 1.59766) (layers *.Cu *.Mask)
      (net 19 /A9))
    (pad 10 thru_hole circle (at -8.5552 8.89) (size 1.6002 1.6002) (drill 1.59766) (layers *.Cu *.Mask)
      (net 20 /D1) (zone_connect 0))
    (pad 21 thru_hole circle (at 8.5552 -6.35 180) (size 1.6002 1.6002) (drill 1.59766) (layers *.Cu *.Mask)
      (net 11 /A11))
    (pad 9 thru_hole circle (at -8.5552 6.35) (size 1.6002 1.6002) (drill 1.59766) (layers *.Cu *.Mask)
      (net 18 /D0) (zone_connect 0))
    (pad 20 thru_hole circle (at 8.5552 -3.81 180) (size 1.6002 1.6002) (drill 1.59766) (layers *.Cu *.Mask)
      (net 13 /~OE))
    (pad 8 thru_hole circle (at -8.5552 3.81) (size 1.6002 1.6002) (drill 1.59766) (layers *.Cu *.Mask)
      (net 16 /A0) (zone_connect 0))
    (pad 19 thru_hole circle (at 8.5552 -1.27 180) (size 1.6002 1.6002) (drill 1.59766) (layers *.Cu *.Mask)
      (net 2 /A10))
    (pad 7 thru_hole circle (at -8.5552 1.27) (size 1.6002 1.6002) (drill 1.59766) (layers *.Cu *.Mask)
      (net 15 /A1) (zone_connect 0))
    (pad 18 thru_hole circle (at 8.5552 1.27 180) (size 1.6002 1.6002) (drill 1.59766) (layers *.Cu *.Mask)
      (net 23 /~CE))
    (pad 6 thru_hole circle (at -8.5552 -1.27) (size 1.6002 1.6002) (drill 1.59766) (layers *.Cu *.Mask)
      (net 14 /A2) (zone_connect 0))
    (pad 17 thru_hole circle (at 8.5552 3.81 180) (size 1.6002 1.6002) (drill 1.59766) (layers *.Cu *.Mask)
      (net 9 /D7))
    (pad 5 thru_hole circle (at -8.5552 -3.81) (size 1.6002 1.6002) (drill 1.59766) (layers *.Cu *.Mask)
      (net 12 /A3) (zone_connect 0))
    (pad 16 thru_hole circle (at 8.5552 6.35 180) (size 1.6002 1.6002) (drill 1.59766) (layers *.Cu *.Mask)
      (net 7 /D6))
    (pad 4 thru_hole circle (at -8.5552 -6.35) (size 1.6002 1.6002) (drill 1.59766) (layers *.Cu *.Mask)
      (net 10 /A4) (zone_connect 0))
    (pad 15 thru_hole circle (at 8.5552 8.89 180) (size 1.6002 1.6002) (drill 1.59766) (layers *.Cu *.Mask)
      (net 5 /D5))
    (pad 3 thru_hole circle (at -8.5552 -8.89) (size 1.6002 1.6002) (drill 1.59766) (layers *.Cu *.Mask)
      (net 8 /A5) (zone_connect 0))
    (pad 14 thru_hole circle (at 8.5552 11.43 180) (size 1.6002 1.6002) (drill 1.59766) (layers *.Cu *.Mask)
      (net 3 /D4))
    (pad 2 thru_hole circle (at -8.5552 -11.43) (size 1.6002 1.6002) (drill 1.59766) (layers *.Cu *.Mask)
      (net 6 /A6) (zone_connect 0))
    (pad 13 thru_hole circle (at 8.5552 13.97 180) (size 1.6002 1.6002) (drill 1.59766) (layers *.Cu *.Mask)
      (net 1 /D3))
    (pad 1 thru_hole circle (at -8.5552 -13.97) (size 1.6002 1.6002) (drill 1.59766) (layers *.Cu *.Mask)
      (net 4 /A7) (zone_connect 0))
    (model ${KIPRJMOD}/000_LOCAL.pretty/3d/Molex78802_PCB_24.step
      (offset (xyz 0 0 -0.16))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module 000_LOCAL:R_0805 (layer Top) (tedit 60997F9A)
    (at 143.4684 88.737 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0.0635 0 270 unlocked) (layer F.SilkS))
    (fp_text value 100k (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.95 0 180) (size 0.7 1.3) (layers Top F.Paste F.Mask) (roundrect_rratio 0.1)
      (net 27 "Net-(R2-Pad1)"))
    (pad 2 smd roundrect (at 0.95 0 180) (size 0.7 1.3) (layers Top F.Paste F.Mask) (roundrect_rratio 0.1)
      (net 26 GND))
    (model ${KIPRJMOD}/000_LOCAL.pretty/3d/R_0805.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000_LOCAL:SOIC-28W (layer Top) (tedit 60AC7F09)
    (at 147.2184 99.187)
    (descr "28-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1 (at 0 0 -90) (layer F.SilkS) hide)
    (fp_text value 28C64 (at 0 0 -90) (layer F.SilkS))
    (fp_text user %R (at 0 0 -90) (layer F.Fab))
    (pad 1 smd roundrect (at -4.7 -8.255) (size 1.5 0.6) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at -4.7 -6.985) (size 1.5 0.6) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 /A12))
    (pad 3 smd roundrect (at -4.7 -5.715) (size 1.5 0.6) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 /A7))
    (pad 4 smd roundrect (at -4.7 -4.445) (size 1.5 0.6) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 /A6))
    (pad 5 smd roundrect (at -4.7 -3.175) (size 1.5 0.6) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 /A5))
    (pad 6 smd roundrect (at -4.7 -1.905) (size 1.5 0.6) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 /A4))
    (pad 7 smd roundrect (at -4.7 -0.635) (size 1.5 0.6) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 /A3))
    (pad 8 smd roundrect (at -4.7 0.635) (size 1.5 0.6) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 /A2))
    (pad 9 smd roundrect (at -4.7 1.905) (size 1.5 0.6) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 /A1))
    (pad 10 smd roundrect (at -4.7 3.175) (size 1.5 0.6) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 /A0))
    (pad 11 smd roundrect (at -4.7 4.445) (size 1.5 0.6) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /D0))
    (pad 12 smd roundrect (at -4.7 5.715) (size 1.5 0.6) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 /D1))
    (pad 13 smd roundrect (at -4.7 6.985) (size 1.5 0.6) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 /D2))
    (pad 14 smd roundrect (at -4.7 8.255) (size 1.5 0.6) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 GND))
    (pad 15 smd roundrect (at 4.7 8.255) (size 1.5 0.6) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 /D3))
    (pad 16 smd roundrect (at 4.7 6.985) (size 1.5 0.6) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /D4))
    (pad 17 smd roundrect (at 4.7 5.715) (size 1.5 0.6) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /D5))
    (pad 18 smd roundrect (at 4.7 4.445) (size 1.5 0.6) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 /D6))
    (pad 19 smd roundrect (at 4.7 3.175) (size 1.5 0.6) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 /D7))
    (pad 20 smd roundrect (at 4.7 1.905) (size 1.5 0.6) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 /~CE))
    (pad 21 smd roundrect (at 4.7 0.635) (size 1.5 0.6) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /A10))
    (pad 22 smd roundrect (at 4.7 -0.635) (size 1.5 0.6) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 /~OE))
    (pad 23 smd roundrect (at 4.7 -1.905) (size 1.5 0.6) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 /A11))
    (pad 24 smd roundrect (at 4.7 -3.175) (size 1.5 0.6) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 /A9))
    (pad 25 smd roundrect (at 4.7 -4.445) (size 1.5 0.6) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 /A8))
    (pad 26 smd roundrect (at 4.7 -5.715) (size 1.5 0.6) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 27 smd roundrect (at 4.7 -6.985) (size 1.5 0.6) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 /~WE))
    (pad 28 smd roundrect (at 4.7 -8.255) (size 1.5 0.6) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 VCC))
    (model ${KIPRJMOD}/000_LOCAL.pretty/3d/SW3dPS-SOIC28-300.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module 000_LOCAL:R_0805 (layer Top) (tedit 60997F9A)
    (at 150.9684 88.687)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at -0.0508 0.0127 -90 unlocked) (layer F.SilkS))
    (fp_text value 100k (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.95 0) (size 0.7 1.3) (layers Top F.Paste F.Mask) (roundrect_rratio 0.1)
      (net 24 /~WE))
    (pad 2 smd roundrect (at 0.95 0) (size 0.7 1.3) (layers Top F.Paste F.Mask) (roundrect_rratio 0.1)
      (net 25 VCC))
    (model ${KIPRJMOD}/000_LOCAL.pretty/3d/R_0805.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "SW1: CL-SB-12C-02 or CL-SB-12C-12" (at 142.7184 84.187 90) (layer B.SilkS))
  (gr_text "BANK 1" (at 152.3184 110.937 -90) (layer F.SilkS))
  (gr_text "BANK 0" (at 141.9684 110.937 -90) (layer F.SilkS))
  (gr_line (start 140.7184 82.727) (end 138.9184 84.527) (layer Edge.Cuts) (width 0.01))
  (gr_line (start 138.9184 115.647) (end 138.9184 84.527) (layer Edge.Cuts) (width 0.01))
  (gr_line (start 155.5184 115.647) (end 155.5184 82.727) (layer Edge.Cuts) (width 0.01))
  (gr_text "28C64 to Molex 78805, 2732 pinout" (at 153.8224 99.187 -90) (layer F.SilkS))
  (gr_text 1 (at 140.3604 85.217) (layer F.SilkS))
  (gr_text 28C64 (at 145.3134 89.387) (layer F.SilkS))
  (gr_line (start 140.7184 82.727) (end 155.5184 82.727) (layer Edge.Cuts) (width 0.01))
  (gr_line (start 155.5184 115.647) (end 138.9184 115.647) (layer Edge.Cuts) (width 0.01))
  (gr_text "Carrier: Molex78802_PCB_24 v004" (at 144.2184 84.187 90) (layer B.SilkS))
  (gr_text github.com/bkw777/Teeprom (at 153.5684 99.187 90) (layer B.SilkS))
  (gr_text "R1, R2, R3: 100k" (at 141.2184 84.187 90) (layer B.SilkS))
  (gr_text "2732 pinout" (at 140.8684 84.201) (layer F.SilkS))
  (zone (net 26) (net_name GND) (layer Top) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.2) (thermal_bridge_width 0.3) (smoothing fillet) (radius 0.1))
    (polygon
      (pts
        (xy 155.5184 115.647) (xy 138.9184 115.647) (xy 138.9184 82.727) (xy 155.5184 82.727)
      )
    )
  )
  (zone (net 26) (net_name GND) (layer Bottom) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.2) (thermal_bridge_width 0.3) (smoothing fillet) (radius 0.1))
    (polygon
      (pts
        (xy 155.5184 115.647) (xy 138.9184 115.647) (xy 138.9184 82.727) (xy 155.5184 82.727)
      )
    )
  )
)
