(kicad_pcb (version 20171130) (host pcbnew 5.1.10-88a1d61d58~88~ubuntu20.10.1)
  (general
    (thickness 1.6)
    (drawings 44)
    (tracks 48)
    (zones 0)
    (modules 5)
    (nets 11)
  )
  (page USLetter)
  (title_block
    (title "TPDD Cable")
    (date 2021-04-27)
    (rev 004)
    (company b.kenyon.w@gmail.com)
  )
  (layers
    (0 Top signal)
    (31 Bottom signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.2)
    (user_trace_width 0.4)
    (trace_clearance 0.2)
    (zone_clearance 0.16)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.5)
    (via_drill 0.3)
    (via_min_size 0.5)
    (via_min_drill 0.3)
    (uvia_size 0.5)
    (uvia_drill 0.3)
    (uvias_allowed no)
    (uvia_min_size 0.5)
    (uvia_min_drill 0.3)
    (edge_width 0.0127)
    (segment_width 0.2032)
    (pcb_text_width 0.1524)
    (pcb_text_size 1.2192 1.2192)
    (mod_edge_width 0.0508)
    (mod_text_size 0.6096 0.6096)
    (mod_text_width 0.0508)
    (pad_size 1.524 1.524)
    (pad_drill 0.889)
    (pad_to_mask_clearance 0)
    (solder_mask_min_width 0.22)
    (aux_axis_origin 0 0)
    (grid_origin 144.993 83.6295)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "GERBER_TPDD_Cable_004"))
  )
  (net 0 "")
  (net 1 /RTS)
  (net 2 /DTR)
  (net 3 /RX_TTL)
  (net 4 /CTS_TTL)
  (net 5 /DSR_TTL)
  (net 6 /TX)
  (net 7 /CTS)
  (net 8 /DSR)
  (net 9 /SG)
  (net 10 /RX)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.5)
    (via_drill 0.3)
    (uvia_dia 0.5)
    (uvia_drill 0.3)
    (diff_pair_width 0.2)
    (diff_pair_gap 0.2)
    (add_net /CTS)
    (add_net /CTS_TTL)
    (add_net /DSR)
    (add_net /DSR_TTL)
    (add_net /DTR)
    (add_net /RTS)
    (add_net /RX)
    (add_net /RX_TTL)
    (add_net /SG)
    (add_net /TX)
  )
  (module 000_LOCAL:D7_1.5mm_wirepads (layer Top) (tedit 608685CE)
    (at 144.993 87.8795)
    (descr "Through hole straight pin header, 1x07, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x07 1.27mm single row")
    (fp_text reference J1 (at 0 -1.695) (layer F.SilkS) hide)
    (fp_text value "Wire Solder Pads" (at 0 9.315 180 unlocked) (layer F.Fab) hide)
    (fp_text user %R (at 0 3.81 90) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 3 0.75 270) (size 1.4 1.4) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 /RTS))
    (pad 7 thru_hole circle (at 4.5 -0.75 270) (size 1.4 1.4) (drill 0.65) (layers *.Cu *.Mask)
      (net 9 /SG))
    (pad 4 thru_hole circle (at 0 0.75 270) (size 1.4 1.4) (drill 0.65) (layers *.Cu *.Mask)
      (net 7 /CTS))
    (pad 5 thru_hole circle (at 1.5 -0.75 270) (size 1.4 1.4) (drill 0.65) (layers *.Cu *.Mask)
      (net 8 /DSR))
    (pad 3 thru_hole circle (at -1.5 -0.75 270) (size 1.4 1.4) (drill 0.65) (layers *.Cu *.Mask)
      (net 2 /DTR))
    (pad 2 thru_hole circle (at -3 0.75 270) (size 1.4 1.4) (drill 0.65) (layers *.Cu *.Mask)
      (net 10 /RX))
    (pad 1 thru_hole circle (at -4.5 -0.75 270) (size 1.4 1.4) (drill 0.65) (layers *.Cu *.Mask)
      (net 6 /TX))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x07_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000_LOCAL:2-6-2_tpdd (layer Top) (tedit 608678DD)
    (at 148.803 82.2795)
    (attr smd)
    (fp_text reference J2 (at -1.27 -0.127 -90 unlocked) (layer F.SilkS) hide)
    (fp_text value TPDD (at -3.81 2.286) (layer F.Fab))
    (fp_text user 8 (at -7.0866 1.85 unlocked) (layer B.SilkS))
    (fp_text user 2 (at -0.5334 1.85 unlocked) (layer B.SilkS))
    (fp_text user 7 (at -7.31 1.85 unlocked) (layer F.SilkS))
    (fp_text user 1 (at -0.31 1.85 unlocked) (layer F.SilkS))
    (pad 2 smd roundrect (at 0 0) (size 1.5 2.7) (layers Bottom B.Mask) (roundrect_rratio 0.1)
      (net 1 /RTS))
    (pad 4 smd roundrect (at -2.54 0) (size 1.5 2.7) (layers Bottom B.Mask) (roundrect_rratio 0.1)
      (net 4 /CTS_TTL))
    (pad 6 smd roundrect (at -5.08 0) (size 1.5 2.7) (layers Bottom B.Mask) (roundrect_rratio 0.1)
      (net 3 /RX_TTL))
    (pad 8 smd roundrect (at -7.62 0) (size 1.5 2.7) (layers Bottom B.Mask) (roundrect_rratio 0.1))
    (pad 7 smd roundrect (at -7.62 0) (size 1.5 2.7) (layers Top F.Mask) (roundrect_rratio 0.1)
      (net 6 /TX))
    (pad 5 smd roundrect (at -5.08 0) (size 1.5 2.7) (layers Top F.Mask) (roundrect_rratio 0.1)
      (net 2 /DTR))
    (pad 3 smd roundrect (at -2.54 0) (size 1.5 2.7) (layers Top F.Mask) (roundrect_rratio 0.1)
      (net 5 /DSR_TTL))
    (pad 1 smd roundrect (at 0 0) (size 1.5 2.7) (layers Top F.Mask) (roundrect_rratio 0.1)
      (net 9 /SG))
    (model ${KIPRJMOD}/000_LOCAL.pretty/3dshapes/PinSocket_2x03_P2.54mm_Vertical_2pulled.step
      (offset (xyz -5.08 1.47 2.93))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 180 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/3dshapes/PinSocket_1x02_P2.54mm_Vertical.step
      (offset (xyz 0 1.47 -2.15))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/3dshapes/PinSocket_1x02_P2.54mm_Vertical.step
      (offset (xyz -7.62 1.47 -2.15))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (module 000_LOCAL:SC-59 (layer Bottom) (tedit 5F2C749B)
    (at 141.945 85.5345 270)
    (descr "SC-59, https://lib.chipdip.ru/images/import_diod/original/SOT-23_SC-59.jpg")
    (tags SC-59)
    (attr smd)
    (fp_text reference Q3 (at -0.3175 0.762 unlocked) (layer B.SilkS))
    (fp_text value DTA114EKA (at -1.905 -3.175 90) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -1.2 0.95 270) (size 0.762 0.635) (layers Bottom B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 9 /SG))
    (pad 2 smd roundrect (at -1.2 -0.95 270) (size 0.762 0.635) (layers Bottom B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 /RX_TTL))
    (pad 3 smd roundrect (at 1.2 0 270) (size 0.762 0.635) (layers Bottom B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 10 /RX))
    (model ${KIPRJMOD}/000_LOCAL.pretty/3dshapes/SC-59.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000_LOCAL:SC-59 (layer Bottom) (tedit 5F2C749B)
    (at 144.993 85.5345 270)
    (descr "SC-59, https://lib.chipdip.ru/images/import_diod/original/SOT-23_SC-59.jpg")
    (tags SC-59)
    (attr smd)
    (fp_text reference Q2 (at -0.381 0.8255 unlocked) (layer B.SilkS))
    (fp_text value DTA114EKA (at -1.905 -3.175 90) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -1.2 0.95 270) (size 0.762 0.635) (layers Bottom B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 9 /SG))
    (pad 2 smd roundrect (at -1.2 -0.95 270) (size 0.762 0.635) (layers Bottom B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 /CTS_TTL))
    (pad 3 smd roundrect (at 1.2 0 270) (size 0.762 0.635) (layers Bottom B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 7 /CTS))
    (model ${KIPRJMOD}/000_LOCAL.pretty/3dshapes/SC-59.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000_LOCAL:SC-59 (layer Bottom) (tedit 5F2C749B)
    (at 148.041 85.5345 270)
    (descr "SC-59, https://lib.chipdip.ru/images/import_diod/original/SOT-23_SC-59.jpg")
    (tags SC-59)
    (attr smd)
    (fp_text reference Q1 (at -0.3175 0.762 unlocked) (layer B.SilkS))
    (fp_text value DTA114EKA (at -1.905 -3.175 90) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -1.2 0.95 270) (size 0.762 0.635) (layers Bottom B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 9 /SG))
    (pad 2 smd roundrect (at -1.2 -0.95 270) (size 0.762 0.635) (layers Bottom B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 5 /DSR_TTL))
    (pad 3 smd roundrect (at 1.2 0 270) (size 0.762 0.635) (layers Bottom B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 8 /DSR))
    (model ${KIPRJMOD}/000_LOCAL.pretty/3dshapes/SC-59.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_arc (start 148.493 93.3795) (end 148.493 94.1295) (angle -180) (layer Edge.Cuts) (width 0.0127))
  (gr_arc (start 141.493 93.3795) (end 141.493 92.6295) (angle -180) (layer Edge.Cuts) (width 0.0127))
  (gr_line (start 139.793 86.5295) (end 140.243 86.0795) (layer Edge.Cuts) (width 0.0127))
  (gr_line (start 139.793 87.6795) (end 139.793 86.5295) (layer Edge.Cuts) (width 0.0127))
  (gr_line (start 141.743 89.6295) (end 139.793 87.6795) (layer Edge.Cuts) (width 0.0127))
  (gr_line (start 150.193 86.5295) (end 149.743 86.0795) (layer Edge.Cuts) (width 0.0127))
  (gr_line (start 150.193 87.6795) (end 150.193 86.5295) (layer Edge.Cuts) (width 0.0127))
  (gr_line (start 148.243 89.6295) (end 150.193 87.6795) (layer Edge.Cuts) (width 0.0127))
  (gr_arc (start 148.243 92.3795) (end 147.993 92.3795) (angle -90) (layer Edge.Cuts) (width 0.0127))
  (gr_arc (start 141.743 92.3795) (end 141.743 92.6295) (angle -90) (layer Edge.Cuts) (width 0.0127))
  (gr_arc (start 141.743 89.8795) (end 141.993 89.8795) (angle -90) (layer Edge.Cuts) (width 0.0127))
  (gr_arc (start 148.243 89.8795) (end 148.243 89.6295) (angle -90) (layer Edge.Cuts) (width 0.0127))
  (gr_line (start 147.993 89.8795) (end 147.993 92.3795) (layer Edge.Cuts) (width 0.0127))
  (gr_line (start 149.743 80.8795) (end 149.743 86.0795) (layer Edge.Cuts) (width 0.0127))
  (gr_line (start 140.243 80.8795) (end 149.743 80.8795) (layer Edge.Cuts) (width 0.0127))
  (gr_line (start 140.243 86.0795) (end 140.243 80.8795) (layer Edge.Cuts) (width 0.0127))
  (gr_line (start 141.993 92.3795) (end 141.993 89.8795) (layer Edge.Cuts) (width 0.0127))
  (gr_line (start 148.493 92.6295) (end 148.243 92.6295) (layer Edge.Cuts) (width 0.0127))
  (gr_line (start 141.743 92.6295) (end 141.493 92.6295) (layer Edge.Cuts) (width 0.0127))
  (gr_line (start 141.493 94.1295) (end 148.493 94.1295) (layer Edge.Cuts) (width 0.0127))
  (gr_text tandy.wiki/TPDD (at 144.943 93.3795) (layer F.SilkS))
  (gr_text THIS (at 147.483 82.296 -90) (layer F.SilkS))
  (gr_text SIDE (at 144.9295 82.296 -90) (layer F.SilkS))
  (gr_text UP (at 142.453 82.296 -90) (layer F.SilkS))
  (gr_text THIS (at 142.523 82.2995 -270) (layer B.SilkS))
  (gr_text SIDE (at 145.003 82.2995 -270) (layer B.SilkS))
  (gr_text "Q* DTA114EKA" (at 145.018 93.3795) (layer B.SilkS))
  (gr_text DB25M (at 144.993 90.3295) (layer F.SilkS))
  (gr_text DOWN (at 147.5584 82.4611 -270) (layer B.SilkS))
  (gr_text 4 (at 147.993 87.4045) (layer F.SilkS))
  (gr_text 5 (at 144.993 87.4045) (layer F.SilkS))
  (gr_text 3 (at 141.993 87.4045) (layer F.SilkS))
  (gr_text 2 (at 140.793 85.9045) (layer F.SilkS))
  (gr_text 20 (at 143.493 85.9045) (layer F.SilkS))
  (gr_text 6 (at 146.493 85.9045) (layer F.SilkS))
  (gr_text 7 (at 149.218 85.9545) (layer F.SilkS))
  (gr_text TPDD (at 144.993 84.6295) (layer F.SilkS))
)
