<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="57.4675" y1="0" x2="57.4675" y2="26.035" width="0" layer="20"/>
<wire x1="57.4675" y1="26.035" x2="0" y2="26.035" width="0" layer="20"/>
<wire x1="0" y1="26.035" x2="0" y2="0" width="0" layer="20"/>
<wire x1="0" y1="0" x2="57.4675" y2="0" width="0" layer="20"/>
<text>7</text>
<text>6</text>
<text>5</text>
<text>4</text>
<text>3</text>
<text>2</text>
<text>1</text>
<text>0</text>
<text>AL</text>
<text>RD</text>
<text>3V</text>
<text>GND</text>
<text>WR</text>
<text>CS</text>
<text>PSP</text>
<text>14</text>
<text>13</text>
<text>12</text>
<text>11</text>
<text>10</text>
<text>9</text>
<text>8</text>
<text>INT</text>
<text>CLK</text>
<text>C4</text>
<text>v1 2014-11-22</text>
<text>Design by</text>
<text>Josh Stone</text>
</plain>
<libraries>
<library name="josh">
<packages>
<package name="TQFP-44">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="C0603">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="HC49/S">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="MAGJACK">
</package>
<package name="1X12_NO_SILK">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="josh" package="TQFP-44" value="ENC424J600">
<attribute name="VALUE"/>
</element>
<element name="C3" library="adafruit" package="C0603" value="10 uF">
<attribute name="NAME"/>
</element>
<element name="R4" library="adafruit" package="R0603" value="100">
<attribute name="NAME"/>
</element>
<element name="C8" library="adafruit" package="C0603" value="10 pF">
<attribute name="NAME"/>
</element>
<element name="C7" library="adafruit" package="C0603" value="10 pF">
<attribute name="NAME"/>
</element>
<element name="Q1" library="adafruit" package="HC49/S" value="25 mHz">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1667008"/>
</element>
<element name="R6" library="adafruit" package="R0603" value="12.4 k">
<attribute name="NAME"/>
</element>
<element name="R3" library="adafruit" package="R0603" value="49.9">
<attribute name="NAME"/>
</element>
<element name="R1" library="adafruit" package="R0603" value="49.9">
<attribute name="NAME"/>
</element>
<element name="C2" library="adafruit" package="C0603" value="10 pF">
<attribute name="NAME"/>
</element>
<element name="C1" library="adafruit" package="C0603" value="6.8 nF">
<attribute name="NAME"/>
</element>
<element name="C4" library="adafruit" package="C0603" value="6.8 nF"/>
<element name="R8" library="adafruit" package="R0603" value="49.9">
<attribute name="NAME"/>
</element>
<element name="R7" library="adafruit" package="R0603" value="49.9">
<attribute name="NAME"/>
</element>
<element name="R5" library="adafruit" package="R0603" value="10">
<attribute name="NAME"/>
</element>
<element name="C6" library="adafruit" package="C0603" value="0.01 uF">
<attribute name="NAME"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="MAGJACK" value="MAGJACK"/>
<element name="R2" library="adafruit" package="R0603" value="330">
<attribute name="NAME"/>
</element>
<element name="R9" library="adafruit" package="R0603" value="330">
<attribute name="NAME"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="1X12_NO_SILK" value="M12NO_SILK"/>
<element name="JP1" library="SparkFun-Connectors" package="1X12_NO_SILK" value="M12NO_SILK"/>
<element name="C10" library="adafruit" package="C0603" value="1 uF">
<attribute name="NAME"/>
</element>
<element name="C9" library="adafruit" package="C0603" value="0.1 uF">
<attribute name="NAME"/>
</element>
<element name="C5" library="adafruit" package="C0603" value="0.01 uF">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="VDD">
<contactref element="U$1" pad="P$12"/>
<contactref element="U$1" pad="P$15"/>
<contactref element="U$1" pad="P$18"/>
<contactref element="R8" pad="2"/>
<contactref element="R7" pad="2"/>
<contactref element="R5" pad="2"/>
<contactref element="JP2" pad="11"/>
<contactref element="U$1" pad="P$4"/>
<contactref element="U$1" pad="P$44"/>
<contactref element="C10" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="C5" pad="1"/>
</signal>
<signal name="GND">
<contactref element="U$1" pad="P$1"/>
<contactref element="C3" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="R6" pad="1"/>
<contactref element="U$1" pad="P$13"/>
<contactref element="U$1" pad="P$14"/>
<contactref element="U$1" pad="P$19"/>
<contactref element="U$1" pad="P$22"/>
<contactref element="C6" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="J1" pad="12"/>
<contactref element="J1" pad="10"/>
<contactref element="J1" pad="M2"/>
<contactref element="J1" pad="M1"/>
<contactref element="JP2" pad="12"/>
<contactref element="U$1" pad="P$33"/>
<contactref element="U$1" pad="P$42"/>
<contactref element="C9" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="C5" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="U$1" pad="P$2"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="R4" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="Q1" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="Q1" pad="2"/>
<contactref element="C7" pad="1"/>
<contactref element="U$1" pad="P$3"/>
</signal>
<signal name="N$5">
<contactref element="U$1" pad="P$11"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="U$1" pad="P$16"/>
<contactref element="R3" pad="2"/>
<contactref element="C4" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="U$1" pad="P$17"/>
<contactref element="R1" pad="2"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="R3" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="J1" pad="6"/>
</signal>
<signal name="N$11">
<contactref element="U$1" pad="P$21"/>
<contactref element="R8" pad="1"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="U$1" pad="P$20"/>
<contactref element="R7" pad="1"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="R5" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="N$15">
<contactref element="C1" pad="2"/>
<contactref element="J1" pad="8"/>
</signal>
<signal name="N$6">
<contactref element="C4" pad="2"/>
<contactref element="J1" pad="7"/>
</signal>
<signal name="N$14">
<contactref element="J1" pad="11"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$17">
<contactref element="J1" pad="9"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="LEDA">
<contactref element="R2" pad="1"/>
<contactref element="U$1" pad="P$10"/>
</signal>
<signal name="LEDB">
<contactref element="R9" pad="1"/>
<contactref element="U$1" pad="P$9"/>
</signal>
<signal name="AD7">
<contactref element="JP2" pad="1"/>
<contactref element="U$1" pad="P$8"/>
</signal>
<signal name="AD6">
<contactref element="JP2" pad="2"/>
<contactref element="U$1" pad="P$7"/>
</signal>
<signal name="AD5">
<contactref element="U$1" pad="P$6"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="AD4">
<contactref element="U$1" pad="P$5"/>
<contactref element="JP2" pad="4"/>
</signal>
<signal name="AD3">
<contactref element="JP2" pad="5"/>
<contactref element="U$1" pad="P$41"/>
</signal>
<signal name="AD2">
<contactref element="JP2" pad="6"/>
<contactref element="U$1" pad="P$40"/>
</signal>
<signal name="AD1">
<contactref element="JP2" pad="7"/>
<contactref element="U$1" pad="P$39"/>
</signal>
<signal name="AD0">
<contactref element="JP2" pad="8"/>
<contactref element="U$1" pad="P$38"/>
</signal>
<signal name="SI/RD/RW">
<contactref element="JP2" pad="10"/>
<contactref element="U$1" pad="P$36"/>
</signal>
<signal name="CLKOUT">
<contactref element="JP1" pad="1"/>
<contactref element="U$1" pad="P$23"/>
</signal>
<signal name="INT/SPISEL">
<contactref element="JP1" pad="2"/>
<contactref element="U$1" pad="P$24"/>
</signal>
<signal name="AD8">
<contactref element="JP1" pad="3"/>
<contactref element="U$1" pad="P$25"/>
</signal>
<signal name="AD9">
<contactref element="JP1" pad="4"/>
<contactref element="U$1" pad="P$26"/>
</signal>
<signal name="AD10">
<contactref element="JP1" pad="5"/>
<contactref element="U$1" pad="P$27"/>
</signal>
<signal name="AD11">
<contactref element="JP1" pad="6"/>
<contactref element="U$1" pad="P$28"/>
</signal>
<signal name="AD12">
<contactref element="JP1" pad="7"/>
<contactref element="U$1" pad="P$29"/>
</signal>
<signal name="AD13">
<contactref element="JP1" pad="8"/>
<contactref element="U$1" pad="P$30"/>
</signal>
<signal name="AD14">
<contactref element="JP1" pad="9"/>
<contactref element="U$1" pad="P$31"/>
</signal>
<signal name="PSPCFG0">
<contactref element="JP1" pad="10"/>
<contactref element="U$1" pad="P$32"/>
</signal>
<signal name="CS/CS">
<contactref element="JP1" pad="11"/>
<contactref element="U$1" pad="P$34"/>
</signal>
<signal name="SO/WR/EN">
<contactref element="JP1" pad="12"/>
<contactref element="U$1" pad="P$35"/>
</signal>
<signal name="SCK/AL">
<contactref element="U$1" pad="P$37"/>
<contactref element="JP2" pad="9"/>
</signal>
<signal name="N$38">
<contactref element="U$1" pad="P$43"/>
<contactref element="C3" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
