(kicad_pcb (version 20171130) (host pcbnew "(5.0.0)")
  (general
    (thickness 1.6)
    (drawings 8)
    (tracks 104)
    (zones 0)
    (modules 3)
    (nets 32)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.2)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.254)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.01 0.01)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010d0_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference false)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "GERBER/"))
  )
  (net 0 "")
  (net 1 "Net-(U1-Pad25)")
  (net 2 "Net-(U1-Pad24)")
  (net 3 "Net-(U1-Pad22)")
  (net 4 "Net-(U1-Pad18)")
  (net 5 "Net-(U1-Pad17)")
  (net 6 "Net-(U1-Pad16)")
  (net 7 "Net-(U1-Pad15)")
  (net 8 "Net-(U1-Pad14)")
  (net 9 "Net-(U1-Pad13)")
  (net 10 "Net-(U1-Pad12)")
  (net 11 "Net-(U1-Pad11)")
  (net 12 "Net-(U1-Pad10)")
  (net 13 "Net-(U1-Pad9)")
  (net 14 "Net-(U1-Pad5)")
  (net 15 "Net-(U1-Pad1)")
  (net 16 VBUS)
  (net 17 GND)
  (net 18 "Net-(J1-Pad8)")
  (net 19 "Net-(J1-Pad7)")
  (net 20 "Net-(J1-Pad6)")
  (net 21 "Net-(J1-Pad5)")
  (net 22 "Net-(J1-Pad4)")
  (net 23 "Net-(J2-Pad1)")
  (net 24 "Net-(J2-Pad2)")
  (net 25 "Net-(J2-Pad3)")
  (net 26 "Net-(J2-Pad4)")
  (net 27 "Net-(J2-Pad5)")
  (net 28 "Net-(J2-Pad6)")
  (net 29 "Net-(J2-Pad7)")
  (net 30 "Net-(J1-Pad3)")
  (net 31 "Net-(J1-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(J2-Pad6)")
    (add_net "Net-(J2-Pad7)")
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad11)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U1-Pad13)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U1-Pad15)")
    (add_net "Net-(U1-Pad16)")
    (add_net "Net-(U1-Pad17)")
    (add_net "Net-(U1-Pad18)")
    (add_net "Net-(U1-Pad22)")
    (add_net "Net-(U1-Pad24)")
    (add_net "Net-(U1-Pad25)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad9)")
    (add_net VBUS)
  )
  (module Housings_DFN_QFN:QFN-24-1EP_4x4mm_Pitch0.5mm (layer B.Cu) (tedit 5BC295AF)
    (at 140.94 90.18 135)
    (descr "24-Lead Plastic Quad Flat, No Lead Package (MJ) - 4x4x0.9 mm Body [QFN]; (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFN 0.5")
    (attr smd)
    (fp_text reference U1 (at 0.700036 3.358757 135) (layer B.SilkS))
    (fp_text value CP2104 (at 0 -3.374999 135) (layer B.Fab))
    (pad 25 smd rect (at -0.65 0.65 135) (size 1.3 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(U1-Pad25)") (solder_paste_margin_ratio -0.2))
    (pad 25 smd rect (at -0.65 -0.65 135) (size 1.3 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(U1-Pad25)") (solder_paste_margin_ratio -0.2))
    (pad 25 smd rect (at 0.65 0.65 135) (size 1.3 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(U1-Pad25)") (solder_paste_margin_ratio -0.2))
    (pad 25 smd rect (at 0.65 -0.65 135) (size 1.3 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(U1-Pad25)") (solder_paste_margin_ratio -0.2))
    (pad 24 smd rect (at -1.25 1.95 45) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(U1-Pad24)"))
    (pad 23 smd rect (at -0.75 1.95 45) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 27 "Net-(J2-Pad5)"))
    (pad 22 smd rect (at -0.25 1.95 45) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(U1-Pad22)"))
    (pad 21 smd rect (at 0.25 1.95 45) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 31 "Net-(J1-Pad2)"))
    (pad 20 smd rect (at 0.75 1.95 45) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 30 "Net-(J1-Pad3)"))
    (pad 19 smd rect (at 1.25 1.95 45) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 28 "Net-(J2-Pad6)"))
    (pad 18 smd rect (at 1.95 1.25 135) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(U1-Pad18)"))
    (pad 17 smd rect (at 1.95 0.75 135) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(U1-Pad17)"))
    (pad 16 smd rect (at 1.95 0.25 135) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(U1-Pad16)"))
    (pad 15 smd rect (at 1.95 -0.25 135) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(U1-Pad15)"))
    (pad 14 smd rect (at 1.95 -0.75 135) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(U1-Pad14)"))
    (pad 13 smd rect (at 1.95 -1.25 135) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(U1-Pad13)"))
    (pad 12 smd rect (at 1.25 -1.95 45) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(U1-Pad12)"))
    (pad 11 smd rect (at 0.75 -1.95 45) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(U1-Pad11)"))
    (pad 10 smd rect (at 0.25 -1.95 45) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(U1-Pad10)"))
    (pad 9 smd rect (at -0.25 -1.95 45) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(U1-Pad9)"))
    (pad 8 smd rect (at -0.75 -1.95 45) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 16 VBUS))
    (pad 7 smd rect (at -1.25 -1.95 45) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 16 VBUS))
    (pad 6 smd rect (at -1.95 -1.25 135) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(U1-Pad5)"))
    (pad 5 smd rect (at -1.95 -0.75 135) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(U1-Pad5)"))
    (pad 4 smd rect (at -1.95 -0.25 135) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(J1-Pad6)"))
    (pad 3 smd rect (at -1.95 0.25 135) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 21 "Net-(J1-Pad5)"))
    (pad 2 smd rect (at -1.95 0.75 135) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 17 GND))
    (pad 1 smd rect (at -1.95 1.25 135) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(U1-Pad1)"))
    (model ${KISYS3DMOD}/Housings_DFN_QFN.3dshapes/QFN-24-1EP_4x4mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x08_Pitch1.27mm (layer F.Cu) (tedit 59650535)
    (at 137.34 94.63 180)
    (descr "Through hole straight pin header, 1x08, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x08 1.27mm single row")
    (fp_text reference J1 (at 0 -1.695 180) (layer F.SilkS))
    (fp_text value Conn_01x08_Male (at 0 10.585 180) (layer F.Fab))
    (fp_text user %R (at 0 4.445 270) (layer F.Fab))
    (pad 8 thru_hole oval (at 0 8.89 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 18 "Net-(J1-Pad8)"))
    (pad 7 thru_hole oval (at 0 7.62 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 19 "Net-(J1-Pad7)"))
    (pad 6 thru_hole oval (at 0 6.35 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 20 "Net-(J1-Pad6)"))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 21 "Net-(J1-Pad5)"))
    (pad 4 thru_hole oval (at 0 3.81 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 22 "Net-(J1-Pad4)"))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 30 "Net-(J1-Pad3)"))
    (pad 2 thru_hole oval (at 0 1.27 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 31 "Net-(J1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 17 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x08_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x08_Pitch1.27mm (layer F.Cu) (tedit 59650535)
    (at 144.54 85.74)
    (descr "Through hole straight pin header, 1x08, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x08 1.27mm single row")
    (fp_text reference J2 (at 0 -1.695) (layer F.SilkS))
    (fp_text value Conn_01x08_Male (at 0 10.585) (layer F.Fab))
    (fp_text user %R (at 0 4.445 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 23 "Net-(J2-Pad1)"))
    (pad 2 thru_hole oval (at 0 1.27) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 24 "Net-(J2-Pad2)"))
    (pad 3 thru_hole oval (at 0 2.54) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 25 "Net-(J2-Pad3)"))
    (pad 4 thru_hole oval (at 0 3.81) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 26 "Net-(J2-Pad4)"))
    (pad 5 thru_hole oval (at 0 5.08) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 27 "Net-(J2-Pad5)"))
    (pad 6 thru_hole oval (at 0 6.35) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 28 "Net-(J2-Pad6)"))
    (pad 7 thru_hole oval (at 0 7.62) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 29 "Net-(J2-Pad7)"))
    (pad 8 thru_hole oval (at 0 8.89) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 16 VBUS))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x08_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 137.34 84.68) (end 144.56 84.68) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 144.55 95.62) (end 144.54 95.62) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 144.56 95.62) (end 144.55 95.62) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 137.34 95.62) (end 144.56 95.62) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 144.54 94.68) (end 144.54 95.6) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 137.34 94.66) (end 137.34 95.6) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 137.34 94.64) (end 137.34 84.7) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 144.54 94.65) (end 144.55 84.7) (layer Edge.Cuts) (width 0.254))
)
