(kicad_pcb (version 4) (host pcbnew 4.0.1-stable)
  (general
    (links 34)
    (no_connects 0)
    (area 167.564999 95.174999 185.495001 113.105001)
    (thickness 1.6)
    (drawings 20)
    (tracks 141)
    (zones 0)
    (modules 18)
    (nets 13)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.3048)
    (user_trace_width 0.3048)
    (trace_clearance 0.1524)
    (zone_clearance 0.1524)
    (zone_45_only yes)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.9)
    (pad_to_mask_clearance 0.0762)
    (aux_axis_origin 176.53 104.14)
    (grid_origin 176.53 104.14)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(Cin1-Pad1)")
  (net 2 GND)
  (net 3 +3V3)
  (net 4 "Net-(D1-Pad2)")
  (net 5 "Net-(R1-Pad2)")
  (net 6 "Net-(D2-Pad2)")
  (net 7 "Net-(R2-Pad2)")
  (net 8 "Net-(PR1-Pad2)")
  (net 9 "Net-(R4-Pad2)")
  (net 10 "Net-(Rbot1-Pad1)")
  (net 11 "Net-(SW1-Pad1)")
  (net 12 "Net-(L1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net +3V3)
    (add_net GND)
    (add_net "Net-(Cin1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(L1-Pad1)")
    (add_net "Net-(PR1-Pad2)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(R4-Pad2)")
    (add_net "Net-(Rbot1-Pad1)")
    (add_net "Net-(SW1-Pad1)")
  )
  (module Pin_Headers:Pin_Header_Straight_1x05_Pitch1.27mm (layer F.Cu) (tedit 5A2E9E01)
    (at 184.785 101.6)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (fp_text reference icsp (at -0.762 -2.286 270) (layer F.SilkS))
    (fp_text value PICKIT3_ICSP (at 8.89 13.462) (layer F.Fab))
    (fp_text user %R (at 2.5 2.5 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 11 "Net-(SW1-Pad1)"))
    (pad 2 thru_hole oval (at 0 1.27) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 3 thru_hole rect (at 0 2.54) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 3.81) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 7 "Net-(R2-Pad2)"))
    (pad 5 thru_hole oval (at 0 5.08) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 5 "Net-(R1-Pad2)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x05_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_SMD:SW_SPST_EVQPE1 (layer F.Cu) (tedit 5A2E90A3)
    (at 176.53 96.266 180)
    (descr "Light Touch Switch, https://industrial.panasonic.com/cdbs/www-data/pdf/ATK0000/ATK0000CE7.pdf")
    (attr smd)
    (fp_text reference bt (at 0 0.5 180) (layer F.SilkS))
    (fp_text value SW_PUSH (at -14.224 -24.003 180) (layer F.Fab))
    (fp_text user %R (at 0 -2.65 180) (layer F.Fab))
    (pad 2 smd rect (at 4.5 0 180) (size 2 1) (layers F.Cu F.Mask)
      (net 9 "Net-(R4-Pad2)"))
    (pad 1 smd rect (at -4.5 0 180) (size 2 1) (layers F.Cu F.Mask)
      (net 11 "Net-(SW1-Pad1)"))
    (pad 1 smd rect (at -4.5 0 180) (size 2 1) (layers B.Cu B.Mask)
      (net 11 "Net-(SW1-Pad1)"))
    (pad 2 smd rect (at 4.5 0 180) (size 2 1) (layers B.Cu B.Mask)
      (net 9 "Net-(R4-Pad2)"))
    (model ${KISYS3DMOD}/Buttons_Switches_SMD.3dshapes/SW_SPST_EVQPE1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm_FlatTop (layer F.Cu) (tedit 5A2E90DF)
    (at 168.656 102.87 270)
    (descr "LED, Round, FlatTop, diameter 3.0mm, 2 pins, http://www.kingbright.com/attachments/file/psearch/000/00/00/L-47XEC(Ver.9A).pdf")
    (tags "LED Round FlatTop diameter 3.0mm 2 pins")
    (fp_text reference PR (at -1.778 0.127 270) (layer F.SilkS))
    (fp_text value Photores (at 19.685 -18.415 360) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 8 "Net-(PR1-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm_FlatTop.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom2:VariousLED (layer F.Cu) (tedit 5A2E8C9B)
    (at 176.53 107.14 180)
    (fp_text reference D1 (at 1.27 -4.112 180) (layer F.SilkS))
    (fp_text value LED (at 15.367 -12.621 180) (layer F.Fab) hide)
    (fp_text user K (at 3 -3.8 180) (layer F.SilkS))
    (fp_text user A (at -1.9 -2.1 180) (layer F.SilkS))
    (pad 2 smd rect (at -1.1 -2.8 180) (size 1.2 0.8) (layers F.Cu F.Mask)
      (net 4 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at 1.25 -2.8 180) (size 2.5 0.8) (layers F.Cu F.Mask)
      (net 2 GND))
  )
  (module custom2:VariousLED (layer F.Cu) (tedit 5A2E90B2)
    (at 176.53 101.14)
    (fp_text reference D2 (at 1.778 -3.858) (layer F.SilkS))
    (fp_text value LED (at -16.002 16.335) (layer F.Fab) hide)
    (fp_text user K (at 3 -2) (layer F.SilkS))
    (fp_text user A (at -1.9 -2.1) (layer F.SilkS))
    (pad 2 smd rect (at -1.1 -2.8) (size 1.2 0.8) (layers F.Cu F.Mask)
      (net 6 "Net-(D2-Pad2)"))
    (pad 1 smd rect (at 1.25 -2.8) (size 2.5 0.8) (layers F.Cu F.Mask)
      (net 2 GND))
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 5A2EA7D3)
    (at 176.53 104.14)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference "Vin +" (at 4.699 0.254 90) (layer B.SilkS) hide)
    (fp_text value Batt (at -9.906 16.764) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 5 5) (layers B.Cu B.Mask)
      (net 1 "Net-(Cin1-Pad1)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5A2EAA99)
    (at 172.212 106.934)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference Cin (at -0.254 1.397) (layer F.SilkS))
    (fp_text value 4.7u (at -1.778 11.303) (layer F.Fab))
    (fp_text user %R (at 0 -1.5) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Mask)
      (net 1 "Net-(Cin1-Pad1)"))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5A2E8C84)
    (at 182.88 104.14 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference Cout (at 0 1.27 270) (layer F.SilkS))
    (fp_text value 10u (at 12.827 -10.668 360) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5A2EA9C3)
    (at 180.34 109.22 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 1.143 -1.397 180) (layer F.SilkS))
    (fp_text value R (at 0.889 -8.763 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Mask)
      (net 4 "Net-(D1-Pad2)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Mask)
      (net 5 "Net-(R1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5A2E8CB3)
    (at 176.53 101.346)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0.508 -1.27) (layer F.SilkS))
    (fp_text value R (at 8.001 16.764) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Mask)
      (net 6 "Net-(D2-Pad2)"))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Mask)
      (net 7 "Net-(R2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5A2E90F2)
    (at 170.942 104.14 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 1.905 0 180) (layer F.SilkS))
    (fp_text value 10K (at -14.478 22.606 180) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Mask)
      (net 8 "Net-(PR1-Pad2)"))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5A2E8C8D)
    (at 181.356 100.33 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 0 1.524 180) (layer F.SilkS))
    (fp_text value 10K (at -12.446 -21.717 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Mask)
      (net 9 "Net-(R4-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5A2E8346)
    (at 181.356 106.934)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference Rbot (at -2.032 0 90) (layer F.SilkS))
    (fp_text value 309K (at -7.366 11.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Mask)
      (net 10 "Net-(Rbot1-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5A2EADA8)
    (at 176.657 107.569 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference Rtop (at -0.127 1.397 360) (layer F.SilkS))
    (fp_text value 536K (at 2.794 -8.509 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Mask)
      (net 10 "Net-(Rbot1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-6 (layer F.Cu) (tedit 5A2E905B)
    (at 174.244 104.14)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U1 (at 0.127 -2.032) (layer F.SilkS))
    (fp_text value MCP1623/24 (at 0.8509 19.7104) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Mask)
      (net 12 "Net-(L1-Pad1)"))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Mask)
      (net 1 "Net-(Cin1-Pad1)"))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Mask)
      (net 10 "Net-(Rbot1-Pad1)"))
    (pad 6 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Mask)
      (net 1 "Net-(Cin1-Pad1)"))
    (pad 5 smd rect (at 1.1 0) (size 1.06 0.65) (layers F.Cu F.Mask)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-6 (layer F.Cu) (tedit 5A2E8335)
    (at 178.816 104.14)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U2 (at 0.508 -2.032) (layer F.SilkS))
    (fp_text value PIC10F320/322 (at -2.54 16.764) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Mask)
      (net 7 "Net-(R2-Pad2)"))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Mask)
      (net 5 "Net-(R1-Pad2)"))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Mask)
      (net 8 "Net-(PR1-Pad2)"))
    (pad 6 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Mask)
      (net 11 "Net-(SW1-Pad1)"))
    (pad 5 smd rect (at 1.1 0) (size 1.06 0.65) (layers F.Cu F.Mask)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5A2E9080)
    (at 172.212 100.33)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference L (at 0.762 -1.397) (layer F.SilkS))
    (fp_text value 4.7u (at 16.764 18.161 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.5) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Mask)
      (net 12 "Net-(L1-Pad1)"))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Mask)
      (net 1 "Net-(Cin1-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom2:LOGO (layer B.Cu) (tedit 5A2EA503)
    (at 176.276 103.505 180)
    (fp_text reference logo (at 10.287 -14.732 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 10.668 -13.843 180) (layer B.SilkS) hide)
  )
  (gr_text clk (at 183.515 106.68) (layer B.SilkS))
  (gr_text dat (at 183.388 105.41) (layer B.SilkS))
  (gr_text GND (at 183.261 104.14) (layer B.SilkS))
  (gr_text Vdd (at 183.388 102.743) (layer B.SilkS))
  (gr_text Vpp (at 183.388 101.346) (layer B.SilkS))
  (gr_text "Another Candle" (at 176.784 108.966) (layer B.SilkS))
  (gr_text "Vin (+)" (at 173.101 101.981 55) (layer B.SilkS))
  (gr_text pierremuth.wordpress.com (at 182.626 111.379) (layer B.SilkS))
  (gr_text "PIC10F320 & MCP1624" (at 176.403 110.236) (layer B.Mask))
  (gr_line (start 180.34 95.25) (end 172.72 95.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 185.42 100.33) (end 185.42 107.95) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 172.72 113.03) (end 180.34 113.03) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 167.64 100.33) (end 167.64 107.95) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 180.34 107.95) (end 185.42 107.95) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 172.72 107.95) (end 172.72 113.03) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 172.72 100.33) (end 167.64 100.33) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 180.34 100.33) (end 180.34 95.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 16) (thermal_gap 0.1524) (thermal_bridge_width 0.254) (smoothing fillet))
    (polygon
      (pts
        (xy 167.64 94.996) (xy 185.674 94.996) (xy 185.674 113.284) (xy 167.64 113.284)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 16) (thermal_gap 0.1524) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 173.228 94.996) (xy 173.228 97.028) (xy 180.086 97.028) (xy 180.086 94.996) (xy 185.674 94.996)
        (xy 185.674 113.284) (xy 167.513 113.284) (xy 167.513 94.996)
      )
    )
  )
)
