(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "unconnected-(J1-Pin_1-Pad1)")
  (net 2 "unconnected-(J1-Pin_2-Pad2)")
  (net 3 "unconnected-(J1-Pin_3-Pad3)")
  (net 4 "unconnected-(J1-Pin_4-Pad4)")
  (net 5 "unconnected-(J1-Pin_5-Pad5)")
  (net 6 "Net-(J1-Pin_6)")
  (net 7 "unconnected-(J1-Pin_7-Pad7)")
  (net 8 "unconnected-(J1-Pin_8-Pad8)")
  (net 9 "unconnected-(J2-Pin_1-Pad1)")
  (net 10 "unconnected-(J2-Pin_2-Pad2)")
  (net 11 "Net-(J2-Pin_3)")
  (net 12 "Net-(J2-Pin_4)")
  (net 13 "unconnected-(J2-Pin_5-Pad5)")
  (net 14 "unconnected-(J2-Pin_6-Pad6)")
  (net 15 "unconnected-(J2-Pin_7-Pad7)")
  (net 16 "unconnected-(J2-Pin_8-Pad8)")
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x08_P2.54mm_Vertical" (layer "F.Cu")
    (at 96.52 70.611)
    (descr "Through hole straight socket strip, 1x08, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x08 2.54mm single row")
    (property "Sheetfile" "cp2102n-hat.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connectable mounting pin connector, single row, 01x08, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J2" (at 0 -2.77) (layer "F.SilkS"))
    (fp_text value "Conn_01x08_MountingPin" (at 0 20.55) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 8.89 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 9 "unconnected-(J2-Pin_1-Pad1)") (pinfunction "Pin_1") (pintype "passive+no_connect"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 10 "unconnected-(J2-Pin_2-Pad2)") (pinfunction "Pin_2") (pintype "passive+no_connect"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(J2-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(J2-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 13 "unconnected-(J2-Pin_5-Pad5)") (pinfunction "Pin_5") (pintype "passive+no_connect"))
    (pad "6" thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 14 "unconnected-(J2-Pin_6-Pad6)") (pinfunction "Pin_6") (pintype "passive+no_connect"))
    (pad "7" thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 15 "unconnected-(J2-Pin_7-Pad7)") (pinfunction "Pin_7") (pintype "passive+no_connect"))
    (pad "8" thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 16 "unconnected-(J2-Pin_8-Pad8)") (pinfunction "Pin_8") (pintype "passive+no_connect"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Slots:Slot_For_Zipties" (layer "F.Cu")
    (at 87.63 73.66)
    (descr "Mounting Hole 5.5mm")
    (tags "mounting hole 5.5mm")
    (property "Sheetfile" "cp2102n-hat.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H1" (at 0 -6.5) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 6.5) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 3.048 7.62) (drill oval 1.905 6.35) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x03_P2.54mm_Vertical" (layer "F.Cu")
    (at 87.63 85.09 90)
    (descr "Through hole straight socket strip, 1x03, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x03 2.54mm single row")
    (property "Sheetfile" "cp2102n-hat.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connectable mounting pin connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J3" (at 0 -2.77 90) (layer "F.SilkS"))
    (fp_text value "Conn_01x03_MountingPin" (at 0 7.85 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.54) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(J2-Pin_3)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(J1-Pin_6)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(J2-Pin_4)") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Slots:Slot_For_Zipties" (layer "F.Cu")
    (at 92.71 73.66)
    (descr "Mounting Hole 5.5mm")
    (tags "mounting hole 5.5mm")
    (property "Sheetfile" "cp2102n-hat.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H2" (at 0 -6.5) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 6.5) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 3.048 7.62) (drill oval 1.905 6.35) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x08_P2.54mm_Vertical" (layer "F.Cu")
    (at 83.82 70.611)
    (descr "Through hole straight socket strip, 1x08, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x08 2.54mm single row")
    (property "Sheetfile" "cp2102n-hat.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connectable mounting pin connector, single row, 01x08, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J1" (at 0 -2.77) (layer "F.SilkS"))
    (fp_text value "Conn_01x08_MountingPin" (at 0 20.55) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 8.89 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "unconnected-(J1-Pin_1-Pad1)") (pinfunction "Pin_1") (pintype "passive+no_connect"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "unconnected-(J1-Pin_2-Pad2)") (pinfunction "Pin_2") (pintype "passive+no_connect"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "unconnected-(J1-Pin_3-Pad3)") (pinfunction "Pin_3") (pintype "passive+no_connect"))
    (pad "4" thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 4 "unconnected-(J1-Pin_4-Pad4)") (pinfunction "Pin_4") (pintype "passive+no_connect"))
    (pad "5" thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 5 "unconnected-(J1-Pin_5-Pad5)") (pinfunction "Pin_5") (pintype "passive+no_connect"))
    (pad "6" thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(J1-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "unconnected-(J1-Pin_7-Pad7)") (pinfunction "Pin_7") (pintype "passive+no_connect"))
    (pad "8" thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 8 "unconnected-(J1-Pin_8-Pad8)") (pinfunction "Pin_8") (pintype "passive+no_connect"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_rect (start 81.28 66.548) (end 99.06 90.932)
    (fill none) (layer "Edge.Cuts"))
  (gr_text "UART adapter\nmates with\nAdafruit 5335" (at 93.98 82.296) (layer "B.SilkS"))
  (zone (net 6) (net_name "Net-(J1-Pin_6)") (layer "F.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 99.06 66.548)
        (xy 99.06 90.932)
        (xy 81.28 90.932)
        (xy 81.28 66.548)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0))
    (min_thickness 0.25) (filled_areas_thickness no)
    (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed) (copperpour allowed) (footprints allowed))
    (fill (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 81.28 66.548)
        (xy 99.06 66.548)
        (xy 99.06 90.932)
        (xy 81.28 90.932)
      )
    )
  )
  (zone (net 6) (net_name "Net-(J1-Pin_6)") (layer "B.Cu") (hatch edge 0.5)
    (priority 1)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 81.28 66.548)
        (xy 99.06 66.548)
        (xy 99.06 90.932)
        (xy 81.28 90.932)
      )
    )
  )
)
