(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "+5V")
  (net 2 "GNDREF")
  (net 3 "Net-(D1-K)")
  (net 4 "Net-(D1-A)")
  (net 5 "Net-(J2-Pin_1)")
  (net 6 "+3V3")
  (net 7 "Net-(Q1-B)")
  (net 8 "Net-(Q1-C)")
  (net 9 "Net-(Q2-B)")
  (net 10 "Net-(Q2-C)")
  (net 11 "Net-(U2-1_TX1_CTX2_MISO1)")
  (net 12 "Net-(U5-C1)")
  (net 13 "Net-(U1-LBO)")
  (net 14 "Net-(U2-0_RX1_CRX2_CS1)")
  (net 15 "unconnected-(U1-Vsh-Pad3)")
  (net 16 "Net-(J3-Pin_1)")
  (net 17 "unconnected-(U1-USB-5V-Pad5V)")
  (net 18 "unconnected-(U1-USB-D+-PadD+)")
  (net 19 "unconnected-(U1-USB-D--PadD-)")
  (net 20 "unconnected-(U1-USB-GND-PadUG)")
  (net 21 "unconnected-(U2-5_IN2-Pad7)")
  (net 22 "unconnected-(U2-6_OUT1D-Pad8)")
  (net 23 "unconnected-(U2-7_RX2_OUT1A-Pad9)")
  (net 24 "unconnected-(U2-8_TX2_IN1-Pad10)")
  (net 25 "unconnected-(U2-9_OUT1C-Pad11)")
  (net 26 "unconnected-(U2-10_CS_MQSR-Pad12)")
  (net 27 "unconnected-(U2-11_MOSI_CTX1-Pad13)")
  (net 28 "unconnected-(U2-12_MISO_MQSL-Pad14)")
  (net 29 "unconnected-(U2-3V3-Pad15)")
  (net 30 "unconnected-(U2-24_A10_TX6_SCL2-Pad16)")
  (net 31 "unconnected-(U2-25_A11_RX6_SDA2-Pad17)")
  (net 32 "unconnected-(U2-28_RX7-Pad20)")
  (net 33 "unconnected-(U2-29_TX7-Pad21)")
  (net 34 "unconnected-(U2-30_CRX3-Pad22)")
  (net 35 "unconnected-(U2-31_CTX3-Pad23)")
  (net 36 "unconnected-(U2-32_OUT1B-Pad24)")
  (net 37 "unconnected-(U2-33_MCLK2-Pad25)")
  (net 38 "unconnected-(U2-34_RX8-Pad26)")
  (net 39 "unconnected-(U2-35_TX8-Pad27)")
  (net 40 "unconnected-(U2-36_CS-Pad28)")
  (net 41 "unconnected-(U2-37_CS-Pad29)")
  (net 42 "unconnected-(U2-40_A16-Pad32)")
  (net 43 "unconnected-(U2-41_A17-Pad33)")
  (net 44 "unconnected-(U2-13_SCK_LED-Pad35)")
  (net 45 "unconnected-(U2-14_A0_TX3_SPDIF_OUT-Pad36)")
  (net 46 "unconnected-(U2-15_A1_RX3_SPDIF_IN-Pad37)")
  (net 47 "Net-(U2-16_A2_RX4_SCL1)")
  (net 48 "Net-(U2-17_A3_TX4_SDA1)")
  (net 49 "unconnected-(U2-20_A6_TX5_LRCLK1-Pad42)")
  (net 50 "unconnected-(U2-21_A7_RX5_BCLK1-Pad43)")
  (net 51 "unconnected-(U2-22_A8_CTX1-Pad44)")
  (net 52 "unconnected-(U2-23_A9_CRX1_MCLK1-Pad45)")
  (net 53 "unconnected-(U2-VUSB-Pad49)")
  (net 54 "unconnected-(U2-VBAT-Pad50)")
  (net 55 "unconnected-(U2-3V3-Pad51)")
  (net 56 "unconnected-(U2-GND-Pad52)")
  (net 57 "unconnected-(U2-PROGRAM-Pad53)")
  (net 58 "unconnected-(U2-ON_OFF-Pad54)")
  (net 59 "unconnected-(U2-R+-Pad60)")
  (net 60 "unconnected-(U2-LED-Pad61)")
  (net 61 "unconnected-(U2-T--Pad62)")
  (net 62 "unconnected-(U2-T+-Pad63)")
  (net 63 "unconnected-(U2-GND-Pad64)")
  (net 64 "unconnected-(U2-R--Pad65)")
  (net 65 "unconnected-(U2-D--Pad66)")
  (net 66 "unconnected-(U2-D+-Pad67)")
  (net 67 "unconnected-(U3-0_RX1_CRX2_CS1-Pad2)")
  (net 68 "unconnected-(U3-1_TX1_CTX2_MISO1-Pad3)")
  (net 69 "unconnected-(U3-2_OUT2-Pad4)")
  (net 70 "unconnected-(U3-3_LRCLK2-Pad5)")
  (net 71 "unconnected-(U3-4_BCLK2-Pad6)")
  (net 72 "unconnected-(U3-5_IN2-Pad7)")
  (net 73 "Net-(U3-6_OUT1D)")
  (net 74 "Net-(U3-7_RX2_OUT1A)")
  (net 75 "Net-(U3-8_TX2_IN1)")
  (net 76 "unconnected-(U3-9_OUT1C-Pad11)")
  (net 77 "Net-(U3-10_CS_MQSR)")
  (net 78 "Net-(U3-11_MOSI_CTX1)")
  (net 79 "Net-(U3-12_MISO_MQSL)")
  (net 80 "unconnected-(U3-VBAT-Pad15)")
  (net 81 "unconnected-(U3-3V3-Pad16)")
  (net 82 "unconnected-(U3-GND-Pad17)")
  (net 83 "unconnected-(U3-PROGRAM-Pad18)")
  (net 84 "unconnected-(U3-ON_OFF-Pad19)")
  (net 85 "Net-(U3-13_SCK_CRX1_LED)")
  (net 86 "unconnected-(U3-14_A0_TX3_SPDIF_OUT-Pad21)")
  (net 87 "Net-(U3-15_A1_RX3_SPDIF_IN)")
  (net 88 "Net-(U3-18_A4_SDA0)")
  (net 89 "Net-(U3-19_A5_SCL0)")
  (net 90 "Net-(U3-20_A6_TX5_LRCLK1)")
  (net 91 "Net-(U3-21_A7_RX5_BCLK1)")
  (net 92 "unconnected-(U3-22_A8_CTX1-Pad29)")
  (net 93 "Net-(U3-23_A9_CRX1_MCLK1)")
  (net 94 "Net-(U4-3V3)")
  (net 95 "unconnected-(U3-VUSB-Pad34)")
  (net 96 "unconnected-(U3-24_A10_TX6_SCL2-Pad35)")
  (net 97 "unconnected-(U3-25_A11_RX6_SDA2-Pad36)")
  (net 98 "unconnected-(U3-26_A12_MOSI1-Pad37)")
  (net 99 "unconnected-(U3-27_A13_SCK1-Pad38)")
  (net 100 "unconnected-(U3-28_RX7-Pad39)")
  (net 101 "unconnected-(U3-29_TX7-Pad40)")
  (net 102 "unconnected-(U3-30_CRX3-Pad41)")
  (net 103 "unconnected-(U3-31_CTX3-Pad42)")
  (net 104 "unconnected-(U3-32_OUT1B-Pad43)")
  (net 105 "unconnected-(U3-33_MCLK2-Pad44)")
  (net 106 "unconnected-(U5-NC-Pad1)")
  (net 107 "unconnected-(U5-NC-Pad4)")
  (net 108 "unconnected-(U5-VO1-Pad7)")
  (net 109 "Net-(U2-27_A13_SCK1)")
  (net 110 "Net-(U2-26_A12_MOSI1)")
  (net 111 "unconnected-(U1-BAT-Pad2)")
  (net 112 "Net-(J1-Pin_1)")
  (net 113 "Net-(J3-Pin_2)")
  (net 114 "Net-(J3-Pin_3)")
  (net 115 "Net-(J5-Pin_1)")
  (net 116 "Net-(J5-Pin_2)")
  (net 117 "Net-(J5-Pin_3)")
  (net 118 "unconnected-(J6-Pin_36-Pad36)")
  (net 119 "Net-(J6-Pin_35)")
  (net 120 "Net-(J6-Pin_34)")
  (net 121 "Net-(J6-Pin_10)")
  (net 122 "unconnected-(J6-Pin_32-Pad32)")
  (net 123 "unconnected-(J6-Pin_31-Pad31)")
  (net 124 "unconnected-(J6-Pin_30-Pad30)")
  (net 125 "unconnected-(J6-Pin_29-Pad29)")
  (net 126 "unconnected-(J6-Pin_28-Pad28)")
  (net 127 "unconnected-(J6-Pin_27-Pad27)")
  (net 128 "unconnected-(J6-Pin_26-Pad26)")
  (net 129 "unconnected-(J6-Pin_25-Pad25)")
  (net 130 "unconnected-(J6-Pin_24-Pad24)")
  (net 131 "unconnected-(J6-Pin_23-Pad23)")
  (net 132 "unconnected-(J6-Pin_22-Pad22)")
  (net 133 "unconnected-(J6-Pin_21-Pad21)")
  (net 134 "unconnected-(J6-Pin_20-Pad20)")
  (net 135 "unconnected-(J6-Pin_19-Pad19)")
  (net 136 "unconnected-(J6-Pin_18-Pad18)")
  (net 137 "unconnected-(J6-Pin_17-Pad17)")
  (net 138 "unconnected-(J6-Pin_16-Pad16)")
  (net 139 "unconnected-(J6-Pin_15-Pad15)")
  (net 140 "unconnected-(J6-Pin_14-Pad14)")
  (net 141 "unconnected-(J6-Pin_13-Pad13)")
  (net 142 "unconnected-(J6-Pin_12-Pad12)")
  (net 143 "Net-(J6-Pin_11)")
  (net 144 "unconnected-(J6-Pin_9-Pad9)")
  (net 145 "Net-(J6-Pin_8)")
  (net 146 "Net-(J6-Pin_7)")
  (net 147 "Net-(J6-Pin_6)")
  (net 148 "Net-(J6-Pin_5)")
  (net 149 "Net-(J7-Pin_3)")
  (net 150 "Net-(J7-Pin_4)")
  (footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P2.50mm" (layer "F.Cu")
    (at 193.04 78.74 -90)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 5mm width 2.5mm Capacitor")
    (property "Sheetfile" "Teensy-MIDI-RA8875-PolySynth.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C6" (at -4.826 0.254 -180) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 1.25 2.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GNDREF") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P2.50mm" (layer "F.Cu")
    (at 55.88 96.52 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 5mm width 2.5mm Capacitor")
    (property "Sheetfile" "Teensy-MIDI-RA8875-PolySynth.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C7" (at 4.064 -2.794 180) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 1.25 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GNDREF") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal" (layer "F.Cu")
    (at 63.754 92.71 90)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (property "Sheetfile" "Teensy-MIDI-RA8875-PolySynth.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D1" (at -2.54 0) (layer "F.SilkS"))
    (fp_text value "1N4148" (at 3.81 2.12 90) (layer "F.Fab"))
    (fp_text user "K" (at 0 -2.286 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 4.11 0 90) (layer "F.Fab"))
    (fp_text user "K" (at 0 2.032 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(D1-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(D1-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical" (layer "F.Cu")
    (at 39.37 16.256 -90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "Teensy-MIDI-RA8875-PolySynth.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J3" (at 0 -2.33 90) (layer "F.SilkS"))
    (fp_text value "LINE_OUT" (at 0 7.41 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 16 "Net-(J3-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 113 "Net-(J3-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 114 "Net-(J3-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical" (layer "F.Cu")
    (at 39.37 10.16 -90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "Teensy-MIDI-RA8875-PolySynth.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J4" (at 0 -2.33 90) (layer "F.SilkS"))
    (fp_text value "LINE_OUT_SCOPE" (at 0 7.41 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 16 "Net-(J3-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 113 "Net-(J3-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 114 "Net-(J3-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical" (layer "F.Cu")
    (at 189.484 59.69 180)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (property "Sheetfile" "Teensy-MIDI-RA8875-PolySynth.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x05, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J5" (at 0 -2.33) (layer "F.SilkS"))
    (fp_text value "USB_HOST" (at 0 12.49) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.08 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 115 "Net-(J5-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 116 "Net-(J5-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 117 "Net-(J5-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GNDREF") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GNDREF") (pinfunction "Pin_5") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-92_Inline" (layer "F.Cu")
    (at 141.112 76.2 90)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (property "Sheetfile" "Teensy-MIDI-RA8875-PolySynth.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "0.2A Ic, 40V Vce, Small Signal NPN Transistor, TO-92")
    (property "ki_keywords" "NPN Transistor")
    (attr through_hole)
    (fp_text reference "Q1" (at 7.62 0) (layer "F.SilkS"))
    (fp_text value "2N3904" (at 1.27 2.79 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 2 "GNDREF") (pinfunction "E") (pintype "passive"))
    (pad "2" thru_hole oval (at 1.27 0 90) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(Q1-B)") (pinfunction "B") (pintype "passive"))
    (pad "3" thru_hole oval (at 2.54 0 90) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(Q1-C)") (pinfunction "C") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-92_Inline" (layer "F.Cu")
    (at 149.748 76.2 90)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (property "Sheetfile" "Teensy-MIDI-RA8875-PolySynth.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "-0.2A Ic, -40V Vce, Small Signal PNP Transistor, TO-92")
    (property "ki_keywords" "PNP Transistor")
    (attr through_hole)
    (fp_text reference "Q2" (at 7.692435 0) (layer "F.SilkS"))
    (fp_text value "2N3906" (at 1.27 2.79 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 6 "+3V3") (pinfunction "E") (pintype "passive"))
    (pad "2" thru_hole oval (at 1.27 0 90) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(Q2-B)") (pinfunction "B") (pintype "input"))
    (pad "3" thru_hole oval (at 2.54 0 90) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(Q2-C)") (pinfunction "C") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal" (layer "F.Cu")
    (at 186.69 24.13)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "Teensy-MIDI-RA8875-PolySynth.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R2" (at 7.62 -0.508) (layer "F.SilkS"))
    (fp_text value "100" (at 2.54 1.92) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 110 "Net-(U2-26_A12_MOSI1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 5.08 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 146 "Net-(J6-Pin_7)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal" (layer "F.Cu")
    (at 71.12 92.964 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "Teensy-MIDI-RA8875-PolySynth.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R4" (at 7.112 0) (layer "F.SilkS"))
    (fp_text value "2K2" (at 2.54 1.626 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 6 "+3V3") (pintype "passive"))
    (pad "2" thru_hole oval (at 5.08 0 90) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 120 "Net-(J6-Pin_34)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal" (layer "F.Cu")
    (at 144.922 89.154)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "Teensy-MIDI-RA8875-PolySynth.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R5" (at -3.19 -1.016) (layer "F.SilkS"))
    (fp_text value "1M" (at 2.54 1.92) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 13 "Net-(U1-LBO)") (pintype "passive"))
    (pad "2" thru_hole oval (at 5.08 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal" (layer "F.Cu")
    (at 40.64 93.98)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "Teensy-MIDI-RA8875-PolySynth.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R6" (at -3.302 -1.016) (layer "F.SilkS"))
    (fp_text value "220" (at 2.54 1.92) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(D1-K)") (pintype "passive"))
    (pad "2" thru_hole oval (at 5.08 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(U5-C1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal" (layer "F.Cu")
    (at 150.114 85.09 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "Teensy-MIDI-RA8875-PolySynth.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R7" (at 8.128 1.016) (layer "F.SilkS"))
    (fp_text value "470K" (at 2.54 1.92) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 13 "Net-(U1-LBO)") (pintype "passive"))
    (pad "2" thru_hole oval (at 5.08 0 180) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(Q1-B)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal" (layer "F.Cu")
    (at 45.72 90.17 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "Teensy-MIDI-RA8875-PolySynth.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R8" (at 8.382 1.016) (layer "F.SilkS"))
    (fp_text value "22K" (at 2.54 1.92) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(Q1-C)") (pintype "passive"))
    (pad "2" thru_hole oval (at 5.08 0 180) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 6 "+3V3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal" (layer "F.Cu")
    (at 144.78 92.71)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "Teensy-MIDI-RA8875-PolySynth.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R9" (at -2.794 -0.762) (layer "F.SilkS"))
    (fp_text value "470" (at 2.54 1.92) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 6 "+3V3") (pintype "passive"))
    (pad "2" thru_hole oval (at 5.08 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 14 "Net-(U2-0_RX1_CRX2_CS1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal" (layer "F.Cu")
    (at 81.28 92.964 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "Teensy-MIDI-RA8875-PolySynth.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R10" (at 7.112 0 180) (layer "F.SilkS"))
    (fp_text value "2K2" (at 2.794 1.124 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(Q1-C)") (pintype "passive"))
    (pad "2" thru_hole oval (at 5.08 0 90) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(Q2-B)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MJC:PowerBoost1000C" (layer "F.Cu")
    (at 149.86 33.02 180)
    (property "Sheetfile" "Teensy-MIDI-RA8875-PolySynth.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U1" (at 0 -19.05) (layer "F.SilkS"))
    (fp_text value "Powerboost1000C" (at 0 19.05) (layer "F.Fab"))
    (fp_text user "PowerBoost 1000C" (at -0.08 0) (layer "F.SilkS"))
    (pad "1" thru_hole rect (at -10.16 -5.08 180) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 112 "Net-(J1-Pin_1)") (pinfunction "USB") (pintype "power_in"))
    (pad "2" thru_hole circle (at -10.16 -2.54 180) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 111 "unconnected-(U1-BAT-Pad2)") (pinfunction "BAT") (pintype "power_in+no_connect"))
    (pad "3" thru_hole circle (at -10.16 0 180) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 15 "unconnected-(U1-Vsh-Pad3)") (pinfunction "Vsh") (pintype "passive+no_connect"))
    (pad "4" thru_hole circle (at -10.16 2.54 180) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(J2-Pin_1)") (pinfunction "EN") (pintype "input"))
    (pad "5" thru_hole circle (at -10.16 5.08 180) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 2 "GNDREF") (pinfunction "GND") (pintype "passive"))
    (pad "5V" thru_hole circle (at -3.81 12.7 180) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 17 "unconnected-(U1-USB-5V-Pad5V)") (pinfunction "USB-5V") (pintype "passive+no_connect"))
    (pad "6" thru_hole circle (at -10.16 7.62 180) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 13 "Net-(U1-LBO)") (pinfunction "LBO") (pintype "output"))
    (pad "7" thru_hole circle (at -10.16 10.16 180) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 2 "GNDREF") (pinfunction "G") (pintype "passive"))
    (pad "8" thru_hole circle (at -10.16 12.7 180) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pinfunction "5Vo") (pintype "power_out"))
    (pad "D+" thru_hole circle (at 1.27 12.7 180) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 18 "unconnected-(U1-USB-D+-PadD+)") (pinfunction "USB-D+") (pintype "passive+no_connect"))
    (pad "D-" thru_hole circle (at -1.27 12.7 180) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 19 "unconnected-(U1-USB-D--PadD-)") (pinfunction "USB-D-") (pintype "passive+no_connect"))
    (pad "UG" thru_hole circle (at 3.81 12.7 180) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 20 "unconnected-(U1-USB-GND-PadUG)") (pinfunction "USB-GND") (pintype "passive+no_connect"))
    (model "${KICAD_USER_DIR}/teensy.pretty/Teensy_4.0_Assembly.STEP"
      (offset (xyz 33 9.5 -11))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "teensy:Teensy41" (layer "F.Cu")
    (at 175.26 36.83 90)
    (property "Sheetfile" "Teensy-MIDI-RA8875-PolySynth.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U2" (at 0 -10.16 90) (layer "F.SilkS"))
    (fp_text value "Teensy4.1" (at 0 10.16 90) (layer "F.Fab"))
    (fp_text user "DVJ6A" (at -2.54 -0.18 180) (layer "F.SilkS"))
    (fp_text user "USB" (at -26.67 0 180) (layer "F.SilkS"))
    (fp_text user "USB Host" (at -18.4658 2.4892 90) (layer "F.SilkS"))
    (fp_text user "Micro SD" (at 24.13 0 90) (layer "F.SilkS"))
    (fp_text user "MIMXRT1062" (at -1.27 0 180) (layer "F.SilkS"))
    (fp_text user "Ethernet" (at -12.065 -3.2766) (layer "F.SilkS"))
    (pad "1" thru_hole rect (at -29.21 7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 2 "GNDREF") (pinfunction "GND") (pintype "power_in"))
    (pad "2" thru_hole circle (at -26.67 7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 14 "Net-(U2-0_RX1_CRX2_CS1)") (pinfunction "0_RX1_CRX2_CS1") (pintype "bidirectional"))
    (pad "3" thru_hole circle (at -24.13 7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(U2-1_TX1_CTX2_MISO1)") (pinfunction "1_TX1_CTX2_MISO1") (pintype "bidirectional"))
    (pad "4" thru_hole circle (at -21.59 7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 121 "Net-(J6-Pin_10)") (pinfunction "2_OUT2") (pintype "bidirectional"))
    (pad "5" thru_hole circle (at -19.05 7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 143 "Net-(J6-Pin_11)") (pinfunction "3_LRCLK2") (pintype "bidirectional"))
    (pad "6" thru_hole circle (at -16.51 7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(Q2-C)") (pinfunction "4_BCLK2") (pintype "bidirectional"))
    (pad "7" thru_hole circle (at -13.97 7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 21 "unconnected-(U2-5_IN2-Pad7)") (pinfunction "5_IN2") (pintype "bidirectional+no_connect"))
    (pad "8" thru_hole circle (at -11.43 7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 22 "unconnected-(U2-6_OUT1D-Pad8)") (pinfunction "6_OUT1D") (pintype "bidirectional+no_connect"))
    (pad "9" thru_hole circle (at -8.89 7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 23 "unconnected-(U2-7_RX2_OUT1A-Pad9)") (pinfunction "7_RX2_OUT1A") (pintype "bidirectional+no_connect"))
    (pad "10" thru_hole circle (at -6.35 7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 24 "unconnected-(U2-8_TX2_IN1-Pad10)") (pinfunction "8_TX2_IN1") (pintype "bidirectional+no_connect"))
    (pad "11" thru_hole circle (at -3.81 7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 25 "unconnected-(U2-9_OUT1C-Pad11)") (pinfunction "9_OUT1C") (pintype "bidirectional+no_connect"))
    (pad "12" thru_hole circle (at -1.27 7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 26 "unconnected-(U2-10_CS_MQSR-Pad12)") (pinfunction "10_CS_MQSR") (pintype "bidirectional+no_connect"))
    (pad "13" thru_hole circle (at 1.27 7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 27 "unconnected-(U2-11_MOSI_CTX1-Pad13)") (pinfunction "11_MOSI_CTX1") (pintype "bidirectional+no_connect"))
    (pad "14" thru_hole circle (at 3.81 7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 28 "unconnected-(U2-12_MISO_MQSL-Pad14)") (pinfunction "12_MISO_MQSL") (pintype "bidirectional+no_connect"))
    (pad "15" thru_hole circle (at 6.35 7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 29 "unconnected-(U2-3V3-Pad15)") (pinfunction "3V3") (pintype "power_out+no_connect"))
    (pad "16" thru_hole circle (at 8.89 7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 30 "unconnected-(U2-24_A10_TX6_SCL2-Pad16)") (pinfunction "24_A10_TX6_SCL2") (pintype "bidirectional+no_connect"))
    (pad "17" thru_hole circle (at 11.43 7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 31 "unconnected-(U2-25_A11_RX6_SDA2-Pad17)") (pinfunction "25_A11_RX6_SDA2") (pintype "bidirectional+no_connect"))
    (pad "18" thru_hole circle (at 13.97 7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 110 "Net-(U2-26_A12_MOSI1)") (pinfunction "26_A12_MOSI1") (pintype "bidirectional"))
    (pad "19" thru_hole circle (at 16.51 7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 109 "Net-(U2-27_A13_SCK1)") (pinfunction "27_A13_SCK1") (pintype "bidirectional"))
    (pad "20" thru_hole circle (at 19.05 7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 32 "unconnected-(U2-28_RX7-Pad20)") (pinfunction "28_RX7") (pintype "bidirectional+no_connect"))
    (pad "21" thru_hole circle (at 21.59 7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 33 "unconnected-(U2-29_TX7-Pad21)") (pinfunction "29_TX7") (pintype "bidirectional+no_connect"))
    (pad "22" thru_hole circle (at 24.13 7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 34 "unconnected-(U2-30_CRX3-Pad22)") (pinfunction "30_CRX3") (pintype "bidirectional+no_connect"))
    (pad "23" thru_hole circle (at 26.67 7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 35 "unconnected-(U2-31_CTX3-Pad23)") (pinfunction "31_CTX3") (pintype "bidirectional+no_connect"))
    (pad "24" thru_hole circle (at 29.21 7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 36 "unconnected-(U2-32_OUT1B-Pad24)") (pinfunction "32_OUT1B") (pintype "bidirectional+no_connect"))
    (pad "25" thru_hole circle (at 29.21 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 37 "unconnected-(U2-33_MCLK2-Pad25)") (pinfunction "33_MCLK2") (pintype "bidirectional+no_connect"))
    (pad "26" thru_hole circle (at 26.67 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 38 "unconnected-(U2-34_RX8-Pad26)") (pinfunction "34_RX8") (pintype "bidirectional+no_connect"))
    (pad "27" thru_hole circle (at 24.13 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 39 "unconnected-(U2-35_TX8-Pad27)") (pinfunction "35_TX8") (pintype "bidirectional+no_connect"))
    (pad "28" thru_hole circle (at 21.59 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 40 "unconnected-(U2-36_CS-Pad28)") (pinfunction "36_CS") (pintype "bidirectional+no_connect"))
    (pad "29" thru_hole circle (at 19.05 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 41 "unconnected-(U2-37_CS-Pad29)") (pinfunction "37_CS") (pintype "bidirectional+no_connect"))
    (pad "30" thru_hole circle (at 16.51 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 148 "Net-(J6-Pin_5)") (pinfunction "38_CS1_IN1") (pintype "bidirectional"))
    (pad "31" thru_hole circle (at 13.97 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 147 "Net-(J6-Pin_6)") (pinfunction "39_MISO1_OUT1A") (pintype "bidirectional"))
    (pad "32" thru_hole circle (at 11.43 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 42 "unconnected-(U2-40_A16-Pad32)") (pinfunction "40_A16") (pintype "bidirectional+no_connect"))
    (pad "33" thru_hole circle (at 8.89 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 43 "unconnected-(U2-41_A17-Pad33)") (pinfunction "41_A17") (pintype "bidirectional+no_connect"))
    (pad "34" thru_hole circle (at 6.35 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 2 "GNDREF") (pinfunction "GND") (pintype "power_in"))
    (pad "35" thru_hole circle (at 3.81 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 44 "unconnected-(U2-13_SCK_LED-Pad35)") (pinfunction "13_SCK_LED") (pintype "bidirectional+no_connect"))
    (pad "36" thru_hole circle (at 1.27 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 45 "unconnected-(U2-14_A0_TX3_SPDIF_OUT-Pad36)") (pinfunction "14_A0_TX3_SPDIF_OUT") (pintype "bidirectional+no_connect"))
    (pad "37" thru_hole circle (at -1.27 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 46 "unconnected-(U2-15_A1_RX3_SPDIF_IN-Pad37)") (pinfunction "15_A1_RX3_SPDIF_IN") (pintype "bidirectional+no_connect"))
    (pad "38" thru_hole circle (at -3.81 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 47 "Net-(U2-16_A2_RX4_SCL1)") (pinfunction "16_A2_RX4_SCL1") (pintype "bidirectional"))
    (pad "39" thru_hole circle (at -6.35 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 48 "Net-(U2-17_A3_TX4_SDA1)") (pinfunction "17_A3_TX4_SDA1") (pintype "bidirectional"))
    (pad "40" thru_hole circle (at -8.89 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 120 "Net-(J6-Pin_34)") (pinfunction "18_A4_SDA") (pintype "bidirectional"))
    (pad "41" thru_hole circle (at -11.43 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 119 "Net-(J6-Pin_35)") (pinfunction "19_A5_SCL") (pintype "bidirectional"))
    (pad "42" thru_hole circle (at -13.97 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 49 "unconnected-(U2-20_A6_TX5_LRCLK1-Pad42)") (pinfunction "20_A6_TX5_LRCLK1") (pintype "bidirectional+no_connect"))
    (pad "43" thru_hole circle (at -16.51 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 50 "unconnected-(U2-21_A7_RX5_BCLK1-Pad43)") (pinfunction "21_A7_RX5_BCLK1") (pintype "bidirectional+no_connect"))
    (pad "44" thru_hole circle (at -19.05 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 51 "unconnected-(U2-22_A8_CTX1-Pad44)") (pinfunction "22_A8_CTX1") (pintype "bidirectional+no_connect"))
    (pad "45" thru_hole circle (at -21.59 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 52 "unconnected-(U2-23_A9_CRX1_MCLK1-Pad45)") (pinfunction "23_A9_CRX1_MCLK1") (pintype "bidirectional+no_connect"))
    (pad "46" thru_hole circle (at -24.13 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 6 "+3V3") (pinfunction "3V3") (pintype "power_out"))
    (pad "47" thru_hole circle (at -26.67 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 2 "GNDREF") (pinfunction "GND") (pintype "power_out"))
    (pad "48" thru_hole circle (at -29.21 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pinfunction "VIN") (pintype "power_in"))
    (pad "49" thru_hole circle (at -26.67 -5.08 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 53 "unconnected-(U2-VUSB-Pad49)") (pinfunction "VUSB") (pintype "power_out+no_connect"))
    (pad "50" thru_hole circle (at 16.51 5.08 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 54 "unconnected-(U2-VBAT-Pad50)") (pinfunction "VBAT") (pintype "power_in+no_connect"))
    (pad "51" thru_hole circle (at 16.51 2.54 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 55 "unconnected-(U2-3V3-Pad51)") (pinfunction "3V3") (pintype "power_in+no_connect"))
    (pad "52" thru_hole circle (at 16.51 0 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 56 "unconnected-(U2-GND-Pad52)") (pinfunction "GND") (pintype "input+no_connect"))
    (pad "53" thru_hole circle (at 16.51 -2.54 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 57 "unconnected-(U2-PROGRAM-Pad53)") (pinfunction "PROGRAM") (pintype "input+no_connect"))
    (pad "54" thru_hole circle (at 16.51 -5.08 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 58 "unconnected-(U2-ON_OFF-Pad54)") (pinfunction "ON_OFF") (pintype "input+no_connect"))
    (pad "55" thru_hole rect (at -22.9108 4.5692 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 115 "Net-(J5-Pin_1)") (pinfunction "5V") (pintype "power_out"))
    (pad "56" thru_hole circle (at -20.3708 4.5692 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 116 "Net-(J5-Pin_2)") (pinfunction "D-") (pintype "bidirectional"))
    (pad "57" thru_hole circle (at -17.8308 4.5692 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 117 "Net-(J5-Pin_3)") (pinfunction "D+") (pintype "bidirectional"))
    (pad "58" thru_hole circle (at -15.2908 4.5692 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 2 "GNDREF") (pinfunction "GND") (pintype "power_in"))
    (pad "59" thru_hole circle (at -12.7508 4.5692 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 2 "GNDREF") (pinfunction "GND") (pintype "power_in"))
    (pad "60" thru_hole rect (at -16.24 -5.1816 90) (size 1.3 1.3) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 59 "unconnected-(U2-R+-Pad60)") (pinfunction "R+") (pintype "bidirectional+no_connect"))
    (pad "61" thru_hole circle (at -16.24 -3.1816 90) (size 1.3 1.3) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 60 "unconnected-(U2-LED-Pad61)") (pinfunction "LED") (pintype "bidirectional+no_connect"))
    (pad "62" thru_hole circle (at -16.24 -1.1816 90) (size 1.3 1.3) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 61 "unconnected-(U2-T--Pad62)") (pinfunction "T-") (pintype "bidirectional+no_connect"))
    (pad "63" thru_hole circle (at -14.24 -1.1816 90) (size 1.3 1.3) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 62 "unconnected-(U2-T+-Pad63)") (pinfunction "T+") (pintype "bidirectional+no_connect"))
    (pad "64" thru_hole circle (at -14.24 -3.1816 90) (size 1.3 1.3) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 63 "unconnected-(U2-GND-Pad64)") (pinfunction "GND") (pintype "power_in+no_connect"))
    (pad "65" thru_hole circle (at -14.24 -5.1816 90) (size 1.3 1.3) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 64 "unconnected-(U2-R--Pad65)") (pinfunction "R-") (pintype "bidirectional+no_connect"))
    (pad "66" thru_hole circle (at -28.48 -1.27 90) (size 1.3 1.3) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 65 "unconnected-(U2-D--Pad66)") (pinfunction "D-") (pintype "bidirectional+no_connect"))
    (pad "67" thru_hole circle (at -28.48 1.27 90) (size 1.3 1.3) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 66 "unconnected-(U2-D+-Pad67)") (pinfunction "D+") (pintype "bidirectional+no_connect"))
    (model "${KICAD_USER_DIR}/teensy.pretty/Teensy_4.1_Assembly.STEP"
      (offset (xyz 0 0 0.762))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "teensy:Teensy40" (layer "F.Cu")
    (at 66.04 31.75)
    (property "Sheetfile" "Teensy-MIDI-RA8875-PolySynth.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U3" (at -5.08 -10.668) (layer "F.SilkS"))
    (fp_text value "Teensy4.0" (at 0 10.16) (layer "F.Fab"))
    (fp_text user "DVL6A" (at 1.778 0 90) (layer "F.SilkS"))
    (fp_text user "MIMXRT1062" (at 0.254 0 90) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at -16.51 7.62) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 2 "GNDREF") (pinfunction "GND") (pintype "power_in"))
    (pad "2" thru_hole circle (at -13.97 7.62) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 67 "unconnected-(U3-0_RX1_CRX2_CS1-Pad2)") (pinfunction "0_RX1_CRX2_CS1") (pintype "bidirectional+no_connect"))
    (pad "3" thru_hole circle (at -11.43 7.62) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 68 "unconnected-(U3-1_TX1_CTX2_MISO1-Pad3)") (pinfunction "1_TX1_CTX2_MISO1") (pintype "bidirectional+no_connect"))
    (pad "4" thru_hole circle (at -8.89 7.62) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 69 "unconnected-(U3-2_OUT2-Pad4)") (pinfunction "2_OUT2") (pintype "bidirectional+no_connect"))
    (pad "5" thru_hole circle (at -6.35 7.62) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 70 "unconnected-(U3-3_LRCLK2-Pad5)") (pinfunction "3_LRCLK2") (pintype "bidirectional+no_connect"))
    (pad "6" thru_hole circle (at -3.81 7.62) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 71 "unconnected-(U3-4_BCLK2-Pad6)") (pinfunction "4_BCLK2") (pintype "bidirectional+no_connect"))
    (pad "7" thru_hole circle (at -1.27 7.62) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 72 "unconnected-(U3-5_IN2-Pad7)") (pinfunction "5_IN2") (pintype "bidirectional+no_connect"))
    (pad "8" thru_hole circle (at 1.27 7.62) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 73 "Net-(U3-6_OUT1D)") (pinfunction "6_OUT1D") (pintype "bidirectional"))
    (pad "9" thru_hole circle (at 3.81 7.62) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 74 "Net-(U3-7_RX2_OUT1A)") (pinfunction "7_RX2_OUT1A") (pintype "bidirectional"))
    (pad "10" thru_hole circle (at 6.35 7.62) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 75 "Net-(U3-8_TX2_IN1)") (pinfunction "8_TX2_IN1") (pintype "bidirectional"))
    (pad "11" thru_hole circle (at 8.89 7.62) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 76 "unconnected-(U3-9_OUT1C-Pad11)") (pinfunction "9_OUT1C") (pintype "bidirectional+no_connect"))
    (pad "12" thru_hole circle (at 11.43 7.62) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 77 "Net-(U3-10_CS_MQSR)") (pinfunction "10_CS_MQSR") (pintype "bidirectional"))
    (pad "13" thru_hole circle (at 13.97 7.62) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 78 "Net-(U3-11_MOSI_CTX1)") (pinfunction "11_MOSI_CTX1") (pintype "bidirectional"))
    (pad "14" thru_hole circle (at 16.51 7.62) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 79 "Net-(U3-12_MISO_MQSL)") (pinfunction "12_MISO_MQSL") (pintype "bidirectional"))
    (pad "15" thru_hole circle (at 16.51 5.08) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 80 "unconnected-(U3-VBAT-Pad15)") (pinfunction "VBAT") (pintype "power_in+no_connect"))
    (pad "16" thru_hole circle (at 16.51 2.54) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 81 "unconnected-(U3-3V3-Pad16)") (pinfunction "3V3") (pintype "power_in+no_connect"))
    (pad "17" thru_hole circle (at 16.51 0) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 82 "unconnected-(U3-GND-Pad17)") (pinfunction "GND") (pintype "power_in+no_connect"))
    (pad "18" thru_hole circle (at 16.51 -2.54) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 83 "unconnected-(U3-PROGRAM-Pad18)") (pinfunction "PROGRAM") (pintype "input+no_connect"))
    (pad "19" thru_hole circle (at 16.51 -5.08) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 84 "unconnected-(U3-ON_OFF-Pad19)") (pinfunction "ON_OFF") (pintype "input+no_connect"))
    (pad "20" thru_hole circle (at 16.51 -7.62) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 85 "Net-(U3-13_SCK_CRX1_LED)") (pinfunction "13_SCK_CRX1_LED") (pintype "bidirectional"))
    (pad "21" thru_hole circle (at 13.97 -7.62) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 86 "unconnected-(U3-14_A0_TX3_SPDIF_OUT-Pad21)") (pinfunction "14_A0_TX3_SPDIF_OUT") (pintype "bidirectional+no_connect"))
    (pad "22" thru_hole circle (at 11.43 -7.62) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 87 "Net-(U3-15_A1_RX3_SPDIF_IN)") (pinfunction "15_A1_RX3_SPDIF_IN") (pintype "bidirectional"))
    (pad "23" thru_hole circle (at 8.89 -7.62) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 48 "Net-(U2-17_A3_TX4_SDA1)") (pinfunction "16_A2_RX4_SCL1") (pintype "bidirectional"))
    (pad "24" thru_hole circle (at 6.35 -7.62) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 47 "Net-(U2-16_A2_RX4_SCL1)") (pinfunction "17_A3_TX4_SDA1") (pintype "bidirectional"))
    (pad "25" thru_hole circle (at 3.81 -7.62) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 88 "Net-(U3-18_A4_SDA0)") (pinfunction "18_A4_SDA0") (pintype "bidirectional"))
    (pad "26" thru_hole circle (at 1.27 -7.62) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 89 "Net-(U3-19_A5_SCL0)") (pinfunction "19_A5_SCL0") (pintype "bidirectional"))
    (pad "27" thru_hole circle (at -1.27 -7.62) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 90 "Net-(U3-20_A6_TX5_LRCLK1)") (pinfunction "20_A6_TX5_LRCLK1") (pintype "bidirectional"))
    (pad "28" thru_hole circle (at -3.81 -7.62) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 91 "Net-(U3-21_A7_RX5_BCLK1)") (pinfunction "21_A7_RX5_BCLK1") (pintype "bidirectional"))
    (pad "29" thru_hole circle (at -6.35 -7.62) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 92 "unconnected-(U3-22_A8_CTX1-Pad29)") (pinfunction "22_A8_CTX1") (pintype "bidirectional+no_connect"))
    (pad "30" thru_hole circle (at -8.89 -7.62) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 93 "Net-(U3-23_A9_CRX1_MCLK1)") (pinfunction "23_A9_CRX1_MCLK1") (pintype "bidirectional"))
    (pad "31" thru_hole circle (at -11.43 -7.62) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 94 "Net-(U4-3V3)") (pinfunction "3V3") (pintype "power_out"))
    (pad "32" thru_hole circle (at -13.97 -7.62) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 2 "GNDREF") (pinfunction "GND") (pintype "power_in"))
    (pad "33" thru_hole circle (at -16.51 -7.62) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pinfunction "VIN") (pintype "power_in"))
    (pad "34" thru_hole circle (at -13.97 -5.08) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 95 "unconnected-(U3-VUSB-Pad34)") (pinfunction "VUSB") (pintype "power_out+no_connect"))
    (pad "35" thru_hole circle (at 11.43 -5.08) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 96 "unconnected-(U3-24_A10_TX6_SCL2-Pad35)") (pinfunction "24_A10_TX6_SCL2") (pintype "bidirectional+no_connect"))
    (pad "36" thru_hole circle (at 8.89 -5.08) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 97 "unconnected-(U3-25_A11_RX6_SDA2-Pad36)") (pinfunction "25_A11_RX6_SDA2") (pintype "bidirectional+no_connect"))
    (pad "37" thru_hole circle (at 11.43 -2.54) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 98 "unconnected-(U3-26_A12_MOSI1-Pad37)") (pinfunction "26_A12_MOSI1") (pintype "bidirectional+no_connect"))
    (pad "38" thru_hole circle (at 8.89 -2.54) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 99 "unconnected-(U3-27_A13_SCK1-Pad38)") (pinfunction "27_A13_SCK1") (pintype "bidirectional+no_connect"))
    (pad "39" thru_hole circle (at 11.43 0) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 100 "unconnected-(U3-28_RX7-Pad39)") (pinfunction "28_RX7") (pintype "bidirectional+no_connect"))
    (pad "40" thru_hole circle (at 8.89 0) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 101 "unconnected-(U3-29_TX7-Pad40)") (pinfunction "29_TX7") (pintype "bidirectional+no_connect"))
    (pad "41" thru_hole circle (at 11.43 2.54) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 102 "unconnected-(U3-30_CRX3-Pad41)") (pinfunction "30_CRX3") (pintype "bidirectional+no_connect"))
    (pad "42" thru_hole circle (at 8.89 2.54) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 103 "unconnected-(U3-31_CTX3-Pad42)") (pinfunction "31_CTX3") (pintype "bidirectional+no_connect"))
    (pad "43" thru_hole circle (at 11.43 5.08) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 104 "unconnected-(U3-32_OUT1B-Pad43)") (pinfunction "32_OUT1B") (pintype "bidirectional+no_connect"))
    (pad "44" thru_hole circle (at 8.89 5.08) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 105 "unconnected-(U3-33_MCLK2-Pad44)") (pinfunction "33_MCLK2") (pintype "bidirectional+no_connect"))
    (model "${KICAD_USER_DIR}/teensy.pretty/Teensy_4.0_Assembly.STEP"
      (offset (xyz 33 9.5 -11))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "MJC:AudioAdapterRevD" (layer "F.Cu")
    (at 66.04 59.69)
    (property "Sheetfile" "Teensy-MIDI-RA8875-PolySynth.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U4" (at 0 22.86) (layer "F.SilkS"))
    (fp_text value "AudioAdapterRevD" (at 0 21.59) (layer "F.Fab"))
    (fp_text user "R" (at -2.62 -9.5) (layer "F.SilkS"))
    (fp_text user "R" (at -0.08 -9.5) (layer "F.SilkS"))
    (fp_text user "LINE IN" (at -10.16 -12.7) (layer "F.SilkS"))
    (fp_text user "Audio Adapter Rev D" (at -0.08 -0.61) (layer "F.SilkS"))
    (fp_text user "G" (at -5.16 -15.5) (layer "F.SilkS"))
    (fp_text user "MIC" (at -14 -2.54) (layer "F.SilkS"))
    (fp_text user "G" (at -2.62 -15.5) (layer "F.SilkS"))
    (fp_text user "G" (at 2.46 -9.5) (layer "F.SilkS"))
    (fp_text user "L" (at 5 -9.5) (layer "F.SilkS"))
    (fp_text user "GND" (at -14 0) (layer "F.SilkS"))
    (fp_text user "L" (at -5.16 -9.5) (layer "F.SilkS"))
    (fp_text user "LINE OUT" (at 10.16 -12.7) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at -16.51 7.62) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 2 "GNDREF") (pinfunction "GND") (pintype "power_in"))
    (pad "2" thru_hole circle (at -13.97 7.62) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask"))
    (pad "3" thru_hole circle (at -11.43 7.62) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask"))
    (pad "4" thru_hole circle (at -8.89 7.62) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask"))
    (pad "5" thru_hole circle (at -6.35 7.62) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask"))
    (pad "6" thru_hole circle (at -3.81 7.62) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask"))
    (pad "7" thru_hole circle (at -1.27 7.62) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask"))
    (pad "8" thru_hole circle (at 1.27 7.62) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 73 "Net-(U3-6_OUT1D)") (pinfunction "6_MEMCS") (pintype "bidirectional"))
    (pad "9" thru_hole circle (at 3.81 7.62) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 74 "Net-(U3-7_RX2_OUT1A)") (pinfunction "7_DIN") (pintype "bidirectional"))
    (pad "10" thru_hole circle (at 6.35 7.62) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 75 "Net-(U3-8_TX2_IN1)") (pinfunction "8_DOUT") (pintype "bidirectional"))
    (pad "11" thru_hole circle (at 8.89 7.62) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask"))
    (pad "12" thru_hole circle (at 11.43 7.62) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 77 "Net-(U3-10_CS_MQSR)") (pinfunction "10_SDCS") (pintype "bidirectional"))
    (pad "13" thru_hole circle (at 13.97 7.62) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 78 "Net-(U3-11_MOSI_CTX1)") (pinfunction "11_MOSI") (pintype "bidirectional"))
    (pad "14" thru_hole circle (at 16.51 7.62) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 79 "Net-(U3-12_MISO_MQSL)") (pinfunction "12_MISO") (pintype "bidirectional"))
    (pad "15" thru_hole circle (at 16.51 -7.62) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 85 "Net-(U3-13_SCK_CRX1_LED)") (pinfunction "13_SCK") (pintype "bidirectional"))
    (pad "16" thru_hole circle (at 13.97 -7.62) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask"))
    (pad "17" thru_hole circle (at 11.43 -7.62) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 87 "Net-(U3-15_A1_RX3_SPDIF_IN)") (pinfunction "15_A1_VOL") (pintype "bidirectional"))
    (pad "18" thru_hole circle (at 8.89 -7.62) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask"))
    (pad "19" thru_hole circle (at 6.35 -7.62) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask"))
    (pad "20" thru_hole circle (at 3.81 -7.62) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 88 "Net-(U3-18_A4_SDA0)") (pinfunction "18_SDA") (pintype "bidirectional"))
    (pad "21" thru_hole circle (at 1.27 -7.62) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 89 "Net-(U3-19_A5_SCL0)") (pinfunction "19_SCL") (pintype "bidirectional"))
    (pad "22" thru_hole circle (at -1.27 -7.62) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 90 "Net-(U3-20_A6_TX5_LRCLK1)") (pinfunction "20_LRCLK") (pintype "bidirectional"))
    (pad "23" thru_hole circle (at -3.81 -7.62) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 91 "Net-(U3-21_A7_RX5_BCLK1)") (pinfunction "21_BCLK") (pintype "bidirectional"))
    (pad "24" thru_hole circle (at -6.35 -7.62) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask"))
    (pad "25" thru_hole circle (at -8.89 -7.62) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 93 "Net-(U3-23_A9_CRX1_MCLK1)") (pinfunction "23_MCLK") (pintype "bidirectional"))
    (pad "26" thru_hole circle (at -11.43 -7.62) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 94 "Net-(U4-3V3)") (pinfunction "3V3") (pintype "power_in"))
    (pad "27" thru_hole circle (at -13.97 -7.62) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 2 "GNDREF") (pinfunction "GND") (pintype "power_in"))
    (pad "28" thru_hole circle (at -16.51 -7.62) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask"))
    (pad "LI-L" thru_hole circle (at -5.08 -11.43) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask"))
    (pad "LI-L-G" thru_hole circle (at -5.08 -13.97) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask"))
    (pad "LI-R" thru_hole circle (at -2.54 -11.43) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask"))
    (pad "LI-R-G" thru_hole circle (at -2.54 -13.97) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask"))
    (pad "LO-G" thru_hole circle (at 2.54 -11.43) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 113 "Net-(J3-Pin_2)") (pinfunction "LINE-OUT-GND") (pintype "output"))
    (pad "LO-L1" thru_hole circle (at 5.08 -11.43) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 16 "Net-(J3-Pin_1)") (pinfunction "LINE-OUT-L1") (pintype "output"))
    (pad "LO-L2" thru_hole circle (at 5.08 -13.97) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask"))
    (pad "LO-R1" thru_hole circle (at 0 -11.43) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 114 "Net-(J3-Pin_3)") (pinfunction "LINE-OUT-R1") (pintype "output"))
    (pad "LO-R2" thru_hole circle (at 0 -13.97) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask"))
    (pad "MIC" thru_hole circle (at -16.51 -2.54) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask"))
    (pad "MIC-G" thru_hole circle (at -16.51 0) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask"))
    (model "${KICAD_USER_DIR}/teensy.pretty/Teensy_4.0_Assembly.STEP"
      (offset (xyz 33 9.5 -11))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Package_DIP:DIP-8_W7.62mm_LongPads" (layer "F.Cu")
    (at 58.42 82.804 -90)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads")
    (property "Sheetfile" "Teensy-MIDI-RA8875-PolySynth.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Low Input Current high Gain Split Darlington Optocouplers, -0.5V to 7V VDD, DIP-8")
    (property "ki_keywords" "darlington optocoupler")
    (attr through_hole)
    (fp_text reference "U5" (at 10.16 7.62 180) (layer "F.SilkS"))
    (fp_text value "6N138" (at 3.81 9.95 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 3.81 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 106 "unconnected-(U5-NC-Pad1)") (pinfunction "NC") (pintype "no_connect"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(U5-C1)") (pinfunction "C1") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(D1-A)") (pinfunction "C2") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 107 "unconnected-(U5-NC-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" thru_hole oval (at 7.62 7.62 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GNDREF") (pinfunction "GND") (pintype "passive"))
    (pad "6" thru_hole oval (at 7.62 5.08 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 14 "Net-(U2-0_RX1_CRX2_CS1)") (pinfunction "VO2") (pintype "passive"))
    (pad "7" thru_hole oval (at 7.62 2.54 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 108 "unconnected-(U5-VO1-Pad7)") (pinfunction "VO1") (pintype "passive+no_connect"))
    (pad "8" thru_hole oval (at 7.62 0 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pinfunction "VCC") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-8_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D10.0mm_P5.00mm_P7.50mm" (layer "F.Cu")
    (at 55.88 15.24 180)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm 7.50mm, , diameter=10mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm 7.50mm  diameter 10mm Electrolytic Capacitor")
    (property "Sheetfile" "Teensy-MIDI-RA8875-PolySynth.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C3" (at 5.842 -6.35) (layer "F.SilkS"))
    (fp_text value "10uF" (at 2.5 6.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at -0.672144 -2 180) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pintype "passive"))
    (pad "1" thru_hole rect (at 0 0 180) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 180) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GNDREF") (pintype "passive"))
    (pad "2" thru_hole circle (at 5.672144 2 180) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GNDREF") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D10.0mm_P5.00mm_P7.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D10.0mm_P5.00mm_P7.50mm" (layer "F.Cu")
    (at 187.484 89.7461 90)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm 7.50mm, , diameter=10mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm 7.50mm  diameter 10mm Electrolytic Capacitor")
    (property "Sheetfile" "Teensy-MIDI-RA8875-PolySynth.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C5" (at 3.894144 8.858 180) (layer "F.SilkS"))
    (fp_text value "10uF" (at 2.5 6.25 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at -0.672144 -2 90) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pintype "passive"))
    (pad "1" thru_hole rect (at 0 0 90) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 90) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GNDREF") (pintype "passive"))
    (pad "2" thru_hole circle (at 5.672144 2 90) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GNDREF") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D10.0mm_P5.00mm_P7.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal" (layer "F.Cu")
    (at 186.69 20.32)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "Teensy-MIDI-RA8875-PolySynth.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R1" (at 7.62 -0.508) (layer "F.SilkS"))
    (fp_text value "100" (at 2.54 1.92) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 109 "Net-(U2-27_A13_SCK1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 5.08 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 145 "Net-(J6-Pin_8)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P2.50mm" (layer "F.Cu")
    (at 161.564 71.882)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 5mm width 2.5mm Capacitor")
    (property "Sheetfile" "Teensy-MIDI-RA8875-PolySynth.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C2" (at -2.052 -2.794) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 1.25 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.428 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GNDREF") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D10.0mm_P5.00mm_P7.50mm" (layer "F.Cu")
    (at 158.75 64.77 90)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm 7.50mm, , diameter=10mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm 7.50mm  diameter 10mm Electrolytic Capacitor")
    (property "Sheetfile" "Teensy-MIDI-RA8875-PolySynth.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C1" (at 9.144 -2.875 180) (layer "F.SilkS"))
    (fp_text value "10uF" (at 2.5 6.25 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at -0.672144 -2 90) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pintype "passive"))
    (pad "1" thru_hole rect (at 0 0 90) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 90) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GNDREF") (pintype "passive"))
    (pad "2" thru_hole circle (at 5.672144 2 90) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GNDREF") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D10.0mm_P5.00mm_P7.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal" (layer "F.Cu")
    (at 76.454 92.964 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "Teensy-MIDI-RA8875-PolySynth.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R3" (at 7.112 0 180) (layer "F.SilkS"))
    (fp_text value "2K2" (at 2.54 1.524 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 6 "+3V3") (pintype "passive"))
    (pad "2" thru_hole oval (at 5.08 0 90) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 119 "Net-(J6-Pin_35)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (at 147.574 10.16 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "Teensy-MIDI-RA8875-PolySynth.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J2" (at 2.54 -5.08) (layer "F.SilkS"))
    (fp_text value "DISABLE_SWITCH" (at 2.794 2.286) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.27) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(J2-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GNDREF") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.5mm" (layer "F.Cu")
    (at 161.09 97.59)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (property "Sheetfile" "Teensy-MIDI-RA8875-PolySynth.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H5" (at 0 -3.5) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 3.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers "*.Cu" "*.Mask"))
  )
  (footprint "MountingHole:MountingHole_2.5mm" (layer "F.Cu")
    (at 167.64 104.14)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (property "Sheetfile" "Teensy-MIDI-RA8875-PolySynth.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H8" (at 0 -3.5) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 3.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers "*.Cu" "*.Mask"))
  )
  (footprint "MountingHole:MountingHole_2.5mm" (layer "F.Cu")
    (at 33.328 35.306)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (property "Sheetfile" "Teensy-MIDI-RA8875-PolySynth.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H2" (at 0 -3.5) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 3.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (at 162.814 54.356)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (property "Sheetfile" "Teensy-MIDI-RA8875-PolySynth.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J1" (at -4.318 -0.762) (layer "F.SilkS"))
    (fp_text value "VUSB" (at 0 2.33) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 112 "Net-(J1-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.5mm" (layer "F.Cu")
    (at 33.328 28.756)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (property "Sheetfile" "Teensy-MIDI-RA8875-PolySynth.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H1" (at 0 -3.5) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 3.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers "*.Cu" "*.Mask"))
  )
  (footprint "MountingHole:MountingHole_2.5mm" (layer "F.Cu")
    (at 39.878 28.756)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (property "Sheetfile" "Teensy-MIDI-RA8875-PolySynth.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H3" (at 0 -3.5) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 3.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal" (layer "F.Cu")
    (at 40.64 85.852)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "Teensy-MIDI-RA8875-PolySynth.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R12" (at -3.302 -1.016) (layer "F.SilkS"))
    (fp_text value "47" (at 2.54 1.92) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 6 "+3V3") (pintype "passive"))
    (pad "2" thru_hole oval (at 5.08 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 149 "Net-(J7-Pin_3)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.5mm" (layer "F.Cu")
    (at 167.64 97.59)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (property "Sheetfile" "Teensy-MIDI-RA8875-PolySynth.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H7" (at 0 -3.5) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 3.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers "*.Cu" "*.Mask"))
  )
  (footprint "MountingHole:MountingHole_2.5mm" (layer "F.Cu")
    (at 39.878 35.306)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (property "Sheetfile" "Teensy-MIDI-RA8875-PolySynth.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H4" (at 0 -3.5) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 3.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers "*.Cu" "*.Mask"))
  )
  (footprint "MountingHole:MountingHole_2.5mm" (layer "F.Cu")
    (at 161.09 104.14)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (property "Sheetfile" "Teensy-MIDI-RA8875-PolySynth.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H6" (at 0 -3.5) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 3.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P2.50mm" (layer "F.Cu")
    (at 63.5 16.116 90)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 5mm width 2.5mm Capacitor")
    (property "Sheetfile" "Teensy-MIDI-RA8875-PolySynth.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C4" (at 2.146 4.064 180) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 1.25 2.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GNDREF") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x09_P2.54mm_Vertical" (layer "F.Cu")
    (at 40.64 49.53)
    (descr "Through hole straight pin header, 1x09, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x09 2.54mm single row")
    (property "Sheetfile" "Teensy-MIDI-RA8875-PolySynth.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x09, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J7" (at -0.086 -3.334 180) (layer "F.SilkS") hide)
    (fp_text value "MIDI EXT" (at 0 22.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 10.16 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(D1-K)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(D1-A)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 149 "Net-(J7-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 150 "Net-(J7-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GNDREF") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 150 "Net-(J7-Pin_4)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 149 "Net-(J7-Pin_3)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(D1-A)") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(D1-K)") (pinfunction "Pin_9") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x09_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal" (layer "F.Cu")
    (at 150.114 61.214 -90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "Teensy-MIDI-RA8875-PolySynth.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R11" (at -4.064 0) (layer "F.SilkS"))
    (fp_text value "2K2" (at 2.54 -1.524 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 2 "GNDREF") (pintype "passive"))
    (pad "2" thru_hole oval (at 5.08 0 270) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(Q2-C)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal" (layer "F.Cu")
    (at 145.034 81.28)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "Teensy-MIDI-RA8875-PolySynth.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R13" (at -3.302 -0.762) (layer "F.SilkS"))
    (fp_text value "47" (at 2.398 1.92) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 150 "Net-(J7-Pin_4)") (pintype "passive"))
    (pad "2" thru_hole oval (at 5.08 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(U2-1_TX1_CTX2_MISO1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MJC:RA8875" (layer "B.Cu")
    (at 110.864 56.166)
    (descr "Through hole straight pin header, 2x20, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x20 2.54mm double row")
    (property "Sheetfile" "Teensy-MIDI-RA8875-PolySynth.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, double row, 02x20, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J6" (at 88.27 27.568) (layer "B.SilkS"))
    (fp_text value "RA8875" (at 93.35 -0.162 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 88.27 1.108 90) (layer "F.Fab"))
    (pad "" thru_hole circle (at -86 50.238) (size 5 5) (drill 3.2) (layers "*.Cu" "*.Mask"))
    (pad "" thru_hole circle (at -85.9 -47.662) (size 5 5) (drill 3.2) (layers "*.Cu" "*.Mask"))
    (pad "" thru_hole circle (at 88 50.238) (size 5 5) (drill 3.2) (layers "*.Cu" "*.Mask"))
    (pad "" thru_hole circle (at 88.1 -47.662) (size 5 5) (drill 3.2) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole rect (at 89.54 25.238) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GNDREF") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 87 25.238) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GNDREF") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 89.54 22.698) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 87 22.698) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 89.54 20.158) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 148 "Net-(J6-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 87 20.158) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 147 "Net-(J6-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 89.54 17.618) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 146 "Net-(J6-Pin_7)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 87 17.618) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 145 "Net-(J6-Pin_8)") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval (at 89.54 15.078) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 144 "unconnected-(J6-Pin_9-Pad9)") (pinfunction "Pin_9") (pintype "passive+no_connect"))
    (pad "10" thru_hole oval (at 87 15.078) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 121 "Net-(J6-Pin_10)") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole oval (at 89.54 12.538) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 143 "Net-(J6-Pin_11)") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole oval (at 87 12.538) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 142 "unconnected-(J6-Pin_12-Pad12)") (pinfunction "Pin_12") (pintype "passive+no_connect"))
    (pad "13" thru_hole oval (at 89.54 9.998) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 141 "unconnected-(J6-Pin_13-Pad13)") (pinfunction "Pin_13") (pintype "passive+no_connect"))
    (pad "14" thru_hole oval (at 87 9.998) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 140 "unconnected-(J6-Pin_14-Pad14)") (pinfunction "Pin_14") (pintype "passive+no_connect"))
    (pad "15" thru_hole oval (at 89.54 7.458) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 139 "unconnected-(J6-Pin_15-Pad15)") (pinfunction "Pin_15") (pintype "passive+no_connect"))
    (pad "16" thru_hole oval (at 87 7.458) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 138 "unconnected-(J6-Pin_16-Pad16)") (pinfunction "Pin_16") (pintype "passive+no_connect"))
    (pad "17" thru_hole oval (at 89.54 4.918) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 137 "unconnected-(J6-Pin_17-Pad17)") (pinfunction "Pin_17") (pintype "passive+no_connect"))
    (pad "18" thru_hole oval (at 87 4.918) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 136 "unconnected-(J6-Pin_18-Pad18)") (pinfunction "Pin_18") (pintype "passive+no_connect"))
    (pad "19" thru_hole oval (at 89.54 2.378) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 135 "unconnected-(J6-Pin_19-Pad19)") (pinfunction "Pin_19") (pintype "passive+no_connect"))
    (pad "20" thru_hole oval (at 87 2.378) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 134 "unconnected-(J6-Pin_20-Pad20)") (pinfunction "Pin_20") (pintype "passive+no_connect"))
    (pad "21" thru_hole oval (at 89.54 -0.162) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 133 "unconnected-(J6-Pin_21-Pad21)") (pinfunction "Pin_21") (pintype "passive+no_connect"))
    (pad "22" thru_hole oval (at 87 -0.162) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 132 "unconnected-(J6-Pin_22-Pad22)") (pinfunction "Pin_22") (pintype "passive+no_connect"))
    (pad "23" thru_hole oval (at 89.54 -2.702) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 131 "unconnected-(J6-Pin_23-Pad23)") (pinfunction "Pin_23") (pintype "passive+no_connect"))
    (pad "24" thru_hole oval (at 87 -2.702) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 130 "unconnected-(J6-Pin_24-Pad24)") (pinfunction "Pin_24") (pintype "passive+no_connect"))
    (pad "25" thru_hole oval (at 89.54 -5.242) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 129 "unconnected-(J6-Pin_25-Pad25)") (pinfunction "Pin_25") (pintype "passive+no_connect"))
    (pad "26" thru_hole oval (at 87 -5.242) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 128 "unconnected-(J6-Pin_26-Pad26)") (pinfunction "Pin_26") (pintype "passive+no_connect"))
    (pad "27" thru_hole oval (at 89.54 -7.782) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 127 "unconnected-(J6-Pin_27-Pad27)") (pinfunction "Pin_27") (pintype "passive+no_connect"))
    (pad "28" thru_hole oval (at 87 -7.782) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 126 "unconnected-(J6-Pin_28-Pad28)") (pinfunction "Pin_28") (pintype "passive+no_connect"))
    (pad "29" thru_hole oval (at 89.54 -10.322) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 125 "unconnected-(J6-Pin_29-Pad29)") (pinfunction "Pin_29") (pintype "passive+no_connect"))
    (pad "30" thru_hole oval (at 87 -10.322) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 124 "unconnected-(J6-Pin_30-Pad30)") (pinfunction "Pin_30") (pintype "passive+no_connect"))
    (pad "31" thru_hole oval (at 89.54 -12.862) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 123 "unconnected-(J6-Pin_31-Pad31)") (pinfunction "Pin_31") (pintype "passive+no_connect"))
    (pad "32" thru_hole oval (at 87 -12.862) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 122 "unconnected-(J6-Pin_32-Pad32)") (pinfunction "Pin_32") (pintype "passive+no_connect"))
    (pad "33" thru_hole oval (at 89.54 -15.402) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 121 "Net-(J6-Pin_10)") (pinfunction "Pin_33") (pintype "passive"))
    (pad "34" thru_hole oval (at 87 -15.402) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 120 "Net-(J6-Pin_34)") (pinfunction "Pin_34") (pintype "passive"))
    (pad "35" thru_hole oval (at 89.54 -17.942) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 119 "Net-(J6-Pin_35)") (pinfunction "Pin_35") (pintype "passive"))
    (pad "36" thru_hole oval (at 87 -17.942) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 118 "unconnected-(J6-Pin_36-Pad36)") (pinfunction "Pin_36") (pintype "passive+no_connect"))
    (pad "37" thru_hole oval (at 89.54 -20.482) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pinfunction "Pin_37") (pintype "passive"))
    (pad "38" thru_hole oval (at 87 -20.482) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pinfunction "Pin_38") (pintype "passive"))
    (pad "39" thru_hole oval (at 89.54 -23.022) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GNDREF") (pinfunction "Pin_39") (pintype "passive"))
    (pad "40" thru_hole oval (at 87 -23.022) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GNDREF") (pinfunction "Pin_40") (pintype "passive"))
    (pad "JP2-1" thru_hole rect (at 89.54 43.018 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
    (pad "JP2-2" thru_hole oval (at 87 43.018) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
    (pad "JP2-3" thru_hole oval (at 89.54 40.478) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
    (pad "JP2-4" thru_hole oval (at 87 40.478) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
    (pad "JP2-5" thru_hole oval (at 89.54 37.938) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
    (pad "JP2-6" thru_hole oval (at 87 37.938) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
    (pad "JP2-7" thru_hole oval (at 89.54 35.398) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
    (pad "JP2-8" thru_hole oval (at 87 35.398) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
    (pad "JP2-9" thru_hole oval (at 89.54 32.858) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
    (pad "JP2-10" thru_hole oval (at 87 32.858) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
    (pad "JP4-1" thru_hole rect (at 87 -40.802 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
    (pad "JP4-2" thru_hole oval (at 89.54 -40.802 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
    (pad "JP4-3" thru_hole oval (at 87 -38.262 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
    (pad "JP4-4" thru_hole oval (at 89.54 -38.262 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
    (pad "JP4-5" thru_hole oval (at 87 -35.722 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
    (pad "JP4-6" thru_hole oval (at 89.54 -35.722 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
    (pad "JP4-7" thru_hole oval (at 87 -33.182 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
    (pad "JP4-8" thru_hole oval (at 89.54 -33.182 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x20_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 20.32 3.81) (end 203.2 3.81)
    (layer "Edge.Cuts"))
  (gr_line (start 20.32 3.81) (end 20.32 110.49)
    (layer "Edge.Cuts"))
  (gr_line (start 203.2 110.49) (end 20.32 110.49)
    (layer "Edge.Cuts"))
  (gr_line (start 203.2 3.81) (end 203.2 110.49)
    (layer "Edge.Cuts"))
  (gr_text "Teensy MIDI PolySynth (TMPS) v5 (20240128) - Mark J Culross (KD5RXT)" (at 91.948 7.62) (layer "B.SilkS"))
  (gr_text "." (at 39.37 17.78) (layer "F.SilkS"))
  (gr_text "." (at 38.1 48.26) (layer "F.SilkS"))
  (gr_text "." (at 58.42 79.756) (layer "F.SilkS"))
  (gr_text "." (at 185.42 64.77) (layer "F.SilkS"))
  (gr_text "220" (at 37.338 94.742) (layer "F.SilkS"))
  (gr_text "1N4148" (at 63.754 96.774) (layer "F.SilkS"))
  (gr_text "Teensy MIDI PolySynth (TMPS) v5 (20240128) - Mark J Culross (KD5RXT)" (at 91.694 7.62) (layer "F.SilkS"))
  (gr_text "0.1 uF" (at 56.642 99.314) (layer "F.SilkS"))
  (gr_text "L  GND  R" (at 36.83 20.32) (layer "F.SilkS"))
  (gr_text "L  GND  R" (at 36.83 6.35) (layer "F.SilkS"))
  (gr_text "LINE\nOUT" (at 29.21 13.97) (layer "F.SilkS"))
  (gr_text "B\n\nB\n\nG\n\nW\n\nR" (at 191.77 54.61) (layer "F.SilkS"))
  (gr_text "EXT\nMIDI" (at 40.64 45.974) (layer "F.SilkS"))
  (gr_text "1M" (at 141.732 89.916) (layer "F.SilkS"))
  (gr_text "Teensy 4.1 (Display/MIDI)" (at 165.1 24.13 90) (layer "F.SilkS"))
  (gr_text "100" (at 194.31 25.146) (layer "F.SilkS"))
  (gr_text "10 uF" (at 196.596 87.63) (layer "F.SilkS"))
  (gr_text "." (at 193.04 58.42) (layer "F.SilkS"))
  (gr_text "47" (at 141.732 82.042) (layer "F.SilkS"))
  (gr_text "IN-4\n\nIN-5\n\nOUT-4\n\nOUT-5\n\nGND\n\nOUT-5\n\nOUT-4\n\nIN-5\n\nIN-4" (at 44.45 59.69) (layer "F.SilkS"))
  (gr_text "2K2" (at 81.28 95.25) (layer "F.SilkS"))
  (gr_text "USB\nHOST" (at 189.23 64.77) (layer "F.SilkS"))
  (gr_text "VUSB" (at 158.496 55.372) (layer "F.SilkS"))
  (gr_text "470K" (at 141.986 85.852) (layer "F.SilkS"))
  (gr_text "2K2\n" (at 71.12 95.25) (layer "F.SilkS"))
  (gr_text "470" (at 141.986 93.98) (layer "F.SilkS"))
  (gr_text "47" (at 37.338 86.614) (layer "F.SilkS"))
  (gr_text "100" (at 194.31 21.336) (layer "F.SilkS"))
  (gr_text "PowerBoost 1000C" (at 149.86 53.34) (layer "F.SilkS"))
  (gr_text "10 uF" (at 160.02 55.626) (layer "F.SilkS"))
  (gr_text "2K2" (at 76.454 95.25) (layer "F.SilkS"))
  (gr_text "." (at 39.37 11.43) (layer "F.SilkS"))
  (gr_text "6N138" (at 56.896 92.964) (layer "F.SilkS"))
  (gr_text "2K2" (at 150.114 58.674) (layer "F.SilkS"))
  (gr_text "22K" (at 37.338 90.932) (layer "F.SilkS"))
  (gr_text "J7" (at 40.64 43.18) (layer "F.SilkS"))
  (gr_text "DISABLE\nSWITCH" (at 141.986 10.16) (layer "F.SilkS"))
  (gr_text "0.1 uF" (at 67.818 15.748) (layer "F.SilkS"))
  (gr_text "Audio Adapter Rev D" (at 76.2 82.55) (layer "F.SilkS"))
  (gr_text "0.1 uF" (at 164.084 69.088) (layer "F.SilkS"))
  (gr_text "0.1 uF" (at 192.786 75.692) (layer "F.SilkS"))
  (gr_text "10 uF" (at 54.61 21.59) (layer "F.SilkS"))
  (gr_text "2N3904" (at 141.112 70.612) (layer "F.SilkS"))
  (gr_text "2N3906" (at 149.748 70.358035) (layer "F.SilkS"))
  (gr_text "Teensy 4.0 / 4.1 (Audio)" (at 73.66 21.082) (layer "F.SilkS"))
)
