(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad1)")
  (net 2 "VCC")
  (net 3 "Net-(J1-Pad3)")
  (net 4 "Net-(J1-Pad4)")
  (net 5 "Net-(J1-Pad5)")
  (net 6 "GND")
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 151.13 107.95 90)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (property "Sheetfile" "koko_prog.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at 0 -2.33 90) (layer "F.SilkS"))
    (fp_text value "Conn_01x06" (at 0 15.03 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 6.35) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "VCC") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad4)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad3)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "GND") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 151.145 101.605 90)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (property "Sheetfile" "koko_prog.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at 1.27 -2.33 90) (layer "F.SilkS"))
    (fp_text value "AVR-ISP-6" (at 1.27 7.41 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 2.54) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)") (pinfunction "MISO") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "VCC") (pinfunction "VCC") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad3)") (pinfunction "SCK") (pintype "passive"))
    (pad "4" thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad4)") (pinfunction "MOSI") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad5)") (pinfunction "~{RST}") (pintype "passive"))
    (pad "6" thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "GND") (pinfunction "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 147.32 111.76) (end 147.32 95.25) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 167.64 95.25) (end 167.64 111.76) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 147.32 95.25) (end 167.64 95.25) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 167.64 111.76) (end 147.32 111.76) (layer "Edge.Cuts") (width 0.1))
  (gr_text "@Petezah" (at 157.48 104.14) (layer "B.SilkS"))
  (gr_text "SCK" (at 153.67 104.14) (layer "F.SilkS"))
  (gr_text "RST" (at 156.21 104.14) (layer "F.SilkS"))
  (gr_text "VCC" (at 151.13 110.49) (layer "F.SilkS"))
  (gr_text "PB5" (at 161.29 105.41) (layer "F.SilkS"))
  (gr_text "MOSI" (at 153.67 96.52) (layer "F.SilkS"))
  (gr_text "VCC" (at 151.13 96.52) (layer "F.SilkS"))
  (gr_text "GND" (at 156.21 96.52) (layer "F.SilkS"))
  (gr_text "PB1" (at 156.21 105.41) (layer "F.SilkS"))
  (gr_text "GND" (at 163.83 110.49) (layer "F.SilkS"))
  (gr_text "PB0" (at 153.67 105.41) (layer "F.SilkS"))
  (gr_text "MISO" (at 151.13 104.14) (layer "F.SilkS"))
  (gr_text "PB2" (at 158.75 105.41) (layer "F.SilkS"))
  (zone (net 6) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 167.64 111.76)
        (xy 147.32 111.76)
        (xy 147.32 95.25)
        (xy 167.64 95.25)
      )
    )
  )
  (zone (net 6) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 167.64 111.76)
        (xy 147.32 111.76)
        (xy 147.32 95.25)
        (xy 167.64 95.25)
      )
    )
  )
)
