<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.3">
<drawing>
<board>
<plain>
<wire x1="45.7" y1="22.86" x2="45.7" y2="52.6925" width="0" layer="20"/>
<wire x1="45.7" y1="52.6925" x2="44.43" y2="53.9625" width="0" layer="20" curve="90"/>
<wire x1="44.43" y1="53.9625" x2="1.27" y2="53.9625" width="0" layer="20"/>
<wire x1="1.27" y1="53.9625" x2="0" y2="52.6925" width="0" layer="20" curve="90"/>
<wire x1="0" y1="52.6925" x2="0" y2="22.86" width="0" layer="20"/>
<wire x1="0" y1="22.86" x2="2.54" y2="20.32" width="0" layer="20" curve="90"/>
<wire x1="2.54" y1="20.32" x2="43.16" y2="20.32" width="0" layer="20"/>
<wire x1="43.16" y1="20.32" x2="45.7" y2="22.86" width="0" layer="20" curve="90"/>
</plain>
<libraries>
<library name="40xx-2">
<description>&lt;b&gt;CMOS Logic Devices, 4000 Series&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Motorola &lt;i&gt;CMOS LOGIC DATA&lt;/i&gt;; book, 02/88, DL131 REV 1
&lt;li&gt;http://www.elexp.com
&lt;li&gt;http://www.intersil.com
&lt;li&gt;http://www.ls3c.com.tw/product/1/COMOS.html
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL14">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="gm-diodes">
<description>&lt;b&gt;Diodes&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;Zener 1N47xx (as in protection for the MOSFET in the AMZ MOSFET Booster)
&lt;li&gt;rectifier 1N4001-1N4008 (for polarity reversal protection in power supply sections)
&lt;li&gt;clipping 1N914 (as in a TS808)
&lt;li&gt;LED (light emitting diode, 3mm and 5mm)
&lt;li&gt;mostly gathered from Eagle libraries
&lt;/ul&gt;</description>
<packages>
<package name="DO41-3">
<description>&lt;b&gt;DO-41 0.3" pad spacing&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="gm-trans">
<description>&lt;b&gt;Transistors&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;small signal amps (e.g., 2N508x)
&lt;li&gt;switching transistors (e.g., 2N2222, 2N390x)
&lt;li&gt;JFETs (e.g., J201, 2N3819, 2N5457)
&lt;li&gt;MOSFETs (e.g., BS170, BS250)
&lt;li&gt;mostly copied from Eagle libraries
&lt;/ul&gt;</description>
<packages>
<package name="TO92-">
</package>
</packages>
</library>
<library name="gm-supply">
<description>&lt;b&gt;Supply&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;input, output, ground, and power supply.  
&lt;li&gt;these are used on a schematic for placeholders and on a board for pads for off-board components like jacks.
&lt;/ul&gt;</description>
<packages>
<package name="ROUND">
<description>&lt;b&gt;Round Pad&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;drill diameter 0.7 mm&lt;/li&gt;&lt;/ul&gt;</description>
</package>
</packages>
</library>
<library name="gm-switches2">
<description>&lt;b&gt;Switches&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;SPST, SPDT, DPDT, 3PDT
&lt;/ul&gt;</description>
<packages>
<package name="FUJITSU">
</package>
</packages>
</library>
<library name="gm-caps-electro-pol">
<description>&lt;b&gt;Capacitors, Polar Electrolytic, Radial &lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;large value capacitors: .22 - 470uF (uF = µF = mF)
&lt;li&gt;often used in power supply filters
&lt;/ul&gt;</description>
<packages>
<package name="050_020_1">
<description>&lt;b&gt;5mm diameter, 2mm lead spacing, 0.1" pad spacing&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="jacks">
<description>&lt;b&gt;Jacks&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;audio and power jacks
&lt;li&gt;off-board versions and just pads for the circuit board
&lt;/ul&gt;</description>
<packages>
<package name="NMJ6HCD2">
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED3MM-NS">
<description>&lt;h3&gt;LED 3MM - No Silk&lt;/h3&gt;
3 mm, round</description>
</package>
</packages>
</library>
<library name="resistors">
<description>&lt;b&gt;Resistors&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;6mm long -- the size of 1/4 watt resistors
&lt;li&gt; all resistor values have the same size package; you choose the value of resistance 
&lt;/ul&gt;</description>
<packages>
<package name="R0207/3">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
length: 6mm&lt;br&gt;
format: 0.1" (perfboard)&lt;br&gt;
spacing: 3 holes

&lt;p&gt;This length resistor applies to 1/4 watt metal film.</description>
</package>
<package name="R0207/2V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
vertical placement&lt;br&gt;
format: 0.1" (perfboard)&lt;br&gt;
spacing: 2 holes

&lt;p&gt;This length resistor applies to 1/4 watt metal film.</description>
</package>
<package name="0805">
</package>
</packages>
</library>
<library name="capacitors-film">
<description>&lt;b&gt;Capacitors, Ceramic&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;very small capacitances: 1 - 1000pF
&lt;/ul&gt;</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="switches">
<description>&lt;b&gt;Switches&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;SPST, SPDT, DPDT, 3PDT
&lt;/ul&gt;</description>
<packages>
<package name="SPST">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="40xx-2" package="DIL14" value="40106N"/>
<element name="R1" library="resistors" package="0805" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="resistors" package="0805" value="1M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="resistors" package="0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="capacitors-film" package="0805" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="capacitors-film" package="0805" value="220n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SW1" library="switches" package="SPST" value="MOMENTARY">
<attribute name="NAME"/>
</element>
<element name="D2" library="SparkFun-LED" package="LED3MM-NS" value="LED">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="gm-diodes" package="DO41-3" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="resistors" package="R0207/3" value="150k"/>
<element name="R5" library="resistors" package="R0207/2V" value="15k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="resistors" package="R0207/2V" value="47R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="gm-trans" package="TO92-" value="2N3904">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="Q2" library="gm-trans" package="TO92-" value="2N3906">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="V" library="gm-supply" package="ROUND" value="">
<attribute name="NAME"/>
</element>
<element name="G" library="gm-supply" package="ROUND" value="">
<attribute name="NAME"/>
</element>
<element name="SND" library="gm-supply" package="ROUND" value="">
<attribute name="NAME"/>
</element>
<element name="RET" library="gm-supply" package="ROUND" value="">
<attribute name="NAME"/>
</element>
<element name="REL1" library="gm-switches2" package="FUJITSU" value="SLATCH"/>
<element name="C3" library="gm-caps-electro-pol" package="050_020_1" value="100u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="gm-caps-electro-pol" package="050_020_1" value="100u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IN" library="jacks" package="NMJ6HCD2" value="STEREOSW">
<attribute name="NAME"/>
</element>
<element name="OUT" library="jacks" package="NMJ6HCD2" value="STEREOSW">
<attribute name="NAME"/>
</element>
<element name="G1" library="gm-supply" package="ROUND" value="">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="D1" pad="C"/>
<contactref element="Q2" pad="3"/>
<contactref element="R6" pad="2"/>
<contactref element="C3" pad="+"/>
</signal>
<signal name="N$2">
<contactref element="Q1" pad="1"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="Q1" pad="2"/>
<contactref element="Q2" pad="1"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="Q2" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="D1" pad="A"/>
<contactref element="IC1" pad="6"/>
</signal>
<signal name="N$5">
<contactref element="REL1" pad="P$1"/>
<contactref element="C3" pad="-"/>
</signal>
<signal name="N$6">
<contactref element="IC1" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="SW1" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="IC1" pad="3"/>
<contactref element="IC1" pad="2"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="C2" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="SW1" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="IC1" pad="4"/>
<contactref element="IC1" pad="5"/>
<contactref element="R3" pad="1"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="LED">
<contactref element="R3" pad="2"/>
<contactref element="D2" pad="K"/>
</signal>
<signal name="GND">
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="R5" pad="1"/>
<contactref element="Q1" pad="3"/>
<contactref element="R4" pad="1"/>
<contactref element="IC1" pad="7"/>
<contactref element="G" pad="1"/>
<contactref element="REL1" pad="P$2"/>
<contactref element="C4" pad="-"/>
<contactref element="IC1" pad="10"/>
<contactref element="IC1" pad="13"/>
<contactref element="IC1" pad="8"/>
<contactref element="IC1" pad="12"/>
<contactref element="IC1" pad="9"/>
<contactref element="IC1" pad="11"/>
<contactref element="REL1" pad="P$6"/>
<contactref element="OUT" pad="S"/>
<contactref element="IN" pad="S"/>
<contactref element="G1" pad="1"/>
</signal>
<signal name="V">
<contactref element="IC1" pad="14"/>
<contactref element="V" pad="1"/>
<contactref element="D2" pad="A"/>
<contactref element="C4" pad="+"/>
</signal>
<signal name="N$12">
<contactref element="REL1" pad="P$4"/>
<contactref element="REL1" pad="P$7"/>
<contactref element="IN" pad="T"/>
</signal>
<signal name="N$13">
<contactref element="REL1" pad="P$3"/>
<contactref element="SND" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="RET" pad="1"/>
<contactref element="REL1" pad="P$9"/>
</signal>
<signal name="N$15">
<contactref element="REL1" pad="P$8"/>
<contactref element="OUT" pad="T"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
