(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 0)
    (no_connects 0)
    (area 0 0 0 0)
    (thickness 1.6)
    (drawings 4)
    (tracks 0)
    (zones 0)
    (modules 8)
    (nets 1)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user hide)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFEFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module Mounting_Holes:MountingHole_3mm (layer F.Cu) (tedit 587C2ADA)
    (at 147.32 114.3)
    (descr "Mounting Hole 3mm, no annular")
    (tags "mounting hole 3mm no annular")
    (fp_text reference REF** (at 0 -4) (layer F.SilkS) hide)
    (fp_text value MountingHole_3mm (at 0 4) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3mm (layer F.Cu) (tedit 587C2AE2)
    (at 101.6 114.3)
    (descr "Mounting Hole 3mm, no annular")
    (tags "mounting hole 3mm no annular")
    (fp_text reference REF** (at 0 -4) (layer F.SilkS) hide)
    (fp_text value MountingHole_3mm (at 0 4) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3mm (layer F.Cu) (tedit 587C2AE5)
    (at 101.6 68.58)
    (descr "Mounting Hole 3mm, no annular")
    (tags "mounting hole 3mm no annular")
    (fp_text reference REF** (at 0 -4) (layer F.SilkS) hide)
    (fp_text value MountingHole_3mm (at 0 4) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers *.Cu *.Mask))
  )
  (module SOC:COPPER3000 (layer F.Cu) (tedit 0)
    (at 124.46 91.44)
    (fp_text reference G*** (at 0 0) (layer F.Cu) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.Cu) hide)
  )
  (module SOC:MASK3000 (layer F.Cu) (tedit 0)
    (at 124.46 91.44)
    (fp_text reference G*** (at 0 0) (layer F.Mask) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.Mask) hide)
  )
  (module SOC:SILK3000 (layer F.Cu) (tedit 0)
    (at 124.46 91.44)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module Mounting_Holes:MountingHole_3mm (layer F.Cu) (tedit 587C2ADD)
    (at 147.32 68.58)
    (descr "Mounting Hole 3mm, no annular")
    (tags "mounting hole 3mm no annular")
    (fp_text reference REF** (at 0 -4) (layer F.SilkS) hide)
    (fp_text value MountingHole_3mm (at 0 4) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers *.Cu *.Mask))
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 587C2AEA)
    (at 123.825 113.665)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference REF** (at 0 2.1) (layer B.SilkS) hide)
    (fp_text value C_0805_HandSoldering (at 0 -2.1) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 149.86 66.04) (end 99.06 66.04) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 149.86 116.84) (end 149.86 66.04) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 99.06 116.84) (end 149.86 116.84) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 99.06 66.04) (end 99.06 116.84) (angle 90) (layer Edge.Cuts) (width 0.15))
)
