(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 112)
    (no_connects 0)
    (area 132.424999 61.174999 172.575001 83.825001)
    (thickness 1.6)
    (drawings 15)
    (tracks 133)
    (zones 0)
    (modules 85)
    (nets 23)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (44 Edge.Cuts user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.3)
    (zone_45_only yes)
    (trace_min 0.006)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.027)
    (via_min_drill 0.013)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.2 0.75)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFEFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VCC)
  (net 2 GND)
  (net 3 +5V)
  (net 4 GNDA)
  (net 5 "Net-(L1-Pad1)")
  (net 6 "Net-(L2-Pad1)")
  (net 7 "Net-(D1-Pad2)")
  (net 8 /VDD1)
  (net 9 /VDD2)
  (net 10 /SPU)
  (net 11 /SPD)
  (net 12 /UD+)
  (net 13 /UD-)
  (net 14 /DD+)
  (net 15 /DD-)
  (net 16 /UD2+)
  (net 17 /DD2+)
  (net 18 /UD2-)
  (net 19 /DD2-)
  (net 20 "Net-(L3-Pad1)")
  (net 21 "Net-(L4-Pad2)")
  (net 22 "Net-(L5-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /DD+)
    (add_net /DD-)
    (add_net /DD2+)
    (add_net /DD2-)
    (add_net /SPD)
    (add_net /SPU)
    (add_net /UD+)
    (add_net /UD-)
    (add_net /UD2+)
    (add_net /UD2-)
    (add_net /VDD1)
    (add_net /VDD2)
    (add_net GND)
    (add_net GNDA)
    (add_net "Net-(D1-Pad2)")
  )
  (net_class pwr ""
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net "Net-(L1-Pad1)")
    (add_net "Net-(L2-Pad1)")
    (add_net "Net-(L3-Pad1)")
    (add_net "Net-(L4-Pad2)")
    (add_net "Net-(L5-Pad2)")
    (add_net VCC)
  )
  (module USB_Iso:Via-0.6 (layer F.Cu) (tedit 58A3A694)
    (at 170 65)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value Via-0.6 (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 4 GNDA) (zone_connect 2))
  )
  (module USB_Iso:Via-0.6 (layer F.Cu) (tedit 58A3A694)
    (at 170 67.5)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value Via-0.6 (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 4 GNDA) (zone_connect 2))
  )
  (module USB_Iso:Via-0.6 (layer F.Cu) (tedit 58A3A694)
    (at 170 70)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value Via-0.6 (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 4 GNDA) (zone_connect 2))
  )
  (module USB_Iso:Via-0.6 (layer F.Cu) (tedit 58A3A694)
    (at 170 72.5)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value Via-0.6 (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 4 GNDA) (zone_connect 2))
  )
  (module USB_Iso:Via-0.6 (layer F.Cu) (tedit 58A3A694)
    (at 170 75)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value Via-0.6 (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 4 GNDA) (zone_connect 2))
  )
  (module USB_Iso:Via-0.6 (layer F.Cu) (tedit 58A3A694)
    (at 170 80)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value Via-0.6 (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 4 GNDA) (zone_connect 2))
  )
  (module USB_Iso:Via-0.6 (layer F.Cu) (tedit 58A3A694)
    (at 170 77.5)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value Via-0.6 (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 4 GNDA) (zone_connect 2))
  )
  (module USB_Iso:Via-0.6 (layer F.Cu) (tedit 58A3A694)
    (at 167.5 77.5)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value Via-0.6 (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 4 GNDA) (zone_connect 2))
  )
  (module USB_Iso:Via-0.6 (layer F.Cu) (tedit 58A3A694)
    (at 167.5 82.5)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value Via-0.6 (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 4 GNDA) (zone_connect 2))
  )
  (module USB_Iso:Via-0.6 (layer F.Cu) (tedit 58A2BF80)
    (at 142.5 80)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value Via-0.6 (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module USB_Iso:Via-0.6 (layer F.Cu) (tedit 58A2BF80)
    (at 137.5 82.5)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value Via-0.6 (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module USB_Iso:Via-0.6 (layer F.Cu) (tedit 58A2BF80)
    (at 135 80)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value Via-0.6 (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module USB_Iso:Via-0.6 (layer F.Cu) (tedit 58A2BF80)
    (at 135 77.5)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value Via-0.6 (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module USB_Iso:Via-0.6 (layer F.Cu) (tedit 58A2BF80)
    (at 135 75)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value Via-0.6 (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module USB_Iso:Via-0.6 (layer F.Cu) (tedit 58A2BF80)
    (at 135 72.5)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value Via-0.6 (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module USB_Iso:Via-0.6 (layer F.Cu) (tedit 58A2BF80)
    (at 135 70)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value Via-0.6 (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module USB_Iso:Via-0.6 (layer F.Cu) (tedit 58A2BF80)
    (at 135 67.5)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value Via-0.6 (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module USB_Iso:Via-0.6 (layer F.Cu) (tedit 58A2BF80)
    (at 137.5 67.5)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value Via-0.6 (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module USB_Iso:Via-0.6 (layer F.Cu) (tedit 58A2BF80)
    (at 135 65)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value Via-0.6 (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module USB_Iso:Via-0.6 (layer F.Cu) (tedit 58A2BF80)
    (at 135 62.5)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value Via-0.6 (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module USB_Iso:Via-0.6 (layer F.Cu) (tedit 58A2BF80)
    (at 137.5 62.5)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value Via-0.6 (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module USB_Iso:Via-0.6 (layer F.Cu) (tedit 58A3A694)
    (at 160 76.5)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value Via-0.6 (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 4 GNDA) (zone_connect 2))
  )
  (module USB_Iso:Via-0.6 (layer F.Cu) (tedit 58A2BF80)
    (at 142.5 67.5)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value Via-0.6 (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module USB_Iso:Via-0.6 (layer F.Cu) (tedit 58A3A694)
    (at 155 65)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value Via-0.6 (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 4 GNDA) (zone_connect 2))
  )
  (module USB_Iso:Via-0.6 (layer F.Cu) (tedit 58A3A694)
    (at 162.5 67.5)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value Via-0.6 (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 4 GNDA) (zone_connect 2))
  )
  (module USB_Iso:Via-0.6 (layer F.Cu) (tedit 58A3A694)
    (at 160 67.5)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value Via-0.6 (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 4 GNDA) (zone_connect 2))
  )
  (module USB_Iso:Via-0.6 (layer F.Cu) (tedit 58A2BF80)
    (at 150 77.5)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value Via-0.6 (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module USB_Iso:Via-0.6 (layer F.Cu) (tedit 58A3A694)
    (at 155 77.5)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value Via-0.6 (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 4 GNDA) (zone_connect 2))
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 541A9B4D)
    (at 160.75 73.5 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference L2 (at -2.75 0 90) (layer F.SilkS))
    (fp_text value Ferrite_Bead_Small (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Mask)
      (net 6 "Net-(L2-Pad1)"))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Mask)
      (net 3 +5V))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module USB_Iso:Via-0.6 (layer F.Cu) (tedit 58A3A694)
    (at 157.5 62.5)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value Via-0.6 (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 4 GNDA) (zone_connect 2))
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 541A9B4D)
    (at 159.25 78.75 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (zone_connect 2)
    (attr smd)
    (fp_text reference C4 (at 0 1.5 90) (layer F.SilkS))
    (fp_text value 0u1 (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Mask)
      (net 4 GNDA) (zone_connect 2))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Mask)
      (net 9 /VDD2) (zone_connect 2))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module USB_Iso:Via-0.6 (layer F.Cu) (tedit 58A3A694)
    (at 155 72.5)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value Via-0.6 (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 4 GNDA) (zone_connect 2))
  )
  (module USB_Iso:Via-0.6 (layer F.Cu) (tedit 58A2BF80)
    (at 150 82.5)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value Via-0.6 (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module USB_Iso:Via-0.6 (layer F.Cu) (tedit 58A2BF80)
    (at 147.5 82.5)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value Via-0.6 (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module USB_Iso:Via-0.6 (layer F.Cu) (tedit 58A3A694)
    (at 155 82.5)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value Via-0.6 (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 4 GNDA) (zone_connect 2))
  )
  (module USB_Iso:Via-0.6 (layer F.Cu) (tedit 58A3A694)
    (at 157.5 82.5)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value Via-0.6 (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 4 GNDA) (zone_connect 2))
  )
  (module USB_Iso:Via-0.6 (layer F.Cu) (tedit 58A2BF80)
    (at 137.5 75)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value Via-0.6 (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module USB_Iso:Via-0.6 (layer F.Cu) (tedit 58A2BF80)
    (at 137.5 72.5)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value Via-0.6 (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module USB_Iso:Via-0.6 (layer F.Cu) (tedit 58A2BF80)
    (at 137.5 70)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value Via-0.6 (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module USB_Iso:Via-0.6 (layer F.Cu) (tedit 58A3A694)
    (at 167.5 75)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value Via-0.6 (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 4 GNDA) (zone_connect 2))
  )
  (module USB_Iso:Via-0.6 (layer F.Cu) (tedit 58A3A694)
    (at 167.5 72.5)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value Via-0.6 (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 4 GNDA) (zone_connect 2))
  )
  (module USB_Iso:Via-0.6 (layer F.Cu) (tedit 58A3A694)
    (at 167.5 70)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value Via-0.6 (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 4 GNDA) (zone_connect 2))
  )
  (module USB_Iso:Via-0.6 (layer F.Cu) (tedit 58A2BF80)
    (at 140 62.5)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value Via-0.6 (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module USB_Iso:Via-0.6 (layer F.Cu) (tedit 58A3A694)
    (at 165 82.5)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value Via-0.6 (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 4 GNDA) (zone_connect 2))
  )
  (module USB_Iso:Via-0.6 (layer F.Cu) (tedit 58A3A694)
    (at 162.5 82.5)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value Via-0.6 (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 4 GNDA) (zone_connect 2))
  )
  (module USB_Iso:Via-0.6 (layer F.Cu) (tedit 58A3A694)
    (at 160 82.5)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value Via-0.6 (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 4 GNDA) (zone_connect 2))
  )
  (module USB_Iso:Via-0.6 (layer F.Cu) (tedit 58A3A694)
    (at 165 70)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value Via-0.6 (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 4 GNDA) (zone_connect 2))
  )
  (module USB_Iso:Via-0.6 (layer F.Cu) (tedit 58A3A694)
    (at 162.5 65)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value Via-0.6 (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 4 GNDA) (zone_connect 2))
  )
  (module USB_Iso:Via-0.6 (layer F.Cu) (tedit 58A3A694)
    (at 160 65)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value Via-0.6 (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 4 GNDA) (zone_connect 2))
  )
  (module USB_Iso:Via-0.6 (layer F.Cu) (tedit 58A3A694)
    (at 155 62.5)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value Via-0.6 (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 4 GNDA) (zone_connect 2))
  )
  (module USB_Iso:Via-0.6 (layer F.Cu) (tedit 58A2BF80)
    (at 150 72.5)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value Via-0.6 (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module USB_Iso:Via-0.6 (layer F.Cu) (tedit 58A2BF80)
    (at 140 75)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value Via-0.6 (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module USB_Iso:Via-0.6 (layer F.Cu) (tedit 58A2BF80)
    (at 140 72.5)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value Via-0.6 (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module USB_Iso:Via-0.6 (layer F.Cu) (tedit 58A2BF80)
    (at 140 70)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value Via-0.6 (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module USB_Iso:Via-0.6 (layer F.Cu) (tedit 58A2BF80)
    (at 142.5 65)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value Via-0.6 (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module USB_Iso:Via-0.6 (layer F.Cu) (tedit 58A2BF80)
    (at 142.5 62.5)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value Via-0.6 (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module USB_Iso:Via-0.6 (layer F.Cu) (tedit 58A2BF80)
    (at 145 62.5)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value Via-0.6 (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module USB_Iso:Via-0.6 (layer F.Cu) (tedit 58A2BF80)
    (at 147.5 62.5)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value Via-0.6 (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module USB_Iso:Via-0.6 (layer F.Cu) (tedit 58A2BF80)
    (at 150 62.5)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value Via-0.6 (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module USB_Iso:Via-0.6 (layer F.Cu) (tedit 58A2BF80)
    (at 140 82.5)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value Via-0.6 (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module USB_Iso:Via-0.6 (layer F.Cu) (tedit 58A2BF80)
    (at 142.5 82.5)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value Via-0.6 (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Housings_SOIC:SOIC-16W_7.5x10.3mm_Pitch1.27mm (layer F.Cu) (tedit 58A3A2F5)
    (at 152.5 77)
    (descr "16-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (zone_connect 2)
    (attr smd)
    (fp_text reference U1 (at 0 -4.25) (layer F.SilkS))
    (fp_text value ADUM4160 (at 0 6.25) (layer F.Fab))
    (pad 1 smd rect (at -4.65 -4.445) (size 1.5 0.6) (layers F.Cu F.Mask)
      (net 1 VCC) (zone_connect 2))
    (pad 2 smd rect (at -4.65 -3.175) (size 1.5 0.6) (layers F.Cu F.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 3 smd rect (at -4.65 -1.905) (size 1.5 0.6) (layers F.Cu F.Mask)
      (net 8 /VDD1) (zone_connect 2))
    (pad 4 smd rect (at -4.65 -0.635) (size 1.5 0.6) (layers F.Cu F.Mask)
      (net 8 /VDD1) (zone_connect 2))
    (pad 5 smd rect (at -4.65 0.635) (size 1.5 0.6) (layers F.Cu F.Mask)
      (net 10 /SPU) (zone_connect 2))
    (pad 6 smd rect (at -4.65 1.905) (size 1.5 0.6) (layers F.Cu F.Mask)
      (net 18 /UD2-) (zone_connect 2))
    (pad 7 smd rect (at -4.65 3.175) (size 1.5 0.6) (layers F.Cu F.Mask)
      (net 16 /UD2+) (zone_connect 2))
    (pad 8 smd rect (at -4.65 4.445) (size 1.5 0.6) (layers F.Cu F.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 9 smd rect (at 4.65 4.445) (size 1.5 0.6) (layers F.Cu F.Mask)
      (net 4 GNDA) (zone_connect 2))
    (pad 10 smd rect (at 4.65 3.175) (size 1.5 0.6) (layers F.Cu F.Mask)
      (net 17 /DD2+) (zone_connect 2))
    (pad 11 smd rect (at 4.65 1.905) (size 1.5 0.6) (layers F.Cu F.Mask)
      (net 19 /DD2-) (zone_connect 2))
    (pad 12 smd rect (at 4.65 0.635) (size 1.5 0.6) (layers F.Cu F.Mask)
      (net 9 /VDD2) (zone_connect 2))
    (pad 13 smd rect (at 4.65 -0.635) (size 1.5 0.6) (layers F.Cu F.Mask)
      (net 11 /SPD) (zone_connect 2))
    (pad 14 smd rect (at 4.65 -1.905) (size 1.5 0.6) (layers F.Cu F.Mask)
      (net 9 /VDD2) (zone_connect 2))
    (pad 15 smd rect (at 4.65 -3.175) (size 1.5 0.6) (layers F.Cu F.Mask)
      (net 4 GNDA) (zone_connect 2))
    (pad 16 smd rect (at 4.65 -4.445) (size 1.5 0.6) (layers F.Cu F.Mask)
      (net 3 +5V) (zone_connect 2))
    (model Housings_SOIC.3dshapes/SOIC-16_7.5x10.3mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module USB_Iso:Via-0.6 (layer F.Cu) (tedit 58A2BF80)
    (at 145 82.5)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value Via-0.6 (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Connect:USB_A (layer F.Cu) (tedit 58A2EEC0)
    (at 163.08 76.07 90)
    (descr "USB A connector")
    (tags "USB USB_A")
    (fp_text reference P2 (at 3.57 3.17 90) (layer F.SilkS))
    (fp_text value USB_A (at 3.84 7.44 90) (layer F.Fab))
    (pad 4 thru_hole circle (at 7.11 0) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(L5-Pad2)") (zone_connect 2))
    (pad 3 thru_hole circle (at 4.57 0) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 14 /DD+))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 15 /DD-))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(L2-Pad1)"))
    (pad 5 thru_hole circle (at 10.16 2.67) (size 3 3) (drill 2.3) (layers *.Cu *.Mask)
      (net 4 GNDA))
    (pad 5 thru_hole circle (at -3.56 2.67) (size 3 3) (drill 2.3) (layers *.Cu *.Mask)
      (net 4 GNDA))
    (model Connectors.3dshapes/USB_A.wrl
      (at (xyz 0.14 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 541A9B8D)
    (at 156.25 70.25 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (zone_connect 2)
    (attr smd)
    (fp_text reference C6 (at 3.25 0.5 180) (layer F.SilkS))
    (fp_text value 10u (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Mask)
      (net 3 +5V) (zone_connect 2))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Mask)
      (net 4 GNDA) (zone_connect 2))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 541A9B4D)
    (at 145.75 73.5 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (zone_connect 2)
    (attr smd)
    (fp_text reference C1 (at 0 1.5 270) (layer F.SilkS))
    (fp_text value 0u1 (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Mask)
      (net 1 VCC) (zone_connect 2))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Mask)
      (net 2 GND) (zone_connect 2))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58C51A44)
    (at 159.25 73.5 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (zone_connect 2)
    (attr smd)
    (fp_text reference C2 (at 2.75 0 270) (layer F.SilkS))
    (fp_text value 0u1 (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Mask)
      (net 3 +5V) (zone_connect 2))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Mask)
      (net 4 GNDA) (zone_connect 2))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 541A9B4D)
    (at 145.75 77.25 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (zone_connect 2)
    (attr smd)
    (fp_text reference C3 (at 2.75 0 270) (layer F.SilkS))
    (fp_text value 0u1 (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Mask)
      (net 8 /VDD1) (zone_connect 2))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Mask)
      (net 2 GND) (zone_connect 2))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:USB_A (layer F.Cu) (tedit 58A3A7AF)
    (at 142 68.96 270)
    (descr "USB A connector")
    (tags "USB USB_A")
    (fp_text reference P1 (at 3.54 3.25 270) (layer F.SilkS))
    (fp_text value USB_A (at 3.84 7.44 270) (layer F.Fab))
    (pad 4 thru_hole circle (at 7.11 0 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(L4-Pad2)") (zone_connect 2))
    (pad 3 thru_hole circle (at 4.57 0 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 12 /UD+))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 13 /UD-))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(L1-Pad1)"))
    (pad 5 thru_hole circle (at 10.16 2.67 180) (size 3 3) (drill 2.3) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 5 thru_hole circle (at -3.56 2.67 180) (size 3 3) (drill 2.3) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Connectors.3dshapes/USB_A.wrl
      (at (xyz 0.14 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 169.25 63 180)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D1 (at 0 -3 180) (layer F.SilkS))
    (fp_text value LED (at 0 1.55 180) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0) (size 1.2 1.2) (layers F.Cu F.Mask)
      (net 7 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -1.1 0) (size 1.2 1.2) (layers F.Cu F.Mask)
      (net 4 GNDA))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module USB_Iso:CRE1 (layer F.Cu) (tedit 58BFDDB1)
    (at 153.77 67.5)
    (fp_text reference U2 (at -0.02 -3.75) (layer F.SilkS))
    (fp_text value CRE1 (at 0 -5.4) (layer F.Fab))
    (pad 1 thru_hole oval (at -3.81 0) (size 1.4 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 2 thru_hole oval (at -1.27 0) (size 1.4 2) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(L3-Pad1)") (zone_connect 2))
    (pad 3 thru_hole oval (at 1.27 0) (size 1.4 2) (drill 1) (layers *.Cu *.Mask)
      (net 4 GNDA) (zone_connect 2))
    (pad 4 thru_hole oval (at 3.81 0) (size 1.4 2) (drill 1) (layers *.Cu *.Mask)
      (net 3 +5V) (zone_connect 2))
    (model D:/Dropbox/Electronics/KiCad/USB_Iso/3d/CRE1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58AA848B)
    (at 145.5 70.25)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference L1 (at -1.25 1.3) (layer F.SilkS))
    (fp_text value Ferrite_Bead_Small (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 -1.25) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Mask)
      (net 5 "Net-(L1-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Mask)
      (net 1 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 58AA848B)
    (at 146.75 80.25 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference R1 (at 2.75 0 180) (layer B.SilkS))
    (fp_text value 22 (at 0 -1.5 180) (layer B.Fab))
    (fp_text user %R (at 0 1.25 180) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Mask)
      (net 16 /UD2+))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Mask)
      (net 12 /UD+))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 58AA848B)
    (at 158.25 80.25 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference R2 (at -2.75 0 180) (layer B.SilkS))
    (fp_text value 22 (at 0 -1.5 180) (layer B.Fab))
    (fp_text user %R (at 0 1.25 180) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Mask)
      (net 14 /DD+))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Mask)
      (net 17 /DD2+))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 58AA848B)
    (at 146.75 78.75 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference R3 (at 2.75 0 180) (layer B.SilkS))
    (fp_text value 22 (at 0 -1.5 180) (layer B.Fab))
    (fp_text user %R (at 0 1.25 180) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Mask)
      (net 18 /UD2-))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Mask)
      (net 13 /UD-))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 58AA848B)
    (at 158.25 78.75 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference R4 (at -2.75 0 180) (layer B.SilkS))
    (fp_text value 22 (at 0 -1.5 180) (layer B.Fab))
    (fp_text user %R (at 0 1.25 180) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Mask)
      (net 15 /DD-))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Mask)
      (net 19 /DD2-))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer B.Cu) (tedit 58BFDC64)
    (at 151 75.7 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference R5 (at 0 1.27 270) (layer B.SilkS) hide)
    (fp_text value R (at 0 -1.27 270) (layer B.Fab))
    (fp_text user %R (at 0 1.27 270) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Mask)
      (net 8 /VDD1))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Mask)
      (net 10 /SPU))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer B.Cu) (tedit 58BFDC5F)
    (at 154 75.7 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference R6 (at 0 1.27 270) (layer B.SilkS) hide)
    (fp_text value R (at 0 -1.27 270) (layer B.Fab))
    (fp_text user %R (at 0 1.27 270) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Mask)
      (net 9 /VDD2))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Mask)
      (net 11 /SPD))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer B.Cu) (tedit 58BFDC68)
    (at 151 76.8 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference R7 (at 0 1.27 270) (layer B.SilkS) hide)
    (fp_text value R (at 0 -1.27 270) (layer B.Fab))
    (fp_text user %R (at 0 1.27 270) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Mask)
      (net 10 /SPU))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer B.Cu) (tedit 58BFDC58)
    (at 154 76.8 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference R8 (at 0 1.27 270) (layer B.SilkS) hide)
    (fp_text value R (at 0 -1.27 270) (layer B.Fab))
    (fp_text user %R (at 0 1.27 270) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Mask)
      (net 11 /SPD))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Mask)
      (net 4 GNDA))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 163 63)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference R9 (at 3.25 0) (layer F.SilkS))
    (fp_text value R (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Mask)
      (net 3 +5V))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Mask)
      (net 7 "Net-(D1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58AA848B)
    (at 144.25 77.25 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference L4 (at -2.75 0 90) (layer F.SilkS))
    (fp_text value Ferrite_Bead_Small (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Mask)
      (net 21 "Net-(L4-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58AA848B)
    (at 160.75 69.75 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference L5 (at 2.75 0 90) (layer F.SilkS))
    (fp_text value Ferrite_Bead_Small (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Mask)
      (net 4 GNDA))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Mask)
      (net 22 "Net-(L5-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58AA848B)
    (at 149.25 70.25)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at 2.75 0.75) (layer F.SilkS))
    (fp_text value 1u (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 -1.25) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module USB_Iso:Panasonic_Series_G_Inductor (layer F.Cu) (tedit 58C7CF31)
    (at 145.5 67 270)
    (fp_text reference L3 (at -2.75 0 540) (layer F.SilkS))
    (fp_text value 10u (at 0 -3 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1.4 3.2) (layers F.Cu F.Mask)
      (net 20 "Net-(L3-Pad1)"))
    (pad 2 smd rect (at 1 0 270) (size 1.4 3.2) (layers F.Cu F.Mask)
      (net 1 VCC))
  )
  (gr_text Out (at 169.75 82) (layer B.SilkS))
  (gr_text In (at 134.25 82) (layer B.SilkS))
  (gr_text v2.0 (at 155.5 63) (layer B.SilkS))
  (gr_text Out (at 169.75 82) (layer F.SilkS))
  (gr_text "In\n" (at 134.25 82) (layer F.SilkS))
  (gr_text "USB Isolator" (at 165 62.75) (layer B.SilkS))
  (dimension 22.5 (width 0.3) (layer Dwgs.User)
    (gr_text "22.500 mm" (at 180.35 72.5 270) (layer Dwgs.User))
    (feature1 (pts (xy 172.5 83.75) (xy 181.7 83.75)))
    (feature2 (pts (xy 172.5 61.25) (xy 181.7 61.25)))
    (crossbar (pts (xy 179 61.25) (xy 179 83.75)))
    (arrow1a (pts (xy 179 83.75) (xy 178.413579 82.623496)))
    (arrow1b (pts (xy 179 83.75) (xy 179.586421 82.623496)))
    (arrow2a (pts (xy 179 61.25) (xy 178.413579 62.376504)))
    (arrow2b (pts (xy 179 61.25) (xy 179.586421 62.376504)))
  )
  (dimension 40 (width 0.3) (layer Dwgs.User)
    (gr_text "40.000 mm" (at 152.5 57.15) (layer Dwgs.User))
    (feature1 (pts (xy 172.5 61.25) (xy 172.5 55.8)))
    (feature2 (pts (xy 132.5 61.25) (xy 132.5 55.8)))
    (crossbar (pts (xy 132.5 58.5) (xy 172.5 58.5)))
    (arrow1a (pts (xy 172.5 58.5) (xy 171.373496 59.086421)))
    (arrow1b (pts (xy 172.5 58.5) (xy 171.373496 57.913579)))
    (arrow2a (pts (xy 132.5 58.5) (xy 133.626504 59.086421)))
    (arrow2b (pts (xy 132.5 58.5) (xy 133.626504 57.913579)))
  )
  (gr_text "FS\n-\nLS" (at 152.5 76.15) (layer B.SilkS))
  (gr_line (start 132.5 61.25) (end 132.5 83.75) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 172.5 61.25) (end 172.5 83.75) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 132.5 61.25) (end 172.5 61.25) (layer Edge.Cuts) (width 0.15))
  (dimension 3 (width 0.3) (layer Dwgs.User)
    (gr_text "3.000 mm" (at 131 86.1) (layer Dwgs.User))
    (feature1 (pts (xy 129.5 82.5) (xy 129.5 87.45)))
    (feature2 (pts (xy 132.5 82.5) (xy 132.5 87.45)))
    (crossbar (pts (xy 132.5 84.75) (xy 129.5 84.75)))
    (arrow1a (pts (xy 129.5 84.75) (xy 130.626504 84.163579)))
    (arrow1b (pts (xy 129.5 84.75) (xy 130.626504 85.336421)))
    (arrow2a (pts (xy 132.5 84.75) (xy 131.373496 84.163579)))
    (arrow2b (pts (xy 132.5 84.75) (xy 131.373496 85.336421)))
  )
  (dimension 3 (width 0.3) (layer Dwgs.User)
    (gr_text "3.000 mm" (at 174.048329 85.800275) (layer Dwgs.User))
    (feature1 (pts (xy 175.548329 82.450275) (xy 175.548329 87.150275)))
    (feature2 (pts (xy 172.548329 82.450275) (xy 172.548329 87.150275)))
    (crossbar (pts (xy 172.548329 84.450275) (xy 175.548329 84.450275)))
    (arrow1a (pts (xy 175.548329 84.450275) (xy 174.421825 85.036696)))
    (arrow1b (pts (xy 175.548329 84.450275) (xy 174.421825 83.863854)))
    (arrow2a (pts (xy 172.548329 84.450275) (xy 173.674833 85.036696)))
    (arrow2b (pts (xy 172.548329 84.450275) (xy 173.674833 83.863854)))
  )
  (gr_line (start 132.5 83.75) (end 172.5 83.75) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads thru_hole_only (clearance 0.3))
    (min_thickness 0.3)
    (fill yes (arc_segments 32) (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 132.5 61.25) (xy 151.25 61.25) (xy 151.25 83.75) (xy 132.5 83.75)
      )
    )
  )
  (zone (net 4) (net_name GNDA) (layer F.Cu) (hatch edge 0.508)
    (connect_pads thru_hole_only (clearance 0.3))
    (min_thickness 0.3)
    (fill yes (arc_segments 32) (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 172.5 61.25) (xy 153.75 61.25) (xy 153.75 83.75) (xy 172.5 83.75)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads thru_hole_only (clearance 0.3))
    (min_thickness 0.3)
    (fill yes (arc_segments 32) (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 132.5 61.25) (xy 151.25 61.25) (xy 151.25 83.75) (xy 132.5 83.75)
      )
    )
  )
  (zone (net 4) (net_name GNDA) (layer B.Cu) (hatch edge 0.508)
    (connect_pads thru_hole_only (clearance 0.3))
    (min_thickness 0.3)
    (fill yes (arc_segments 32) (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 172.5 61.25) (xy 153.75 61.25) (xy 153.75 83.75) (xy 172.5 83.75)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 153.75 65.5) (xy 154.5 66.25) (xy 154.5 68.5) (xy 153.75 69.25) (xy 153.25 69.25)
        (xy 153.25 65.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 153.75 65.5) (xy 154.5 66.25) (xy 154.5 68.5) (xy 153.75 69.25) (xy 153.25 69.25)
        (xy 153.25 65.5)
      )
    )
  )
)
