(kicad_pcb (version 20171130) (host pcbnew "(5.1.7)-1")
  (general
    (thickness 1.6)
    (drawings 13)
    (tracks 61)
    (zones 0)
    (modules 14)
    (nets 16)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 5 10)
    (pad_drill 0)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +12V)
  (net 2 GND)
  (net 3 "Net-(R1-Pad2)")
  (net 4 "Net-(R1-Pad1)")
  (net 5 "Net-(R2-Pad1)")
  (net 6 "Net-(Rbottom1-Pad1)")
  (net 7 "Net-(U1-Pad14)")
  (net 8 "Net-(U1-Pad13)")
  (net 9 "Net-(U1-Pad12)")
  (net 10 "Net-(U1-Pad10)")
  (net 11 "Net-(U1-Pad9)")
  (net 12 "Net-(U1-Pad8)")
  (net 13 "Net-(U1-Pad7)")
  (net 14 "Net-(U1-Pad6)")
  (net 15 "Net-(U1-Pad5)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net GND)
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(Rbottom1-Pad1)")
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U1-Pad13)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(U1-Pad8)")
    (add_net "Net-(U1-Pad9)")
  )
  (module Connector_Wire:SolderWirePad_1x01_SMD_5x10mm (layer B.Cu) (tedit 5640A485)
    (at 90.17 102.235)
    (descr "Wire Pad, Square, SMD Pad,  5mm x 10mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (attr smd virtual)
    (fp_text reference REF** (at 0 3.81) (layer B.SilkS))
    (fp_text value SolderWirePad_1x01_SMD_5x10mm (at 0 -6.35) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 5 10) (layers B.Cu B.Paste B.Mask))
  )
  (module Connector_Wire:SolderWirePad_1x01_SMD_5x10mm (layer B.Cu) (tedit 5640A485)
    (at 90.17 90.17)
    (descr "Wire Pad, Square, SMD Pad,  5mm x 10mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (attr smd virtual)
    (fp_text reference REF** (at 0 3.81) (layer B.SilkS))
    (fp_text value SolderWirePad_1x01_SMD_5x10mm (at 0 -6.35) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 5 10) (layers B.Cu B.Paste B.Mask))
  )
  (module Connector_Wire:SolderWirePad_1x01_SMD_5x10mm (layer F.Cu) (tedit 5FA0C765)
    (at 128.905 82.55 90)
    (descr "Wire Pad, Square, SMD Pad,  5mm x 10mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (fp_text reference REF** (at 0 -3.81 90) (layer F.SilkS))
    (fp_text value SolderWirePad_1x01_SMD_5x10mm (at 0 6.35 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad "Signal in" smd rect (at 0 0 90) (size 5 10) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(R1-Pad2)"))
  )
  (module Connector_Wire:SolderWirePad_1x01_SMD_5x10mm (layer F.Cu) (tedit 5FA0C779)
    (at 140.97 82.55 90)
    (descr "Wire Pad, Square, SMD Pad,  5mm x 10mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (attr smd virtual)
    (fp_text reference REF** (at 0 -3.81 90) (layer F.SilkS))
    (fp_text value SolderWirePad_1x01_SMD_5x10mm (at 0 6.35 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad "Signal Out" smd rect (at 0 0 90) (size 5 10) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(R2-Pad1)"))
  )
  (module Single_Wire_V5_Footprints:XL6009E1_Buck_Hybrid (layer B.Cu) (tedit 5FA0C5A0)
    (at 124.46 96.52)
    (fp_text reference REF** (at 0 -0.5) (layer B.SilkS))
    (fp_text value XL6009E1_Buck_Hybrid (at 0 0.5) (layer B.Fab))
    (fp_text user IN+ (at -16.4592 8.5725) (layer B.SilkS))
    (fp_text user IN- (at -16.6116 -8.509) (layer B.SilkS))
    (fp_text user OUT- (at 15.7861 -8.5217) (layer B.SilkS))
    (fp_text user OUT+ (at 16.2941 8.9408) (layer B.SilkS))
    (pad 2 smd rect (at -20 -8.5) (size 3.5 3.5) (layers B.Cu B.Paste B.Mask))
    (pad 1 smd rect (at -20 8.5) (size 3.5 3.5) (layers B.Cu B.Paste B.Mask))
    (pad 4 smd rect (at 20 8.5) (size 3.5 3.5) (layers B.Cu B.Paste B.Mask)
      (net 1 +12V))
    (pad 3 smd rect (at 20 -8.5) (size 3.5 3.5) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 98.425 96.52 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference REF** (at 0 1.68 270) (layer B.SilkS))
    (fp_text value C_0805_2012Metric (at 0 -1.68 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -0.95 0 270) (size 1 1.45) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at 0.95 0 270) (size 1 1.45) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:CP_Elec_3x5.3 (layer B.Cu) (tedit 5B303299)
    (at 97.79 87.63)
    (descr "SMT capacitor, aluminium electrolytic, 3x5.3, Cornell Dubilier Electronics ")
    (tags "Capacitor Electrolytic")
    (attr smd)
    (fp_text reference REF** (at 0 2.7) (layer B.SilkS))
    (fp_text value CP_Elec_3x5.3 (at 0 -2.7) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0) (size 2.2 1.6) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd rect (at 1.5 0) (size 2.2 1.6) (layers B.Cu B.Paste B.Mask))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/CP_Elec_3x5.3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:CP_Elec_3x5.3 (layer B.Cu) (tedit 5B303299)
    (at 97.79 104.775)
    (descr "SMT capacitor, aluminium electrolytic, 3x5.3, Cornell Dubilier Electronics ")
    (tags "Capacitor Electrolytic")
    (attr smd)
    (fp_text reference REF** (at 0 2.7) (layer B.SilkS))
    (fp_text value CP_Elec_3x5.3 (at 0 -2.7) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0) (size 2.2 1.6) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd rect (at 1.5 0) (size 2.2 1.6) (layers B.Cu B.Paste B.Mask))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/CP_Elec_3x5.3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 135.255 87.63)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference Rtop1 (at -2.54 0 -90) (layer F.SilkS))
    (fp_text value 3.665k (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1 0) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 6 "Net-(Rbottom1-Pad1)"))
    (pad 1 smd roundrect (at -1 0) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 1 +12V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-14W_7.5x9mm_P1.27mm (layer F.Cu) (tedit 5D9F72B1)
    (at 135.92 99.06)
    (descr "SOIC, 14 Pin (JEDEC MS-013AF, https://www.analog.com/media/en/package-pcb-resources/package/54614177245586rw_14.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference U1 (at 0 -5.45) (layer F.SilkS))
    (fp_text value LM324AM (at 0 5.45) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 14 smd roundrect (at 4.65 -3.81) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(U1-Pad14)"))
    (pad 13 smd roundrect (at 4.65 -2.54) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 "Net-(U1-Pad13)"))
    (pad 12 smd roundrect (at 4.65 -1.27) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 "Net-(U1-Pad12)"))
    (pad 11 smd roundrect (at 4.65 0) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 10 smd roundrect (at 4.65 1.27) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(U1-Pad10)"))
    (pad 9 smd roundrect (at 4.65 2.54) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(U1-Pad9)"))
    (pad 8 smd roundrect (at 4.65 3.81) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(U1-Pad8)"))
    (pad 7 smd roundrect (at -4.65 3.81) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(U1-Pad7)"))
    (pad 6 smd roundrect (at -4.65 2.54) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(U1-Pad6)"))
    (pad 5 smd roundrect (at -4.65 1.27) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 "Net-(U1-Pad5)"))
    (pad 4 smd roundrect (at -4.65 0) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +12V))
    (pad 3 smd roundrect (at -4.65 -1.27) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(Rbottom1-Pad1)"))
    (pad 2 smd roundrect (at -4.65 -2.54) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(R1-Pad1)"))
    (pad 1 smd roundrect (at -4.65 -3.81) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(R2-Pad1)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-14W_7.5x9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 139.065 90.17)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference Rbottom1 (at 3.175 0 -90) (layer F.SilkS))
    (fp_text value 1.067k (at 0 1.65) (layer F.Fab))
    (pad 2 smd roundrect (at 1 0) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 2 GND))
    (pad 1 smd roundrect (at -1 0) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 6 "Net-(Rbottom1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 128.27 96.25 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at 0 1.651 90) (layer F.SilkS))
    (fp_text value 1k (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1 0 270) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 4 "Net-(R1-Pad1)"))
    (pad 1 smd roundrect (at -1 0 270) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 5 "Net-(R2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 128.905 88.9 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 0 1.524 90) (layer F.SilkS))
    (fp_text value 1k (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 3 "Net-(R1-Pad2)"))
    (pad 1 smd roundrect (at -1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 4 "Net-(R1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder (layer F.Cu) (tedit 5F68FEEF)
    (at 137.16 92.71 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C1 (at 3.0695 -0.0215 270) (layer F.SilkS))
    (fp_text value 104pF (at 0 1.68) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.0375 0 180) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.212766)
      (net 1 +12V))
    (pad 1 smd roundrect (at -1.0375 0 180) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.212766)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 86.36 110.49) (end 85.09 110.49) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 85.09 109.22) (end 83.82 109.22) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 83.82 82.55) (end 83.82 109.22) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 119.38 81.28) (end 85.09 81.28) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 149.86 110.49) (end 86.36 110.49) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 151.13 77.47) (end 151.13 109.22) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 121.92 76.2) (end 149.86 76.2) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 120.65 77.47) (end 120.65 80.01) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 85.09 82.55) (end 85.09 81.28) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 119.38 80.01) (end 119.38 81.28) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 121.92 77.47) (end 121.92 76.2) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 149.86 77.47) (end 151.13 77.47) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 149.86 109.22) (end 149.86 110.49) (angle -90) (layer Edge.Cuts) (width 0.05))
  (zone (net 1) (net_name +12V) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 107.315 108.585) (xy 86.36 108.585) (xy 86.36 83.82) (xy 107.315 83.82)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 149.225 108.585) (xy 122.555 108.585) (xy 122.555 78.74) (xy 149.225 78.74)
      )
    )
  )
  (zone (net 1) (net_name +12V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 149.225 108.585) (xy 122.555 108.585) (xy 122.555 78.74) (xy 149.225 78.74)
      )
    )
  )
)
