<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="16.51" y2="0" width="0" layer="20"/>
<wire x1="16.51" y1="0" x2="16.51" y2="6.35" width="0" layer="20"/>
<wire x1="16.51" y1="6.35" x2="0" y2="6.35" width="0" layer="20"/>
<wire x1="0" y1="6.35" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="common components">
<packages>
<package name="1206_SMT_RES">
</package>
</packages>
</library>
<library name="LM74610">
<packages>
<package name="MSOP-8">
</package>
</packages>
</library>
<library name="transistor-fet">
<description>&lt;b&gt;Field Effect Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;p&gt;
&lt;p&gt;
Symbols changed according to IEC617&lt;p&gt; 
All types, packages and assignment to symbols and pins checked&lt;p&gt;
Package outlines partly checked&lt;p&gt;
&lt;p&gt;
JFET = junction FET&lt;p&gt;
IGBT-x = insulated gate bipolar transistor&lt;p&gt;
x=N: NPN; x=P: PNP&lt;p&gt;
IGFET-mc-nnn; (IGFET=insulated gate field effect transistor)&lt;P&gt;
m=D: depletion mode (Verdr&amp;auml;ngungstyp)&lt;p&gt;
m=E: enhancement mode (Anreicherungstyp)&lt;p&gt;
c: N=N-channel; P=P-Channel&lt;p&gt;
nnn=GDS:  gate, drain, source&lt;p&gt;
2GDS: 2 x gate, drain, source&lt;p&gt;
GnDS: gate, n x drain, source&lt;p&gt;
GDSB: gate, drain, source, bulk&lt;p&gt;
&lt;p&gt;
by R. Vogg  15.March.2002</description>
<packages>
<package name="SOT669">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="common components" package="1206_SMT_RES" value="1uF">
<attribute name="NAME"/>
</element>
<element name="U1" library="LM74610" package="MSOP-8" value="LM74610-Q1">
<attribute name="NAME"/>
</element>
<element name="Q1" library="transistor-fet" package="SOT669" value="BUK9Y4R8"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="U1" pad="7"/>
<contactref element="C1" pad="P$1"/>
</signal>
<signal name="N$2">
<contactref element="U1" pad="1"/>
<contactref element="C1" pad="P$2"/>
</signal>
<signal name="G">
<contactref element="U1" pad="6"/>
<contactref element="Q1" pad="4"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="S">
<contactref element="Q1" pad="3"/>
<contactref element="U1" pad="4"/>
<contactref element="Q1" pad="1"/>
<contactref element="Q1" pad="2"/>
</signal>
<signal name="D">
<contactref element="Q1" pad="TAB"/>
<contactref element="U1" pad="8"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
