(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(1 "In1.Cu" signal)
		(2 "In2.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "N$1")
	(net 3 "N$2")
	(net 4 "N$3")
	(net 5 "N$4")
	(net 6 "N$5")
	(net 7 "N$6")
	(net 8 "N$7")
	(net 9 "N$8")
	(net 10 "N$9")
	(net 11 "N$10")
	(net 12 "N$11")
	(net 13 "N$12")
	(net 14 "N$13")
	(net 15 "N$14")
	(net 16 "N$15")
	(net 17 "N$16")
	(net 18 "N$17")
	(net 19 "N$18")
	(net 20 "N$19")
	(net 21 "N$20")
	(net 22 "N$21")
	(net 23 "N$22")
	(net 24 "N$23")
	(net 25 "N$24")
	(net 26 "N$25")
	(net 27 "N$26")
	(net 28 "N$27")
	(net 29 "N$28")
	(net 30 "N$29")
	(net 31 "N$30")
	(net 32 "N$31")
	(net 33 "N$32")
	(net 34 "N$33")
	(footprint "DIL16_SOCKET"
		(layer "F.Cu")
		(at 150.4061 98.81235 -90)
		(property "Reference" "S3"
			(at 0 0 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "DIP16_SOCKET"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole roundrect
			(at 1.68765 -5.3939)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(chamfer_ratio 0.2928932188)
			(chamfer top_left top_right bottom_left bottom_right)
			(net 19 "N$18")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "2" thru_hole roundrect
			(at 1.88765 -3.81)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(chamfer_ratio 0.2928932188)
			(chamfer top_left top_right bottom_left bottom_right)
			(net 20 "N$19")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "3" thru_hole roundrect
			(at 1.88765 7.62)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(chamfer_ratio 0.2928932188)
			(chamfer top_left top_right bottom_left bottom_right)
			(net 21 "N$20")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "4" thru_hole roundrect
			(at 1.88765 3.81)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(chamfer_ratio 0.2928932188)
			(chamfer top_left top_right bottom_left bottom_right)
			(net 22 "N$21")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "5" thru_hole roundrect
			(at 3.94 3.81)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(chamfer_ratio 0.2928932188)
			(chamfer top_left top_right bottom_left bottom_right)
			(net 23 "N$22")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "6" thru_hole roundrect
			(at 5.78 3.81)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(chamfer_ratio 0.2928932188)
			(chamfer top_left top_right bottom_left bottom_right)
			(net 24 "N$23")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "7" thru_hole roundrect
			(at 8.22 3.81)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(chamfer_ratio 0.2928932188)
			(chamfer top_left top_right bottom_left bottom_right)
			(net 25 "N$24")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "8" thru_hole roundrect
			(at 10.6609 3.81)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(chamfer_ratio 0.2928932188)
			(chamfer top_left top_right bottom_left bottom_right)
			(net 26 "N$25")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "9" thru_hole roundrect
			(at 11.6609 -6.81)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(chamfer_ratio 0.2928932188)
			(chamfer top_left top_right bottom_left bottom_right)
			(net 34 "N$33")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "10" thru_hole roundrect
			(at 9.220005 -6.81)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(chamfer_ratio 0.2928932188)
			(chamfer top_left top_right bottom_left bottom_right)
			(net 33 "N$32")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "11" thru_hole roundrect
			(at 6.78 -6.81)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(chamfer_ratio 0.2928932188)
			(chamfer top_left top_right bottom_left bottom_right)
			(net 32 "N$31")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "12" thru_hole roundrect
			(at 4.44 -6.81)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(chamfer_ratio 0.2928932188)
			(chamfer top_left top_right bottom_left bottom_right)
			(net 31 "N$30")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "13" thru_hole roundrect
			(at 10.6609 -3.81)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(chamfer_ratio 0.2928932188)
			(chamfer top_left top_right bottom_left bottom_right)
			(net 30 "N$29")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "14" thru_hole roundrect
			(at 8.22 -3.81)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(chamfer_ratio 0.2928932188)
			(chamfer top_left top_right bottom_left bottom_right)
			(net 29 "N$28")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "15" thru_hole roundrect
			(at 5.78 -3.81)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(chamfer_ratio 0.2928932188)
			(chamfer top_left top_right bottom_left bottom_right)
			(net 28 "N$27")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "16" thru_hole roundrect
			(at 3.94 -3.81)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(chamfer_ratio 0.2928932188)
			(chamfer top_left top_right bottom_left bottom_right)
			(net 27 "N$26")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint "TESTPOINT_SMALL"
		(layer "F.Cu")
		(at 137.8 112 180)
		(property "Reference" "GND0"
			(at -1 1.3 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "TESTPOINT_SMALL"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole roundrect
			(at 0 0 270)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(chamfer_ratio 0.2928932188)
			(chamfer top_left top_right bottom_left bottom_right)
			(net 1 "GND")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint "DIL16_SOCKET"
		(layer "F.Cu")
		(at 146.5961 98.81235 -90)
		(property "Reference" "S2"
			(at 0 0 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "DIP16_SOCKET"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole roundrect
			(at 3.94 3.81)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(chamfer_ratio 0.2928932188)
			(chamfer top_left top_right bottom_left bottom_right)
			(net 10 "N$9")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "2" thru_hole roundrect
			(at 5.78 3.81)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(chamfer_ratio 0.2928932188)
			(chamfer top_left top_right bottom_left bottom_right)
			(net 9 "N$8")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "3" thru_hole roundrect
			(at 8.22 3.81)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(chamfer_ratio 0.2928932188)
			(chamfer top_left top_right bottom_left bottom_right)
			(net 8 "N$7")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "4" thru_hole roundrect
			(at 10.6609 3.81)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(chamfer_ratio 0.2928932188)
			(chamfer top_left top_right bottom_left bottom_right)
			(net 7 "N$6")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "5" thru_hole roundrect
			(at 4.44 6.81)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(chamfer_ratio 0.2928932188)
			(chamfer top_left top_right bottom_left bottom_right)
			(net 6 "N$5")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "6" thru_hole roundrect
			(at 6.78 6.81)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(chamfer_ratio 0.2928932188)
			(chamfer top_left top_right bottom_left bottom_right)
			(net 5 "N$4")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "7" thru_hole roundrect
			(at 9.22 6.81)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(chamfer_ratio 0.2928932188)
			(chamfer top_left top_right bottom_left bottom_right)
			(net 4 "N$3")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "8" thru_hole roundrect
			(at 11.6609 6.81)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(chamfer_ratio 0.2928932188)
			(chamfer top_left top_right bottom_left bottom_right)
			(net 3 "N$2")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "9" thru_hole roundrect
			(at 10.6609 -3.81)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(chamfer_ratio 0.2928932188)
			(chamfer top_left top_right bottom_left bottom_right)
			(net 11 "N$10")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "10" thru_hole roundrect
			(at 8.22 -3.81)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(chamfer_ratio 0.2928932188)
			(chamfer top_left top_right bottom_left bottom_right)
			(net 12 "N$11")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "11" thru_hole roundrect
			(at 5.78 -3.81)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(chamfer_ratio 0.2928932188)
			(chamfer top_left top_right bottom_left bottom_right)
			(net 13 "N$12")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "12" thru_hole roundrect
			(at 3.94 -3.81)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(chamfer_ratio 0.2928932188)
			(chamfer top_left top_right bottom_left bottom_right)
			(net 14 "N$13")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "13" thru_hole roundrect
			(at 1.88765 -3.81)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(chamfer_ratio 0.2928932188)
			(chamfer top_left top_right bottom_left bottom_right)
			(net 15 "N$14")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "14" thru_hole roundrect
			(at 2.38765 -10.62)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(chamfer_ratio 0.2928932188)
			(chamfer top_left top_right bottom_left bottom_right)
			(net 16 "N$15")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "15" thru_hole roundrect
			(at 2.68765 6.81)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(chamfer_ratio 0.2928932188)
			(chamfer top_left top_right bottom_left bottom_right)
			(net 17 "N$16")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "16" thru_hole roundrect
			(at 1.68765 5.5961)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(chamfer_ratio 0.2928932188)
			(chamfer top_left top_right bottom_left bottom_right)
			(net 18 "N$17")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint "clipboard:f6e2a30f-1d4b-43ef-b59b-0bcdac681adb"
		(layer "F.Cu")
		(at 138.2 115.45)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 20 0)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "N$25")
			(solder_mask_margin 0.102)
		)
		(pad "2" thru_hole circle
			(at 18.75 0)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "N$24")
			(solder_mask_margin 0.102)
		)
		(pad "3" thru_hole circle
			(at 17.5 0)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "N$23")
			(solder_mask_margin 0.102)
		)
		(pad "4" thru_hole circle
			(at 16.25 0)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "N$22")
			(solder_mask_margin 0.102)
		)
		(pad "5" thru_hole circle
			(at 15 0)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "N$21")
			(solder_mask_margin 0.102)
		)
		(pad "6" thru_hole circle
			(at 13.75 0)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "N$20")
			(solder_mask_margin 0.102)
		)
		(pad "7" thru_hole circle
			(at 12.5 0)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "N$19")
			(solder_mask_margin 0.102)
		)
		(pad "8" thru_hole circle
			(at 11.25 0)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "N$18")
			(solder_mask_margin 0.102)
		)
		(pad "9" thru_hole circle
			(at 10 0)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "N$17")
			(solder_mask_margin 0.102)
		)
		(pad "10" thru_hole circle
			(at 8.75 0)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "N$16")
			(solder_mask_margin 0.102)
		)
		(pad "11" thru_hole circle
			(at 7.5 0)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "N$15")
			(solder_mask_margin 0.102)
		)
		(pad "12" thru_hole circle
			(at 6.25 0)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "N$14")
			(solder_mask_margin 0.102)
		)
		(pad "13" thru_hole circle
			(at 5 0)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "N$13")
			(solder_mask_margin 0.102)
		)
		(pad "14" thru_hole circle
			(at 3.75 0)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "N$12")
			(solder_mask_margin 0.102)
		)
		(pad "15" thru_hole circle
			(at 2.5 0)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "N$11")
			(solder_mask_margin 0.102)
		)
		(pad "16" thru_hole circle
			(at 1.25 0)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "N$10")
			(solder_mask_margin 0.102)
		)
		(pad "17" thru_hole circle
			(at 0 0)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(solder_mask_margin 0.102)
		)
		(pad "18" thru_hole circle
			(at 20 1.25)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "N$1")
			(solder_mask_margin 0.102)
		)
		(pad "19" thru_hole circle
			(at 18.75 1.25)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "N$33")
			(solder_mask_margin 0.102)
		)
		(pad "20" thru_hole circle
			(at 17.5 1.25)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "N$32")
			(solder_mask_margin 0.102)
		)
		(pad "21" thru_hole circle
			(at 16.25 1.25)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "N$31")
			(solder_mask_margin 0.102)
		)
		(pad "22" thru_hole circle
			(at 15 1.25)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "N$30")
			(solder_mask_margin 0.102)
		)
		(pad "23" thru_hole circle
			(at 13.75 1.25)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "N$29")
			(solder_mask_margin 0.102)
		)
		(pad "24" thru_hole circle
			(at 12.5 1.25)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "N$28")
			(solder_mask_margin 0.102)
		)
		(pad "25" thru_hole circle
			(at 11.25 1.25)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "N$27")
			(solder_mask_margin 0.102)
		)
		(pad "26" thru_hole circle
			(at 10 1.25)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "N$26")
			(solder_mask_margin 0.102)
		)
		(pad "27" thru_hole circle
			(at 8.75 1.25)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "N$9")
			(solder_mask_margin 0.102)
		)
		(pad "28" thru_hole circle
			(at 7.5 1.25)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "N$8")
			(solder_mask_margin 0.102)
		)
		(pad "29" thru_hole circle
			(at 6.25 1.25)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "N$7")
			(solder_mask_margin 0.102)
		)
		(pad "30" thru_hole circle
			(at 5 1.25)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "N$6")
			(solder_mask_margin 0.102)
		)
		(pad "31" thru_hole circle
			(at 3.75 1.25)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "N$5")
			(solder_mask_margin 0.102)
		)
		(pad "32" thru_hole circle
			(at 2.5 1.25)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "N$4")
			(solder_mask_margin 0.102)
		)
		(pad "33" thru_hole circle
			(at 1.25 1.25)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "N$3")
			(solder_mask_margin 0.102)
		)
		(pad "34" thru_hole circle
			(at 0 1.25)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "N$2")
			(solder_mask_margin 0.102)
		)
	)
	(footprint "TESTPOINT_SMALL"
		(layer "F.Cu")
		(at 158.7 112.3 180)
		(property "Reference" "REF0"
			(at 0.7 0.4 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "TESTPOINT_SMALL"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole roundrect
			(at 0 0 270)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(chamfer_ratio 0.2928932188)
			(chamfer top_left top_right bottom_left bottom_right)
			(net 2 "N$1")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(gr_line
		(start 138.3 108.45)
		(end 136.7 110)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 159.9 119.3)
		(end 159.9 110.1)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 158.5 108.4)
		(end 159.9 110.1)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 158.5 99.3)
		(end 138.3 99.3)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 138.3 99.3)
		(end 138.3 108.45)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 159.9 119.3)
		(end 136.7 119.3)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 136.7 119.3)
		(end 136.7 110)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 158.5 99.3)
		(end 158.5 108.4)
		(layer "Edge.Cuts")
	)
	(gr_text "3"
		(at 142.2 110.7 0)
		(layer "F.SilkS")
	)
	(gr_text "0\n"
		(at 142.1 103.2 0)
		(layer "F.SilkS")
	)
	(gr_text "www.intantech.com"
		(at 148.7 110.7 90)
		(layer "F.SilkS")
	)
	(gr_text "22"
		(at 147.1 108.3 0)
		(layer "F.SilkS")
	)
	(gr_text "5"
		(at 139.1 106.2 0)
		(layer "F.SilkS")
	)
	(gr_text "1"
		(at 142.3 105.6 0)
		(layer "F.SilkS")
	)
	(gr_text "7"
		(at 139.4 110 0)
		(layer "F.SilkS")
	)
	(gr_text "14"
		(at 138.4 102.1 0)
		(layer "F.SilkS")
	)
	(gr_text "6"
		(at 139.2 108.9 0)
		(layer "F.SilkS")
	)
	(gr_text "21"
		(at 147.7 105.8 0)
		(layer "F.SilkS")
	)
	(gr_text "29"
		(at 154.6 108.2 0)
		(layer "F.SilkS")
	)
	(gr_text "27"
		(at 157.6 104.2 0)
		(layer "F.SilkS")
	)
	(gr_text "15"
		(at 139.6 100.1 0)
		(layer "F.SilkS")
	)
	(gr_text "13"
		(at 157.4 102.2 0)
		(layer "F.SilkS")
	)
	(gr_text "19"
		(at 148.1 101.2 0)
		(layer "F.SilkS")
	)
	(gr_text "16"
		(at 157.2 100.1 0)
		(layer "F.SilkS")
	)
	(gr_text "24"
		(at 157.5 111.5 0)
		(layer "F.SilkS")
	)
	(gr_text "20"
		(at 146 103.4 0)
		(layer "F.SilkS")
	)
	(gr_text "31"
		(at 154.9 103.4 0)
		(layer "F.SilkS")
	)
	(gr_text "17"
		(at 155.3 101.7 0)
		(layer "F.SilkS")
	)
	(gr_text "23"
		(at 146.5 110.7 0)
		(layer "F.SilkS")
	)
	(gr_text "30"
		(at 154.6 105.7 0)
		(layer "F.SilkS")
	)
	(gr_text "9"
		(at 150.8 108.1 0)
		(layer "F.SilkS")
	)
	(gr_text "4"
		(at 139.2 104 0)
		(layer "F.SilkS")
	)
	(gr_text "28"
		(at 154.5 110.6 0)
		(layer "F.SilkS")
	)
	(gr_text "25"
		(at 157.5 109.1 0)
		(layer "F.SilkS")
	)
	(gr_text "26"
		(at 157.6 106.5 0)
		(layer "F.SilkS")
	)
	(gr_text "2"
		(at 142.4 108.1 0)
		(layer "F.SilkS")
	)
	(gr_text "11"
		(at 151 103.3 0)
		(layer "F.SilkS")
	)
	(gr_text "8"
		(at 149.7 110.6 0)
		(layer "F.SilkS")
	)
	(gr_text "HART LAB - 32CH EIB"
		(at 143.8 113.2 0)
		(layer "F.SilkS")
	)
	(gr_text "12"
		(at 151 101.2 0)
		(layer "F.SilkS")
	)
	(gr_text "10"
		(at 150.6 105.8 0)
		(layer "F.SilkS")
	)
	(gr_text "18"
		(at 142.4 101.6 0)
		(layer "F.SilkS")
	)
)
