<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="48.26" x2="36.5" y2="48.26" width="0" layer="20"/>
<wire x1="36.5" y1="48.26" x2="36.5" y2="80" width="0" layer="20"/>
<wire x1="36.5" y1="80" x2="0" y2="80" width="0" layer="20"/>
<wire x1="0" y1="80" x2="0" y2="48.26" width="0" layer="20"/>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="USB-A-H">
<description>&lt;h3&gt;USB Type 'A' Male Connector - PTH&lt;/h3&gt;
Shield pins may be grounded.
&lt;br&gt; tDocu shows plug end. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://www.4uconnector.com/online/object/4udrawing/10016.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;USB_A&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X05">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X02">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="SparkFun-Connectors" package="USB-A-H" value="USB_A_PTH_MALE">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-08367"/>
<attribute name="SF_ID" value="PRT-00437"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="pinhead" package="1X05" value="">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="69"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="pinhead" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="98"/>
<attribute name="VALUE"/>
</element>
<element name="JP3" library="pinhead" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="98"/>
<attribute name="VALUE"/>
</element>
<element name="JP4" library="pinhead" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="98"/>
<attribute name="VALUE"/>
</element>
<element name="JP5" library="pinhead" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="92"/>
<attribute name="VALUE"/>
</element>
<element name="JP6" library="pinhead" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="98"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="JP5" pad="3"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="JP5" pad="1"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="JP3" pad="2"/>
<contactref element="JP4" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="JP4" pad="2"/>
<contactref element="JP6" pad="1"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="N$5">
<contactref element="JP6" pad="2"/>
<contactref element="JP3" pad="1"/>
<contactref element="JP1" pad="4"/>
<contactref element="J1" pad="GND"/>
</signal>
<signal name="N$6">
<contactref element="JP1" pad="5"/>
<contactref element="J1" pad="VBUS"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
