(kicad_pcb (version 4) (host pcbnew 4.0.4+e1-6308~48~ubuntu16.04.1-stable)
  (general
    (links 33)
    (no_connects 0)
    (area 159.68 77.563809 211.384762 120.925001)
    (thickness 1.6)
    (drawings 26)
    (tracks 61)
    (zones 0)
    (modules 17)
    (nets 16)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.508)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 GND)
  (net 3 "Net-(D1-Pad2)")
  (net 4 GNDA)
  (net 5 "Net-(J1-Pad3)")
  (net 6 "Net-(J1-Pad2)")
  (net 7 "Net-(J1-Pad6)")
  (net 8 "Net-(J1-Pad5)")
  (net 9 +12V)
  (net 10 "Net-(K1-Pad14)")
  (net 11 "Net-(K1-Pad3)")
  (net 12 "Net-(Q1-Pad1)")
  (net 13 "Net-(R1-Pad2)")
  (net 14 "Net-(J2-Pad2)")
  (net 15 "Net-(J2-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.508)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net GND)
    (add_net GNDA)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(K1-Pad14)")
    (add_net "Net-(K1-Pad3)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(R1-Pad2)")
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 582BFE78)
    (at 189.865 82.55)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C1 (at 0 -2.3) (layer F.SilkS))
    (fp_text value 22uF (at -0.635 -3.81) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:SMB_Handsoldering (layer B.Cu) (tedit 582BFEA6)
    (at 190.5 95.885)
    (descr "Diode SMB Handsoldering")
    (tags "Diode SMB Handsoldering")
    (attr smd)
    (fp_text reference D1 (at 17.145 -0.635) (layer B.SilkS))
    (fp_text value 1N4001 (at 17.78 -5.08) (layer B.Fab))
    (fp_text user K (at 16.51 -1.905) (layer B.SilkS))
    (fp_text user A (at 16.51 -1.905) (layer B.SilkS))
    (pad 1 smd rect (at -2.70002 0) (size 3.50012 2.30124) (layers B.Cu B.Paste B.Mask)
      (net 9 +12V))
    (pad 2 smd rect (at 2.70002 0) (size 3.50012 2.30124) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(D1-Pad2)"))
    (model Diodes_SMD.3dshapes/SMB_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 180))
    )
  )
  (module Libraries:NRJ6HF (layer F.Cu) (tedit 582BFE3F)
    (at 174.625 111.76)
    (fp_text reference J1 (at 0.635 1.27) (layer F.SilkS))
    (fp_text value JACK_TRS_6PINS (at -1.27 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 7.239 -4.2418) (size 2.54 2.54) (drill 1.4986) (layers *.Cu *.Mask)
      (net 4 GNDA))
    (pad 3 thru_hole circle (at 7.239 -10.5918) (size 2.54 2.54) (drill 1.4986) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad3)"))
    (pad 2 thru_hole circle (at 7.239 -16.9418) (size 2.54 2.54) (drill 1.4986) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad2)"))
    (pad 4 thru_hole circle (at -4.191 -4.2418) (size 2.54 2.54) (drill 1.4986) (layers *.Cu *.Mask)
      (net 4 GNDA))
    (pad 6 thru_hole circle (at -4.191 -10.5918) (size 2.54 2.54) (drill 1.4986) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad6)"))
    (pad 5 thru_hole circle (at -4.191 -16.9418) (size 2.54 2.54) (drill 1.4986) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad5)"))
    (pad "" np_thru_hole circle (at 7.239 -7.4422) (size 2.032 2.032) (drill 2.032) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -4.191 -7.4422) (size 2.032 2.032) (drill 2.032) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 5.1054 -13.7922) (size 2.9972 2.9972) (drill 2.9972) (layers *.Cu *.Mask))
  )
  (module Libraries:Relay_HK19F (layer F.Cu) (tedit 582BFE92)
    (at 190.5 99.695 270)
    (fp_text reference K1 (at -1.905 -16.51 270) (layer F.SilkS))
    (fp_text value RELAY_2RT (at 0.635 -16.51 270) (layer F.Fab))
    (pad 8 thru_hole circle (at -7.62 -3.81 270) (size 2 2) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(D1-Pad2)"))
    (pad 9 thru_hole circle (at -7.62 3.81 270) (size 2 2) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 9 +12V))
    (pad 12 thru_hole circle (at 0 -3.81 270) (size 2 2) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(J2-Pad2)"))
    (pad 5 thru_hole circle (at 0 3.81 270) (size 2 2) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(J2-Pad3)"))
    (pad 14 thru_hole circle (at 5.08 -3.81 270) (size 2 2) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(K1-Pad14)"))
    (pad 3 thru_hole circle (at 5.08 3.81 270) (size 2 2) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(K1-Pad3)"))
    (pad 16 thru_hole circle (at 10.16 -3.81 270) (size 2 2) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(J1-Pad2)"))
    (pad 1 thru_hole circle (at 10.16 3.81 270) (size 2 2) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(J1-Pad3)"))
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 582BFE44)
    (at 174.625 83.82 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at -1.905 -13.97 90) (layer F.SilkS))
    (fp_text value CONN_01X02 (at -3.81 -12.7 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 +12V))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 582BFEBA)
    (at 198.12 97.155 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at 0.635 10.16 90) (layer F.SilkS))
    (fp_text value CONN_01X03 (at -1.905 9.525 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 14 "Net-(J2-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 "Net-(J2-Pad3)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 GNDA))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 582BFE3A)
    (at 165.735 98.425)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P3 (at 0 15.24) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 3.81 15.24) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad5)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad6)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 GNDA))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 582BFE90)
    (at 198.755 92.075 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at -8.255 -0.635 180) (layer F.SilkS))
    (fp_text value MMBT3904 (at 0 13.335 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.00076 180) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at 0.95 1.00076 180) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 0 -0.99822 180) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D1-Pad2)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 582BFE52)
    (at 181.61 85.725 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R1 (at -0.635 -20.955 90) (layer F.SilkS))
    (fp_text value 200k (at -5.08 -20.32 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 9 +12V))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 582BFE8B)
    (at 184.15 85.725 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R2 (at -6.985 -2.54 270) (layer F.SilkS))
    (fp_text value 10k (at 2.54 22.86 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R1-Pad2)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 582BFE87)
    (at 195.58 86.36 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R3 (at 7.62 -1.905 90) (layer F.SilkS))
    (fp_text value 4.7k (at 0 11.43 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 9 +12V))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(Q1-Pad1)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer B.Cu) (tedit 582BFE61)
    (at 189.23 106.68 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R4 (at 7.62 2.54 270) (layer B.SilkS))
    (fp_text value 150 (at 6.985 -2.54 270) (layer B.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(K1-Pad3)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 4 GNDA))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer B.Cu) (tedit 582BFE64)
    (at 191.77 106.68 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R5 (at 6.985 2.54 270) (layer B.SilkS))
    (fp_text value 150 (at 7.62 -1.905 270) (layer B.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(K1-Pad14)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 4 GNDA))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 582BFE82)
    (at 189.865 86.995)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1 (at 0.635 -7.62) (layer F.SilkS))
    (fp_text value TL7700 (at 1.27 -8.255) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at -2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R1-Pad2)"))
    (pad 3 smd rect (at -2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at -2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 +12V))
    (pad 6 smd rect (at 2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at 2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at 2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(Q1-Pad1)"))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 582BFE45)
    (at 167.005 85.09)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF** (at -0.635 -5.08) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at 5.715 28.575) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 582BFE6E)
    (at 201.295 85.09)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF** (at 0 -5.715) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at -2.54 -6.35) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Libraries:PJ321-3.5mm-TRS (layer F.Cu) (tedit 582BFE68)
    (at 200.66 111.76 90)
    (fp_text reference J2 (at 5.715 7.62 90) (layer F.SilkS))
    (fp_text value JACK_TRS_6PINS (at 6.35 6.985 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 3.5 -2.9 90) (size 2 1.6) (drill oval 1.4 1) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(J2-Pad2)"))
    (pad 2 thru_hole oval (at 3.5 2.9 90) (size 2 1.6) (drill oval 1.4 1) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(J2-Pad2)"))
    (pad 3 thru_hole oval (at 11 -2.3 90) (size 2 1.6) (drill oval 1.4 1) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(J2-Pad3)"))
    (pad 1 thru_hole oval (at 11 2.3 90) (size 2 1.6) (drill oval 1.4 1) (layers *.Cu *.Mask F.SilkS)
      (net 4 GNDA))
    (pad "" np_thru_hole circle (at 7 -2.5 90) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 7 2.5 90) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask F.SilkS))
  )
  (gr_text mark@halibut.com (at 197.485 87.63) (layer B.SilkS))
  (gr_text "Mark Smith 2016 BY-NC-SA" (at 197.485 85.725) (layer B.SilkS))
  (gr_text "Pop Stopper v1.0a" (at 197.485 83.82) (layer B.SilkS))
  (gr_text G (at 203.2 94.615) (layer F.SilkS))
  (gr_text R (at 200.66 94.615) (layer F.SilkS))
  (gr_text L (at 198.12 94.615) (layer F.SilkS))
  (gr_text GND (at 165.735 95.885) (layer F.SilkS))
  (gr_text Right (at 165.735 93.98) (layer F.SilkS))
  (gr_text Left (at 165.735 92.075) (layer F.SilkS))
  (gr_text "2x 150" (at 190.5 102.87) (layer B.SilkS))
  (gr_text TL7700 (at 189.865 90.17) (layer F.SilkS))
  (gr_text 3904 (at 201.93 92.075) (layer F.SilkS))
  (gr_text 4.7k (at 195.58 90.17) (layer F.SilkS))
  (gr_text 22uF (at 193.04 81.915) (layer F.SilkS))
  (gr_text 10k (at 184.785 89.535) (layer F.SilkS))
  (gr_text 200k (at 181.61 89.535) (layer F.SilkS))
  (gr_text GND (at 177.8 86.36) (layer F.SilkS))
  (gr_text +12v (at 173.355 86.36) (layer F.SilkS))
  (gr_line (start 205.105 81.28) (end 203.2 81.28) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 205.105 111.76) (end 205.105 81.28) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 203.2 111.76) (end 205.105 111.76) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 163.195 111.76) (end 184.15 111.76) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 163.195 81.28) (end 163.195 111.76) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 203.2 81.28) (end 163.195 81.28) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 202.565 111.76) (end 203.2 111.76) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 184.15 111.76) (end 202.565 111.76) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 171.45 81.28) (xy 171.45 90.17) (xy 184.785 90.17) (xy 184.785 97.155) (xy 195.58 97.155)
        (xy 195.58 93.98) (xy 202.565 93.98) (xy 202.565 88.9) (xy 197.485 88.9) (xy 197.485 81.28)
      )
    )
  )
  (zone (net 9) (net_name +12V) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 171.45 81.28) (xy 171.45 90.17) (xy 184.785 90.17) (xy 184.785 97.155) (xy 195.58 97.155)
        (xy 195.58 93.98) (xy 202.565 93.98) (xy 202.565 88.9) (xy 197.485 88.9) (xy 197.485 81.28)
      )
    )
  )
  (zone (net 4) (net_name GNDA) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 163.195 90.805) (xy 184.15 90.805) (xy 184.15 97.79) (xy 196.215 97.79) (xy 196.215 94.615)
        (xy 205.105 94.615) (xy 205.105 111.76) (xy 163.195 111.76)
      )
    )
  )
)
