<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.1.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="19" y2="0" width="0" layer="20"/>
<wire x1="19" y1="0" x2="19" y2="45" width="0" layer="20"/>
<wire x1="19" y1="45" x2="0" y2="45" width="0" layer="20"/>
<wire x1="0" y1="45" x2="0" y2="0" width="0" layer="20"/>
<text>mojo 
power module rev 1.0</text>
</plain>
<libraries>
<library name="Capacitors">
<packages>
<package name="CAPC3225X280">
<description>3225 Metric (1210 Standard),
Chip: 3.20 X 2.50 X 2.80 mm body
&lt;p&gt;Chip package with body size 3.20 X 2.50 X 2.80 mm&lt;/p&gt;</description>
</package>
<package name="CAPC3216X180">
<description>Chip, 3.20 X 1.60 X 1.80 mm body
&lt;p&gt;Chip package with body size 3.20 X 1.60 X 1.80 mm&lt;/p&gt;</description>
</package>
<package name="CAPAE1030X1050">
<description>ECAP (Aluminum Electrolytic Capacitor), 10.30 X 10.50 mm body
&lt;p&gt;ECAP (Aluminum Electrolytic Capacitor) package with body size 10.30 X 10.50 mm&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="Resistors">
<packages>
<package name="RESC1005X35">
<description>Chip, 1.00 X 0.50 X 0.35 mm body
&lt;p&gt;Chip package with body size 1.00 X 0.50 X 0.35 mm&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="Integrated_Circuits">
<packages>
<package name="RLX0041A">
<description>RLX0041A Footprint for the TI LMZM33606</description>
</package>
</packages>
</library>
<library name="Connectors">
<description>Various connectors</description>
<packages>
<package name="HDRRA6W64P254_2X3_762X254X483B">
<description>Double-row, 6-pin Pin Header (Male) Right Angle, 2.54 mm (0.10 in) row pitch, 2.54 mm (0.10 in) col pitch, 5.84 mm mating length, 7.62 X 2.54 X 4.83 mm body
&lt;p&gt;Double-row (2X3), 6-pin Pin Header (Male) Right Angle package with 2.54 mm (0.10 in) row pitch, 2.54 mm (0.10 in) col pitch, 0.64 mm lead width, 3.05 mm tail length and 5.84 mm mating length with body size 7.62 X 2.54 X 4.83 mm, pin pattern - zigzag from bottom left&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="Capacitors" package="CAPC3225X280" value="100uF">
<attribute name="DIGI-KEY_PRT_NUM" value="445-1437-1-ND"/>
<attribute name="MFG" value="TDK"/>
<attribute name="MFG_PRT_NUM" value="C3225X5R0J107M250AC"/>
<attribute name="NAME"/>
<attribute name="PACKAGE_M" value="3225"/>
<attribute name="TOLERANCE" value="20%"/>
<attribute name="VOLTAGE" value="6.3V"/>
</element>
<element name="C2" library="Capacitors" package="CAPC3225X280" value="100uF">
<attribute name="DIGI-KEY_PRT_NUM" value="445-1437-1-ND"/>
<attribute name="MFG" value="TDK"/>
<attribute name="MFG_PRT_NUM" value="C3225X5R0J107M250AC"/>
<attribute name="NAME"/>
<attribute name="PACKAGE_M" value="3225"/>
<attribute name="TOLERANCE" value="20%"/>
<attribute name="VOLTAGE" value="6.3V"/>
</element>
<element name="C3" library="Capacitors" package="CAPC3225X280" value="100uF">
<attribute name="DIGI-KEY_PRT_NUM" value="445-1437-1-ND"/>
<attribute name="MFG" value="TDK"/>
<attribute name="MFG_PRT_NUM" value="C3225X5R0J107M250AC"/>
<attribute name="NAME"/>
<attribute name="PACKAGE_M" value="3225"/>
<attribute name="TOLERANCE" value="20%"/>
<attribute name="VOLTAGE" value="6.3V"/>
</element>
<element name="C4" library="Capacitors" package="CAPC3216X180" value="10uF">
<attribute name="DIGI-KEY_PRT_NUM" value="490-12456-1-ND"/>
<attribute name="MFG" value="Murata Electronics North America"/>
<attribute name="MFG_PRT_NUM" value="GRT31CR61H106KE01L"/>
<attribute name="NAME"/>
<attribute name="PACKAGE_M" value="3216"/>
<attribute name="TOLERANCE" value="10%"/>
<attribute name="VOLTAGE" value="50V"/>
</element>
<element name="C5" library="Capacitors" package="CAPC3216X180" value="10uF">
<attribute name="DIGI-KEY_PRT_NUM" value="490-12456-1-ND"/>
<attribute name="MFG" value="Murata Electronics North America"/>
<attribute name="MFG_PRT_NUM" value="GRT31CR61H106KE01L"/>
<attribute name="NAME"/>
<attribute name="PACKAGE_M" value="3216"/>
<attribute name="TOLERANCE" value="10%"/>
<attribute name="VOLTAGE" value="50V"/>
</element>
<element name="C6" library="Capacitors" package="CAPAE1030X1050" value="100uF">
<attribute name="DIGI-KEY_PRT_NUM" value="PCE3942CT-ND"/>
<attribute name="MFG" value="Panasonic"/>
<attribute name="MFG-PRT-NUM" value="EEE-1JA101P"/>
<attribute name="NAME"/>
<attribute name="PACKAGE_M" value="10.3x10.3"/>
<attribute name="TOLERANCE" value="20"/>
<attribute name="VOLTAGE" value="63V"/>
</element>
<element name="R1" library="Resistors" package="RESC1005X35" value="40.2K">
<attribute name="DIGI-KEY_PRT_NUM" value="541-4097-1-ND"/>
<attribute name="MFG" value="Vishay Dale"/>
<attribute name="MFG_PRT_NUM" value="CRCW040240K2FKEDC"/>
<attribute name="NAME"/>
<attribute name="PACKAGE_M" value="1005"/>
<attribute name="POWER" value="0.063W"/>
<attribute name="TOLERANCE" value="1%"/>
</element>
<element name="R2" library="Resistors" package="RESC1005X35" value="10k">
<attribute name="DIGI-KEY_PRT_NUM" value="541-2954-1-ND"/>
<attribute name="MFG" value="Vishay Dale"/>
<attribute name="MFG_PRT_NUM" value="CRCW040210K0FKEE"/>
<attribute name="NAME"/>
<attribute name="PACKAGE_M" value="1005"/>
<attribute name="POWER" value="0.063W"/>
<attribute name="TOLERANCE" value="1%"/>
</element>
<element name="U1" library="Integrated_Circuits" package="RLX0041A" value="LMZM33606">
<attribute name="NAME"/>
</element>
<element name="J1" library="Connectors" package="HDRRA6W64P254_2X3_762X254X483B" value="">
<attribute name="COL" value="3"/>
<attribute name="DIGI-KEY_PRT_NUM" value="609-3352-ND"/>
<attribute name="MFG" value="Amphenol FCI"/>
<attribute name="MFG_PRT_NUM" value="68021-406HLF"/>
<attribute name="NAME"/>
<attribute name="PINS" value="6"/>
<attribute name="PITCH" value="2.54"/>
<attribute name="ROW" value="2"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="Resistors" package="RESC1005X35" value="64.9k">
<attribute name="DIGI-KEY_PRT_NUM" value="311-64.9KLRCT-ND"/>
<attribute name="MFG" value="Yageo"/>
<attribute name="MFG_PRT_NUM" value="RC0402FR-0764K9L"/>
<attribute name="NAME"/>
<attribute name="PACKAGE_M" value="1005"/>
<attribute name="POWER" value="0.063W"/>
<attribute name="TOLERANCE" value="1%"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="AGND">
<contactref element="U1" pad="16"/>
<contactref element="U1" pad="21"/>
<contactref element="R2" pad="1"/>
<contactref element="U1" pad="19"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="GND">
<contactref element="U1" pad="8"/>
<contactref element="U1" pad="11"/>
<contactref element="U1" pad="23"/>
<contactref element="U1" pad="30"/>
<contactref element="U1" pad="34"/>
<contactref element="U1" pad="35"/>
<contactref element="U1" pad="38"/>
<contactref element="U1" pad="40"/>
<contactref element="U1" pad="41"/>
<contactref element="U1" pad="10"/>
<contactref element="C6" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="J1" pad="4"/>
<contactref element="J1" pad="2"/>
<contactref element="J1" pad="3"/>
<contactref element="U1" pad="PGND$1"/>
<contactref element="U1" pad="PGND$2"/>
<contactref element="U1" pad="PGND$19"/>
<contactref element="U1" pad="PGND$20"/>
<contactref element="U1" pad="PGND$15"/>
<contactref element="U1" pad="PGND$16"/>
<contactref element="U1" pad="PGND$17"/>
<contactref element="U1" pad="PGND$18"/>
<contactref element="U1" pad="PGND$21"/>
<contactref element="U1" pad="PGND$22"/>
<contactref element="U1" pad="PGND$23"/>
<contactref element="U1" pad="PGND$24"/>
<contactref element="U1" pad="PGND$25"/>
<contactref element="U1" pad="PGND$6"/>
<contactref element="U1" pad="PGND$7"/>
<contactref element="U1" pad="PGND$8"/>
<contactref element="U1" pad="PGND$9"/>
<contactref element="U1" pad="PGND$10"/>
<contactref element="U1" pad="PGND$11"/>
<contactref element="U1" pad="PGND$12"/>
<contactref element="U1" pad="PGND$13"/>
<contactref element="U1" pad="PGND$14"/>
<contactref element="U1" pad="PGND$3"/>
<contactref element="U1" pad="PGND$4"/>
<contactref element="U1" pad="PGND$5"/>
</signal>
<signal name="V+">
<contactref element="U1" pad="22"/>
<contactref element="C6" pad="1"/>
<contactref element="U1" pad="39"/>
<contactref element="U1" pad="20"/>
<contactref element="C4" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="J1" pad="1"/>
<contactref element="U1" pad="VIN$1"/>
<contactref element="U1" pad="VIN$2"/>
</signal>
<signal name="+5V">
<contactref element="U1" pad="37"/>
<contactref element="U1" pad="24"/>
<contactref element="C1" pad="1"/>
<contactref element="U1" pad="25"/>
<contactref element="U1" pad="26"/>
<contactref element="U1" pad="27"/>
<contactref element="U1" pad="28"/>
<contactref element="U1" pad="29"/>
<contactref element="U1" pad="36"/>
<contactref element="C3" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="J1" pad="6"/>
<contactref element="J1" pad="5"/>
<contactref element="U1" pad="VOUT$1"/>
<contactref element="U1" pad="VOUT$2"/>
<contactref element="U1" pad="VOUT$3"/>
<contactref element="U1" pad="VOUT$4"/>
<contactref element="U1" pad="VOUT$5"/>
<contactref element="U1" pad="VOUT$6"/>
<contactref element="U1" pad="VOUT$7"/>
<contactref element="U1" pad="VOUT$8"/>
<contactref element="U1" pad="VOUT$9"/>
<contactref element="U1" pad="VOUT$10"/>
<contactref element="U1" pad="VOUT$11"/>
</signal>
<signal name="FB">
<contactref element="U1" pad="15"/>
<contactref element="R1" pad="1"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="RT">
<contactref element="U1" pad="12"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="SW">
<contactref element="U1" pad="1"/>
<contactref element="U1" pad="33"/>
<contactref element="U1" pad="32"/>
<contactref element="U1" pad="2"/>
<contactref element="U1" pad="3"/>
<contactref element="U1" pad="4"/>
<contactref element="U1" pad="5"/>
<contactref element="U1" pad="6"/>
<contactref element="U1" pad="31"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
