<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="32" y2="0" width="0" layer="20"/>
<wire x1="32" y1="0" x2="32" y2="32" width="0" layer="20"/>
<wire x1="32" y1="32" x2="0" y2="32" width="0" layer="20"/>
<wire x1="0" y1="32" x2="0" y2="0" width="0" layer="20"/>
<hole x="2" y="2" drill="1.5"/>
<hole x="30" y="2" drill="1.5"/>
<hole x="2" y="30" drill="1.5"/>
<hole x="30" y="30" drill="1.5"/>
<text>Desgined in Thailand
By TinLethax</text>
<text>ComeNCapture 3.0</text>
<text>ComeNCapture 3.0</text>
<text>ComeNCapture 3.0</text>
<text>rev2.1</text>
<text>Designed in Thailand
By TinLethax</text>
<text>ComeNCapture 3.0</text>
</plain>
<libraries>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="2X05">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="FM25V01">
<packages>
<package name="SOIC127P601X172-8N">
<description>8-SOIC, 1.27 mm pitch, 6.02 mm span, 4.89 X 3.89 X 1.73 mm body
&lt;p&gt;8-pin SOIC package with 1.27 mm pitch, 6.02 mm span with body size 4.89 X 3.89 X 1.73 mm&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="STM8L151F3">
<packages>
<package name="UFQFPN-20">
<description>UFQFPN20 Package 3x3mm</description>
</package>
</packages>
</library>
<library name="SN74LVC157APWR">
<description>QUADRUPLE 2-LINE TO 1-LINE DATA SELECTORS/MULTIPLEXERS</description>
<packages>
<package name="SOP65P640X120-16L">
<description>16-SOP, 0.65 mm pitch, 6.40 mm span, 5.00 X 4.40 X 1.20 mm body
&lt;p&gt;16-pin SOP package with 0.65 mm pitch, 6.40 mm span with body size 5.00 X 4.40 X 1.20 mm&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="CH330">
<packages>
<package name="SOIC127P600X150-8N">
<description>8-SOIC, 1.27 mm pitch, 6.00 mm span, 4.95 X 3.95 X 1.50 mm body
&lt;p&gt;8-pin SOIC package with 1.27 mm pitch, 6.00 mm span with body size 4.95 X 3.95 X 1.50 mm&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="AMS1117">
<packages>
<package name="SOT223">
<description>&lt;b&gt;Smal Outline Transistor&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="C0603">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="C0805">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="C1206">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="testpad">
<description>&lt;b&gt;Test Pins/Pads&lt;/b&gt;&lt;p&gt;
Cream on SMD OFF.&lt;br&gt;
new: Attribute TP_SIGNAL_NAME&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TP20R">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Switches">
<description>&lt;h3&gt;SparkFun Switches, Buttons, Encoders&lt;/h3&gt;
In this library you'll find switches, buttons, joysticks, and anything that moves to create or disrupt an electrical connection.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE_SWITCH_SMD_5.2MM">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST - SMD, 5.2mm Square&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons).&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.sparkfun.com/datasheets/Components/Buttons/SMD-Button.pdf"&gt;Dimensional Drawing&lt;/a&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="TO-3227BC_LED">
<description>TO-3227BC-MRMGEE
Surface Mount Device LED
AlGaInP High Bright Red
Water Clear
AlGaInP High Bright Green</description>
<packages>
<package name="DIODFN320X270X40-4L">
<description>DFN4, 3.21 X 2.71 X 0.40 mm body
&lt;p&gt;DFN4 package with body size 3.21 X 2.71 X 0.40 mm&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="oshw">
<description>&lt;p&gt;&lt;strong&gt;Open Source Hardware PCB Logos&lt;/strong&gt;
&lt;p&gt;A simple polygon based version of the OSHWA logos for use on Eagle PCB's
&lt;p&gt;For use please refer to the OSHWA definition at &lt;a href="http://www.oshwa.org/definition/"&gt;http://www.oshwa.org/definition/&lt;/a&gt;
&lt;p&gt;Based on the NBitWonder version (&lt;a href="http://nbitwonder.com"&gt;http://nbitwonder.com&lt;/a&gt;)
&lt;p&gt;&lt;strong&gt;Andrew Cooper&lt;/strong&gt;&lt;br&gt;28Nov2016&lt;br&gt;&lt;a href="http://www.darkerview.com"&gt;www.DarkerView.com&lt;/a&gt;</description>
<packages>
<package name="OSHW_5MM">
</package>
</packages>
</library>
<library name="USB-C-Breakout">
<description>Generated from &lt;b&gt;USB-C-Breakout.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="SPARKFUN-CONNECTORS_USB-C-16P">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP1" library="pinhead" package="2X05" value="">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="35"/>
<attribute name="VALUE"/>
</element>
<element name="M0" library="FM25V01" package="SOIC127P601X172-8N" value="FM25V01">
<attribute name="NAME"/>
<attribute name="PARTNO" value="FM52V01"/>
<attribute name="VALUE"/>
</element>
<element name="M1" library="FM25V01" package="SOIC127P601X172-8N" value="FM25V01">
<attribute name="NAME"/>
<attribute name="PARTNO" value="FM52V01"/>
<attribute name="VALUE"/>
</element>
<element name="M2" library="FM25V01" package="SOIC127P601X172-8N" value="FM25V01">
<attribute name="NAME"/>
<attribute name="PARTNO" value="FM52V01"/>
<attribute name="VALUE"/>
</element>
<element name="M3" library="FM25V01" package="SOIC127P601X172-8N" value="FM25V01">
<attribute name="NAME"/>
<attribute name="PARTNO" value="FM52V01"/>
<attribute name="VALUE"/>
</element>
<element name="M4" library="FM25V01" package="SOIC127P601X172-8N" value="FM25V01">
<attribute name="NAME"/>
<attribute name="PARTNO" value="FM52V01"/>
<attribute name="VALUE"/>
</element>
<element name="M5" library="FM25V01" package="SOIC127P601X172-8N" value="FM25V01">
<attribute name="NAME"/>
<attribute name="PARTNO" value="FM52V01"/>
<attribute name="VALUE"/>
</element>
<element name="M6" library="FM25V01" package="SOIC127P601X172-8N" value="FM25V01">
<attribute name="NAME"/>
<attribute name="PARTNO" value="FM52V01"/>
<attribute name="VALUE"/>
</element>
<element name="M7" library="FM25V01" package="SOIC127P601X172-8N" value="FM25V01">
<attribute name="NAME"/>
<attribute name="PARTNO" value="FM52V01"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="STM8L151F3" package="UFQFPN-20" value="STM8L151F3"/>
<element name="U2" library="SN74LVC157APWR" package="SOP65P640X120-16L" value="SN74LVC157APWR">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U3" library="SN74LVC157APWR" package="SOP65P640X120-16L" value="SN74LVC157APWR">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U4" library="CH330" package="SOIC127P600X150-8N" value="CH330">
<attribute name="DESCRIPTION" value="CH330 Super small Serial to USB chip  "/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="SOP8"/>
<attribute name="PARTNO" value="CH330"/>
<attribute name="VALUE"/>
</element>
<element name="U5" library="AMS1117" package="SOT223" value="AMS1117">
<attribute name="NAME"/>
<attribute name="PARTNO" value="AMS1117"/>
<attribute name="VALUE"/>
</element>
<element name="USB-C" library="USB-C-Breakout" package="SPARKFUN-CONNECTORS_USB-C-16P" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-14122"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="adafruit" package="C0603" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="adafruit" package="C0603" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="adafruit" package="C0603" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="adafruit" package="C0603" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="adafruit" package="C0603" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="adafruit" package="C0603" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="adafruit" package="C0603" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="adafruit" package="C0603" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="adafruit" package="C0603" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="adafruit" package="C0603" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="adafruit" package="C0805" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="adafruit" package="C0805" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="adafruit" package="C1206" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C14" library="adafruit" package="C1206" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="adafruit" package="R0603" value="5.1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="adafruit" package="R0603" value="5.1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RST" library="testpad" package="TP20R" value="TPSQTP20R">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="2"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="SWIM" library="testpad" package="TP20R" value="TPSQTP20R">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="2"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="adafruit" package="R0603" value="4.7k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="adafruit" package="R0603" value="4.7k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S1" library="SparkFun-Switches" package="TACTILE_SWITCH_SMD_5.2MM" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="SWCH-08247"/>
<attribute name="SF_SKU" value="COM-08720"/>
<attribute name="VALUE"/>
</element>
<element name="C15" library="adafruit" package="C1206" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED" library="TO-3227BC_LED" package="DIODFN320X270X40-4L" value="TO-3227BC">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="GOLD_ORB_SM1" library="oshw" package="OSHW_5MM" value="OSHWLOGOLOGO5MM"/>
</elements>
<signals>
<signal name="B0">
<contactref element="U1" pad="PB0"/>
<contactref element="M0" pad="2"/>
</signal>
<signal name="B1">
<contactref element="U1" pad="PB1"/>
<contactref element="M1" pad="2"/>
</signal>
<signal name="B2">
<contactref element="U1" pad="PB2"/>
<contactref element="M2" pad="2"/>
</signal>
<signal name="B3">
<contactref element="U1" pad="PB3"/>
<contactref element="M3" pad="2"/>
</signal>
<signal name="B4">
<contactref element="U1" pad="PB4"/>
<contactref element="M4" pad="2"/>
</signal>
<signal name="B5">
<contactref element="U1" pad="PB5"/>
<contactref element="M5" pad="2"/>
</signal>
<signal name="B6">
<contactref element="U1" pad="PB6"/>
<contactref element="M6" pad="2"/>
</signal>
<signal name="B7">
<contactref element="U1" pad="PB7"/>
<contactref element="M7" pad="2"/>
</signal>
<signal name="/CS">
<contactref element="M1" pad="1"/>
<contactref element="M2" pad="1"/>
<contactref element="M3" pad="1"/>
<contactref element="M6" pad="1"/>
<contactref element="M5" pad="1"/>
<contactref element="M4" pad="1"/>
<contactref element="M0" pad="1"/>
<contactref element="M7" pad="1"/>
<contactref element="U2" pad="15"/>
<contactref element="U3" pad="15"/>
<contactref element="U1" pad="PC0"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="+3V3">
<contactref element="M2" pad="3"/>
<contactref element="M2" pad="7"/>
<contactref element="M2" pad="8"/>
<contactref element="M6" pad="3"/>
<contactref element="M6" pad="7"/>
<contactref element="M6" pad="8"/>
<contactref element="M5" pad="3"/>
<contactref element="M5" pad="7"/>
<contactref element="M5" pad="8"/>
<contactref element="M4" pad="3"/>
<contactref element="M4" pad="7"/>
<contactref element="M4" pad="8"/>
<contactref element="M0" pad="3"/>
<contactref element="M0" pad="7"/>
<contactref element="M0" pad="8"/>
<contactref element="M7" pad="3"/>
<contactref element="M7" pad="7"/>
<contactref element="M7" pad="8"/>
<contactref element="M1" pad="7"/>
<contactref element="M1" pad="8"/>
<contactref element="M1" pad="3"/>
<contactref element="M3" pad="3"/>
<contactref element="M3" pad="7"/>
<contactref element="M3" pad="8"/>
<contactref element="U1" pad="VDD"/>
<contactref element="U2" pad="16"/>
<contactref element="U3" pad="16"/>
<contactref element="U5" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="C11" pad="1"/>
<contactref element="U4" pad="8"/>
<contactref element="U4" pad="5"/>
<contactref element="C10" pad="1"/>
<contactref element="C13" pad="1"/>
<contactref element="C12" pad="1"/>
<contactref element="C14" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="R3" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="LED" pad="4"/>
<contactref element="LED" pad="3"/>
</signal>
<signal name="SCK">
<contactref element="M0" pad="6"/>
<contactref element="M1" pad="6"/>
<contactref element="M2" pad="6"/>
<contactref element="M3" pad="6"/>
<contactref element="M4" pad="6"/>
<contactref element="M5" pad="6"/>
<contactref element="M6" pad="6"/>
<contactref element="M7" pad="6"/>
<contactref element="U1" pad="PC4"/>
</signal>
<signal name="CMD">
<contactref element="U2" pad="2"/>
<contactref element="U2" pad="5"/>
<contactref element="U2" pad="11"/>
<contactref element="U2" pad="14"/>
<contactref element="U3" pad="2"/>
<contactref element="U3" pad="5"/>
<contactref element="U3" pad="11"/>
<contactref element="U3" pad="14"/>
<contactref element="U1" pad="PD0"/>
</signal>
<signal name="SI0">
<contactref element="U2" pad="4"/>
<contactref element="M0" pad="5"/>
</signal>
<signal name="SI1">
<contactref element="U2" pad="7"/>
<contactref element="M1" pad="5"/>
</signal>
<signal name="SI2">
<contactref element="U2" pad="9"/>
<contactref element="M2" pad="5"/>
</signal>
<signal name="SI3">
<contactref element="U2" pad="12"/>
<contactref element="M3" pad="5"/>
</signal>
<signal name="SI4">
<contactref element="U3" pad="4"/>
<contactref element="M4" pad="5"/>
</signal>
<signal name="SI5">
<contactref element="U3" pad="7"/>
<contactref element="M5" pad="5"/>
</signal>
<signal name="SI6">
<contactref element="U3" pad="9"/>
<contactref element="M6" pad="5"/>
</signal>
<signal name="SI7">
<contactref element="U3" pad="12"/>
<contactref element="M7" pad="5"/>
</signal>
<signal name="SEL">
<contactref element="U2" pad="1"/>
<contactref element="U3" pad="1"/>
<contactref element="U1" pad="PC1"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="GND">
<contactref element="U3" pad="8"/>
<contactref element="U2" pad="8"/>
<contactref element="M0" pad="4"/>
<contactref element="M1" pad="4"/>
<contactref element="M7" pad="4"/>
<contactref element="M6" pad="4"/>
<contactref element="M2" pad="4"/>
<contactref element="M5" pad="4"/>
<contactref element="M3" pad="4"/>
<contactref element="M4" pad="4"/>
<contactref element="JP1" pad="10"/>
<contactref element="C1" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="U5" pad="1"/>
<contactref element="C11" pad="2"/>
<contactref element="U4" pad="3"/>
<contactref element="C10" pad="2"/>
<contactref element="C14" pad="2"/>
<contactref element="C12" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="USB-C" pad="GND"/>
<contactref element="USB-C" pad="GND2"/>
<contactref element="R2" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="USB-C" pad="SHLD2" route="any" routetag="J1.SHLD"/>
<contactref element="USB-C" pad="SHLD8" route="any" routetag="J1.SHLD"/>
<contactref element="USB-C" pad="SHLD7" route="any" routetag="J1.SHLD"/>
<contactref element="USB-C" pad="SHLD4" route="any" routetag="J1.SHLD"/>
<contactref element="USB-C" pad="SHLD5" route="any" routetag="J1.SHLD"/>
<contactref element="USB-C" pad="SHLD6" route="any" routetag="J1.SHLD"/>
<contactref element="USB-C" pad="SHLD1" route="any" routetag="J1.SHLD"/>
<contactref element="USB-C" pad="SHLD3" route="any" routetag="J1.SHLD"/>
<contactref element="C9" pad="2"/>
<contactref element="U1" pad="VSS"/>
<contactref element="S1" pad="3"/>
<contactref element="S1" pad="4"/>
<contactref element="C15" pad="2"/>
<contactref element="JP1" pad="9"/>
<contactref element="LED" pad="1"/>
</signal>
<signal name="IN0">
<contactref element="U2" pad="3"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="IN1">
<contactref element="U2" pad="6"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="IN2">
<contactref element="U2" pad="10"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="IN3">
<contactref element="U2" pad="13"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="IN4">
<contactref element="U3" pad="3"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="IN5">
<contactref element="U3" pad="6"/>
<contactref element="JP1" pad="6"/>
</signal>
<signal name="IN6">
<contactref element="U3" pad="10"/>
<contactref element="JP1" pad="7"/>
</signal>
<signal name="IN7">
<contactref element="U3" pad="13"/>
<contactref element="JP1" pad="8"/>
</signal>
<signal name="DP">
<contactref element="USB-C" pad="B6" route="any" routetag="J1.D+"/>
<contactref element="USB-C" pad="A6" route="any" routetag="J1.D+"/>
<contactref element="U4" pad="1"/>
</signal>
<signal name="DM">
<contactref element="USB-C" pad="B7"/>
<contactref element="USB-C" pad="A7"/>
<contactref element="U4" pad="2"/>
</signal>
<signal name="MCU_TX">
<contactref element="U4" pad="7"/>
<contactref element="U1" pad="PA2"/>
</signal>
<signal name="MCU_RX">
<contactref element="U4" pad="6"/>
<contactref element="U1" pad="PA3"/>
</signal>
<signal name="5V">
<contactref element="USB-C" pad="VBUS1"/>
<contactref element="USB-C" pad="VBUS2"/>
<contactref element="U5" pad="3"/>
</signal>
<signal name="N$1">
<contactref element="USB-C" pad="A5"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="USB-C" pad="B5"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="RST">
<contactref element="U1" pad="NRST/PA1"/>
<contactref element="RST" pad="TP"/>
<contactref element="S1" pad="1"/>
<contactref element="S1" pad="2"/>
<contactref element="C15" pad="1"/>
</signal>
<signal name="SWIM">
<contactref element="U1" pad="PA0"/>
<contactref element="SWIM" pad="TP"/>
</signal>
<signal name="LED_STAT">
<contactref element="U1" pad="PC5"/>
<contactref element="LED" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
