(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 117)
    (no_connects 0)
    (area 123.924999 68.924999 176.075001 122.075001)
    (thickness 1.6)
    (drawings 24)
    (tracks 421)
    (zones 0)
    (modules 42)
    (nets 101)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.3048)
    (user_trace_width 0.254)
    (user_trace_width 0.3048)
    (user_trace_width 0.4064)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad1)")
  (net 2 +5V)
  (net 3 "Net-(D2-Pad1)")
  (net 4 "Net-(D3-Pad1)")
  (net 5 "Net-(D4-Pad1)")
  (net 6 "Net-(D5-Pad1)")
  (net 7 "Net-(D6-Pad1)")
  (net 8 "Net-(D7-Pad1)")
  (net 9 "Net-(D8-Pad1)")
  (net 10 "Net-(D9-Pad1)")
  (net 11 "Net-(D10-Pad1)")
  (net 12 "Net-(D11-Pad1)")
  (net 13 "Net-(D12-Pad1)")
  (net 14 "Net-(D13-Pad1)")
  (net 15 "Net-(D14-Pad1)")
  (net 16 "Net-(D15-Pad1)")
  (net 17 "Net-(D16-Pad1)")
  (net 18 "Net-(D17-Pad1)")
  (net 19 /A0)
  (net 20 /A1)
  (net 21 /A2)
  (net 22 GND)
  (net 23 "Net-(R1-Pad1)")
  (net 24 "Net-(R2-Pad1)")
  (net 25 "Net-(R3-Pad1)")
  (net 26 "Net-(R4-Pad1)")
  (net 27 "Net-(R5-Pad1)")
  (net 28 "Net-(R6-Pad1)")
  (net 29 "Net-(R7-Pad1)")
  (net 30 "Net-(R8-Pad1)")
  (net 31 "Net-(R9-Pad1)")
  (net 32 "Net-(R10-Pad1)")
  (net 33 "Net-(R11-Pad1)")
  (net 34 "Net-(R12-Pad1)")
  (net 35 "Net-(R13-Pad1)")
  (net 36 "Net-(R14-Pad1)")
  (net 37 "Net-(R15-Pad1)")
  (net 38 "Net-(R16-Pad1)")
  (net 39 /SCL)
  (net 40 /SDA)
  (net 41 "Net-(U1-Pad19)")
  (net 42 "Net-(U1-Pad20)")
  (net 43 "Net-(U2-Pad19)")
  (net 44 "Net-(U2-Pad20)")
  (net 45 "Net-(U3-Pad19)")
  (net 46 "Net-(U3-Pad20)")
  (net 47 "Net-(XA1-PadVIN)")
  (net 48 "Net-(XA1-Pad3V3)")
  (net 49 "Net-(XA1-PadRST1)")
  (net 50 "Net-(XA1-PadIORF)")
  (net 51 "Net-(XA1-PadD0)")
  (net 52 "Net-(XA1-PadD1)")
  (net 53 "Net-(XA1-PadD2)")
  (net 54 "Net-(XA1-PadD3)")
  (net 55 "Net-(XA1-PadD4)")
  (net 56 "Net-(XA1-PadD5)")
  (net 57 "Net-(XA1-PadD6)")
  (net 58 "Net-(XA1-PadD7)")
  (net 59 "Net-(XA1-PadD8)")
  (net 60 "Net-(XA1-PadD9)")
  (net 61 "Net-(XA1-PadD10)")
  (net 62 "Net-(XA1-PadAREF)")
  (net 63 "Net-(XA1-PadD13)")
  (net 64 "Net-(XA1-PadD12)")
  (net 65 "Net-(XA1-PadD11)")
  (net 66 "Net-(XA1-PadA4)")
  (net 67 "Net-(XA1-PadA5)")
  (net 68 /OUT1)
  (net 69 /OUT2)
  (net 70 /OUT3)
  (net 71 /OUT4)
  (net 72 /OUT5)
  (net 73 /OUT6)
  (net 74 /OUT7)
  (net 75 /OUT8)
  (net 76 /IN1)
  (net 77 /IN2)
  (net 78 /IN3)
  (net 79 /IN4)
  (net 80 /IN5)
  (net 81 /IN6)
  (net 82 /IN7)
  (net 83 /IN8)
  (net 84 /OUT9)
  (net 85 /OUT10)
  (net 86 /OUT11)
  (net 87 /OUT12)
  (net 88 /OUT13)
  (net 89 /OUT14)
  (net 90 /OUT15)
  (net 91 /OUT16)
  (net 92 /IN9)
  (net 93 /IN10)
  (net 94 /IN11)
  (net 95 /IN12)
  (net 96 /IN13)
  (net 97 /IN14)
  (net 98 /IN15)
  (net 99 /IN16)
  (net 100 /A3)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net /A0)
    (add_net /A1)
    (add_net /A2)
    (add_net /A3)
    (add_net /IN1)
    (add_net /IN10)
    (add_net /IN11)
    (add_net /IN12)
    (add_net /IN13)
    (add_net /IN14)
    (add_net /IN15)
    (add_net /IN16)
    (add_net /IN2)
    (add_net /IN3)
    (add_net /IN4)
    (add_net /IN5)
    (add_net /IN6)
    (add_net /IN7)
    (add_net /IN8)
    (add_net /IN9)
    (add_net /OUT1)
    (add_net /OUT10)
    (add_net /OUT11)
    (add_net /OUT12)
    (add_net /OUT13)
    (add_net /OUT14)
    (add_net /OUT15)
    (add_net /OUT16)
    (add_net /OUT2)
    (add_net /OUT3)
    (add_net /OUT4)
    (add_net /OUT5)
    (add_net /OUT6)
    (add_net /OUT7)
    (add_net /OUT8)
    (add_net /OUT9)
    (add_net /SCL)
    (add_net /SDA)
    (add_net GND)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D10-Pad1)")
    (add_net "Net-(D11-Pad1)")
    (add_net "Net-(D12-Pad1)")
    (add_net "Net-(D13-Pad1)")
    (add_net "Net-(D14-Pad1)")
    (add_net "Net-(D15-Pad1)")
    (add_net "Net-(D16-Pad1)")
    (add_net "Net-(D17-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(D5-Pad1)")
    (add_net "Net-(D6-Pad1)")
    (add_net "Net-(D7-Pad1)")
    (add_net "Net-(D8-Pad1)")
    (add_net "Net-(D9-Pad1)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R10-Pad1)")
    (add_net "Net-(R11-Pad1)")
    (add_net "Net-(R12-Pad1)")
    (add_net "Net-(R13-Pad1)")
    (add_net "Net-(R14-Pad1)")
    (add_net "Net-(R15-Pad1)")
    (add_net "Net-(R16-Pad1)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R4-Pad1)")
    (add_net "Net-(R5-Pad1)")
    (add_net "Net-(R6-Pad1)")
    (add_net "Net-(R7-Pad1)")
    (add_net "Net-(R8-Pad1)")
    (add_net "Net-(R9-Pad1)")
    (add_net "Net-(U1-Pad19)")
    (add_net "Net-(U1-Pad20)")
    (add_net "Net-(U2-Pad19)")
    (add_net "Net-(U2-Pad20)")
    (add_net "Net-(U3-Pad19)")
    (add_net "Net-(U3-Pad20)")
    (add_net "Net-(XA1-Pad3V3)")
    (add_net "Net-(XA1-PadA4)")
    (add_net "Net-(XA1-PadA5)")
    (add_net "Net-(XA1-PadAREF)")
    (add_net "Net-(XA1-PadD0)")
    (add_net "Net-(XA1-PadD1)")
    (add_net "Net-(XA1-PadD10)")
    (add_net "Net-(XA1-PadD11)")
    (add_net "Net-(XA1-PadD12)")
    (add_net "Net-(XA1-PadD13)")
    (add_net "Net-(XA1-PadD2)")
    (add_net "Net-(XA1-PadD3)")
    (add_net "Net-(XA1-PadD4)")
    (add_net "Net-(XA1-PadD5)")
    (add_net "Net-(XA1-PadD6)")
    (add_net "Net-(XA1-PadD7)")
    (add_net "Net-(XA1-PadD8)")
    (add_net "Net-(XA1-PadD9)")
    (add_net "Net-(XA1-PadIORF)")
    (add_net "Net-(XA1-PadRST1)")
    (add_net "Net-(XA1-PadVIN)")
  )
  (module footprints:Arduino_Uno_Shield locked (layer F.Cu) (tedit 5FB3F857)
    (at 107.25 122.25)
    (descr https://store.arduino.cc/arduino-uno-rev3)
    (fp_text reference XA1 (at 2.54 -54.356) (layer F.SilkS))
    (fp_text value Arduino_Uno_Shield (at 15.494 -54.356) (layer F.Fab))
    (pad A0 thru_hole oval (at 50.8 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 /A0))
    (pad VIN thru_hole oval (at 45.72 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 47 "Net-(XA1-PadVIN)"))
    (pad GND3 thru_hole oval (at 43.18 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 22 GND))
    (pad GND2 thru_hole oval (at 40.64 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 22 GND))
    (pad 5V1 thru_hole oval (at 38.1 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 3V3 thru_hole oval (at 35.56 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 48 "Net-(XA1-Pad3V3)"))
    (pad RST1 thru_hole oval (at 33.02 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 49 "Net-(XA1-PadRST1)"))
    (pad IORF thru_hole oval (at 30.48 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 50 "Net-(XA1-PadIORF)"))
    (pad D0 thru_hole oval (at 63.5 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 51 "Net-(XA1-PadD0)"))
    (pad D1 thru_hole oval (at 60.96 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 52 "Net-(XA1-PadD1)"))
    (pad D2 thru_hole oval (at 58.42 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 53 "Net-(XA1-PadD2)"))
    (pad D3 thru_hole oval (at 55.88 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 54 "Net-(XA1-PadD3)"))
    (pad D4 thru_hole oval (at 53.34 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 55 "Net-(XA1-PadD4)"))
    (pad D5 thru_hole oval (at 50.8 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 56 "Net-(XA1-PadD5)"))
    (pad D6 thru_hole oval (at 48.26 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 57 "Net-(XA1-PadD6)"))
    (pad D7 thru_hole oval (at 45.72 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 58 "Net-(XA1-PadD7)"))
    (pad GND1 thru_hole oval (at 26.416 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 22 GND))
    (pad D8 thru_hole oval (at 41.656 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 59 "Net-(XA1-PadD8)"))
    (pad D9 thru_hole oval (at 39.116 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 60 "Net-(XA1-PadD9)"))
    (pad D10 thru_hole oval (at 36.576 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 61 "Net-(XA1-PadD10)"))
    (pad SCL thru_hole oval (at 18.796 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 39 /SCL))
    (pad SDA thru_hole oval (at 21.336 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 40 /SDA))
    (pad AREF thru_hole oval (at 23.876 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 62 "Net-(XA1-PadAREF)"))
    (pad D13 thru_hole oval (at 28.956 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 63 "Net-(XA1-PadD13)"))
    (pad D12 thru_hole oval (at 31.496 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 64 "Net-(XA1-PadD12)"))
    (pad D11 thru_hole oval (at 34.036 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 65 "Net-(XA1-PadD11)"))
    (pad "" thru_hole oval (at 27.94 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad A1 thru_hole oval (at 53.34 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 /A1))
    (pad A2 thru_hole oval (at 55.88 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 /A2))
    (pad A3 thru_hole oval (at 58.42 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 100 /A3))
    (pad A4 thru_hole oval (at 60.96 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 66 "Net-(XA1-PadA4)"))
    (pad A5 thru_hole oval (at 63.5 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 67 "Net-(XA1-PadA5)"))
  )
  (module footprints:LED_0805_HandSoldering (layer F.Cu) (tedit 5FB314E9)
    (at 127 111.76 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference D17 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value PWR (at 3.81 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(D17-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:LED_0805_HandSoldering (layer F.Cu) (tedit 5FB31340)
    (at 171.45 111.76 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference D16 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 16 (at 3 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(D16-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:LED_0805_HandSoldering (layer F.Cu) (tedit 5FB31340)
    (at 168.91 111.76 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference D15 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 15 (at 3 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(D15-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:LED_0805_HandSoldering (layer F.Cu) (tedit 5FB31340)
    (at 166.37 111.76 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference D14 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 14 (at 3 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(D14-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:LED_0805_HandSoldering (layer F.Cu) (tedit 5FB31340)
    (at 163.83 111.76 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference D13 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 13 (at 3 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D13-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:LED_0805_HandSoldering (layer F.Cu) (tedit 5FB31340)
    (at 161.29 111.76 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference D12 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 12 (at 3 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(D12-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:LED_0805_HandSoldering (layer F.Cu) (tedit 5FB31340)
    (at 158.75 111.76 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference D11 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 11 (at 3 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(D11-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:LED_0805_HandSoldering (layer F.Cu) (tedit 5FB31340)
    (at 156.21 111.76 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference D10 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 10 (at 3 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(D10-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:LED_0805_HandSoldering (layer F.Cu) (tedit 5FB31340)
    (at 153.67 111.76 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference D9 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 9 (at 3 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D9-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:LED_0805_HandSoldering (layer F.Cu) (tedit 5FB31340)
    (at 151.13 111.76 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference D8 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 8 (at 3 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D8-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:LED_0805_HandSoldering (layer F.Cu) (tedit 5FB31340)
    (at 148.59 111.76 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference D7 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 7 (at 3 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D7-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:LED_0805_HandSoldering (layer F.Cu) (tedit 5FB31340)
    (at 146.05 111.76 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference D6 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 6 (at 3 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D6-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:LED_0805_HandSoldering (layer F.Cu) (tedit 5FB31340)
    (at 143.51 111.76 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference D5 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 5 (at 3 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D5-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:LED_0805_HandSoldering (layer F.Cu) (tedit 5FB31340)
    (at 140.97 111.76 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference D4 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 4 (at 3 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D4-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:LED_0805_HandSoldering (layer F.Cu) (tedit 5FB31340)
    (at 138.43 111.76 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference D3 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 3 (at 3 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D3-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:LED_0805_HandSoldering (layer F.Cu) (tedit 5FB31340)
    (at 135.89 111.76 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference D2 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 2 (at 3 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:LED_0805_HandSoldering (layer F.Cu) (tedit 5FB31340)
    (at 133.35 111.76 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference D1 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 1 (at 3 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0805_HandSoldering (layer F.Cu) (tedit 5FB3142F)
    (at 138.43 106.68 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 330 (at -3.75 0 270) (layer F.SilkS))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(R3-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D3-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0805_HandSoldering (layer F.Cu) (tedit 5FB3142F)
    (at 140.97 106.68 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 330 (at -3.75 0 270) (layer F.SilkS))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(R4-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D4-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0805_HandSoldering (layer F.Cu) (tedit 5FB3142F)
    (at 143.51 106.68 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 330 (at -3.75 0 270) (layer F.SilkS))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(R5-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D5-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0805_HandSoldering (layer F.Cu) (tedit 5FB3142F)
    (at 146.05 106.68 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 330 (at -3.75 0 270) (layer F.SilkS))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(R6-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D6-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0805_HandSoldering (layer F.Cu) (tedit 5FB3142F)
    (at 148.59 106.68 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R7 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 330 (at -3.75 0 270) (layer F.SilkS))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(R7-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D7-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0805_HandSoldering (layer F.Cu) (tedit 5FB3142F)
    (at 151.13 106.68 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R8 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 330 (at -3.75 0 270) (layer F.SilkS))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(R8-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D8-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0805_HandSoldering (layer F.Cu) (tedit 5FB3142F)
    (at 153.67 106.68 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R9 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 330 (at -3.75 0 270) (layer F.SilkS))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(R9-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D9-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0805_HandSoldering (layer F.Cu) (tedit 5FB3142F)
    (at 156.21 106.68 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R10 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 330 (at -3.75 0 270) (layer F.SilkS))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(R10-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(D10-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0805_HandSoldering (layer F.Cu) (tedit 5FB3142F)
    (at 158.75 106.68 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R11 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 330 (at -3.75 0 270) (layer F.SilkS))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(R11-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(D11-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0805_HandSoldering (layer F.Cu) (tedit 5FB3142F)
    (at 161.29 106.68 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R12 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 330 (at -3.75 0 270) (layer F.SilkS))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(R12-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(D12-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0805_HandSoldering (layer F.Cu) (tedit 5FB3142F)
    (at 163.83 106.68 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R13 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 330 (at -3.75 0 270) (layer F.SilkS))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(R13-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D13-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0805_HandSoldering (layer F.Cu) (tedit 5FB3142F)
    (at 166.37 106.68 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R14 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 330 (at -3.75 0 270) (layer F.SilkS))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(R14-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(D14-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0805_HandSoldering (layer F.Cu) (tedit 5FB3142F)
    (at 168.91 106.68 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R15 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 330 (at -3.75 0 270) (layer F.SilkS))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(R15-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(D15-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0805_HandSoldering (layer F.Cu) (tedit 5FB3142F)
    (at 171.45 106.68 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R16 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 330 (at -3.75 0 270) (layer F.SilkS))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(R16-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(D16-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0805_HandSoldering (layer F.Cu) (tedit 5FB3142F)
    (at 127 106.68 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R17 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 330 (at -3.75 0 270) (layer F.SilkS))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 22 GND))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(D17-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0805_HandSoldering (layer F.Cu) (tedit 5FB3142F)
    (at 135.89 106.68 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 330 (at -3.75 0 270) (layer F.SilkS))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(R2-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0805_HandSoldering (layer F.Cu) (tedit 5FB3142F)
    (at 133.35 106.68 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 330 (at -3.75 0 270) (layer F.SilkS))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0805_HandSoldering (layer F.Cu) (tedit 5FB3142F)
    (at 129.54 86.36 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R20 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value 4K7 (at -3.75 0 90) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 40 /SDA))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0805_HandSoldering (layer F.Cu) (tedit 5FB3142F)
    (at 126.365 86.36 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R19 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value 4K7 (at -3.75 0 90) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 39 /SCL))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:Pin_Header_Straight_1x18_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 127 76.2 90)
    (descr "Through hole straight pin header, 1x18, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x18 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value CONN_01X18 (at 0 45.51 90) (layer F.Fab))
    (fp_text user %R (at 0 21.59 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /A2))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 100 /A3))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 69 /OUT2))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 71 /OUT4))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 73 /OUT6))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 75 /OUT8))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 85 /OUT10))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 87 /OUT12))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 89 /OUT14))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 91 /OUT16))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 77 /IN2))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 79 /IN4))
    (pad 13 thru_hole oval (at 0 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 81 /IN6))
    (pad 14 thru_hole oval (at 0 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 83 /IN8))
    (pad 15 thru_hole oval (at 0 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 93 /IN10))
    (pad 16 thru_hole oval (at 0 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 95 /IN12))
    (pad 17 thru_hole oval (at 0 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 97 /IN14))
    (pad 18 thru_hole oval (at 0 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 99 /IN16))
  )
  (module footprints:Pin_Header_Straight_1x18_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 127 96.52 90)
    (descr "Through hole straight pin header, 1x18, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x18 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value CONN_01X18 (at 0 45.51 90) (layer F.Fab))
    (fp_text user %R (at 0 21.59 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /A0))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /A1))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 68 /OUT1))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 70 /OUT3))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 72 /OUT5))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 74 /OUT7))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 84 /OUT9))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 86 /OUT11))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 88 /OUT13))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 90 /OUT15))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 76 /IN1))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 78 /IN3))
    (pad 13 thru_hole oval (at 0 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 80 /IN5))
    (pad 14 thru_hole oval (at 0 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 82 /IN7))
    (pad 15 thru_hole oval (at 0 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 92 /IN9))
    (pad 16 thru_hole oval (at 0 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 94 /IN11))
    (pad 17 thru_hole oval (at 0 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 96 /IN13))
    (pad 18 thru_hole oval (at 0 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 98 /IN15))
  )
  (module footprints:SSOP-28_5.3x10.2mm_Pitch0.65mm (layer F.Cu) (tedit 5FB31525)
    (at 160.02 86.36 90)
    (descr "28-Lead Plastic Shrink Small Outline (SS)-5.30 mm Body [SSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U2 (at 0 -6.25 90) (layer F.SilkS))
    (fp_text value MCP23017 (at 0 6.25 90) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -3.6 -4.225 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 76 /IN1))
    (pad 2 smd rect (at -3.6 -3.575 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 78 /IN3))
    (pad 3 smd rect (at -3.6 -2.925 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 80 /IN5))
    (pad 4 smd rect (at -3.6 -2.275 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 82 /IN7))
    (pad 5 smd rect (at -3.6 -1.625 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 92 /IN9))
    (pad 6 smd rect (at -3.6 -0.975 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 94 /IN11))
    (pad 7 smd rect (at -3.6 -0.325 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 96 /IN13))
    (pad 8 smd rect (at -3.6 0.325 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 98 /IN15))
    (pad 9 smd rect (at -3.6 0.975 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 10 smd rect (at -3.6 1.625 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 22 GND))
    (pad 11 smd rect (at -3.6 2.275 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask))
    (pad 12 smd rect (at -3.6 2.925 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 39 /SCL))
    (pad 13 smd rect (at -3.6 3.575 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 40 /SDA))
    (pad 14 smd rect (at -3.6 4.225 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask))
    (pad 15 smd rect (at 3.6 4.225 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 16 smd rect (at 3.6 3.575 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 22 GND))
    (pad 17 smd rect (at 3.6 2.925 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 22 GND))
    (pad 18 smd rect (at 3.6 2.275 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 19 smd rect (at 3.6 1.625 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(U2-Pad19)"))
    (pad 20 smd rect (at 3.6 0.975 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(U2-Pad20)"))
    (pad 21 smd rect (at 3.6 0.325 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 99 /IN16))
    (pad 22 smd rect (at 3.6 -0.325 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 97 /IN14))
    (pad 23 smd rect (at 3.6 -0.975 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 95 /IN12))
    (pad 24 smd rect (at 3.6 -1.625 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 93 /IN10))
    (pad 25 smd rect (at 3.6 -2.275 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 83 /IN8))
    (pad 26 smd rect (at 3.6 -2.925 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 81 /IN6))
    (pad 27 smd rect (at 3.6 -3.575 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 79 /IN4))
    (pad 28 smd rect (at 3.6 -4.225 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 77 /IN2))
    (model ${KISYS3DMOD}/Housings_SSOP.3dshapes/SSOP-28_5.3x10.2mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:SSOP-28_5.3x10.2mm_Pitch0.65mm (layer F.Cu) (tedit 5FB31525)
    (at 142.24 86.36 90)
    (descr "28-Lead Plastic Shrink Small Outline (SS)-5.30 mm Body [SSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U1 (at 0 -6.25 90) (layer F.SilkS))
    (fp_text value MCP23017 (at 0 6.25 90) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -3.6 -4.225 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 68 /OUT1))
    (pad 2 smd rect (at -3.6 -3.575 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 70 /OUT3))
    (pad 3 smd rect (at -3.6 -2.925 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 72 /OUT5))
    (pad 4 smd rect (at -3.6 -2.275 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 74 /OUT7))
    (pad 5 smd rect (at -3.6 -1.625 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 84 /OUT9))
    (pad 6 smd rect (at -3.6 -0.975 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 86 /OUT11))
    (pad 7 smd rect (at -3.6 -0.325 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 88 /OUT13))
    (pad 8 smd rect (at -3.6 0.325 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 90 /OUT15))
    (pad 9 smd rect (at -3.6 0.975 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 10 smd rect (at -3.6 1.625 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 22 GND))
    (pad 11 smd rect (at -3.6 2.275 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask))
    (pad 12 smd rect (at -3.6 2.925 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 39 /SCL))
    (pad 13 smd rect (at -3.6 3.575 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 40 /SDA))
    (pad 14 smd rect (at -3.6 4.225 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask))
    (pad 15 smd rect (at 3.6 4.225 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 22 GND))
    (pad 16 smd rect (at 3.6 3.575 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 22 GND))
    (pad 17 smd rect (at 3.6 2.925 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 22 GND))
    (pad 18 smd rect (at 3.6 2.275 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 19 smd rect (at 3.6 1.625 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(U1-Pad19)"))
    (pad 20 smd rect (at 3.6 0.975 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(U1-Pad20)"))
    (pad 21 smd rect (at 3.6 0.325 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 91 /OUT16))
    (pad 22 smd rect (at 3.6 -0.325 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 89 /OUT14))
    (pad 23 smd rect (at 3.6 -0.975 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 87 /OUT12))
    (pad 24 smd rect (at 3.6 -1.625 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 85 /OUT10))
    (pad 25 smd rect (at 3.6 -2.275 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 75 /OUT8))
    (pad 26 smd rect (at 3.6 -2.925 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 73 /OUT6))
    (pad 27 smd rect (at 3.6 -3.575 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 71 /OUT4))
    (pad 28 smd rect (at 3.6 -4.225 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 69 /OUT2))
    (model ${KISYS3DMOD}/Housings_SSOP.3dshapes/SSOP-28_5.3x10.2mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:SSOP-28_5.3x10.2mm_Pitch0.65mm (layer B.Cu) (tedit 5FB31525)
    (at 153.67 109.22)
    (descr "28-Lead Plastic Shrink Small Outline (SS)-5.30 mm Body [SSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U3 (at 0 6.25) (layer B.SilkS))
    (fp_text value MCP23017 (at 0 -6.25) (layer B.SilkS))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -3.6 4.225) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 23 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at -3.6 3.575) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(R2-Pad1)"))
    (pad 3 smd rect (at -3.6 2.925) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 25 "Net-(R3-Pad1)"))
    (pad 4 smd rect (at -3.6 2.275) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 26 "Net-(R4-Pad1)"))
    (pad 5 smd rect (at -3.6 1.625) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 27 "Net-(R5-Pad1)"))
    (pad 6 smd rect (at -3.6 0.975) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 28 "Net-(R6-Pad1)"))
    (pad 7 smd rect (at -3.6 0.325) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 29 "Net-(R7-Pad1)"))
    (pad 8 smd rect (at -3.6 -0.325) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 30 "Net-(R8-Pad1)"))
    (pad 9 smd rect (at -3.6 -0.975) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (pad 10 smd rect (at -3.6 -1.625) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 22 GND))
    (pad 11 smd rect (at -3.6 -2.275) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask))
    (pad 12 smd rect (at -3.6 -2.925) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 39 /SCL))
    (pad 13 smd rect (at -3.6 -3.575) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 40 /SDA))
    (pad 14 smd rect (at -3.6 -4.225) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask))
    (pad 15 smd rect (at 3.6 -4.225) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (pad 16 smd rect (at 3.6 -3.575) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (pad 17 smd rect (at 3.6 -2.925) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 22 GND))
    (pad 18 smd rect (at 3.6 -2.275) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (pad 19 smd rect (at 3.6 -1.625) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 45 "Net-(U3-Pad19)"))
    (pad 20 smd rect (at 3.6 -0.975) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 46 "Net-(U3-Pad20)"))
    (pad 21 smd rect (at 3.6 -0.325) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 31 "Net-(R9-Pad1)"))
    (pad 22 smd rect (at 3.6 0.325) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 32 "Net-(R10-Pad1)"))
    (pad 23 smd rect (at 3.6 0.975) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 33 "Net-(R11-Pad1)"))
    (pad 24 smd rect (at 3.6 1.625) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 34 "Net-(R12-Pad1)"))
    (pad 25 smd rect (at 3.6 2.275) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 35 "Net-(R13-Pad1)"))
    (pad 26 smd rect (at 3.6 2.925) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 36 "Net-(R14-Pad1)"))
    (pad 27 smd rect (at 3.6 3.575) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 37 "Net-(R15-Pad1)"))
    (pad 28 smd rect (at 3.6 4.225) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 38 "Net-(R16-Pad1)"))
    (model ${KISYS3DMOD}/Housings_SSOP.3dshapes/SSOP-28_5.3x10.2mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "2  4  6  8 10 12 14 16" (at 161.29 78.74) (layer F.SilkS))
  (gr_text "2  4  6  8 10 12 14 16" (at 140.97 78.74) (layer F.SilkS))
  (gr_text "1  3  5  7  9 11 13 15" (at 161.29 93.98) (layer F.SilkS))
  (gr_text "1  3  5  7  9 11 13 15" (at 140.97 93.98) (layer F.SilkS))
  (gr_text "Rev 0.0\nNov 2020" (at 173.355 114.935) (layer B.SilkS))
  (gr_text "Universal Cable Tester" (at 151.13 117.475) (layer F.SilkS))
  (gr_line (start 126 69) (end 171 69) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 126 122) (end 127 122) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 126 120) (end 126 122) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 124 71) (end 124 120) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 173 122) (end 127 122) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 176 119) (end 173 122) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 176 84) (end 176 119) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 173 81) (end 176 84) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 173 71) (end 173 81) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 171 71) (end 171 69) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 126 71) (end 124 71) (angle 90) (layer Edge.Cuts) (width 0.15))
)
