(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "unconnected-(A1-Pad1)")
  (net 2 "unconnected-(A1-Pad2)")
  (net 3 "unconnected-(A1-Pad3)")
  (net 4 "unconnected-(A1-Pad4)")
  (net 5 "unconnected-(A1-Pad9)")
  (net 6 "unconnected-(A1-Pad15)")
  (net 7 "unconnected-(A1-Pad16)")
  (net 8 "unconnected-(A1-Pad21)")
  (net 9 "unconnected-(A1-Pad23)")
  (net 10 "unconnected-(A1-Pad28)")
  (net 11 "unconnected-(A1-Pad30)")
  (net 12 "unconnected-(A1-Pad31)")
  (net 13 "unconnected-(A1-Pad32)")
  (net 14 "+5V")
  (net 15 "GND")
  (net 16 "Net-(Q1-Pad1)")
  (net 17 "+12V")
  (net 18 "/TACH1")
  (net 19 "/TACH2")
  (net 20 "/PWM1")
  (net 21 "/PWM2")
  (net 22 "Net-(FB3-Pad1)")
  (net 23 "/5V0")
  (net 24 "/PWM")
  (net 25 "Net-(D1-Pad1)")
  (net 26 "Net-(D2-Pad1)")
  (net 27 "Net-(A1-Pad12)")
  (net 28 "/IN-")
  (net 29 "/SDA")
  (net 30 "/SCL")
  (net 31 "/12{slash}5V")
  (net 32 "/5VFAN")
  (net 33 "Net-(F1-Pad1)")
  (net 34 "Net-(F2-Pad2)")
  (net 35 "Net-(A1-Pad19)")
  (net 36 "unconnected-(A1-Pad26)")
  (net 37 "unconnected-(A1-Pad27)")
  (net 38 "unconnected-(A1-Pad20)")
  (net 39 "Net-(A1-Pad22)")
  (net 40 "Net-(A1-Pad10)")
  (net 41 "Net-(A1-Pad11)")
  (net 42 "Net-(D7-Pad1)")
  (net 43 "Net-(D4-Pad1)")
  (net 44 "Net-(D15-Pad1)")
  (net 45 "Net-(D16-Pad1)")
  (net 46 "Net-(R11-Pad1)")
  (net 47 "Net-(R12-Pad2)")
  (net 48 "Net-(R15-Pad1)")
  (net 49 "Net-(R16-Pad2)")
  (footprint "footprints:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 215.03 97.79 -90)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "Sheetfile" "Fan_Shield.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D4" (at 0 -1.43 90) (layer "F.Fab"))
    (fp_text value "OK" (at 2.935 0 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 43 "Net-(D4-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 35 "Net-(A1-Pad19)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:SW_1218_EWI" (layer "F.Cu")
    (tedit 0)
    (at 168.91 120.1439 180)
    (tags "EG1218 ")
    (property "Sheetfile" "Fan_Shield.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW1" (at 0 -2.54 unlocked) (layer "F.SilkS"))
    (fp_text value "SW_SPDT" (at 3.302 2.159 90 unlocked) (layer "F.Fab"))
    (fp_text user "*" (at -1.6129 0 180 unlocked) (layer "F.Fab"))
    (fp_text user "*" (at -1.6129 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 7.239 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.397 1.397) (drill 0.889) (layers *.Cu *.Mask)
      (net 14 "+5V") (pinfunction "A") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 2.5 180) (size 1.397 1.397) (drill 0.889) (layers *.Cu *.Mask)
      (net 22 "Net-(FB3-Pad1)") (pinfunction "B") (pintype "passive"))
    (pad "3" thru_hole circle (at 0 5 180) (size 1.397 1.397) (drill 0.889) (layers *.Cu *.Mask)
      (net 17 "+12V") (pinfunction "C") (pintype "passive"))
    (model "${KIPRJMOD}/3D/EG1218.stp"
      (offset (xyz 0 -2.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (footprint "footprints:CONN_2132250000-SD_04_MOL" (layer "F.Cu")
    (tedit 0)
    (at 188.595 117.475 180)
    (tags "2132250470 ")
    (property "Sheetfile" "Fan_Shield.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "J5" (at 0 3.795001 180 unlocked) (layer "F.Fab"))
    (fp_text value "TORSO" (at 0 -4.445 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 3.795001 180 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -2.250001 3.795001 180) (size 0.8128 2.3876) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "/TACH2") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd rect (at -0.750001 3.795001 180) (size 0.8128 2.3876) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 24 "/PWM") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" smd rect (at 0.750001 3.795001 180) (size 0.8128 2.3876) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "GND") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" smd rect (at 2.250001 3.795001 180) (size 0.8128 2.3876) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 28 "/IN-") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" smd rect (at -4.85 -1.254999 180) (size 1.8034 3.302) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "6" smd rect (at 4.85 -1.254999 180) (size 1.8034 3.302) (layers "F.Cu" "F.Paste" "F.Mask"))
    (model "${KIPRJMOD}/3D/2132250470.stp"
      (offset (xyz 0 0 4))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (footprint "footprints:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 215.0425 93.218 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Fan_Shield.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R19" (at 0 1.27 90) (layer "F.Fab"))
    (fp_text value "1K" (at 0 -1.27 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 43 "Net-(D4-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 215.03 114.3 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Fan_Shield.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R8" (at 0 1.27 90) (layer "F.Fab"))
    (fp_text value "1K" (at 0 -1.27 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 42 "Net-(D7-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 194.31 85.03 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Fan_Shield.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R14" (at 0 -2.54 -90) (layer "F.Fab"))
    (fp_text value "0.1" (at 4.505 0) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "/5VFAN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "+5V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 199.39 103.41)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Fan_Shield.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C2" (at 0 -1.43) (layer "F.Fab"))
    (fp_text value "0.1uF" (at 3.81 0) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 199.53058 81.25)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Fan_Shield.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C3" (at 0 -1.43) (layer "F.Fab"))
    (fp_text value "0.1uF" (at 3.66942 -0.065) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 187.6025 104.2675)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Fan_Shield.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R4" (at 0 -1.43) (layer "F.Fab"))
    (fp_text value "4K7" (at 0 -1.27) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "/TACH1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 208.0025 86.36)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Fan_Shield.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R15" (at 0 0) (layer "F.Fab"))
    (fp_text value "10K" (at 3.0715 0) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "Net-(R15-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 175.26 105.41)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Fan_Shield.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R2" (at 0 -1.43) (layer "F.Fab"))
    (fp_text value "10K" (at 0 -1.27) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "Net-(Q1-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 208.0025 83.82 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Fan_Shield.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R17" (at 0 0) (layer "F.Fab"))
    (fp_text value "4K7" (at -3.0715 0) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "/SDA") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:SOIC-8_3.9x4.9mm_P1.27mm" (layer "F.Cu")
    (tedit 5D9F72B1)
    (at 201.77 107.8175 180)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Sheetfile" "Fan_Shield.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U1" (at 0 0) (layer "F.Fab"))
    (fp_text value "INA219AxD" (at -0.017235 -3.620771) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.475 -1.905 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 47 "Net-(R12-Pad2)") (pinfunction "A1") (pintype "input"))
    (pad "2" smd roundrect (at -2.475 -0.635 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 46 "Net-(R11-Pad1)") (pinfunction "A0") (pintype "input"))
    (pad "3" smd roundrect (at -2.475 0.635 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "/SDA") (pinfunction "SDA") (pintype "bidirectional"))
    (pad "4" smd roundrect (at -2.475 1.905 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "/SCL") (pinfunction "SCL") (pintype "input"))
    (pad "5" smd roundrect (at 2.475 1.905 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "+5V") (pinfunction "VS") (pintype "power_in"))
    (pad "6" smd roundrect (at 2.475 0.635 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "7" smd roundrect (at 2.475 -0.635 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "/IN-") (pinfunction "IN-") (pintype "input"))
    (pad "8" smd roundrect (at 2.475 -1.905 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 31 "/12{slash}5V") (pinfunction "IN+") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 180.34 115.33 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Fan_Shield.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R20" (at 0 -1.43 90) (layer "F.Fab"))
    (fp_text value "1K" (at -0.24 1.27 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 45 "Net-(D16-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 170.5375 105.41)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Fan_Shield.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at 0 -1.43) (layer "F.Fab"))
    (fp_text value "10" (at 0.254724 -1.27) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "/PWM1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "Net-(Q1-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 173.341 117.602 180)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "Sheetfile" "Fan_Shield.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D1" (at 0 1.27) (layer "F.Fab"))
    (fp_text value "12/5" (at 0 1.59925) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "Net-(D1-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 31 "/12{slash}5V") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:R_2512_6332Metric_Pad1.40x3.35mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 194.31 85.03 -90)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Fan_Shield.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R13" (at 0 -0.635 -90) (layer "F.Fab"))
    (fp_text value "0" (at 0 0.635 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -3.05 0 270) (size 1.4 3.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.178571)
      (net 32 "/5VFAN") (pintype "passive"))
    (pad "2" smd roundrect (at 3.05 0 270) (size 1.4 3.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.178571)
      (net 14 "+5V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 174.99 108.585)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Fan_Shield.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "F1" (at 0 -1.65) (layer "F.Fab"))
    (fp_text value "1A" (at -0.238 1.651) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 33 "Net-(F1-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 31 "/12{slash}5V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 208.0025 81.28 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Fan_Shield.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R18" (at 0 0) (layer "F.Fab"))
    (fp_text value "4K7" (at -3.0715 0) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "/SCL") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 195.04 107.185276 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Fan_Shield.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R10" (at 0 -1.43 -90) (layer "F.Fab"))
    (fp_text value "0.1" (at 4.175003 -0.090329) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "/IN-") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 31 "/12{slash}5V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:D_SMA" (layer "F.Cu")
    (tedit 586432E5)
    (at 187.96 107.95 180)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (property "Sheetfile" "Fan_Shield.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D5" (at 0 -2.5 180) (layer "F.SilkS"))
    (fp_text value "KICKBACK" (at 0 2.6 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5 180) (layer "F.Fab"))
    (pad "1" smd rect (at -2 0 180) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "/12{slash}5V") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect (at 2 0 180) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "GND") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 208.28 109.855 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Fan_Shield.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R12" (at 0 0 180) (layer "F.Fab"))
    (fp_text value "10K" (at 0 -1.27 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 47 "Net-(R12-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:SOT-323_SC-70_Handsoldering" (layer "F.Cu")
    (tedit 5A02FF57)
    (at 180.54 108.57)
    (descr "SOT-323, SC-70 Handsoldering")
    (tags "SOT-323 SC-70 Handsoldering")
    (property "Sheetfile" "Fan_Shield.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Q1" (at 0 -2) (layer "F.Fab"))
    (fp_text value "BSS138" (at -0.254 -1.905 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.33 -0.65 270) (size 0.45 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "Net-(Q1-Pad1)") (pinfunction "G") (pintype "input"))
    (pad "2" smd rect (at -1.33 0.65 270) (size 0.45 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "GND") (pinfunction "S") (pintype "passive"))
    (pad "3" smd rect (at 1.33 0 270) (size 0.45 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 24 "/PWM") (pinfunction "D") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-323_SC-70.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 180.34 111.125)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Fan_Shield.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R5" (at 0 -1.43) (layer "F.Fab"))
    (fp_text value "1K" (at 2.6435 -0.000598) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "Net-(D1-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 180.34 104.2675 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Fan_Shield.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R3" (at 0 -1.43) (layer "F.Fab"))
    (fp_text value "4K7" (at -0.254724 1.27) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "/PWM") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:Molex_Pico-Clasp_501331-0407_1x04-1MP_P1.00mm_Vertical" (layer "F.Cu")
    (tedit 5B78AD89)
    (at 207.905 95.665 180)
    (descr "Molex Pico-Clasp series connector, 501331-0407 (http://www.molex.com/pdm_docs/sd/5013310207_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex Pico-Clasp side entry")
    (property "Sheetfile" "Fan_Shield.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "J2" (at 0 -3.3) (layer "F.SilkS") hide)
    (fp_text value "CAMERA" (at -0.003028 -5.005924) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -1.15) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5 1.325 180) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "/PWM") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd roundrect (at -0.5 1.325 180) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "/TACH1") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" smd roundrect (at 0.5 1.325 180) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "/5V0") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" smd roundrect (at 1.5 1.325 180) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "GND") (pinfunction "Pin_4") (pintype "passive"))
    (pad "MP" smd roundrect (at 2.8 -1.2 180) (size 1.2 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333))
    (pad "MP" smd roundrect (at -2.8 -1.2 180) (size 1.2 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333))
    (model "${KIPRJMOD}/3D/PICO-CLASP 2035610403.stp"
      (offset (xyz 0 -1 7))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (footprint "footprints:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 171.6175 98.77 -90)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "Sheetfile" "Fan_Shield.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D2" (at 0 -1.6425 90) (layer "F.Fab"))
    (fp_text value "5V" (at 2.562124 0.069136) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "Net-(D2-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "/5V0") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 179.435 89.535)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Fan_Shield.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "F2" (at 0 -1.65) (layer "F.Fab"))
    (fp_text value "1A" (at 2.905 0) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 23 "/5V0") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 34 "Net-(F2-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 208.28 107.22)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Fan_Shield.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R11" (at 0 0) (layer "F.Fab"))
    (fp_text value "10K" (at 0 -1.175) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 46 "Net-(R11-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "+5V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:Logo" (layer "F.Cu")
    (tedit 0)
    (at 179.07 83.185)
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "G***" (at 0 0) (layer "F.Fab"))
    (fp_text value "LOGO" (at 0.75 0) (layer "F.SilkS") hide)
  )
  (footprint "footprints:Fuse_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 170.529475 108.498438)
    (descr "Fuse SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "fuse handsolder")
    (property "Sheetfile" "Fan_Shield.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "FB3" (at 0 1.737562) (layer "F.SilkS"))
    (fp_text value "FerriteBead" (at 1.27 3.0575) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.875 0) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "Net-(FB3-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.875 0) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 33 "Net-(F1-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Fuse.3dshapes/Fuse_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 189.23 97.5125 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Fan_Shield.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R7" (at 0 -1.43 90) (layer "F.Fab"))
    (fp_text value "DNP" (at 0.2775 -1.27 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "/TACH1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 19 "/TACH2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl" hide
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:SOIC-8_3.9x4.9mm_P1.27mm" (layer "F.Cu")
    (tedit 5D9F72B1)
    (at 201.93 85.79 180)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Sheetfile" "Fan_Shield.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U2" (at 0 0) (layer "F.Fab"))
    (fp_text value "INA219AxD" (at 0 -3.81) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.475 -1.905 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 49 "Net-(R16-Pad2)") (pinfunction "A1") (pintype "input"))
    (pad "2" smd roundrect (at -2.475 -0.635 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "Net-(R15-Pad1)") (pinfunction "A0") (pintype "input"))
    (pad "3" smd roundrect (at -2.475 0.635 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "/SDA") (pinfunction "SDA") (pintype "bidirectional"))
    (pad "4" smd roundrect (at -2.475 1.905 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "/SCL") (pinfunction "SCL") (pintype "input"))
    (pad "5" smd roundrect (at 2.475 1.905 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "+5V") (pinfunction "VS") (pintype "power_in"))
    (pad "6" smd roundrect (at 2.475 0.635 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "7" smd roundrect (at 2.475 -0.635 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "/5VFAN") (pinfunction "IN-") (pintype "input"))
    (pad "8" smd roundrect (at 2.475 -1.905 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "+5V") (pinfunction "IN+") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:Molex_SL_171971-0004_1x04_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5DA36613)
    (at 176.7925 94.845)
    (descr "Molex Stackable Linear Connector, 171971-0004 (compatible alternatives: 171971-0104, 171971-0204), 4 Pins per row (https://www.molex.com/pdm_docs/sd/1719710002_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex SL vertical")
    (property "Sheetfile" "Fan_Shield.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J3" (at 3.81 -3.75) (layer "F.SilkS") hide)
    (fp_text value "CAMERA" (at 3.81 5.83 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.81 1.85) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0) (size 1.74 1.74) (drill 1.09) (layers *.Cu *.Mask) (roundrect_rratio 0.143678)
      (net 23 "/5V0") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0) (size 1.74 1.74) (drill 1.09) (layers *.Cu *.Mask)
      (net 24 "/PWM") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole circle (at 5.08 0) (size 1.74 1.74) (drill 1.09) (layers *.Cu *.Mask)
      (net 18 "/TACH1") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole circle (at 7.62 0) (size 1.74 1.74) (drill 1.09) (layers *.Cu *.Mask)
      (net 15 "GND") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_SL_171971-0004_1x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KIPRJMOD}/3D/SL_705430003.stp"
      (offset (xyz 3.5 0 7.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (footprint "footprints:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 171.6175 94.6825 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Fan_Shield.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R6" (at 0.0675 1.6425 90) (layer "F.Fab"))
    (fp_text value "1K" (at -0.08934 -1.184221 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "Net-(D2-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:Molex_Pico-Clasp_501331-0407_1x04-1MP_P1.00mm_Vertical" (layer "F.Cu")
    (tedit 5B78AD89)
    (at 195.58 95.845 180)
    (descr "Molex Pico-Clasp series connector, 501331-0407 (http://www.molex.com/pdm_docs/sd/5013310207_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex Pico-Clasp side entry")
    (property "Sheetfile" "Fan_Shield.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "J1" (at 0 -3.3) (layer "F.SilkS") hide)
    (fp_text value "ARM / HIP" (at 0 -4.83) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -1.15) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5 1.325 180) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "/5V0") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd roundrect (at -0.5 1.325 180) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "/PWM") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" smd roundrect (at 0.5 1.325 180) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "/TACH1") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" smd roundrect (at 1.5 1.325 180) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "GND") (pinfunction "Pin_4") (pintype "passive"))
    (pad "MP" smd roundrect (at -2.8 -1.2 180) (size 1.2 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333))
    (pad "MP" smd roundrect (at 2.8 -1.2 180) (size 1.2 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333))
    (model "${KIPRJMOD}/3D/PICO-CLASP 2035610403.stp"
      (offset (xyz 0 -1 7))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (footprint "footprints:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 208.0025 88.9 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Fan_Shield.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R16" (at 0 0 180) (layer "F.Fab"))
    (fp_text value "10K" (at -3.0715 0 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 49 "Net-(R16-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 186.69 81.915 180)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Fan_Shield.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C1" (at 0 -1.85 180) (layer "F.Fab"))
    (fp_text value "22uF" (at 0 1.85 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 180) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 32 "/5VFAN") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 180) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 15 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 178.435 120.335 90)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "Sheetfile" "Fan_Shield.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D15" (at 0 1.27 90) (layer "F.Fab"))
    (fp_text value "5V" (at 0.082732 -1.504202 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 44 "Net-(D15-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "Net-(A1-Pad10)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 178.435 115.33 -90)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "Sheetfile" "Fan_Shield.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D16" (at 0 -1.43 90) (layer "User.1"))
    (fp_text value "12V" (at 0 1.43 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 45 "Net-(D16-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "Net-(A1-Pad11)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:Fuse_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 186.45 89.535 180)
    (descr "Fuse SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "fuse handsolder")
    (property "Sheetfile" "Fan_Shield.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "FB1" (at -3.415 0) (layer "F.SilkS"))
    (fp_text value "FerriteBead" (at -0.635 -1.27) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "/5VFAN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 34 "Net-(F2-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Fuse.3dshapes/Fuse_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:SW_PUSH_6mm" (layer "F.Cu")
    (tedit 5A02FE31)
    (at 211.745 110.565 90)
    (descr "https://www.omron.com/ecb/products/pdf/en-b3f.pdf")
    (tags "tact sw push 6mm")
    (property "Sheetfile" "Fan_Shield.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW2" (at 3.25 -2 90) (layer "F.Fab"))
    (fp_text value "INPUT" (at 1.98 2.25 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.25 2.25 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 15 "GND") (pinfunction "1") (pintype "passive"))
    (pad "1" thru_hole circle (at 6.5 0 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 15 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 6.5 4.5 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 27 "Net-(A1-Pad12)") (pinfunction "2") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 4.5 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 27 "Net-(A1-Pad12)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_PUSH_6mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:R_2512_6332Metric_Pad1.40x3.35mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 195.04 106.555 -90)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Fan_Shield.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R9" (at 0 -2.62 -90) (layer "F.Fab"))
    (fp_text value "0" (at 0 1.27 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -3.05 0 270) (size 1.4 3.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.178571)
      (net 28 "/IN-") (pintype "passive"))
    (pad "2" smd roundrect (at 3.05 0 270) (size 1.4 3.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.178571)
      (net 31 "/12{slash}5V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:CONN_2132250000-SD_04_MOL" (layer "F.Cu")
    (tedit 0)
    (at 203.2 117.475 180)
    (tags "2132250470 ")
    (property "Sheetfile" "Fan_Shield.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "J7" (at 0 3.795001 180 unlocked) (layer "F.Fab"))
    (fp_text value "THIGH" (at 0 -4.445 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 3.795001 180 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -2.250001 3.795001 180) (size 0.8128 2.3876) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 28 "/IN-") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd rect (at -0.750001 3.795001 180) (size 0.8128 2.3876) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 24 "/PWM") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" smd rect (at 0.750001 3.795001 180) (size 0.8128 2.3876) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "/TACH2") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" smd rect (at 2.250001 3.795001 180) (size 0.8128 2.3876) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "GND") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" smd rect (at -4.85 -1.254999 180) (size 1.8034 3.302) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "6" smd rect (at 4.85 -1.254999 180) (size 1.8034 3.302) (layers "F.Cu" "F.Paste" "F.Mask"))
    (model "${KIPRJMOD}/3D/2132250470.stp"
      (offset (xyz 0 0 4))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (footprint "footprints:D_SMA" (layer "F.Cu")
    (tedit 586432E5)
    (at 171.45 88.9 180)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (property "Sheetfile" "Fan_Shield.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D3" (at -4.445 0 180) (layer "F.SilkS"))
    (fp_text value "KICKBACK" (at 0 2.6 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5 180) (layer "F.Fab"))
    (pad "1" smd rect (at -2 0 180) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "/5V0") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect (at 2 0 180) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "GND") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 215.03 118.985 -90)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "Sheetfile" "Fan_Shield.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D7" (at 0 -1.43 90) (layer "F.Fab"))
    (fp_text value "OK" (at 2.935 0) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 42 "Net-(D7-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "Net-(A1-Pad22)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 180.34 120.3725 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Fan_Shield.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R21" (at 0 -1.43 90) (layer "F.Fab"))
    (fp_text value "1K" (at 0.2775 -1.27 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 44 "Net-(D15-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:Arduino_UNO_R3" locked (layer "B.Cu")
    (tedit 58AB60FC)
    (at 177.165 125.73)
    (descr "Arduino UNO R3, http://www.mouser.com/pdfdocs/Gravitech_Arduino_Nano3_0.pdf")
    (tags "Arduino UNO R3")
    (property "Sheetfile" "Fan_Shield.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "A1" (at -9.525 0.635 180) (layer "F.Fab"))
    (fp_text value "Arduino_UNO_R3" (at 0 -22.86 180) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -20.32 180) (layer "B.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 1 "unconnected-(A1-Pad1)") (pinfunction "NC") (pintype "no_connect"))
    (pad "2" thru_hole oval locked (at 2.54 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 2 "unconnected-(A1-Pad2)") (pinfunction "IOREF") (pintype "output"))
    (pad "3" thru_hole oval locked (at 5.08 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 3 "unconnected-(A1-Pad3)") (pinfunction "~{RESET}") (pintype "input"))
    (pad "4" thru_hole oval locked (at 7.62 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 4 "unconnected-(A1-Pad4)") (pinfunction "3V3") (pintype "power_out"))
    (pad "5" thru_hole oval locked (at 10.16 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 14 "+5V") (pinfunction "+5V") (pintype "power_out"))
    (pad "6" thru_hole oval locked (at 12.7 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 15 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "7" thru_hole oval locked (at 15.24 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 15 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "8" thru_hole oval locked (at 17.78 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 17 "+12V") (pinfunction "VIN") (pintype "power_in"))
    (pad "9" thru_hole oval locked (at 22.86 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 5 "unconnected-(A1-Pad9)") (pinfunction "A0") (pintype "bidirectional"))
    (pad "10" thru_hole oval locked (at 25.4 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 40 "Net-(A1-Pad10)") (pinfunction "A1") (pintype "bidirectional"))
    (pad "11" thru_hole oval locked (at 27.94 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 41 "Net-(A1-Pad11)") (pinfunction "A2") (pintype "bidirectional"))
    (pad "12" thru_hole oval locked (at 30.48 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(A1-Pad12)") (pinfunction "A3") (pintype "bidirectional"))
    (pad "13" thru_hole oval locked (at 33.02 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 29 "/SDA") (pinfunction "SDA/A4") (pintype "bidirectional"))
    (pad "14" thru_hole oval locked (at 35.56 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 30 "/SCL") (pinfunction "SCL/A5") (pintype "bidirectional"))
    (pad "15" thru_hole oval locked (at 35.56 -48.26 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 6 "unconnected-(A1-Pad15)") (pinfunction "D0/RX") (pintype "bidirectional"))
    (pad "16" thru_hole oval locked (at 33.02 -48.26 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 7 "unconnected-(A1-Pad16)") (pinfunction "D1/TX") (pintype "bidirectional"))
    (pad "17" thru_hole oval locked (at 30.48 -48.26 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 18 "/TACH1") (pinfunction "D2") (pintype "bidirectional"))
    (pad "18" thru_hole oval locked (at 27.94 -48.26 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 19 "/TACH2") (pinfunction "D3") (pintype "bidirectional"))
    (pad "19" thru_hole oval locked (at 25.4 -48.26 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(A1-Pad19)") (pinfunction "D4") (pintype "bidirectional"))
    (pad "20" thru_hole oval locked (at 22.86 -48.26 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 38 "unconnected-(A1-Pad20)") (pinfunction "D5") (pintype "bidirectional"))
    (pad "21" thru_hole oval locked (at 20.32 -48.26 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 8 "unconnected-(A1-Pad21)") (pinfunction "D6") (pintype "bidirectional"))
    (pad "22" thru_hole oval locked (at 17.78 -48.26 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 39 "Net-(A1-Pad22)") (pinfunction "D7") (pintype "bidirectional"))
    (pad "23" thru_hole oval locked (at 13.72 -48.26 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 9 "unconnected-(A1-Pad23)") (pinfunction "D8") (pintype "bidirectional"))
    (pad "24" thru_hole oval locked (at 11.18 -48.26 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 20 "/PWM1") (pinfunction "D9") (pintype "bidirectional"))
    (pad "25" thru_hole oval locked (at 8.64 -48.26 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 21 "/PWM2") (pinfunction "D10") (pintype "bidirectional"))
    (pad "26" thru_hole oval locked (at 6.1 -48.26 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 36 "unconnected-(A1-Pad26)") (pinfunction "D11") (pintype "bidirectional"))
    (pad "27" thru_hole oval locked (at 3.56 -48.26 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 37 "unconnected-(A1-Pad27)") (pinfunction "D12") (pintype "bidirectional"))
    (pad "28" thru_hole oval locked (at 1.02 -48.26 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 10 "unconnected-(A1-Pad28)") (pinfunction "D13") (pintype "bidirectional"))
    (pad "29" thru_hole oval locked (at -1.52 -48.26 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 15 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "30" thru_hole oval locked (at -4.06 -48.26 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 11 "unconnected-(A1-Pad30)") (pinfunction "AREF") (pintype "input"))
    (pad "31" thru_hole oval locked (at -6.6 -48.26 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 12 "unconnected-(A1-Pad31)") (pinfunction "SDA/A4") (pintype "bidirectional"))
    (pad "32" thru_hole oval locked (at -9.14 -48.26 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 13 "unconnected-(A1-Pad32)") (pinfunction "SCL/A5") (pintype "bidirectional"))
    (model "${KICAD6_3DMODEL_DIR}/Module.3dshapes/Arduino_UNO_R3.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:Logo" (layer "B.Cu")
    (tedit 0)
    (at 198.755 91.44 180)
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "G***" (at 0 0) (layer "B.Fab"))
    (fp_text value "LOGO" (at 0.75 0) (layer "B.SilkS") hide)
  )
  (gr_arc (start 167.64 128.27) (mid 165.843949 127.526051) (end 165.1 125.73) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 215.9 125.73) (mid 215.156051 127.526051) (end 213.36 128.27) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 215.9 77.47) (end 215.9 87.63) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 165.1 77.47) (end 165.1 125.73) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 215.9 87.63) (end 218.44 90.17) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 218.44 90.17) (end 218.44 123.19) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 167.64 74.93) (end 213.36 74.93) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 213.36 74.93) (mid 215.156051 75.673949) (end 215.9 77.47) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 213.36 128.27) (end 212.09 128.27) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 167.64 128.27) (end 212.09 128.27) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 165.1 77.47) (mid 165.843949 75.673949) (end 167.64 74.93) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 218.44 123.19) (end 215.9 125.73) (layer "Edge.Cuts") (width 0.1))
  (gr_text "5V OK\nTACH1\nTACH2" (at 205.105 79.375 90) (layer "B.SilkS"))
  (gr_text "D2  TACH1\nD3  TACH2\nD4  5V {dblquote}OK{dblquote}\nD7  5/12V {dblquote}OK{dblquote}\nD9  PWM1\nD10 PWM2\nD15 5V IN\nD16 12V IN\nD17 INPUT\n\n0X40 INA219 5V\n0X41 INA219 5/12V" (at 208.28 105.41) (layer "B.SilkS"))
  (gr_text "Rev 0.0  May 25" (at 181.61 122.555) (layer "B.SilkS"))
  (gr_text "12V OK\n" (at 194.945 79.375 90) (layer "B.SilkS"))
  (gr_text "5V\nGND\nGND\n12V" (at 191.135 123.19 90) (layer "B.SilkS"))
  (gr_text "LED\nLED\nBTN\nSDA\nSCL\n" (at 208.915 123.19 90) (layer "B.SilkS"))
  (gr_text "PWM1\nPWM2" (at 189.865 79.375 90) (layer "B.SilkS"))
  (gr_text "5V0\n\nPWM\n\nTACH1\n\nGND" (at 180.975 95.885 90) (layer "B.SilkS"))
  (gr_text "5V" (at 172.72 121.92) (layer "F.SilkS"))
  (gr_text "12V" (at 173.355 113.665) (layer "F.SilkS"))
  (zone (net 15) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 220.98 132.08)
        (xy 162.56 132.08)
        (xy 162.56 73.66)
        (xy 220.98 73.66)
      )
    )
  )
  (zone (net 15) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 223.52 134.62)
        (xy 160.02 134.62)
        (xy 160.02 71.12)
        (xy 223.52 71.12)
      )
    )
  )
)
