(kicad_pcb (version 20171130) (host pcbnew "(5.1.5)-3")
  (general
    (thickness 1.6)
    (drawings 15)
    (tracks 70)
    (zones 0)
    (modules 8)
    (nets 4)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3.8 3.8)
    (pad_drill 2.2)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "GRBR/"))
  )
  (net 0 "")
  (net 1 GNDD)
  (net 2 +3V3)
  (net 3 Limit_Switch)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net GNDD)
    (add_net Limit_Switch)
  )
  (module Mini_Golden_Talon_Footprints:RPI-1133 (layer F.Cu) (tedit 5F319872)
    (at 130.66 68.94)
    (fp_text reference Co1 (at -2.5 -1.600001) (layer F.SilkS))
    (fp_text value RPI-1133 (at -2.5 -5.08) (layer F.SilkS) hide)
    (fp_text user * (at 0 0) (layer F.Fab))
    (fp_text user * (at 0 0) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
    (pad 3 thru_hole circle (at 0 -0.000001) (size 1.2954 1.2954) (drill 0.7874) (layers *.Cu *.Mask)
      (net 1 GNDD))
    (pad 2 thru_hole circle (at 0 -3.2) (size 1.2954 1.2954) (drill 0.7874) (layers *.Cu *.Mask)
      (net 2 +3V3))
    (pad 4 thru_hole circle (at -2.5 -0.000001) (size 1.2954 1.2954) (drill 0.7874) (layers *.Cu *.Mask)
      (net 3 Limit_Switch))
    (pad 5 thru_hole circle (at -5 -0.000001) (size 1.2954 1.2954) (drill 0.7874) (layers *.Cu *.Mask)
      (net 2 +3V3))
    (pad 1 thru_hole circle (at -5 -3.2) (size 1.2954 1.2954) (drill 0.7874) (layers *.Cu *.Mask)
      (net 1 GNDD))
  )
  (module "Mini_Golden_Talon_Footprints:FH19C-5S-0.5SH(99)" (layer B.Cu) (tedit 5F31D3D0)
    (at 129.13 66.97 180)
    (fp_text reference Co2 (at 1 1.5) (layer B.SilkS))
    (fp_text value RPI-1133 (at 1.5 0.5) (layer B.Fab))
    (pad 1 smd rect (at 0 0 180) (size 0.3 0.8) (layers B.Cu B.Paste B.Mask)
      (net 1 GNDD))
    (pad 2 smd rect (at 0.5 0 180) (size 0.3 0.8) (layers B.Cu B.Paste B.Mask)
      (net 2 +3V3))
    (pad 3 smd rect (at 1 0 180) (size 0.3 0.8) (layers B.Cu B.Paste B.Mask)
      (net 1 GNDD))
    (pad 4 smd rect (at 1.5 0 180) (size 0.3 0.8) (layers B.Cu B.Paste B.Mask)
      (net 3 Limit_Switch))
    (pad 5 smd rect (at 2 0 180) (size 0.3 0.8) (layers B.Cu B.Paste B.Mask)
      (net 2 +3V3))
    (model "${KIPRJMOD}/3D Files/FH19C-5S-0.5SH.igs"
      (offset (xyz 2.42 0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 90))
    )
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2_ISO14580_Pad (layer F.Cu) (tedit 56D1B4CB)
    (at 122.5 67.456)
    (descr "Mounting Hole 2.2mm, M2, ISO14580")
    (tags "mounting hole 2.2mm m2 iso14580")
    (attr virtual)
    (fp_text reference H1 (at 0 -2.9) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.8 3.8) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2_ISO14580_Pad (layer F.Cu) (tedit 56D1B4CB)
    (at 133.8 67.5)
    (descr "Mounting Hole 2.2mm, M2, ISO14580")
    (tags "mounting hole 2.2mm m2 iso14580")
    (attr virtual)
    (fp_text reference H2 (at 0 -2.9) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.8 3.8) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Mini_Golden_Talon_Footprints:RPI-1133 (layer F.Cu) (tedit 5F319872)
    (at 125.7 72.4 180)
    (fp_text reference Co3 (at -2.5 -1.600001) (layer F.SilkS))
    (fp_text value RPI-1133 (at -2.5 -5.08) (layer F.SilkS) hide)
    (fp_text user * (at 0 0) (layer F.Fab))
    (fp_text user * (at 0 0) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
    (pad 3 thru_hole circle (at 0 -0.000001 180) (size 1.2954 1.2954) (drill 0.7874) (layers *.Cu *.Mask)
      (net 1 GNDD))
    (pad 2 thru_hole circle (at 0 -3.2 180) (size 1.2954 1.2954) (drill 0.7874) (layers *.Cu *.Mask)
      (net 2 +3V3))
    (pad 4 thru_hole circle (at -2.5 -0.000001 180) (size 1.2954 1.2954) (drill 0.7874) (layers *.Cu *.Mask)
      (net 3 Limit_Switch))
    (pad 5 thru_hole circle (at -5 -0.000001 180) (size 1.2954 1.2954) (drill 0.7874) (layers *.Cu *.Mask)
      (net 2 +3V3))
    (pad 1 thru_hole circle (at -5 -3.2 180) (size 1.2954 1.2954) (drill 0.7874) (layers *.Cu *.Mask)
      (net 1 GNDD))
  )
  (module "Mini_Golden_Talon_Footprints:FH19C-5S-0.5SH(99)" (layer B.Cu) (tedit 5F31D3D0)
    (at 127.28 74.38)
    (fp_text reference Co4 (at 1 1.5) (layer B.SilkS))
    (fp_text value RPI-1133 (at 1.5 0.5) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 0.3 0.8) (layers B.Cu B.Paste B.Mask)
      (net 1 GNDD))
    (pad 2 smd rect (at 0.5 0) (size 0.3 0.8) (layers B.Cu B.Paste B.Mask)
      (net 2 +3V3))
    (pad 3 smd rect (at 1 0) (size 0.3 0.8) (layers B.Cu B.Paste B.Mask)
      (net 1 GNDD))
    (pad 4 smd rect (at 1.5 0) (size 0.3 0.8) (layers B.Cu B.Paste B.Mask)
      (net 3 Limit_Switch))
    (pad 5 smd rect (at 2 0) (size 0.3 0.8) (layers B.Cu B.Paste B.Mask)
      (net 2 +3V3))
    (model "${KIPRJMOD}/3D Files/FH19C-5S-0.5SH.igs"
      (offset (xyz 2.42 0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 90))
    )
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2_ISO14580_Pad (layer F.Cu) (tedit 56D1B4CB)
    (at 133.9 74 180)
    (descr "Mounting Hole 2.2mm, M2, ISO14580")
    (tags "mounting hole 2.2mm m2 iso14580")
    (attr virtual)
    (fp_text reference H3 (at 0 -2.9) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 3.8 3.8) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2_ISO14580_Pad (layer F.Cu) (tedit 56D1B4CB)
    (at 122.5 74.1 180)
    (descr "Mounting Hole 2.2mm, M2, ISO14580")
    (tags "mounting hole 2.2mm m2 iso14580")
    (attr virtual)
    (fp_text reference H4 (at 0 -2.9) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 3.8 3.8) (drill 2.2) (layers *.Cu *.Mask))
  )
  (gr_circle (center 123.4 70.731058) (end 123.8 70.731058) (layer Edge.Cuts) (width 0.05))
  (gr_circle (center 124.8 70.7) (end 125.2 70.7) (layer Edge.Cuts) (width 0.05))
  (gr_circle (center 126.368942 70.7) (end 126.768942 70.7) (layer Edge.Cuts) (width 0.05))
  (gr_circle (center 128 70.668942) (end 128.4 70.668942) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 133.9 70.2) (end 133.9 71.2) (layer Edge.Cuts) (width 0.05))
  (gr_circle (center 132.6 70.668942) (end 133.1 70.668942) (layer Edge.Cuts) (width 0.05))
  (gr_circle (center 130.968942 70.7) (end 131.468942 70.7) (layer Edge.Cuts) (width 0.05))
  (gr_circle (center 129.4 70.7) (end 129.8 70.7) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 122.5 70.2) (end 122.5 71.2) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 133.9 74) (end 133.9 76.8) (angle -180) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 122.5 76.8) (end 133.9 76.8) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 122.5 74) (end 122.5 71.2) (angle -180) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 122.5 64.6) (end 133.9 64.6) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 133.9 67.4) (end 133.9 70.2) (angle -180) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 122.5 67.4) (end 122.5 64.6) (angle -180) (layer Edge.Cuts) (width 0.05))
)
