(kicad_pcb (version 20171130) (host pcbnew 5.1.10-88a1d61d58~90~ubuntu21.04.1)
  (general
    (thickness 1.6)
    (drawings 15)
    (tracks 124)
    (zones 0)
    (modules 5)
    (nets 24)
  )
  (page USLetter)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.127)
    (user_trace_width 0.254)
    (user_trace_width 0.508)
    (user_trace_width 0.762)
    (trace_clearance 0.127)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.0889)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.45)
    (via_min_drill 0.2)
    (user_via 0.6096 0.3556)
    (user_via 0.8 0.4)
    (user_via 0.889 0.381)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (pad_to_paste_clearance_ratio -0.05)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /T_VCP_TX)
  (net 2 /T_VCP_RX)
  (net 3 /~RST)
  (net 4 "Net-(J1-Pad11)")
  (net 5 /T_JTDI_NC)
  (net 6 /JRCLK_NC)
  (net 7 /JTDO_SWO)
  (net 8 GND)
  (net 9 /JCLK_SWCLK)
  (net 10 /JTMS_SWDIO)
  (net 11 /T_VCC)
  (net 12 "Net-(J1-Pad2)")
  (net 13 "Net-(J1-Pad1)")
  (net 14 "Net-(J2-Pad20)")
  (net 15 /V_SUPPLY)
  (net 16 "Net-(J2-Pad18)")
  (net 17 "Net-(J2-Pad16)")
  (net 18 "Net-(J2-Pad14)")
  (net 19 /JTDI_Tx)
  (net 20 "Net-(J2-Pad3)")
  (net 21 "Net-(J2-Pad2)")
  (net 22 /DBGRQ_Rx)
  (net 23 "Net-(J4-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.127)
    (trace_width 0.254)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net /DBGRQ_Rx)
    (add_net /JCLK_SWCLK)
    (add_net /JRCLK_NC)
    (add_net /JTDI_Tx)
    (add_net /JTDO_SWO)
    (add_net /JTMS_SWDIO)
    (add_net /T_JTDI_NC)
    (add_net /T_VCC)
    (add_net /T_VCP_RX)
    (add_net /T_VCP_TX)
    (add_net /V_SUPPLY)
    (add_net /~RST)
    (add_net GND)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad11)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J2-Pad14)")
    (add_net "Net-(J2-Pad16)")
    (add_net "Net-(J2-Pad18)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad20)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J4-Pad3)")
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical locked (layer F.Cu) (tedit 59FED5CC)
    (at 85.598 87.376 90)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference J5 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value "Serial Header" (at 0 12.49 90) (layer F.Fab))
    (fp_text user %R (at 0 5.08) (layer F.Fab))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /T_VCP_RX))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /T_VCP_TX))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /T_VCC))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /V_SUPPLY))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lib_fp:PinSocket_2x10_P2.54mm_Horizontal_Overhang locked (layer F.Cu) (tedit 61563001)
    (at 76.2 76.2)
    (descr "Through hole angled socket strip, 2x10, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated")
    (tags "Through hole angled socket strip THT 2x10 2.54mm double row")
    (fp_text reference J2 (at 3.429 -11.43 90) (layer F.SilkS))
    (fp_text value J-Link (at 0 14.5) (layer F.Fab))
    (fp_text user %R (at 4.1 0 90) (layer F.Fab))
    (pad 20 thru_hole oval (at -1.27 11.43) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J2-Pad20)"))
    (pad 19 thru_hole oval (at 1.27 11.43) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /V_SUPPLY))
    (pad 18 thru_hole oval (at -1.27 8.89) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J2-Pad18)"))
    (pad 17 thru_hole oval (at 1.27 8.89) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /DBGRQ_Rx))
    (pad 16 thru_hole oval (at -1.27 6.35) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J2-Pad16)"))
    (pad 15 thru_hole oval (at 1.27 6.35) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /~RST))
    (pad 14 thru_hole oval (at -1.27 3.81) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J2-Pad14)"))
    (pad 13 thru_hole oval (at 1.27 3.81) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /JTDO_SWO))
    (pad 12 thru_hole oval (at -1.27 1.27) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 11 thru_hole oval (at 1.27 1.27) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /JRCLK_NC))
    (pad 10 thru_hole oval (at -1.27 -1.27) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 9 thru_hole oval (at 1.27 -1.27) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /JCLK_SWCLK))
    (pad 8 thru_hole oval (at -1.27 -3.81) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 7 thru_hole oval (at 1.27 -3.81) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /JTMS_SWDIO))
    (pad 6 thru_hole oval (at -1.27 -6.35) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 5 thru_hole oval (at 1.27 -6.35) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /JTDI_Tx))
    (pad 4 thru_hole oval (at -1.27 -8.89) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 3 thru_hole oval (at 1.27 -8.89) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(J2-Pad3)"))
    (pad 2 thru_hole oval (at -1.27 -11.43) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(J2-Pad2)"))
    (pad 1 thru_hole rect (at 1.27 -11.43) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /T_VCC))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x10_P2.54mm_Horizontal.wrl
      (offset (xyz 1.27 11.43 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 91.694 65.532)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J4 (at 0 -2.33) (layer F.SilkS))
    (fp_text value "Mode Jumper" (at 0 7.41) (layer F.Fab))
    (fp_text user %R (at 0 2.54 90) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(J4-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /DBGRQ_Rx))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /T_VCP_TX))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 87.884 65.532)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33) (layer F.SilkS))
    (fp_text value "Mode Jumper" (at 0 7.41) (layer F.Fab))
    (fp_text user %R (at 0 2.54 -270) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /T_JTDI_NC))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /JTDI_Tx))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /T_VCP_RX))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lib_fp:Samtec_FTSH-107-01-L-DV-K-A_2x07_P1.27mm locked (layer F.Cu) (tedit 61554151)
    (at 100.33 76.2 90)
    (descr "Samtec FTSH .050\" SMT Micro Header, FTSH-1XX-XX-XXX-DV-XXX-XXX (http://suddendocs.samtec.com/prints/ftsh-1xx-xx-xxx-dv-xxx-footprint.pdf)")
    (tags "connector Samtec HLE top entry")
    (attr smd)
    (fp_text reference J1 (at 0 -5.08 90) (layer F.SilkS))
    (fp_text value STDC14 (at 0 5.08 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 14 smd rect (at 3.81 -2.032 90) (size 0.7366 2.794) (layers F.Cu F.Paste F.Mask)
      (net 1 /T_VCP_TX))
    (pad 13 smd rect (at 3.81 2.032 90) (size 0.7366 2.794) (layers F.Cu F.Paste F.Mask)
      (net 2 /T_VCP_RX))
    (pad 12 smd rect (at 2.54 -2.032 90) (size 0.7366 2.794) (layers F.Cu F.Paste F.Mask)
      (net 3 /~RST))
    (pad 11 smd rect (at 2.54 2.032 90) (size 0.7366 2.794) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-Pad11)"))
    (pad 10 smd rect (at 1.27 -2.032 90) (size 0.7366 2.794) (layers F.Cu F.Paste F.Mask)
      (net 5 /T_JTDI_NC))
    (pad 9 smd rect (at 1.27 2.032 90) (size 0.7366 2.794) (layers F.Cu F.Paste F.Mask)
      (net 6 /JRCLK_NC))
    (pad 8 smd rect (at 0 -2.032 90) (size 0.7366 2.794) (layers F.Cu F.Paste F.Mask)
      (net 7 /JTDO_SWO))
    (pad 7 smd rect (at 0 2.032 90) (size 0.7366 2.794) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 6 smd rect (at -1.27 -2.032 90) (size 0.7366 2.794) (layers F.Cu F.Paste F.Mask)
      (net 9 /JCLK_SWCLK))
    (pad 5 smd rect (at -1.27 2.032 90) (size 0.7366 2.794) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 4 smd rect (at -2.54 -2.032 90) (size 0.7366 2.794) (layers F.Cu F.Paste F.Mask)
      (net 10 /JTMS_SWDIO))
    (pad 3 smd rect (at -2.54 2.032 90) (size 0.7366 2.794) (layers F.Cu F.Paste F.Mask)
      (net 11 /T_VCC))
    (pad 2 smd rect (at -3.81 -2.032 90) (size 0.7366 2.794) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(J1-Pad2)"))
    (pad 1 smd rect (at -3.81 2.032 90) (size 0.7366 2.794) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(J1-Pad1)"))
    (pad "" np_thru_hole circle (at 3.175 0 90) (size 1.016 1.016) (drill 1.016) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -3.175 0 90) (size 1.016 1.016) (drill 1.016) (layers *.Cu *.Mask))
    (model ${KIPRJMOD}/modules/packages3d/lib_fp.3dshapes/FTSH-107-01-L-DV-K-A.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (gr_text VCP_Rx (at 95.758 85.852 90) (layer F.SilkS))
  (gr_text VCP_Rx (at 93.218 85.852 90) (layer F.SilkS))
  (gr_text VCP_Tx (at 90.678 85.852 90) (layer F.SilkS))
  (gr_text T_VCC (at 88.138 85.852 90) (layer F.SilkS))
  (gr_text +5V (at 85.598 85.852 90) (layer F.SilkS))
  (gr_text JTAG (at 93.218 70.612) (layer F.SilkS))
  (gr_text SWD+VCP (at 93.218 65.532) (layer F.SilkS))
  (gr_text STDC14 (at 105.918 76.2 90) (layer F.SilkS))
  (gr_text J-Link (at 79.756 76.2 90) (layer F.SilkS))
  (dimension 38.1 (width 0.15) (layer Cmts.User)
    (gr_text "38.100 mm" (at 91.44 94.009999) (layer Cmts.User))
    (feature1 (pts (xy 110.49 91.44) (xy 110.49 93.29642)))
    (feature2 (pts (xy 72.39 91.44) (xy 72.39 93.29642)))
    (crossbar (pts (xy 72.39 92.709999) (xy 110.49 92.709999)))
    (arrow1a (pts (xy 110.49 92.709999) (xy 109.363496 93.29642)))
    (arrow1b (pts (xy 110.49 92.709999) (xy 109.363496 92.123578)))
    (arrow2a (pts (xy 72.39 92.709999) (xy 73.516504 93.29642)))
    (arrow2b (pts (xy 72.39 92.709999) (xy 73.516504 92.123578)))
  )
  (dimension 27.94 (width 0.15) (layer Cmts.User)
    (gr_text "27.940 mm" (at 68.550001 76.2 270) (layer Cmts.User))
    (feature1 (pts (xy 71.12 90.17) (xy 69.26358 90.17)))
    (feature2 (pts (xy 71.12 62.23) (xy 69.26358 62.23)))
    (crossbar (pts (xy 69.850001 62.23) (xy 69.850001 90.17)))
    (arrow1a (pts (xy 69.850001 90.17) (xy 69.26358 89.043496)))
    (arrow1b (pts (xy 69.850001 90.17) (xy 70.436422 89.043496)))
    (arrow2a (pts (xy 69.850001 62.23) (xy 69.26358 63.356504)))
    (arrow2b (pts (xy 69.850001 62.23) (xy 70.436422 63.356504)))
  )
  (gr_line (start 107.95 90.17) (end 72.39 90.17) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 107.95 62.23) (end 107.95 90.17) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 72.39 62.23) (end 107.95 62.23) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 72.39 62.23) (end 72.39 90.17) (layer Edge.Cuts) (width 0.05))
  (zone (net 8) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 107.95 90.17) (xy 72.39 90.17) (xy 72.39 62.23) (xy 107.95 62.23)
      )
    )
  )
  (zone (net 8) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 107.95 90.17) (xy 72.39 90.17) (xy 72.39 62.23) (xy 107.95 62.23)
      )
    )
  )
)
