(kicad_pcb (version 20171130) (host pcbnew "(5.1.6)-1")
  (general
    (thickness 1.6)
    (drawings 10)
    (tracks 26)
    (zones 0)
    (modules 12)
    (nets 11)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad9)")
  (net 2 "Net-(J1-Pad5)")
  (net 3 "Net-(J1-Pad2)")
  (net 4 "Net-(J1-Pad1)")
  (net 5 "Net-(J1-Pad7)")
  (net 6 "Net-(J1-Pad10)")
  (net 7 "Net-(J1-Pad6)")
  (net 8 "Net-(J1-Pad3)")
  (net 9 "Net-(J1-Pad8)")
  (net 10 "Net-(J1-Pad4)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J1-Pad9)")
  )
  (module Connector_DebugEdge:DebugEdge_URL_Silk (layer B.Cu) (tedit 5F4720B6)
    (at 151.5 98.5 270)
    (fp_text reference Ref** (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value Val** (at 0 0 270) (layer B.SilkS) hide)
  )
  (module Connector_Pin:Pin_D1.0mm_L10.0mm (layer F.Cu) (tedit 5A1DC084)
    (at 154 106 90)
    (descr "solder Pin_ diameter 1.0mm, hole diameter 1.0mm (press fit), length 10.0mm")
    (tags "solder Pin_ press fit")
    (fp_text reference TP10 (at 0 2.25 90) (layer F.SilkS))
    (fp_text value TestPoint (at 0 -2.05 90) (layer F.Fab))
    (fp_text user %R (at 0 2.25 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad10)"))
  )
  (module Connector_Pin:Pin_D1.0mm_L10.0mm (layer F.Cu) (tedit 5A1DC084)
    (at 149 106 90)
    (descr "solder Pin_ diameter 1.0mm, hole diameter 1.0mm (press fit), length 10.0mm")
    (tags "solder Pin_ press fit")
    (fp_text reference TP9 (at 0 2.25 90) (layer F.SilkS))
    (fp_text value TestPoint (at 0 -2.05 90) (layer F.Fab))
    (fp_text user %R (at 0 2.25 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad9)"))
  )
  (module Connector_Pin:Pin_D1.0mm_L10.0mm (layer F.Cu) (tedit 5A1DC084)
    (at 154 92 90)
    (descr "solder Pin_ diameter 1.0mm, hole diameter 1.0mm (press fit), length 10.0mm")
    (tags "solder Pin_ press fit")
    (fp_text reference TP8 (at 0 2.25 90) (layer F.SilkS))
    (fp_text value TestPoint (at 0 -2.05 90) (layer F.Fab))
    (fp_text user %R (at 0 2.25 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad8)"))
  )
  (module Connector_Pin:Pin_D1.0mm_L10.0mm (layer F.Cu) (tedit 5A1DC084)
    (at 149 92 90)
    (descr "solder Pin_ diameter 1.0mm, hole diameter 1.0mm (press fit), length 10.0mm")
    (tags "solder Pin_ press fit")
    (fp_text reference TP7 (at 0 2.25 90) (layer F.SilkS))
    (fp_text value TestPoint (at 0 -2.05 90) (layer F.Fab))
    (fp_text user %R (at 0 2.25 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad7)"))
  )
  (module Connector_Pin:Pin_D1.0mm_L10.0mm (layer F.Cu) (tedit 5A1DC084)
    (at 154 102.5 90)
    (descr "solder Pin_ diameter 1.0mm, hole diameter 1.0mm (press fit), length 10.0mm")
    (tags "solder Pin_ press fit")
    (fp_text reference TP6 (at 0 2.25 90) (layer F.SilkS))
    (fp_text value TestPoint (at 0 -2.05 90) (layer F.Fab))
    (fp_text user %R (at 0 2.25 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad6)"))
  )
  (module Connector_Pin:Pin_D1.0mm_L10.0mm (layer F.Cu) (tedit 5A1DC084)
    (at 149 102.5 90)
    (descr "solder Pin_ diameter 1.0mm, hole diameter 1.0mm (press fit), length 10.0mm")
    (tags "solder Pin_ press fit")
    (fp_text reference TP5 (at 0 2.25 90) (layer F.SilkS))
    (fp_text value TestPoint (at 0 -2.05 90) (layer F.Fab))
    (fp_text user %R (at 0 2.25 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad5)"))
  )
  (module Connector_Pin:Pin_D1.0mm_L10.0mm (layer F.Cu) (tedit 5A1DC084)
    (at 154 99 90)
    (descr "solder Pin_ diameter 1.0mm, hole diameter 1.0mm (press fit), length 10.0mm")
    (tags "solder Pin_ press fit")
    (fp_text reference TP4 (at 0 2.25 90) (layer F.SilkS))
    (fp_text value TestPoint (at 0 -2.05 90) (layer F.Fab))
    (fp_text user %R (at 0 2.25 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad4)"))
  )
  (module Connector_Pin:Pin_D1.0mm_L10.0mm (layer F.Cu) (tedit 5A1DC084)
    (at 154 95.5 90)
    (descr "solder Pin_ diameter 1.0mm, hole diameter 1.0mm (press fit), length 10.0mm")
    (tags "solder Pin_ press fit")
    (fp_text reference TP3 (at 0 2.25 90) (layer F.SilkS))
    (fp_text value TestPoint (at 0 -2.05 90) (layer F.Fab))
    (fp_text user %R (at 0 2.25 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad3)"))
  )
  (module Connector_Pin:Pin_D1.0mm_L10.0mm (layer F.Cu) (tedit 5A1DC084)
    (at 149 99 90)
    (descr "solder Pin_ diameter 1.0mm, hole diameter 1.0mm (press fit), length 10.0mm")
    (tags "solder Pin_ press fit")
    (fp_text reference TP2 (at 0 2.25 90) (layer F.SilkS))
    (fp_text value TestPoint (at 0 -2.05 90) (layer F.Fab))
    (fp_text user %R (at 0 2.25 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad2)"))
  )
  (module Connector_Pin:Pin_D1.0mm_L10.0mm (layer F.Cu) (tedit 5A1DC084)
    (at 149 95.5 90)
    (descr "solder Pin_ diameter 1.0mm, hole diameter 1.0mm (press fit), length 10.0mm")
    (tags "solder Pin_ press fit")
    (fp_text reference TP1 (at 0 2.25 90) (layer F.SilkS))
    (fp_text value TestPoint (at 0 -2.05 90) (layer F.Fab))
    (fp_text user %R (at 0 2.25 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad1)"))
  )
  (module Connector_DebugEdge:DebugEdge_2x05_Target (layer F.Cu) (tedit 5F47DF5F)
    (at 142 99 270)
    (fp_text reference J1 (at -5.5 -2.5 180) (layer F.SilkS))
    (fp_text value DebugEdge_02x05 (at 0 2 90) (layer F.Fab))
    (fp_arc (start -1 -2.8) (end -1.3 -2.8) (angle 180) (layer Edge.Cuts) (width 0.05))
    (fp_line (start -0.7 0) (end 5 0) (layer Edge.Cuts) (width 0.05))
    (fp_line (start -5 0) (end -1.3 0) (layer Edge.Cuts) (width 0.05))
    (fp_line (start -0.7 -2.8) (end -0.7 0) (layer Edge.Cuts) (width 0.05))
    (fp_line (start -1.3 0) (end -1.3 -2.8) (layer Edge.Cuts) (width 0.05))
    (pad 9 smd rect (at 4 -2.5 90) (size 1 4) (layers F.Cu F.Mask)
      (net 1 "Net-(J1-Pad9)"))
    (pad 5 smd rect (at 2 -2.5 90) (size 1 4) (layers F.Cu F.Mask)
      (net 2 "Net-(J1-Pad5)"))
    (pad 2 smd rect (at 0 -2.5 90) (size 1 4) (layers F.Cu F.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (pad 1 smd rect (at -2 -2.5 90) (size 1 4) (layers F.Cu F.Mask)
      (net 4 "Net-(J1-Pad1)"))
    (pad 7 smd rect (at -4 -2.5 90) (size 1 4) (layers F.Cu F.Mask)
      (net 5 "Net-(J1-Pad7)"))
    (pad 10 smd rect (at 4 -2.5 90) (size 1 4) (layers B.Cu B.Mask)
      (net 6 "Net-(J1-Pad10)"))
    (pad 6 smd rect (at 2 -2.5 90) (size 1 4) (layers B.Cu B.Mask)
      (net 7 "Net-(J1-Pad6)"))
    (pad 3 smd rect (at -2 -2.5 90) (size 1 4) (layers B.Cu B.Mask)
      (net 8 "Net-(J1-Pad3)"))
    (pad 8 smd rect (at -4 -2.5 90) (size 1 4) (layers B.Cu B.Mask)
      (net 9 "Net-(J1-Pad8)"))
    (pad 4 smd rect (at 0 -2.5 90) (size 1 4) (layers B.Cu B.Mask)
      (net 10 "Net-(J1-Pad4)"))
  )
  (gr_text "Test\nRev0" (at 144.5 106) (layer F.SilkS))
  (gr_arc (start 144 106.5) (end 142 106.5) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 156 106.5) (end 156 108.5) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 156 91.5) (end 158 91.5) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 144 91.5) (end 144 89.5) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 142 91.5) (end 142 94) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 142 106.5) (end 142 104) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 158 91.5) (end 158 106.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 144 89.5) (end 156 89.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 144 108.5) (end 156 108.5) (layer Edge.Cuts) (width 0.05))
)
