(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(1 "In1.Cu" signal)
		(2 "In2.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "prepreg")
				(thickness 0.1)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In1.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 2"
				(type "core")
				(thickness 1.24)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In2.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 3"
				(type "prepreg")
				(thickness 0.1)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "gerbers/")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "/-5V")
	(net 3 "/+5V")
	(net 4 "/VBIAS")
	(net 5 "Net-(P1-In)")
	(net 6 "Net-(U2-IN-)")
	(net 7 "Net-(U2-OUT)")
	(net 8 "Net-(U1-OUT)")
	(net 9 "unconnected-(J2-Pad1)")
	(net 10 "/LED+")
	(net 11 "Net-(U1-IN-)")
	(net 12 "Net-(J2-Pad10)")
	(net 13 "Net-(J3-Pad10)")
	(net 14 "Net-(U2-IN+)")
	(net 15 "Net-(U1-IN+)")
	(net 16 "unconnected-(J3-Pad1)")
	(net 17 "/TH+")
	(net 18 "Net-(J4-Pad1)")
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 149.25 115.36 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R3"
			(at 0 -1.17 90)
			(layer "F.SilkS")
		)
		(property "Value" "9.09"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Gerard readout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 15 "Net-(U1-IN+)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Samtec:CON20_2X10_DVU_MLE_SAI"
		(layer "F.Cu")
		(at 144.725 108.75 90)
		(tags "MLE-110-01-G-DV ")
		(property "Reference" "J2"
			(at 0.7 -3.8 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "MLE-110-01-G-DV"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_Samtec:CON20_2X10_DVU_MLE_SAI"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "MLE-110-01-G-DV"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CON20_2X10_DVU_MLE_SAI CON20_2X10_DVU_MLE_SAI-M CON20_2X10_DVU_MLE_SAI-L")
		(sheetname "Root")
		(sheetfile "Gerard readout.kicad_sch")
		(attr smd)
		(fp_text user "2"
			(at 5.60959 -1.84785 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "20"
			(at -5.60959 -1.84785 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "1"
			(at 5.60959 1.84785 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "19"
			(at -5.60959 1.84785 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "1"
			(at 5.60959 1.84785 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "2"
			(at 5.60959 -1.84785 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "19"
			(at -5.60959 1.84785 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "20"
			(at -5.60959 -1.84785 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 4.499991 1.84785 90)
			(size 0.3556 1.3335)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "unconnected-(J2-Pad1)")
			(pinfunction "1")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at 4.499991 -1.84785 90)
			(size 0.3556 1.3335)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 17 "/TH+")
			(pinfunction "2")
			(pintype "unspecified")
		)
		(pad "3" smd rect
			(at 3.499993 1.84785 90)
			(size 0.3556 1.3335)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "3")
			(pintype "unspecified")
		)
		(pad "4" smd rect
			(at 3.499993 -1.84785 90)
			(size 0.3556 1.3335)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "/VBIAS")
			(pinfunction "4")
			(pintype "unspecified")
		)
		(pad "5" smd rect
			(at 2.499995 1.84785 90)
			(size 0.3556 1.3335)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 12 "Net-(J2-Pad10)")
			(pinfunction "5")
			(pintype "unspecified")
		)
		(pad "6" smd rect
			(at 2.499995 -1.84785 90)
			(size 0.3556 1.3335)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 12 "Net-(J2-Pad10)")
			(pinfunction "6")
			(pintype "unspecified")
		)
		(pad "7" smd rect
			(at 1.499997 1.84785 90)
			(size 0.3556 1.3335)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "/VBIAS")
			(pinfunction "7")
			(pintype "unspecified")
		)
		(pad "8" smd rect
			(at 1.499997 -1.84785 90)
			(size 0.3556 1.3335)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "/VBIAS")
			(pinfunction "8")
			(pintype "unspecified")
		)
		(pad "9" smd rect
			(at 0.499999 1.84785 90)
			(size 0.3556 1.3335)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 12 "Net-(J2-Pad10)")
			(pinfunction "9")
			(pintype "unspecified")
		)
		(pad "10" smd rect
			(at 0.499999 -1.84785 90)
			(size 0.3556 1.3335)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 12 "Net-(J2-Pad10)")
			(pinfunction "10")
			(pintype "unspecified")
		)
		(pad "11" smd rect
			(at -0.499999 1.84785 90)
			(size 0.3556 1.3335)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "/VBIAS")
			(pinfunction "11")
			(pintype "unspecified")
		)
		(pad "12" smd rect
			(at -0.499999 -1.84785 90)
			(size 0.3556 1.3335)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "/VBIAS")
			(pinfunction "12")
			(pintype "unspecified")
		)
		(pad "13" smd rect
			(at -1.499997 1.84785 90)
			(size 0.3556 1.3335)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 12 "Net-(J2-Pad10)")
			(pinfunction "13")
			(pintype "unspecified")
		)
		(pad "14" smd rect
			(at -1.499997 -1.84785 90)
			(size 0.3556 1.3335)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 12 "Net-(J2-Pad10)")
			(pinfunction "14")
			(pintype "unspecified")
		)
		(pad "15" smd rect
			(at -2.499995 1.84785 90)
			(size 0.3556 1.3335)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "/VBIAS")
			(pinfunction "15")
			(pintype "unspecified")
		)
		(pad "16" smd rect
			(at -2.499995 -1.84785 90)
			(size 0.3556 1.3335)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "/VBIAS")
			(pinfunction "16")
			(pintype "unspecified")
		)
		(pad "17" smd rect
			(at -3.499993 1.84785 90)
			(size 0.3556 1.3335)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 12 "Net-(J2-Pad10)")
			(pinfunction "17")
			(pintype "unspecified")
		)
		(pad "18" smd rect
			(at -3.499993 -1.84785 90)
			(size 0.3556 1.3335)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 12 "Net-(J2-Pad10)")
			(pinfunction "18")
			(pintype "unspecified")
		)
		(pad "19" smd rect
			(at -4.499991 1.84785 90)
			(size 0.3556 1.3335)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "/VBIAS")
			(pinfunction "19")
			(pintype "unspecified")
		)
		(pad "20" smd rect
			(at -4.499991 -1.84785 90)
			(size 0.3556 1.3335)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "20")
			(pintype "unspecified")
		)
		(model "/Users/ldi00a/Downloads/MLE_110_01_G_DV_K/MLE-110-01-G-DV.step"
			(offset
				(xyz 0 0 0.1)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 145.75 101.6 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C1"
			(at -0.85 1.25 90)
			(layer "F.SilkS")
		)
		(property "Value" "3.9pF"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Gerard readout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "Net-(U2-IN-)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "Net-(U2-OUT)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 154.5 101.95)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C5"
			(at 0 -1.68 0)
			(layer "F.SilkS")
		)
		(property "Value" "1 µF KGM43FR72A105KV"
			(at 0 1.68 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "Root")
		(sheetfile "Gerard readout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "/VBIAS")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 153.2 116.35 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C8"
			(at -0.95 1.45 90)
			(layer "F.SilkS")
		)
		(property "Value" "3.9pF"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Gerard readout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 11 "Net-(U1-IN-)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "Net-(U1-OUT)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_0603_1608Metric"
		(layer "F.Cu")
		(at 149.25 112.7 -90)
		(descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "L2"
			(at -2.2 -0.05 90)
			(layer "F.SilkS")
		)
		(property "Value" "220nH"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Inductor_SMD:L_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "Root")
		(sheetfile "Gerard readout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 270)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 13 "Net-(J3-Pad10)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0 270)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 15 "Net-(U1-IN+)")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 151.65 116.5 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R14"
			(at -0.85 -1 90)
			(layer "F.SilkS")
		)
		(property "Value" "301"
			(at 0 1.17 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Gerard readout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 11 "Net-(U1-IN-)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "Net-(U1-OUT)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Samtec:CON20_2X10_DVU_MLE_SAI"
		(layer "F.Cu")
		(at 153.825 108.75 90)
		(tags "MLE-110-01-G-DV ")
		(property "Reference" "J3"
			(at 0 3.55 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "MLE-110-01-G-DV"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_Samtec:CON20_2X10_DVU_MLE_SAI"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "MLE-110-01-G-DV"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CON20_2X10_DVU_MLE_SAI CON20_2X10_DVU_MLE_SAI-M CON20_2X10_DVU_MLE_SAI-L")
		(sheetname "Root")
		(sheetfile "Gerard readout.kicad_sch")
		(attr smd)
		(fp_text user "20"
			(at -5.60959 -1.84785 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "1"
			(at 5.60959 1.84785 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "19"
			(at -5.7 1.84785 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "2"
			(at 5.60959 -1.84785 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "20"
			(at -5.60959 -1.84785 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "2"
			(at 5.60959 -1.84785 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "19"
			(at -5.60959 1.84785 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "1"
			(at 5.60959 1.84785 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 4.499991 1.84785 90)
			(size 0.3556 1.3335)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 16 "unconnected-(J3-Pad1)")
			(pinfunction "1")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at 4.499991 -1.84785 90)
			(size 0.3556 1.3335)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "/LED+")
			(pinfunction "2")
			(pintype "unspecified")
		)
		(pad "3" smd rect
			(at 3.499993 1.84785 90)
			(size 0.3556 1.3335)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "3")
			(pintype "unspecified")
		)
		(pad "4" smd rect
			(at 3.499993 -1.84785 90)
			(size 0.3556 1.3335)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "/VBIAS")
			(pinfunction "4")
			(pintype "unspecified")
		)
		(pad "5" smd rect
			(at 2.499995 1.84785 90)
			(size 0.3556 1.3335)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 13 "Net-(J3-Pad10)")
			(pinfunction "5")
			(pintype "unspecified")
		)
		(pad "6" smd rect
			(at 2.499995 -1.84785 90)
			(size 0.3556 1.3335)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 13 "Net-(J3-Pad10)")
			(pinfunction "6")
			(pintype "unspecified")
		)
		(pad "7" smd rect
			(at 1.499997 1.84785 90)
			(size 0.3556 1.3335)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "/VBIAS")
			(pinfunction "7")
			(pintype "unspecified")
		)
		(pad "8" smd rect
			(at 1.499997 -1.84785 90)
			(size 0.3556 1.3335)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "/VBIAS")
			(pinfunction "8")
			(pintype "unspecified")
		)
		(pad "9" smd rect
			(at 0.499999 1.84785 90)
			(size 0.3556 1.3335)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 13 "Net-(J3-Pad10)")
			(pinfunction "9")
			(pintype "unspecified")
		)
		(pad "10" smd rect
			(at 0.499999 -1.84785 90)
			(size 0.3556 1.3335)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 13 "Net-(J3-Pad10)")
			(pinfunction "10")
			(pintype "unspecified")
		)
		(pad "11" smd rect
			(at -0.499999 1.84785 90)
			(size 0.3556 1.3335)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "/VBIAS")
			(pinfunction "11")
			(pintype "unspecified")
		)
		(pad "12" smd rect
			(at -0.499999 -1.84785 90)
			(size 0.3556 1.3335)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "/VBIAS")
			(pinfunction "12")
			(pintype "unspecified")
		)
		(pad "13" smd rect
			(at -1.499997 1.84785 90)
			(size 0.3556 1.3335)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 13 "Net-(J3-Pad10)")
			(pinfunction "13")
			(pintype "unspecified")
		)
		(pad "14" smd rect
			(at -1.499997 -1.84785 90)
			(size 0.3556 1.3335)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 13 "Net-(J3-Pad10)")
			(pinfunction "14")
			(pintype "unspecified")
		)
		(pad "15" smd rect
			(at -2.499995 1.84785 90)
			(size 0.3556 1.3335)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "/VBIAS")
			(pinfunction "15")
			(pintype "unspecified")
		)
		(pad "16" smd rect
			(at -2.499995 -1.84785 90)
			(size 0.3556 1.3335)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "/VBIAS")
			(pinfunction "16")
			(pintype "unspecified")
		)
		(pad "17" smd rect
			(at -3.499993 1.84785 90)
			(size 0.3556 1.3335)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 13 "Net-(J3-Pad10)")
			(pinfunction "17")
			(pintype "unspecified")
		)
		(pad "18" smd rect
			(at -3.499993 -1.84785 90)
			(size 0.3556 1.3335)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 13 "Net-(J3-Pad10)")
			(pinfunction "18")
			(pintype "unspecified")
		)
		(pad "19" smd rect
			(at -4.499991 1.84785 90)
			(size 0.3556 1.3335)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "/VBIAS")
			(pinfunction "19")
			(pintype "unspecified")
		)
		(pad "20" smd rect
			(at -4.499991 -1.84785 90)
			(size 0.3556 1.3335)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "20")
			(pintype "unspecified")
		)
		(model "/Users/ldi00a/Downloads/MLE_110_01_G_DV_K/MLE-110-01-G-DV.step"
			(offset
				(xyz 0 0 0.1)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_0603_1608Metric"
		(layer "F.Cu")
		(at 149.2 105.9 90)
		(descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "L1"
			(at -2.05 -0.05 90)
			(layer "F.SilkS")
		)
		(property "Value" "220nH"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Inductor_SMD:L_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "Root")
		(sheetfile "Gerard readout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 90)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 12 "Net-(J2-Pad10)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0 90)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 14 "Net-(U2-IN+)")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 149.25 103.14 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R5"
			(at -0.14 -1.15 90)
			(layer "F.SilkS")
		)
		(property "Value" "9.09"
			(at 0 1.17 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Gerard readout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 14 "Net-(U2-IN+)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 142.375 102.15)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C4"
			(at -0.325 -1.3 0)
			(layer "F.SilkS")
		)
		(property "Value" "100nF GRJ188R72A104KE11D"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Gerard readout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "/VBIAS")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 147.15 101.51 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R7"
			(at -0.04 -1.15 90)
			(layer "F.SilkS")
		)
		(property "Value" "301"
			(at 0 1.17 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Gerard readout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "Net-(U2-IN-)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "Net-(U2-OUT)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-6"
		(layer "B.Cu")
		(at 149.2 102.5)
		(descr "SOT, 6 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "U2"
			(at 0.1 -2.25 0)
			(layer "B.SilkS")
		)
		(property "Value" "ADA4895-1ARJZ-R7"
			(at 0 -2.4 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "ADA4895-1ARJZ-R7"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "RJ_6_ADI RJ_6_ADI-M RJ_6_ADI-L")
		(sheetname "Root")
		(sheetfile "Gerard readout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 0.95)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 7 "Net-(U2-OUT)")
			(pinfunction "OUT")
			(pintype "output")
		)
		(pad "2" smd roundrect
			(at -1.1375 0)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 2 "/-5V")
			(pinfunction "VS-")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -1.1375 -0.95)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 14 "Net-(U2-IN+)")
			(pinfunction "IN+")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at 1.1375 -0.95)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 6 "Net-(U2-IN-)")
			(pinfunction "IN-")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at 1.1375 0)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "/+5V")
			(pinfunction "*DISABLE")
			(pintype "unspecified")
		)
		(pad "6" smd roundrect
			(at 1.1375 0.95)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "/+5V")
			(pinfunction "VS+")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "B.Cu")
		(at 148.2 111.8 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R15"
			(at -0.4 -1.1 90)
			(layer "B.SilkS")
		)
		(property "Value" "100"
			(at 0 -1.17 90)
			(layer "B.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Gerard readout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 8 "Net-(U1-OUT)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 5 "Net-(P1-In)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "B.Cu")
		(at 154.075 116.8)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C10"
			(at 0.025 -1.8 0)
			(layer "B.SilkS")
		)
		(property "Value" "2.2uF"
			(at 0 -1.85 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Gerard readout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.217391)
			(net 2 "/-5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.217391)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "B.Cu")
		(at 144.375 102.5 180)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C7"
			(at 0 1.85 0)
			(layer "B.SilkS")
		)
		(property "Value" "2.2uF"
			(at 0 -1.85 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Gerard readout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 180)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.217391)
			(net 2 "/-5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 180)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.217391)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "B.Cu")
		(at 153.925 103.45)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C6"
			(at 3.225 -0.2 0)
			(layer "B.SilkS")
		)
		(property "Value" "2.2uF"
			(at 0 -1.85 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Gerard readout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.217391)
			(net 3 "/+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.217391)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Samtec:CONN_TFM-104-02-L-D_SAI"
		(layer "B.Cu")
		(at 153.705 109.1855)
		(tags "TFM-104-02-L-D ")
		(property "Reference" "J4"
			(at 3.695 -4 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TFM-104-02-L-D"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Footprint" "Connector_Samtec:CONN_TFM-104-02-L-D_SAI"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "TFM-104-02-L-D"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CONN_TFM-104-02-L-D_SAI")
		(sheetname "Root")
		(sheetfile "Gerard readout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -1.905 -1.7145)
			(size 0.7366 2.921)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 18 "Net-(J4-Pad1)")
			(pinfunction "1")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at -1.905 1.7145)
			(size 0.7366 2.921)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 2 "/-5V")
			(pinfunction "2")
			(pintype "unspecified")
		)
		(pad "3" smd rect
			(at -0.635 -1.7145)
			(size 0.7366 2.921)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 3 "/+5V")
			(pinfunction "3")
			(pintype "unspecified")
		)
		(pad "4" smd rect
			(at -0.635 1.7145)
			(size 0.7366 2.921)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pinfunction "4")
			(pintype "unspecified")
		)
		(pad "5" smd rect
			(at 0.635 -1.7145)
			(size 0.7366 2.921)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pinfunction "5")
			(pintype "unspecified")
		)
		(pad "6" smd rect
			(at 0.635 1.7145)
			(size 0.7366 2.921)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 17 "/TH+")
			(pinfunction "6")
			(pintype "unspecified")
		)
		(pad "7" smd rect
			(at 1.905 -1.7145)
			(size 0.7366 2.921)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 10 "/LED+")
			(pinfunction "7")
			(pintype "unspecified")
		)
		(pad "8" smd rect
			(at 1.905 1.7145)
			(size 0.7366 2.921)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pinfunction "8")
			(pintype "unspecified")
		)
		(model "/Users/ldi00a/Downloads/TFM_104_02_L_D-2/TFM-104-02-L-D.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 148.4 108.175 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R4"
			(at 0.65 -1.15 90)
			(layer "B.SilkS")
		)
		(property "Value" "100"
			(at 0 -1.43 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Gerard readout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 4 "/VBIAS")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 18 "Net-(J4-Pad1)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "B.Cu")
		(at 145.65 117.8 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R13"
			(at 2.45 -0.1 0)
			(layer "B.SilkS")
		)
		(property "Value" "30.1"
			(at 0 -1.17 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Gerard readout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 11 "Net-(U1-IN-)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-6"
		(layer "B.Cu")
		(at 149.2 115.9 180)
		(descr "SOT, 6 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "U1"
			(at -0.05 -2.4 0)
			(layer "B.SilkS")
		)
		(property "Value" "ADA4895-1ARJZ-R7"
			(at 0 -2.4 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "ADA4895-1ARJZ-R7"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "RJ_6_ADI RJ_6_ADI-M RJ_6_ADI-L")
		(sheetname "Root")
		(sheetfile "Gerard readout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 0.95 180)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 8 "Net-(U1-OUT)")
			(pinfunction "OUT")
			(pintype "output")
		)
		(pad "2" smd roundrect
			(at -1.1375 0 180)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 2 "/-5V")
			(pinfunction "VS-")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -1.1375 -0.95 180)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 15 "Net-(U1-IN+)")
			(pinfunction "IN+")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at 1.1375 -0.95 180)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 11 "Net-(U1-IN-)")
			(pinfunction "IN-")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at 1.1375 0 180)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "/+5V")
			(pinfunction "*DISABLE")
			(pintype "unspecified")
		)
		(pad "6" smd roundrect
			(at 1.1375 0.95 180)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "/+5V")
			(pinfunction "VS+")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "B.Cu")
		(at 148.1 105.45 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R8"
			(at -0.45 1 90)
			(layer "B.SilkS")
		)
		(property "Value" "100"
			(at 0 -1.17 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Gerard readout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 7 "Net-(U2-OUT)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 5 "Net-(P1-In)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Coaxial:MCX_Molex_73415_vertical"
		(layer "B.Cu")
		(at 143.675 109.15 90)
		(property "Reference" "P1"
			(at 3.85 0.025 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "MCX_Molex_73415"
			(at 0.1 -6.6 -90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Footprint" "Connector_Coaxial:MCX_Molex_73415_vertical"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "{Value}"
			(at 51.125 259.525 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*BNC* *SMA* *SMB* *SMC* *Cinch* *LEMO* *UMRF* *MCX* *U.FL*")
		(sheetname "Root")
		(sheetfile "Gerard readout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.1 -4.8 -90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 90)
			(size 1.6 1.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 5 "Net-(P1-In)")
			(pinfunction "In")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -2.25 -2.25 90)
			(size 1.9 1.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pinfunction "Ext")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd rect
			(at -2.25 2.25 90)
			(size 1.9 1.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pinfunction "Ext")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd rect
			(at 2.25 -2.25 90)
			(size 1.9 1.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pinfunction "Ext")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd rect
			(at 2.25 2.25 90)
			(size 1.9 1.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pinfunction "Ext")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(model "/Users/ldi00a/Downloads/734151692.stp"
			(offset
				(xyz -2.95 -2.95 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "B.Cu")
		(at 153.26 101.5)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R6"
			(at 0.01 -1 0)
			(layer "B.SilkS")
		)
		(property "Value" "30.1"
			(at 0 -1.17 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Gerard readout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 6 "Net-(U2-IN-)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "B.Cu")
		(at 144.275 115.9 180)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C9"
			(at 0 1.85 0)
			(layer "B.SilkS")
		)
		(property "Value" "2.2uF"
			(at 0 -1.85 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Gerard readout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 180)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.217391)
			(net 3 "/+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 180)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.217391)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_poly
		(pts
			(xy 137.35 99.1) (xy 137.35 108.85) (xy 140.05 108.85) (xy 140.05 119.1) (xy 161.05 119.1) (xy 161.05 109.4)
			(xy 158.35 109.4) (xy 158.35 99.1)
		)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 138.9 100.65)
		(end 139.9 100.65)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 159.5 117.55)
		(end 160.5 117.55)
		(fill none)
		(layer "Edge.Cuts")
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads thru_hole_only
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 158.15 99.4) (xy 158.15 118.8) (xy 140.25 118.8) (xy 140.25 99.4)
			)
		)
	)
	(zone
		(net 4)
		(net_name "/VBIAS")
		(layer "In1.Cu")
		(hatch edge 0.5)
		(priority 2)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 140.2 99.35) (xy 158.2 99.35) (xy 158.15 118.85) (xy 140.2 118.8)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 4)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 140.25 99.4) (xy 158.15 99.4) (xy 158.2 118.8) (xy 140.3 118.8)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 5)
		(connect_pads thru_hole_only
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 140.25 99.4) (xy 158.15 99.4) (xy 158.15 118.85) (xy 140.25 118.85)
			)
		)
	)
)
