(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "USLetter")
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "VDD")
	(net 2 "Net-(J2-Pin_1)")
	(net 3 "Net-(D3-A)")
	(net 4 "Net-(U1-RB0{slash}AN12{slash}INT0)")
	(net 5 "Net-(U1-RB1{slash}AN10{slash}INT1)")
	(net 6 "Net-(D4-A)")
	(net 7 "Net-(D2-A)")
	(net 8 "Net-(J4-Pad4)")
	(net 9 "Net-(D5-K)")
	(net 10 "Net-(J3-Pad5)")
	(net 11 "Net-(D6-K)")
	(net 12 "Net-(J3-Pad4)")
	(net 13 "Net-(U1-RX{slash}DT{slash}RC7)")
	(net 14 "Net-(D1-K)")
	(net 15 "GND")
	(net 16 "Net-(D5-A)")
	(net 17 "unconnected-(U3-Pad3)")
	(net 18 "unconnected-(U1-RA2{slash}AN2{slash}Vref--Pad4)")
	(net 19 "unconnected-(U1-RB4{slash}AN11{slash}KBI0-Pad25)")
	(net 20 "unconnected-(U1-RA4{slash}T0CKI{slash}RCV-Pad6)")
	(net 21 "unconnected-(U1-~{UOE}{slash}T1OSI{slash}RC1-Pad12)")
	(net 22 "unconnected-(U1-RA3{slash}AN3{slash}Vref+-Pad5)")
	(net 23 "unconnected-(U1-VM{slash}D-{slash}RC4-Pad15)")
	(net 24 "unconnected-(U1-VP{slash}D+{slash}RC5-Pad16)")
	(net 25 "Net-(J2-Pin_5)")
	(net 26 "Net-(U1-RA6{slash}OSC2{slash}CLKO)")
	(net 27 "Net-(J2-Pin_4)")
	(net 28 "unconnected-(U1-RA0{slash}AN0-Pad2)")
	(net 29 "unconnected-(U1-RA1{slash}AN1-Pad3)")
	(net 30 "unconnected-(U1-RB5{slash}KBI1{slash}PGM-Pad26)")
	(net 31 "unconnected-(U1-RA5{slash}AN4{slash}HLVDIN-Pad7)")
	(net 32 "unconnected-(U1-CCP1{slash}RC2-Pad13)")
	(net 33 "unconnected-(U1-VUSB-Pad14)")
	(net 34 "Net-(U1-OSC1{slash}CLKI)")
	(net 35 "unconnected-(U1-T1OSO{slash}T1CKI{slash}RC0-Pad11)")
	(net 36 "unconnected-(U1-RB3{slash}AN9{slash}VPO-Pad24)")
	(net 37 "unconnected-(U1-RB2{slash}AN8{slash}INT2{slash}VMO-Pad23)")
	(net 38 "unconnected-(J2-Pin_6-Pad6)")
	(net 39 "unconnected-(J2-Pin_7-Pad7)")
	(net 40 "unconnected-(J2-Pin_8-Pad8)")
	(net 41 "unconnected-(J1-Pad3)")
	(net 42 "Net-(D1-A)")
	(net 43 "unconnected-(J3-Pad2)")
	(net 44 "unconnected-(J3-Pad3)")
	(net 45 "unconnected-(J3-Pad1)")
	(net 46 "unconnected-(J4-Pad3)")
	(net 47 "Net-(C6-Pad1)")
	(net 48 "unconnected-(J4-Pad1)")
	(net 49 "unconnected-(J3-SHLD-Pad6)")
	(net 50 "Net-(J4-SHLD)")
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 62.42 69.5)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R5"
			(at 0.08 -2 0)
			(layer "F.SilkS")
		)
		(property "Value" "220"
			(at 5.08 2.37 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "PCB.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "Net-(J4-Pad4)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "Net-(D5-K)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MIDI:CAP_C320_KEM"
		(layer "F.Cu")
		(at 84.46 71)
		(tags "C320C104K5R5TA ")
		(property "Reference" "C7"
			(at -1.96 2 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "0.1µ"
			(at 1.27 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "MIDI:CAP_C320_KEM"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "PCB.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.27 1.27)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "Net-(J4-SHLD)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0)
			(size 1.27 1.27)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "GND")
			(pintype "passive")
		)
	)
	(footprint "Diode_THT:D_5W_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 103.5 80.08 90)
		(descr "Diode, 5W series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=8.9*3.7mm^2, , http://www.diodes.com/_files/packages/8686949.gif")
		(tags "Diode 5W series Axial Horizontal pin pitch 10.16mm  length 8.9mm diameter 3.7mm")
		(property "Reference" "D6"
			(at 3.58 3 -90)
			(layer "F.SilkS")
		)
		(property "Value" "1N5817"
			(at 5.08 2.97 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Diode_THT:D_5W_P10.16mm_Horizontal"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88525/1n5817.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "20V 1A Schottky Barrier Rectifier Diode, DO-41"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*DO?41*")
		(sheetname "Root")
		(sheetfile "PCB.kicad_sch")
		(attr through_hole)
		(fp_text user "K"
			(at 0 -2.4 -90)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 5.7475 0 -90)
			(layer "F.Fab")
		)
		(fp_text user "K"
			(at 0 -2.4 -90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 2.8 2.8)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "Net-(D6-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 90)
			(size 2.8 2.8)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "GND")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Diode_THT.3dshapes/D_5W_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_THT:D_5W_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 105.5 52.07 -90)
		(descr "Diode, 5W series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=8.9*3.7mm^2, , http://www.diodes.com/_files/packages/8686949.gif")
		(tags "Diode 5W series Axial Horizontal pin pitch 10.16mm  length 8.9mm diameter 3.7mm")
		(property "Reference" "D1"
			(at 5.08 -2.97 90)
			(layer "F.SilkS")
		)
		(property "Value" "1N5817"
			(at 5.08 2.97 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Diode_THT:D_5W_P10.16mm_Horizontal"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88525/1n5817.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "20V 1A Schottky Barrier Rectifier Diode, DO-41"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*DO?41*")
		(sheetname "Root")
		(sheetfile "PCB.kicad_sch")
		(attr through_hole)
		(fp_text user "K"
			(at 0 -2.4 90)
			(layer "F.SilkS")
		)
		(fp_text user "K"
			(at 0 -2.4 90)
			(layer "F.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 5.7475 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 2.8 2.8)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "Net-(D1-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 270)
			(size 2.8 2.8)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "Net-(D1-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Diode_THT.3dshapes/D_5W_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MIDI:ABL-8.000MHZ-B2_ABR"
		(layer "F.Cu")
		(at 77.380001 91.5 180)
		(tags "ABL-8.000MHZ-B2 ")
		(property "Reference" "X1"
			(at 2.380001 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "8 MHz"
			(at 2.44 0 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "MIDI:ABL-8.000MHZ-B2_ABR"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Two pin crystal"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Crystal*")
		(sheetname "Root")
		(sheetfile "PCB.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.44 0 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.2192 1.2192)
			(drill 0.7112)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "Net-(U1-RA6{slash}OSC2{slash}CLKO)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 4.880001 0 180)
			(size 1.2192 1.2192)
			(drill 0.7112)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "Net-(U1-OSC1{slash}CLKI)")
			(pinfunction "2")
			(pintype "passive")
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 107.95 74)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R4"
			(at 5.55 -2 0)
			(layer "F.SilkS")
		)
		(property "Value" "470"
			(at 5.08 2.37 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "PCB.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "VDD")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Net-(D2-A)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_THT:LED_D3.0mm"
		(layer "F.Cu")
		(at 116.46 91.5)
		(descr "LED, diameter 3.0mm, 2 pins")
		(tags "LED diameter 3.0mm 2 pins")
		(property "Reference" "D4"
			(at -0.46 -3.5 90)
			(layer "F.SilkS")
		)
		(property "Value" "green"
			(at 1.27 2.96 0)
			(layer "F.Fab")
		)
		(property "Footprint" "LED_THT:LED_D3.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "Root")
		(sheetfile "PCB.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "GND")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "Net-(D4-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_THT.3dshapes/LED_D3.0mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MIDI:CAP_C315C_MOLDED_KEM"
		(layer "F.Cu")
		(at 85.389 91.5 180)
		(tags "C315C180J2G5TA ")
		(property "Reference" "C2"
			(at -2.111 1 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "18p"
			(at 1.27 0 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "MIDI:CAP_C315C_MOLDED_KEM"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "PCB.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 0 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.3716 1.3716)
			(drill 0.8636)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "GND")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0 180)
			(size 1.3716 1.3716)
			(drill 0.8636)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "Net-(U1-RA6{slash}OSC2{slash}CLKO)")
			(pintype "passive")
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 62.08 91.44 180)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R1"
			(at 5.08 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "43k"
			(at 5.08 2.37 180)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "PCB.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "VDD")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(J2-Pin_1)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_THT:D_5W_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 99 69.92 -90)
		(descr "Diode, 5W series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=8.9*3.7mm^2, , http://www.diodes.com/_files/packages/8686949.gif")
		(tags "Diode 5W series Axial Horizontal pin pitch 10.16mm  length 8.9mm diameter 3.7mm")
		(property "Reference" "D7"
			(at 4.58 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "1N5817"
			(at 5.08 2.97 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Diode_THT:D_5W_P10.16mm_Horizontal"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88525/1n5817.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "20V 1A Schottky Barrier Rectifier Diode, DO-41"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*DO?41*")
		(sheetname "Root")
		(sheetfile "PCB.kicad_sch")
		(attr through_hole)
		(fp_text user "K"
			(at 0 -2.4 90)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 5.7475 0 90)
			(layer "F.Fab")
		)
		(fp_text user "K"
			(at 0 -2.4 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 2.8 2.8)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "VDD")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 270)
			(size 2.8 2.8)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "Net-(D6-K)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Diode_THT.3dshapes/D_5W_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MIDI:Sullins_PPPC081LGBN-RC"
		(layer "F.Cu")
		(at 98.5 85.4665)
		(descr "Female Header, Right Angle")
		(property "Reference" "J2"
			(at 8 -1.9665 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "ICSD"
			(at 0 2.54 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "MIDI:Sullins_PPPC081LGBN-RC"
			(at 1.27 2.54 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 1.27 2.54 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x08, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 1.27 2.54 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "PCB.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 11.5 1.0335 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at -8.89 0)
			(size 1.524 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(J2-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -6.35 0)
			(size 1.524 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "VDD")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at -3.81 0)
			(size 1.524 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "GND")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at -1.27 0)
			(size 1.524 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "Net-(J2-Pin_4)")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 1.27 0)
			(size 1.524 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "Net-(J2-Pin_5)")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at 3.81 0)
			(size 1.524 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "unconnected-(J2-Pin_6-Pad6)")
			(pinfunction "Pin_6")
			(pintype "passive+no_connect")
		)
		(pad "7" thru_hole circle
			(at 6.35 0)
			(size 1.524 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "unconnected-(J2-Pin_7-Pad7)")
			(pinfunction "Pin_7")
			(pintype "passive+no_connect")
		)
		(pad "8" thru_hole circle
			(at 8.89 0)
			(size 1.524 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "unconnected-(J2-Pin_8-Pad8)")
			(pinfunction "Pin_8")
			(pintype "passive+no_connect")
		)
	)
	(footprint "MIDI:CONN5_5212044-1_TEC"
		(layer "F.Cu")
		(at 78.74 63.4746 180)
		(tags "5212044-1 ")
		(property "Reference" "J3"
			(at -6.76 -4.5254 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "DIN-5_180degree"
			(at -7.4892 0 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "MIDI:CONN5_5212044-1_TEC"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "5-pin DIN connector (5-pin DIN-5 stereo) with shield"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -7.4892 0 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 180)
			(size 1.62 1.97)
			(drill oval 0.82 1.17)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "unconnected-(J3-Pad1)")
			(pintype "passive+no_connect")
		)
		(pad "2" thru_hole oval
			(at -7.4892 0 180)
			(size 1.62 1.97)
			(drill oval 0.82 1.17)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "unconnected-(J3-Pad2)")
			(pintype "passive+no_connect")
		)
		(pad "3" thru_hole oval
			(at -14.9784 0 180)
			(size 1.62 1.97)
			(drill oval 0.82 1.17)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "unconnected-(J3-Pad3)")
			(pintype "passive+no_connect")
		)
		(pad "4" thru_hole oval
			(at -2.4746 -2.4892 180)
			(size 1.62 1.97)
			(drill oval 0.82 1.17)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "Net-(J3-Pad4)")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at -12.5038 -2.4892 180)
			(size 1.62 1.97)
			(drill oval 0.82 1.17)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "Net-(J3-Pad5)")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at -9.9892 9.906 180)
			(size 2.24 1.23)
			(drill oval 1.44 0.43)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "unconnected-(J3-SHLD-Pad6)")
			(pinfunction "SHLD")
			(pintype "passive+no_connect")
		)
		(pad "6" thru_hole oval
			(at -4.9892 9.906 180)
			(size 2.24 1.23)
			(drill oval 1.44 0.43)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "unconnected-(J3-SHLD-Pad6)")
			(pinfunction "SHLD")
			(pintype "passive+no_connect")
		)
	)
	(footprint "MIDI:CONN5_5212044-1_TEC"
		(layer "F.Cu")
		(at 54.61 63.4746 180)
		(tags "5212044-1 ")
		(property "Reference" "J4"
			(at 0.61 -4.0254 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "DIN-5_180degree"
			(at -7.4892 0 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "MIDI:CONN5_5212044-1_TEC"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "5-pin DIN connector (5-pin DIN-5 stereo) with shield"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -7.4892 0 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 180)
			(size 1.62 1.97)
			(drill oval 0.82 1.17)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "unconnected-(J4-Pad1)")
			(pintype "passive+no_connect")
		)
		(pad "2" thru_hole oval
			(at -7.4892 0 180)
			(size 1.62 1.97)
			(drill oval 0.82 1.17)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "Net-(C6-Pad1)")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at -14.9784 0 180)
			(size 1.62 1.97)
			(drill oval 0.82 1.17)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "unconnected-(J4-Pad3)")
			(pintype "passive+no_connect")
		)
		(pad "4" thru_hole oval
			(at -2.4746 -2.4892 180)
			(size 1.62 1.97)
			(drill oval 0.82 1.17)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "Net-(J4-Pad4)")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at -12.5038 -2.4892 180)
			(size 1.62 1.97)
			(drill oval 0.82 1.17)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "Net-(D5-A)")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at -9.9892 9.906 180)
			(size 2.24 1.23)
			(drill oval 1.44 0.43)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "Net-(J4-SHLD)")
			(pinfunction "SHLD")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at -4.9892 9.906 180)
			(size 2.24 1.23)
			(drill oval 1.44 0.43)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "Net-(J4-SHLD)")
			(pinfunction "SHLD")
			(pintype "passive")
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 94.5 69.92 -90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R6"
			(at -1.920001 -1 180)
			(layer "F.SilkS")
		)
		(property "Value" "220"
			(at 5.08 2.37 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "PCB.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "Net-(J3-Pad5)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "Net-(D6-K)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_THT:D_5W_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 62.42 73.5)
		(descr "Diode, 5W series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=8.9*3.7mm^2, , http://www.diodes.com/_files/packages/8686949.gif")
		(tags "Diode 5W series Axial Horizontal pin pitch 10.16mm  length 8.9mm diameter 3.7mm")
		(property "Reference" "D5"
			(at 10.58 3 0)
			(layer "F.SilkS")
		)
		(property "Value" "1N4148"
			(at 5.08 2.97 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Diode_THT:D_5W_P10.16mm_Horizontal"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/1N4148_1N4448.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "100V 0.15A standard switching diode, DO-35"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*DO?35*")
		(sheetname "Root")
		(sheetfile "PCB.kicad_sch")
		(attr through_hole)
		(fp_text user "K"
			(at 0 -2.4 0)
			(layer "F.SilkS")
		)
		(fp_text user "K"
			(at 0 -2.4 0)
			(layer "F.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 5.7475 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 2.8 2.8)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "Net-(D5-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0)
			(size 2.8 2.8)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "Net-(D5-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Diode_THT.3dshapes/D_5W_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MIDI:CAP_C315C_MOLDED_KEM"
		(layer "F.Cu")
		(at 65 91.5)
		(tags "C315C180J2G5TA ")
		(property "Reference" "C1"
			(at -1.5 -2 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "18p"
			(at 1.27 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "MIDI:CAP_C315C_MOLDED_KEM"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "PCB.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.3716 1.3716)
			(drill 0.8636)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "GND")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0)
			(size 1.3716 1.3716)
			(drill 0.8636)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "Net-(U1-OSC1{slash}CLKI)")
			(pintype "passive")
		)
	)
	(footprint "MIDI:CAP_C320_KEM"
		(layer "F.Cu")
		(at 110 81.27 -90)
		(tags "C320C104K5R5TA ")
		(property "Reference" "C3"
			(at -2.77 2 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "0.1µ"
			(at 1.27 0 -90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "MIDI:CAP_C320_KEM"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "PCB.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 0 -90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.27 1.27)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "VDD")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0 270)
			(size 1.27 1.27)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "GND")
			(pintype "passive")
		)
	)
	(footprint "MIDI:CAP_R82D-7P4X3P6-5P0_KEM"
		(layer "F.Cu")
		(at 104.1844 66.04 180)
		(tags "R82DC3330AA60J ")
		(property "Reference" "C4"
			(at -2.3156 -0.96 -90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "0.33µ"
			(at 2.54 0 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "MIDI:CAP_R82D-7P4X3P6-5P0_KEM"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "PCB.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.54 0 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "Net-(D1-K)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5.08 0 180)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "GND")
			(pintype "passive")
		)
	)
	(footprint "Package_TO_SOT_THT:TO-220-3_Vertical"
		(layer "F.Cu")
		(at 99.695 53.34 -90)
		(descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
		(tags "TO-220-3 Vertical RM 2.54mm")
		(property "Reference" "U2"
			(at 8.66 0.695 180)
			(layer "F.SilkS")
		)
		(property "Value" "L7805"
			(at 2.54 2.5 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/41/4f/b3/b0/12/d4/47/88/CD00000444.pdf/files/CD00000444.pdf/jcr:content/translations/en.CD00000444.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Positive 1.5A 35V Linear Regulator, Fixed Output 5V, TO-220/TO-263/TO-252"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO?252* TO?263* TO?220*")
		(sheetname "Root")
		(sheetfile "PCB.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.54 -4.27 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "Net-(D1-K)")
			(pinfunction "IN")
			(pintype "power_in")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 270)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" thru_hole oval
			(at 5.08 0 270)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "VDD")
			(pinfunction "OUT")
			(pintype "power_out")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-28_W7.62mm"
		(layer "F.Cu")
		(at 52.07 87.63 90)
		(descr "28-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U1"
			(at 7.63 35.43 90)
			(layer "F.SilkS")
		)
		(property "Value" "PIC18F2450-ISP"
			(at 3.81 35.35 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_DIP:DIP-28_W7.62mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39760d.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "16K Flash, 8K SRAM, USB, nanoWatt XLP, SPDIP28"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SPDIP*W7.62mm* DIP*W7.62mm* PDIP*W7.62mm*")
		(sheetname "Root")
		(sheetfile "PCB.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 16.51 -90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(J2-Pin_1)")
			(pinfunction "Vpp/~{MCLR}/RE3")
			(pintype "input")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "unconnected-(U1-RA0{slash}AN0-Pad2)")
			(pinfunction "RA0/AN0")
			(pintype "bidirectional+no_connect")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "unconnected-(U1-RA1{slash}AN1-Pad3)")
			(pinfunction "RA1/AN1")
			(pintype "bidirectional+no_connect")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "unconnected-(U1-RA2{slash}AN2{slash}Vref--Pad4)")
			(pinfunction "RA2/AN2/Vref-")
			(pintype "bidirectional+no_connect")
		)
		(pad "5" thru_hole oval
			(at 0 10.16 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "unconnected-(U1-RA3{slash}AN3{slash}Vref+-Pad5)")
			(pinfunction "RA3/AN3/Vref+")
			(pintype "bidirectional+no_connect")
		)
		(pad "6" thru_hole oval
			(at 0 12.7 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "unconnected-(U1-RA4{slash}T0CKI{slash}RCV-Pad6)")
			(pinfunction "RA4/T0CKI/RCV")
			(pintype "bidirectional+no_connect")
		)
		(pad "7" thru_hole oval
			(at 0 15.24 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "unconnected-(U1-RA5{slash}AN4{slash}HLVDIN-Pad7)")
			(pinfunction "RA5/AN4/HLVDIN")
			(pintype "bidirectional+no_connect")
		)
		(pad "8" thru_hole oval
			(at 0 17.78 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "9" thru_hole oval
			(at 0 20.32 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "Net-(U1-OSC1{slash}CLKI)")
			(pinfunction "OSC1/CLKI")
			(pintype "input")
		)
		(pad "10" thru_hole oval
			(at 0 22.86 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "Net-(U1-RA6{slash}OSC2{slash}CLKO)")
			(pinfunction "RA6/OSC2/CLKO")
			(pintype "output")
		)
		(pad "11" thru_hole oval
			(at 0 25.4 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "unconnected-(U1-T1OSO{slash}T1CKI{slash}RC0-Pad11)")
			(pinfunction "T1OSO/T1CKI/RC0")
			(pintype "bidirectional+no_connect")
		)
		(pad "12" thru_hole oval
			(at 0 27.94 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "unconnected-(U1-~{UOE}{slash}T1OSI{slash}RC1-Pad12)")
			(pinfunction "~{UOE}/T1OSI/RC1")
			(pintype "bidirectional+no_connect")
		)
		(pad "13" thru_hole oval
			(at 0 30.48 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "unconnected-(U1-CCP1{slash}RC2-Pad13)")
			(pinfunction "CCP1/RC2")
			(pintype "bidirectional+no_connect")
		)
		(pad "14" thru_hole oval
			(at 0 33.02 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "unconnected-(U1-VUSB-Pad14)")
			(pinfunction "VUSB")
			(pintype "bidirectional+no_connect")
		)
		(pad "15" thru_hole oval
			(at 7.62 33.02 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "unconnected-(U1-VM{slash}D-{slash}RC4-Pad15)")
			(pinfunction "VM/D-/RC4")
			(pintype "bidirectional+no_connect")
		)
		(pad "16" thru_hole oval
			(at 7.62 30.48 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "unconnected-(U1-VP{slash}D+{slash}RC5-Pad16)")
			(pinfunction "VP/D+/RC5")
			(pintype "bidirectional+no_connect")
		)
		(pad "17" thru_hole oval
			(at 7.62 27.94 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "Net-(D6-K)")
			(pinfunction "TX/CK/RC6")
			(pintype "bidirectional")
		)
		(pad "18" thru_hole oval
			(at 7.62 25.4 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "Net-(U1-RX{slash}DT{slash}RC7)")
			(pinfunction "RX/DT/RC7")
			(pintype "bidirectional")
		)
		(pad "19" thru_hole oval
			(at 7.62 22.86 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "20" thru_hole oval
			(at 7.62 20.32 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "VDD")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "21" thru_hole oval
			(at 7.62 17.78 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(U1-RB0{slash}AN12{slash}INT0)")
			(pinfunction "RB0/AN12/INT0")
			(pintype "bidirectional")
		)
		(pad "22" thru_hole oval
			(at 7.62 15.24 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(U1-RB1{slash}AN10{slash}INT1)")
			(pinfunction "RB1/AN10/INT1")
			(pintype "bidirectional")
		)
		(pad "23" thru_hole oval
			(at 7.62 12.7 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "unconnected-(U1-RB2{slash}AN8{slash}INT2{slash}VMO-Pad23)")
			(pinfunction "RB2/AN8/INT2/VMO")
			(pintype "bidirectional+no_connect")
		)
		(pad "24" thru_hole oval
			(at 7.62 10.16 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "unconnected-(U1-RB3{slash}AN9{slash}VPO-Pad24)")
			(pinfunction "RB3/AN9/VPO")
			(pintype "bidirectional+no_connect")
		)
		(pad "25" thru_hole oval
			(at 7.62 7.62 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "unconnected-(U1-RB4{slash}AN11{slash}KBI0-Pad25)")
			(pinfunction "RB4/AN11/KBI0")
			(pintype "bidirectional+no_connect")
		)
		(pad "26" thru_hole oval
			(at 7.62 5.08 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "unconnected-(U1-RB5{slash}KBI1{slash}PGM-Pad26)")
			(pinfunction "RB5/KBI1/PGM")
			(pintype "bidirectional+no_connect")
		)
		(pad "27" thru_hole oval
			(at 7.62 2.54 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "Net-(J2-Pin_5)")
			(pinfunction "RB6/KBI2/PGC")
			(pintype "bidirectional")
		)
		(pad "28" thru_hole oval
			(at 7.62 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "Net-(J2-Pin_4)")
			(pinfunction "RB7/KBI3/PGD")
			(pintype "bidirectional")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-28_W7.62mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MIDI:CUI_PJ-102AH"
		(layer "F.Cu")
		(at 113.665 57.785 90)
		(property "Reference" "J1"
			(at -7.715 -5.665 -90)
			(layer "F.SilkS")
		)
		(property "Value" "3.5mm barrel"
			(at 0.43042 5.78054 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "MIDI:CUI_PJ-102AH"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "DC Barrel Jack with an internal switch"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "BarrelJack*")
		(sheetname "Root")
		(sheetfile "PCB.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole oval
			(at -6.5 0 90)
			(size 1.508 3.016)
			(drill oval 1 1.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "Net-(D1-A)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" thru_hole oval
			(at -0.5 0 90)
			(size 1.508 3.016)
			(drill oval 1 1.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "3" thru_hole oval
			(at -3.5 -4.7 90)
			(size 3.016 1.508)
			(drill oval 1.6 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "unconnected-(J1-Pad3)")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
		)
	)
	(footprint "MIDI:CAP_C320_KEM"
		(layer "F.Cu")
		(at 77.46 71)
		(tags "C320C104K5R5TA ")
		(property "Reference" "C6"
			(at -1.46 2.5 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "0.1µ"
			(at 1.27 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "MIDI:CAP_C320_KEM"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "PCB.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.27 1.27)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "Net-(C6-Pad1)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0)
			(size 1.27 1.27)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "GND")
			(pintype "passive")
		)
	)
	(footprint "LED_THT:LED_D3.0mm"
		(layer "F.Cu")
		(at 115.565 69.215)
		(descr "LED, diameter 3.0mm, 2 pins")
		(tags "LED diameter 3.0mm 2 pins")
		(property "Reference" "D2"
			(at 1.27 -2.96 0)
			(layer "F.SilkS")
		)
		(property "Value" "red"
			(at 1.27 2.96 0)
			(layer "F.Fab")
		)
		(property "Footprint" "LED_THT:LED_D3.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "Root")
		(sheetfile "PCB.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "GND")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Net-(D2-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_THT.3dshapes/LED_D3.0mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-6_W7.62mm"
		(layer "F.Cu")
		(at 58.04 69.225 -90)
		(descr "6-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U3"
			(at 1.275 -2.33 90)
			(layer "F.SilkS")
		)
		(property "Value" "H11L1"
			(at 3.81 7.41 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_DIP:DIP-6_W7.62mm"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/H11L3M-D.PDF"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Schmitt Trigger Output Optocoupler, High Speed, DIP-6, 1.6mA turn on threshold"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP*W7.62mm* DIP*W10.16mm* SMDIP*W9.53mm*")
		(sheetname "Root")
		(sheetfile "PCB.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 2.54 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "Net-(D5-K)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "Net-(D5-A)")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "unconnected-(U3-Pad3)")
			(pintype "no_connect")
		)
		(pad "4" thru_hole oval
			(at 7.62 5.08 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "Net-(U1-RX{slash}DT{slash}RC7)")
			(pintype "output")
		)
		(pad "5" thru_hole oval
			(at 7.62 2.54 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "GND")
			(pintype "power_in")
		)
		(pad "6" thru_hole oval
			(at 7.62 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "VDD")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-6_W7.62mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 76.42 76)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R8"
			(at 1.08 2 0)
			(layer "F.SilkS")
		)
		(property "Value" "460"
			(at 5.08 2.37 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "PCB.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 7.08 -1 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "VDD")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "Net-(U1-RX{slash}DT{slash}RC7)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 117.5 88.08 90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R3"
			(at 3.08 0.5 -90)
			(layer "F.SilkS")
		)
		(property "Value" "330"
			(at 5.08 2.37 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "PCB.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 11.58 -1.5 -90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "Net-(D4-A)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(U1-RB1{slash}AN10{slash}INT1)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MIDI:CAP_C320_KEM"
		(layer "F.Cu")
		(at 108.96 69.215)
		(tags "C320C104K5R5TA ")
		(property "Reference" "C5"
			(at -1.96 2.285 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "0.1µ"
			(at 1.27 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "MIDI:CAP_C320_KEM"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "PCB.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.27 1.27)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "VDD")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0)
			(size 1.27 1.27)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "GND")
			(pintype "passive")
		)
	)
	(footprint "LED_THT:LED_D3.0mm"
		(layer "F.Cu")
		(at 111 91.58)
		(descr "LED, diameter 3.0mm, 2 pins")
		(tags "LED diameter 3.0mm 2 pins")
		(property "Reference" "D3"
			(at 1 -3.58 90)
			(layer "F.SilkS")
		)
		(property "Value" "green"
			(at 1.27 2.96 0)
			(layer "F.Fab")
		)
		(property "Footprint" "LED_THT:LED_D3.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "Root")
		(sheetfile "PCB.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "GND")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "Net-(D3-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_THT.3dshapes/LED_D3.0mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 90.5 69.92 -90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R7"
			(at -1.92 -0.5 180)
			(layer "F.SilkS")
		)
		(property "Value" "220"
			(at 5.08 2.37 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "PCB.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "Net-(J3-Pad4)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "VDD")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 114 88.08 90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R2"
			(at 11.08 -2 -90)
			(layer "F.SilkS")
		)
		(property "Value" "330"
			(at 5.08 2.37 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "PCB.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 -90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "Net-(D3-A)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(U1-RB0{slash}AN12{slash}INT0)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_rect
		(start 50 50)
		(end 121 95.5)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_text "TX"
		(at 87 59.5 0)
		(layer "B.SilkS")
	)
	(gr_text "RX"
		(at 63 59.5 0)
		(layer "B.SilkS")
	)
	(gr_text "MIDI Processor\nhttp://hekster.org"
		(at 108.5 92.5 0)
		(layer "B.SilkS")
	)
	(zone
		(net 15)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 120.5 94.5) (xy 50.5 94.5) (xy 50.5 50.5) (xy 120.5 50.5)
			)
		)
	)
)