(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "USLetter")
	(title_block
		(title "UsbGpio")
		(date "2024-10-07")
		(rev "1b")
	)
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0.0254)
		(solder_mask_min_width 0.1016)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes no)
			(usegerberadvancedattributes no)
			(creategerberjobfile no)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "+5V")
	(net 3 "Net-(U_MCP2221-VUSB)")
	(net 4 "Net-(F1-Pad2)")
	(net 5 "+3V3")
	(net 6 "SCL")
	(net 7 "SDA")
	(net 8 "TXD")
	(net 9 "RXD")
	(net 10 "unconnected-(J_USBC1-SBU2-PadB8)")
	(net 11 "AIN3")
	(net 12 "USB+")
	(net 13 "USB-")
	(net 14 "Net-(J_USBC1-CC2)")
	(net 15 "Net-(J_USBC1-CC1)")
	(net 16 "AIN0")
	(net 17 "/ADDR")
	(net 18 "/RDY")
	(net 19 "AIN2")
	(net 20 "/OUGP2")
	(net 21 "/OMPG7")
	(net 22 "AIN1")
	(net 23 "/VSER+")
	(net 24 "UGP1")
	(net 25 "unconnected-(J_USBC1-SBU1-PadA8)")
	(net 26 "UGP0")
	(net 27 "UGP2")
	(net 28 "Net-(SP_A2-B)")
	(net 29 "Net-(SP_A3-B)")
	(net 30 "UGP3")
	(net 31 "Net-(U_MCP23008-~{RESET})")
	(net 32 "MGP7")
	(net 33 "Net-(U_MCP2221-~{RST})")
	(net 34 "MGP5")
	(net 35 "MGP1")
	(net 36 "MGP0")
	(net 37 "MGP2")
	(net 38 "MGP3")
	(net 39 "Net-(J_OPT27-Pin_4)")
	(net 40 "MGP4")
	(net 41 "MGP6")
	(net 42 "unconnected-(U_MCP23008-INT-Pad8)")
	(net 43 "unconnected-(U_MCP23008-NC-Pad7)")
	(net 44 "Net-(LED3-A)")
	(net 45 "Net-(SP_UGP3-A)")
	(net 46 "Net-(SP_LED7-B)")
	(net 47 "Net-(SP_USB5-A)")
	(net 48 "Net-(LED7-A)")
	(footprint "MountingHole:MountingHole_3.2mm_M3"
		(layer "F.Cu")
		(at 3.81 3.81)
		(descr "Mounting Hole 3.2mm, no annular, M3")
		(tags "mounting hole 3.2mm no annular m3")
		(property "Reference" "H1"
			(at -0.0762 0.0762 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole"
			(at -0.0762 1.6002 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_3.2mm_M3"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "Root")
		(sheetfile "UsbGpio_v1b.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3"
		(layer "F.Cu")
		(at 52.07 3.81)
		(descr "Mounting Hole 3.2mm, no annular, M3")
		(tags "mounting hole 3.2mm no annular m3")
		(property "Reference" "H2"
			(at -0.0762 0.0762 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole"
			(at -0.0762 1.6002 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_3.2mm_M3"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "Root")
		(sheetfile "UsbGpio_v1b.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 31.5214 20.5514 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "RMGP7"
			(at -0.4318 1.349 0)
			(layer "F.SilkS")
		)
		(property "Value" "10K"
			(at -0.0254 1.27 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digi-Key_PN" "311-10KLGCT-ND"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer Part#" "AC0805FR-0710KL"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "UsbGpio_v1b.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 32 "MGP7")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Fuse:Fuse_1812_4532Metric"
		(layer "F.Cu")
		(at 12.6238 13.4366 90)
		(descr "Fuse SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.nikhef.nl/pub/departments/mt/projects/detectorR_D/dtddice/ERJ2G.pdf), generated with kicad-footprint-generator")
		(tags "fuse")
		(property "Reference" "F1"
			(at 3.3743 -0.0254 180)
			(layer "F.SilkS")
		)
		(property "Value" "500ma"
			(at 0 1.71 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Fuse:Fuse_1812_4532Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digi-Key_PN" "MF-PSMF050X-2CT-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer Part#" "MF-MSMF050-2"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*polyfuse* *PTC*")
		(sheetname "Root")
		(sheetfile "UsbGpio_v1b.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -2.1375 0 90)
			(size 1.125 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 47 "Net-(SP_USB5-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.1375 0 90)
			(size 1.125 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 4 "Net-(F1-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Fuse.3dshapes/Fuse_1812_4532Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 20.7518 23.2195 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "CO1"
			(at 2.3407 -0.0762 180)
			(layer "F.SilkS")
		)
		(property "Value" "4.7uF"
			(at 0 1.2446 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digi-Key_PN" "399-5505-1-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer Part#" "C0805C475K3PACTU"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "UsbGpio_v1b.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -1.0375 0 90)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.212766)
			(net 5 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 90)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_JST:JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal"
		(layer "F.Cu")
		(at 19.9704 38.6888)
		(descr "JST SH series connector, SM04B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST SH horizontal")
		(property "Reference" "J_SER1"
			(at -2.6476 -3.6622 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x04_MountingPin"
			(at 0.0508 1.0668 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Connector_JST:JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connectable mounting pin connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digi-Key_PN" "455-SM04B-SRSS-TBCT-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer Part#" "SM04B-SRSS-TB"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??-1MP*")
		(sheetname "Root")
		(sheetfile "UsbGpio_v1b.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -1.5 -2)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -0.5 -2)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 23 "/VSER+")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.5 -2)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 9 "RXD")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at 1.5 -2)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "TXD")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "MP" smd roundrect
			(at -2.8 1.875)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 1 "GND")
			(pinfunction "MountPin")
			(pintype "passive")
		)
		(pad "MP" smd roundrect
			(at 2.8 1.875)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 1 "GND")
			(pinfunction "MountPin")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_JST.3dshapes/JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 21.59 29.845 90)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "J_VMGP7"
			(at 2.3622 1.3462 180)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02"
			(at 1.524 1.0922 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "UsbGpio_v1b.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "Net-(J_OPT27-Pin_4)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 29.8196 8.1026 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "RUGP3"
			(at 0.1016 1.397 180)
			(layer "F.SilkS")
		)
		(property "Value" "10K"
			(at -0.0254 1.27 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digi-Key_PN" "311-10KLGCT-ND"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer Part#" "AC0805FR-0710KL"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "UsbGpio_v1b.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 5 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 45 "Net-(SP_UGP3-A)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23_Handsoldering"
		(layer "F.Cu")
		(at 27.559 24.487 -90)
		(descr "SOT-23, Handsoldering")
		(tags "SOT-23")
		(property "Reference" "Q_UGP2"
			(at -0.4826 2.2323 -90)
			(layer "F.SilkS")
		)
		(property "Value" "2N7002K"
			(at -0.0508 0.2794 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23_Handsoldering"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/ds30896.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digi-Key_PN" "2N7002KCT-ND"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer Part#" "2N7002K"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "Root")
		(sheetfile "UsbGpio_v1b.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -1.5 -0.95 270)
			(size 1.9 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 27 "UGP2")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -1.5 0.95 270)
			(size 1.9 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.5 0 270)
			(size 1.9 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 20 "/OUGP2")
			(pinfunction "D")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 43.7896 15.9766)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "RADUP1"
			(at 0.1778 -1.3716 0)
			(layer "F.SilkS")
		)
		(property "Value" "10K"
			(at -0.0254 1.27 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digi-Key_PN" "311-10KLGCT-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer Part#" "AC0805FR-0710KL"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "UsbGpio_v1b.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 18 "/RDY")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 5 "+3V3")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_JST:JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal"
		(layer "F.Cu")
		(at 35.8694 38.6822)
		(descr "JST SH series connector, SM04B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST SH horizontal")
		(property "Reference" "J_IO2"
			(at -2.6476 -3.2558 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x04_MountingPin"
			(at 0.0508 1.0668 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Connector_JST:JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connectable mounting pin connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digi-Key_PN" "455-SM04B-SRSS-TBCT-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer Part#" "SM04B-SRSS-TB"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??-1MP*")
		(sheetname "Root")
		(sheetfile "UsbGpio_v1b.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -1.5 -2)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -0.5 -2)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "+3V3")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.5 -2)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 30 "UGP3")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at 1.5 -2)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 41 "MGP6")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "MP" smd roundrect
			(at -2.8 1.875)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 1 "GND")
			(pinfunction "MountPin")
			(pintype "passive")
		)
		(pad "MP" smd roundrect
			(at 2.8 1.875)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 1 "GND")
			(pinfunction "MountPin")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_JST.3dshapes/JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MyParts:USB_C_Receptacle_Palconn_UTC16-G_MOD"
		(layer "F.Cu")
		(at 18.7178 5.168 180)
		(descr "http://www.palpilot.com/wp-content/uploads/2017/05/UTC027-GKN-OR-Rev-A.pdf")
		(tags "USB C Type-C Receptacle USB2.0")
		(property "Reference" "J_USBC1"
			(at 5.715 -1.4224 90)
			(layer "F.SilkS")
		)
		(property "Value" "USB_C_Receptacle_USB2.0"
			(at 0 4.84 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MyParts:USB_C_Receptacle_Palconn_UTC16-G_MOD"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.usb.org/sites/default/files/documents/usb_type-c.zip"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "USB 2.0-only 16P Type-C Receptacle connector"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digi-Key_PN" " 2073-USB4105-GF-ACT-ND"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer Part#" "USB4105-GF-A"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "USB*C*Receptacle*")
		(sheetname "Root")
		(sheetfile "UsbGpio_v1b.kicad_sch")
		(clearance 0.00254)
		(attr smd)
		(fp_text user "PCB Edge"
			(at 0 3.43 0)
			(layer "Dwgs.User")
			(hide yes)
		)
		(fp_text user "${REFERENCE}"
			(at 0 1.18 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "" np_thru_hole circle
			(at -2.89 -1.45)
			(size 0.6 0.6)
			(drill 0.6)
			(layers "F&B.Cu" "*.Mask")
			(clearance 0.1524)
		)
		(pad "" np_thru_hole circle
			(at 2.89 -1.45)
			(size 0.6 0.6)
			(drill 0.6)
			(layers "F&B.Cu" "*.Mask")
			(clearance 0.1524)
		)
		(pad "A1" smd rect
			(at -3.2 -2.51 180)
			(size 0.6 1.16)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(clearance 0.1524)
		)
		(pad "A4" smd rect
			(at -2.4 -2.51 180)
			(size 0.6 1.16)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "Net-(F1-Pad2)")
			(pinfunction "VBUS")
			(pintype "passive")
			(clearance 0.1524)
		)
		(pad "A5" smd rect
			(at -1.25 -2.51)
			(size 0.3 1.16)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 15 "Net-(J_USBC1-CC1)")
			(pinfunction "CC1")
			(pintype "bidirectional")
		)
		(pad "A6" smd rect
			(at -0.25 -2.51)
			(size 0.3 1.16)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 12 "USB+")
			(pinfunction "D+")
			(pintype "bidirectional")
		)
		(pad "A7" smd rect
			(at 0.25 -2.51)
			(size 0.3 1.16)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 13 "USB-")
			(pinfunction "D-")
			(pintype "bidirectional")
		)
		(pad "A8" smd rect
			(at 1.25 -2.51)
			(size 0.3 1.16)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 25 "unconnected-(J_USBC1-SBU1-PadA8)")
			(pinfunction "SBU1")
			(pintype "bidirectional+no_connect")
			(clearance 0.1524)
		)
		(pad "A9" smd rect
			(at 2.4 -2.51 180)
			(size 0.6 1.16)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "Net-(F1-Pad2)")
			(pinfunction "VBUS")
			(pintype "passive")
			(clearance 0.1524)
		)
		(pad "A12" smd rect
			(at 3.2 -2.51 180)
			(size 0.6 1.16)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(clearance 0.1524)
		)
		(pad "B1" smd rect
			(at 3.2 -2.51 180)
			(size 0.6 1.16)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(clearance 0.1524)
		)
		(pad "B4" smd rect
			(at 2.4 -2.51 180)
			(size 0.6 1.16)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "Net-(F1-Pad2)")
			(pinfunction "VBUS")
			(pintype "passive")
			(clearance 0.1524)
		)
		(pad "B5" smd rect
			(at 1.75 -2.51)
			(size 0.3 1.16)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 14 "Net-(J_USBC1-CC2)")
			(pinfunction "CC2")
			(pintype "bidirectional")
		)
		(pad "B6" smd rect
			(at 0.75 -2.51)
			(size 0.3 1.16)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 12 "USB+")
			(pinfunction "D+")
			(pintype "bidirectional")
		)
		(pad "B7" smd rect
			(at -0.75 -2.51)
			(size 0.3 1.16)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 13 "USB-")
			(pinfunction "D-")
			(pintype "bidirectional")
		)
		(pad "B8" smd rect
			(at -1.75 -2.51)
			(size 0.3 1.16)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "unconnected-(J_USBC1-SBU2-PadB8)")
			(pinfunction "SBU2")
			(pintype "bidirectional+no_connect")
			(clearance 0.1524)
		)
		(pad "B9" smd rect
			(at -2.4 -2.51 180)
			(size 0.6 1.16)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "Net-(F1-Pad2)")
			(pinfunction "VBUS")
			(pintype "passive")
			(clearance 0.1524)
		)
		(pad "B12" smd rect
			(at -3.2 -2.51 180)
			(size 0.6 1.16)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(clearance 0.1524)
		)
		(pad "S1" thru_hole oval
			(at -4.32 -1.93 270)
			(size 2 0.9)
			(drill oval 1.7 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
			(clearance 0.1778)
		)
		(pad "S1" thru_hole oval
			(at -4.32 2.24 270)
			(size 1.7 0.9)
			(drill oval 1.4 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
			(clearance 0.1778)
		)
		(pad "S1" thru_hole oval
			(at 4.32 -1.93 270)
			(size 2 0.9)
			(drill oval 1.7 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
			(clearance 0.1778)
		)
		(pad "S1" thru_hole oval
			(at 4.32 2.24 270)
			(size 1.7 0.9)
			(drill oval 1.4 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
			(clearance 0.1778)
		)
		(model "${KICAD6_3DMODEL_DIR}/Connector_USB.3dshapes/USB_C_Receptacle_Palconn_UTC16-G.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 22.8346 23.2195 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "CO2"
			(at 2.3661 0.0254 180)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.2446 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digi-Key_PN" "399-C0805C104K3RAC7800CT-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer Part#" "C0805C104K3RAC7800"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "UsbGpio_v1b.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -1.0375 0 90)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.212766)
			(net 5 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 90)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 33.274 16.1036 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "RMC8"
			(at -0.0254 -1.4478 0)
			(layer "F.SilkS")
		)
		(property "Value" "10K"
			(at -0.0254 1.27 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digi-Key_PN" "311-10KLGCT-ND"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer Part#" "AC0805FR-0710KL"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "UsbGpio_v1b.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 31 "Net-(U_MCP23008-~{RESET})")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 5 "+3V3")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23_Handsoldering"
		(layer "F.Cu")
		(at 31.4452 24.487 -90)
		(descr "SOT-23, Handsoldering")
		(tags "SOT-23")
		(property "Reference" "Q_MGP7"
			(at -0.5842 -2.4413 90)
			(layer "F.SilkS")
		)
		(property "Value" "2N7002K"
			(at -0.0508 0.2794 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23_Handsoldering"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/ds30896.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digi-Key_PN" "2N7002KCT-ND"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer Part#" "2N7002K"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "Root")
		(sheetfile "UsbGpio_v1b.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -1.5 -0.95 270)
			(size 1.9 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 32 "MGP7")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -1.5 0.95 270)
			(size 1.9 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.5 0 270)
			(size 1.9 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 21 "/OMPG7")
			(pinfunction "D")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 11.1252 24.6888 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "CI1"
			(at -2.3368 -0.2286 0)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 1.2446 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digi-Key_PN" "1276-1029-1-ND"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer Part#" "CL21B105KBFNNNE"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "UsbGpio_v1b.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -1.0375 0 270)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.212766)
			(net 2 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 270)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 44.3992 29.6164)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "RA3"
			(at -0.127 1.397 0)
			(layer "F.SilkS")
		)
		(property "Value" "10K"
			(at -0.0254 1.27 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digi-Key_PN" "311-10KLGCT-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer Part#" "AC0805FR-0710KL"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "UsbGpio_v1b.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 29 "Net-(SP_A3-B)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 5 "+3V3")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm"
		(layer "F.Cu")
		(at 29.4998 11.4046 180)
		(descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "SP_UGP3"
			(at -0.0658 -1.8034 180)
			(layer "F.SilkS")
		)
		(property "Value" "SolderJumper_2_Open"
			(at -0.0254 1.3462 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 2-pole, open"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(sheetname "Root")
		(sheetfile "UsbGpio_v1b.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "1" smd rect
			(at -0.65 0 180)
			(size 1 1.5)
			(layers "F.Cu" "F.Mask")
			(net 45 "Net-(SP_UGP3-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.65 0 180)
			(size 1 1.5)
			(layers "F.Cu" "F.Mask")
			(net 30 "UGP3")
			(pinfunction "B")
			(pintype "passive")
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 26.0096 8.128 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "CU1"
			(at 2.286 0.0254 180)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 1.2446 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digi-Key_PN" "1276-1029-1-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer Part#" "CL21B105KBFNNNE"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "UsbGpio_v1b.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -1.0375 0 90)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.212766)
			(net 3 "Net-(U_MCP2221-VUSB)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 90)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:SOIC-18W_7.5x11.6mm_P1.27mm"
		(layer "F.Cu")
		(at 39.0906 6.8308 90)
		(descr "SOIC, 18 Pin (JEDEC MS-013AB, https://www.analog.com/media/en/package-pcb-resources/package/33254132129439rw_18.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U_MCP23008"
			(at -0.1717 -6.4894 90)
			(layer "F.SilkS")
		)
		(property "Value" "MCP23008-xSO"
			(at -0.1524 4.8768 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Package_SO:SOIC-18W_7.5x11.6mm_P1.27mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/MCP23008-MCP23S08-Data-Sheet-20001919F.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "8-bit I/O expander, I2C, interrupts, SOIC-18"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digi-Key_PN" "MCP23008T-E/SOCT-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer Part#" "MCP23008T-E/SO"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOIC*7.5x11.6mm*P1.27mm*")
		(sheetname "Root")
		(sheetfile "UsbGpio_v1b.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -4.65 -5.08 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "SCL")
			(pinfunction "SCL")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -4.65 -3.81 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "SDA")
			(pinfunction "SDA")
			(pintype "bidirectional")
		)
		(pad "3" smd roundrect
			(at -4.65 -2.54 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "A2")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at -4.65 -1.27 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "A1")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at -4.65 0 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at -4.65 1.27 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 31 "Net-(U_MCP23008-~{RESET})")
			(pinfunction "~{RESET}")
			(pintype "input")
		)
		(pad "7" smd roundrect
			(at -4.65 2.54 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 43 "unconnected-(U_MCP23008-NC-Pad7)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "8" smd roundrect
			(at -4.65 3.81 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 42 "unconnected-(U_MCP23008-INT-Pad8)")
			(pinfunction "INT")
			(pintype "output+no_connect")
		)
		(pad "9" smd roundrect
			(at -4.65 5.08 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "10" smd roundrect
			(at 4.65 5.08 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 36 "MGP0")
			(pinfunction "GP0")
			(pintype "bidirectional")
		)
		(pad "11" smd roundrect
			(at 4.65 3.81 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 35 "MGP1")
			(pinfunction "GP1")
			(pintype "bidirectional")
		)
		(pad "12" smd roundrect
			(at 4.65 2.54 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 37 "MGP2")
			(pinfunction "GP2")
			(pintype "bidirectional")
		)
		(pad "13" smd roundrect
			(at 4.65 1.27 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 38 "MGP3")
			(pinfunction "GP3")
			(pintype "bidirectional")
		)
		(pad "14" smd roundrect
			(at 4.65 0 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 40 "MGP4")
			(pinfunction "GP4")
			(pintype "bidirectional")
		)
		(pad "15" smd roundrect
			(at 4.65 -1.27 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 34 "MGP5")
			(pinfunction "GP5")
			(pintype "bidirectional")
		)
		(pad "16" smd roundrect
			(at 4.65 -2.54 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 41 "MGP6")
			(pinfunction "GP6")
			(pintype "bidirectional")
		)
		(pad "17" smd roundrect
			(at 4.65 -3.81 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 32 "MGP7")
			(pinfunction "GP7")
			(pintype "bidirectional")
		)
		(pad "18" smd roundrect
			(at 4.65 -5.08 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "+3V3")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-18W_7.5x11.6mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 3.3274 8.8646 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "RLED3"
			(at -0.127 1.5494 0)
			(layer "F.SilkS")
		)
		(property "Value" "330"
			(at 0 0.735 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digi-Key_PN" "311-330CRCT-ND"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer Part#" "RC0805FR-07330RL"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "UsbGpio_v1b.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 44 "Net-(LED3-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 5 "+3V3")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 25.9334 3.1496 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "RCC1"
			(at 2.1844 0.1016 180)
			(layer "F.SilkS")
		)
		(property "Value" "5K1"
			(at 0 0.735 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digi-Key_PN" "311-5.10KCRCT-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer Part#" "RC0805FR-075K1L"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "UsbGpio_v1b.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 15 "Net-(J_USBC1-CC1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_JST:JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal"
		(layer "F.Cu")
		(at 12.0142 38.6842)
		(descr "JST SH series connector, SM04B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST SH horizontal")
		(property "Reference" "J_I2C1"
			(at -2.667 -3.5306 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x04_MountingPin"
			(at 0.0508 1.0668 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Connector_JST:JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connectable mounting pin connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digi-Key_PN" "455-SM04B-SRSS-TBCT-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer Part#" "SM04B-SRSS-TB"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??-1MP*")
		(sheetname "Root")
		(sheetfile "UsbGpio_v1b.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -1.5 -2)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -0.5 -2)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "+3V3")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.5 -2)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "SDA")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at 1.5 -2)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "SCL")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "MP" smd roundrect
			(at -2.8 1.875)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 1 "GND")
			(pinfunction "MountPin")
			(pintype "passive")
		)
		(pad "MP" smd roundrect
			(at 2.8 1.875)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 1 "GND")
			(pinfunction "MountPin")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_JST.3dshapes/JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_JST:JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal"
		(layer "F.Cu")
		(at 27.94 38.6888)
		(descr "JST SH series connector, SM04B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST SH horizontal")
		(property "Reference" "J_OPT27"
			(at -2.673 -3.9416 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x04_MountingPin"
			(at 0.0508 1.0668 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Connector_JST:JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connectable mounting pin connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digi-Key_PN" "455-SM04B-SRSS-TBCT-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer Part#" "SM04B-SRSS-TB"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??-1MP*")
		(sheetname "Root")
		(sheetfile "UsbGpio_v1b.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -1.5 -2)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 20 "/OUGP2")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -0.5 -2)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+5V")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.5 -2)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 21 "/OMPG7")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at 1.5 -2)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 39 "Net-(J_OPT27-Pin_4)")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "MP" smd roundrect
			(at -2.8 1.875)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 1 "GND")
			(pinfunction "MountPin")
			(pintype "passive")
		)
		(pad "MP" smd roundrect
			(at 2.8 1.875)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 1 "GND")
			(pinfunction "MountPin")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_JST.3dshapes/JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm"
		(layer "F.Cu")
		(at 12.1008 19.558 180)
		(descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "SP_USB5"
			(at -0.2794 1.7272 0)
			(layer "F.SilkS")
		)
		(property "Value" "SolderJumper_2_Open"
			(at -0.0254 1.3462 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 2-pole, open"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(sheetname "Root")
		(sheetfile "UsbGpio_v1b.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "1" smd rect
			(at -0.65 0 180)
			(size 1 1.5)
			(layers "F.Cu" "F.Mask")
			(net 47 "Net-(SP_USB5-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.65 0 180)
			(size 1 1.5)
			(layers "F.Cu" "F.Mask")
			(net 2 "+5V")
			(pinfunction "B")
			(pintype "passive")
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 39.7764 15.9766)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "RADDN1"
			(at -0.2286 -1.4224 0)
			(layer "F.SilkS")
		)
		(property "Value" "10K"
			(at -0.0254 1.27 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digi-Key_PN" "311-10KLGCT-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer Part#" "AC0805FR-0710KL"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "UsbGpio_v1b.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 17 "/ADDR")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3"
		(layer "F.Cu")
		(at 3.81 38.1)
		(descr "Mounting Hole 3.2mm, no annular, M3")
		(tags "mounting hole 3.2mm no annular m3")
		(property "Reference" "H3"
			(at -0.0762 0.0762 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole"
			(at -0.0762 1.6002 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_3.2mm_M3"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "Root")
		(sheetfile "UsbGpio_v1b.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3"
		(layer "F.Cu")
		(at 52.07 38.1)
		(descr "Mounting Hole 3.2mm, no annular, M3")
		(tags "mounting hole 3.2mm no annular m3")
		(property "Reference" "H4"
			(at -0.0762 0.0762 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole"
			(at -0.0762 1.6002 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_3.2mm_M3"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "Root")
		(sheetfile "UsbGpio_v1b.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
	)
	(footprint "Connector_JST:JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal"
		(layer "F.Cu")
		(at 43.7956 38.6888)
		(descr "JST SH series connector, SM04B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST SH horizontal")
		(property "Reference" "J_AD23"
			(at -2.6984 -3.7384 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x04_MountingPin"
			(at 0.0508 1.0668 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Connector_JST:JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connectable mounting pin connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digi-Key_PN" "455-SM04B-SRSS-TBCT-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer Part#" "SM04B-SRSS-TB"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??-1MP*")
		(sheetname "Root")
		(sheetfile "UsbGpio_v1b.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -1.5 -2)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -0.5 -2)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 19 "AIN2")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.5 -2)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at 1.5 -2)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 11 "AIN3")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "MP" smd roundrect
			(at -2.8 1.875)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 1 "GND")
			(pinfunction "MountPin")
			(pintype "passive")
		)
		(pad "MP" smd roundrect
			(at 2.8 1.875)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 1 "GND")
			(pinfunction "MountPin")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_JST.3dshapes/JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 27.5184 20.5994 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "RUGP2"
			(at 0.3404 1.3462 0)
			(layer "F.SilkS")
		)
		(property "Value" "10K"
			(at -0.0254 1.27 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digi-Key_PN" "311-10KLGCT-ND"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer Part#" "AC0805FR-0710KL"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "UsbGpio_v1b.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 27 "UGP2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 11.4788 3.0738 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "RCC2"
			(at 2.1082 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "5K1"
			(at 0 0.735 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digi-Key_PN" "311-5.10KCRCT-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer Part#" "RC0805FR-075K1L"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "UsbGpio_v1b.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 14 "Net-(J_USBC1-CC2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 37.0078 22.5552 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "CAD1"
			(at -0.1016 1.397 -90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.2446 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digi-Key_PN" "399-C0805C104K3RAC7800CT-ND"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer Part#" "C0805C104K3RAC7800"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "UsbGpio_v1b.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -1.0375 0 270)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 270)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.212766)
			(net 5 "+3V3")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 33.5698 30.5562)
		(descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "LED handsolder")
		(property "Reference" "LED7"
			(at -0.1524 1.5494 180)
			(layer "F.SilkS")
		)
		(property "Value" "blue"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digi-Key_PN" "160-1645-1-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer Part#" "C171TBKT"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "Root")
		(sheetfile "UsbGpio_v1b.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -1.025 0)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 21 "/OMPG7")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.025 0)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 48 "Net-(LED7-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
		(layer "F.Cu")
		(at 20.701 13.9842 90)
		(descr "SOIC, 14 Pin (JEDEC MS-012AB, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_14.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U_MCP2221"
			(at 0.0254 -5.1054 90)
			(layer "F.SilkS")
		)
		(property "Value" "MCP2221AxSL"
			(at 0 4.435 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005565B.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "USB to I2C/UART Protocol Converter with GPIO, SOIC-14"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digi-Key_PN" "MCP2221A-I/SL-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer Part#" "MCP2221A-I/SL"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOIC*3.9x8.7mm*P1.27mm*")
		(sheetname "Root")
		(sheetfile "UsbGpio_v1b.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -2.475 -3.81 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "+3V3")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -2.475 -2.54 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 26 "UGP0")
			(pinfunction "GP0")
			(pintype "bidirectional")
		)
		(pad "3" smd roundrect
			(at -2.475 -1.27 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 24 "UGP1")
			(pinfunction "GP1")
			(pintype "bidirectional")
		)
		(pad "4" smd roundrect
			(at -2.475 0 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 33 "Net-(U_MCP2221-~{RST})")
			(pinfunction "~{RST}")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at -2.475 1.27 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 9 "RXD")
			(pinfunction "URx")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at -2.475 2.54 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "TXD")
			(pinfunction "UTx")
			(pintype "output")
		)
		(pad "7" smd roundrect
			(at -2.475 3.81 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 27 "UGP2")
			(pinfunction "GP2")
			(pintype "bidirectional")
		)
		(pad "8" smd roundrect
			(at 2.475 3.81 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 30 "UGP3")
			(pinfunction "GP3")
			(pintype "bidirectional")
		)
		(pad "9" smd roundrect
			(at 2.475 2.54 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "SDA")
			(pinfunction "SDA")
			(pintype "bidirectional")
		)
		(pad "10" smd roundrect
			(at 2.475 1.27 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "SCL")
			(pinfunction "SCL")
			(pintype "bidirectional")
		)
		(pad "11" smd roundrect
			(at 2.475 0 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "Net-(U_MCP2221-VUSB)")
			(pinfunction "VUSB")
			(pintype "passive")
		)
		(pad "12" smd roundrect
			(at 2.475 -1.27 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 13 "USB-")
			(pinfunction "D-")
			(pintype "bidirectional")
		)
		(pad "13" smd roundrect
			(at 2.475 -2.54 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 12 "USB+")
			(pinfunction "D+")
			(pintype "bidirectional")
		)
		(pad "14" smd roundrect
			(at 2.475 -3.81 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-14_3.9x8.7mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 8.89 7.493 180)
		(descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "LED handsolder")
		(property "Reference" "LED3"
			(at 0.0153 1.524 0)
			(layer "F.SilkS")
		)
		(property "Value" "yellow"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digi-Key_PN" "160-1416-1-ND"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer Part#" "LTST-C170KSKT"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "Root")
		(sheetfile "UsbGpio_v1b.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -1.025 0 180)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 1 "GND")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.025 0 180)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 44 "Net-(LED3-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 30.6324 3.2258 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "CMC8"
			(at 2.3114 -0.0762 180)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.2446 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digi-Key_PN" "399-C0805C104K3RAC7800CT-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer Part#" "C0805C104K3RAC7800"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "UsbGpio_v1b.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -1.0375 0 90)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 90)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.212766)
			(net 5 "+3V3")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "UsbGpio:MSOP-10_3x3mm_P0.5mm_MOD"
		(layer "F.Cu")
		(at 41.5544 21.4376)
		(descr "MSOP, 10 Pin (https://www.jedec.org/system/files/docs/mo-187F.pdf variant BA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "MSOP SO")
		(property "Reference" "U_1115"
			(at -0.0508 -2.2352 0)
			(layer "F.SilkS")
		)
		(property "Value" "ADS1115"
			(at 0 1.61 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "UsbGpio:MSOP-10_3x3mm_P0.5mm_MOD"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ads1113.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ultra-Small, Low-Power, I2C-Compatible, 860-SPS, 16-Bit ADCs With Internal Reference, Oscillator, and Programmable Comparator, VSSOP-10"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digi-Key_PN" "296-24934-1-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer Part#" "ADS1115IDGST"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TSSOP*3x3mm*P0.5mm*")
		(sheetname "Root")
		(sheetfile "UsbGpio_v1b.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.0254 1.1684 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -2.1125 -1)
			(size 1.625 0.295)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 17 "/ADDR")
			(pinfunction "ADDR")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -2.1125 -0.5)
			(size 1.625 0.295)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 18 "/RDY")
			(pinfunction "ALERT/RDY")
			(pintype "output")
		)
		(pad "3" smd roundrect
			(at -2.1125 0)
			(size 1.625 0.295)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "4" smd roundrect
			(at -2.1125 0.5)
			(size 1.625 0.295)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 16 "AIN0")
			(pinfunction "AIN0")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at -2.1125 1)
			(size 1.625 0.295)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 22 "AIN1")
			(pinfunction "AIN1")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at 2.1125 1)
			(size 1.625 0.295)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 19 "AIN2")
			(pinfunction "AIN2")
			(pintype "input")
		)
		(pad "7" smd roundrect
			(at 2.1125 0.5)
			(size 1.625 0.295)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 11 "AIN3")
			(pinfunction "AIN3")
			(pintype "input")
		)
		(pad "8" smd roundrect
			(at 2.1125 0)
			(size 1.625 0.295)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "+3V3")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "9" smd roundrect
			(at 2.1125 -0.5)
			(size 1.625 0.295)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "SDA")
			(pinfunction "SDA")
			(pintype "bidirectional")
		)
		(pad "10" smd roundrect
			(at 2.1125 -1)
			(size 1.625 0.295)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "SCL")
			(pinfunction "SCL")
			(pintype "input")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/MSOP-10_3x3mm_P0.5mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_2x08_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 50.8 12.065)
		(descr "Through hole straight pin header, 2x08, 2.54mm pitch, double rows")
		(tags "Through hole pin header THT 2x08 2.54mm double row")
		(property "Reference" "J2"
			(at 1.1684 20.0914 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_02x08_Odd_Even"
			(at 1.1684 15.0622 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_2x08_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, double row, 02x08, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digi-Key_PN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer Part#" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(sheetname "Root")
		(sheetfile "UsbGpio_v1b.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 8.89 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "MGP0")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.54 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "MGP1")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 2.54 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "MGP2")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 2.54 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "MGP3")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 2.54 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" thru_hole oval
			(at 0 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "MGP4")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" thru_hole oval
			(at 2.54 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(pad "11" thru_hole oval
			(at 0 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "MGP5")
			(pinfunction "Pin_11")
			(pintype "passive")
		)
		(pad "12" thru_hole oval
			(at 2.54 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_12")
			(pintype "passive")
		)
		(pad "13" thru_hole oval
			(at 0 15.24)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "AIN3")
			(pinfunction "Pin_13")
			(pintype "passive")
		)
		(pad "14" thru_hole oval
			(at 2.54 15.24)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_14")
			(pintype "passive")
		)
		(pad "15" thru_hole oval
			(at 0 17.78)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "AIN2")
			(pinfunction "Pin_15")
			(pintype "passive")
		)
		(pad "16" thru_hole oval
			(at 2.54 17.78)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_16")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x08_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 35.4857 28.0924)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "RLED7"
			(at 0.0235 -1.397 180)
			(layer "F.SilkS")
		)
		(property "Value" "330"
			(at 0 0.735 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digi-Key_PN" "311-330CRCT-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer Part#" "RC0805FR-07330RL"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "UsbGpio_v1b.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 48 "Net-(LED7-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 46 "Net-(SP_LED7-B)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
		(layer "F.Cu")
		(at 15.9766 25.4508 -90)
		(descr "module CMS SOT223 4 pins")
		(tags "CMS SOT")
		(property "Reference" "U_1117"
			(at -4.826 -0.1778 0)
			(layer "F.SilkS")
		)
		(property "Value" "AZ1117-3.3"
			(at 0.127 3.1496 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AZ1117.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "1A 20V Fixed LDO Linear Regulator, 3.3V, SOT-89/SOT-223/TO-220/TO-252/TO-263"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digi-Key_PN" "AZ1117CH-3.3TRG1DICT-ND"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer Part#" "AZ1117CH-3.3TRG1"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?223* SOT?89* TO?220* TO?252* TO?263*")
		(sheetname "Root")
		(sheetfile "UsbGpio_v1b.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -3.15 -2.3 270)
			(size 2 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -3.15 0 270)
			(size 2 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "+3V3")
			(pinfunction "VO")
			(pintype "power_out")
		)
		(pad "2" smd roundrect
			(at 3.15 0 270)
			(size 2 3.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "+3V3")
			(pinfunction "VO")
			(pintype "power_out")
		)
		(pad "3" smd roundrect
			(at -3.15 2.3 270)
			(size 2 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+5V")
			(pinfunction "VI")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-223.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm"
		(layer "F.Cu")
		(at 40.1932 27.051 180)
		(descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "SP_A2"
			(at -0.0404 1.6764 0)
			(layer "F.SilkS")
		)
		(property "Value" "SolderJumper_2_Open"
			(at -0.0254 1.3462 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 2-pole, open"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(sheetname "Root")
		(sheetfile "UsbGpio_v1b.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "1" smd rect
			(at -0.65 0 180)
			(size 1 1.5)
			(layers "F.Cu" "F.Mask")
			(net 19 "AIN2")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.65 0 180)
			(size 1 1.5)
			(layers "F.Cu" "F.Mask")
			(net 28 "Net-(SP_A2-B)")
			(pinfunction "B")
			(pintype "passive")
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_2x08_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 3.81 12.065)
		(descr "Through hole straight pin header, 2x08, 2.54mm pitch, double rows")
		(tags "Through hole pin header THT 2x08 2.54mm double row")
		(property "Reference" "J1"
			(at 1.397 20.2438 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_02x08_Odd_Even"
			(at 1.1684 15.0622 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_2x08_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, double row, 02x08, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(sheetname "Root")
		(sheetfile "UsbGpio_v1b.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 8.89 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "+5V")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.54 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "+5V")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 2.54 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "+3V3")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "+3V3")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 2.54 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "SDA")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "UGP0")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 2.54 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "SCL")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" thru_hole oval
			(at 0 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "UGP1")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" thru_hole oval
			(at 2.54 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(pad "11" thru_hole oval
			(at 0 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "AIN0")
			(pinfunction "Pin_11")
			(pintype "passive")
		)
		(pad "12" thru_hole oval
			(at 2.54 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "+3V3")
			(pinfunction "Pin_12")
			(pintype "passive")
		)
		(pad "13" thru_hole oval
			(at 0 15.24)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "AIN1")
			(pinfunction "Pin_13")
			(pintype "passive")
		)
		(pad "14" thru_hole oval
			(at 2.54 15.24)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "RXD")
			(pinfunction "Pin_14")
			(pintype "passive")
		)
		(pad "15" thru_hole oval
			(at 0 17.78)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_15")
			(pintype "passive")
		)
		(pad "16" thru_hole oval
			(at 2.54 17.78)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "TXD")
			(pinfunction "Pin_16")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x08_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 40.0718 29.6164 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "RA2"
			(at -0.1364 -1.4224 180)
			(layer "F.SilkS")
		)
		(property "Value" "10K"
			(at -0.0254 1.27 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digi-Key_PN" "311-10KLGCT-ND"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer Part#" "AC0805FR-0710KL"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "UsbGpio_v1b.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 28 "Net-(SP_A2-B)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 5 "+3V3")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm"
		(layer "F.Cu")
		(at 44.4708 27.0764 180)
		(descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "SP_A3"
			(at 0.0462 1.7018 0)
			(layer "F.SilkS")
		)
		(property "Value" "SolderJumper_2_Open"
			(at -0.0254 1.3462 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 2-pole, open"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(sheetname "Root")
		(sheetfile "UsbGpio_v1b.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "1" smd rect
			(at -0.65 0 180)
			(size 1 1.5)
			(layers "F.Cu" "F.Mask")
			(net 11 "AIN3")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.65 0 180)
			(size 1 1.5)
			(layers "F.Cu" "F.Mask")
			(net 29 "Net-(SP_A3-B)")
			(pinfunction "B")
			(pintype "passive")
		)
	)
	(footprint "Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm"
		(layer "B.Cu")
		(at 15.3774 31.3944 180)
		(descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "SP_SERV3"
			(at -0.0404 1.5494 0)
			(layer "B.SilkS")
		)
		(property "Value" "SolderJumper_2_Open"
			(at -0.0254 -1.3462 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 2-pole, open"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(sheetname "Root")
		(sheetfile "UsbGpio_v1b.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "1" smd rect
			(at -0.65 0 180)
			(size 1 1.5)
			(layers "B.Cu" "B.Mask")
			(net 5 "+3V3")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.65 0 180)
			(size 1 1.5)
			(layers "B.Cu" "B.Mask")
			(net 23 "/VSER+")
			(pinfunction "B")
			(pintype "passive")
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D2.0mm"
		(layer "B.Cu")
		(at 12.3952 13.1318 180)
		(descr "SMD pad as test Point, diameter 2.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TRST21"
			(at 0.1016 1.9558 0)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0.1016 -0.6604 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_D2.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "UsbGpio_v1b.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at -0.0508 0.381 0)
			(layer "B.Fab")
			(hide yes)
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 2 2)
			(layers "B.Cu" "B.Mask")
			(net 33 "Net-(U_MCP2221-~{RST})")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Jumper:SolderJumper-3_P1.3mm_Open_Pad1.0x1.5mm"
		(layer "B.Cu")
		(at 32.5374 30.6931)
		(descr "SMD Solder 3-pad Jumper, 1x1.5mm Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "SP_MGP7"
			(at -0.0254 -1.9149 0)
			(layer "B.SilkS")
		)
		(property "Value" "SolderJumper_3_Open"
			(at 0.0254 -1.524 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Jumper:SolderJumper-3_P1.3mm_Open_Pad1.0x1.5mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 3-pole, open"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(sheetname "Root")
		(sheetfile "UsbGpio_v1b.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "1" smd rect
			(at -1.3 0)
			(size 1 1.5)
			(layers "B.Cu" "B.Mask")
			(net 2 "+5V")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0 0)
			(size 1 1.5)
			(layers "B.Cu" "B.Mask")
			(net 39 "Net-(J_OPT27-Pin_4)")
			(pinfunction "C")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 1.3 0)
			(size 1 1.5)
			(layers "B.Cu" "B.Mask")
			(net 5 "+3V3")
			(pinfunction "B")
			(pintype "passive")
		)
	)
	(footprint "Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm"
		(layer "B.Cu")
		(at 33.0858 26.1366)
		(descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "SP_LED7"
			(at 0.1166 -1.5494 0)
			(layer "B.SilkS")
		)
		(property "Value" "SolderJumper_2_Open"
			(at -0.0254 -1.3462 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 2-pole, open"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(sheetname "Root")
		(sheetfile "UsbGpio_v1b.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "1" smd rect
			(at -0.65 0)
			(size 1 1.5)
			(layers "B.Cu" "B.Mask")
			(net 39 "Net-(J_OPT27-Pin_4)")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.65 0)
			(size 1 1.5)
			(layers "B.Cu" "B.Mask")
			(net 46 "Net-(SP_LED7-B)")
			(pinfunction "B")
			(pintype "passive")
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D2.0mm"
		(layer "B.Cu")
		(at 36.1569 5.9817 180)
		(descr "SMD pad as test Point, diameter 2.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TRST08"
			(at 0 1.9812 0)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0.1016 -0.6604 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_D2.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "UsbGpio_v1b.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at -0.0508 0.381 0)
			(layer "B.Fab")
			(hide yes)
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 2 2)
			(layers "B.Cu" "B.Mask")
			(net 31 "Net-(U_MCP23008-~{RESET})")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(gr_line
		(start 52.07 41.91)
		(end 3.81 41.91)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 0 3.81)
		(mid 1.115923 1.115923)
		(end 3.81 0)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 3.81 41.91)
		(mid 1.115923 40.794077)
		(end 0 38.1)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 0 38.1)
		(end 0 3.81)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 55.88 38.1)
		(mid 54.764077 40.794077)
		(end 52.07 41.91)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 52.07 0)
		(mid 54.764077 1.115923)
		(end 55.88 3.81)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 3.81 0)
		(end 52.07 0)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 55.88 3.81)
		(end 55.88 38.1)
		(layer "Edge.Cuts")
	)
	(gr_text "5V"
		(at 31.8516 32.6898 0)
		(layer "B.SilkS")
	)
	(gr_text "Copyright S. Cooper 2024.\nCERN OHL v.1.2  (Open Hardware Licence)\nhttp://ohwr.org/cernohl"
		(at 30.1244 37.6682 0)
		(layer "B.SilkS")
	)
	(gr_text "GND"
		(at 22.5806 32.0802 0)
		(layer "B.SilkS")
	)
	(gr_text "VMGP7"
		(at 24.4094 28.5242 0)
		(layer "B.SilkS")
	)
	(gr_text "3V"
		(at 34.417 32.7152 0)
		(layer "B.SilkS")
	)
	(gr_text "3 Volt logic level only"
		(at 28.194 11.2776 0)
		(layer "B.SilkS")
	)
	(gr_text "UsbGpio\nVersion 1b\n7 Oct 2024"
		(at 28.7782 3.2512 0)
		(layer "B.SilkS")
	)
	(gr_text "V+"
		(at 24.9174 32.0802 0)
		(layer "B.SilkS")
	)
	(gr_text "UsbGpio\nVersion 1b\n7 Oct 2024"
		(at 48.4632 8.3566 0)
		(layer "F.SilkS")
	)
	(gr_text "AIN1"
		(at -0.0508 27.6098 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 18.8736 35.7444 90)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 55.7784 25.8318 90)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 0.0254 30.3276 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 55.7784 20.7772 90)
		(layer "F.SilkS")
	)
	(gr_text "RXD"
		(at 8.2296 27.6606 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 44.6532 35.7378 90)
		(layer "F.SilkS")
	)
	(gr_text "V+"
		(at 23.7744 32.512 0)
		(layer "F.SilkS")
	)
	(gr_text "3V"
		(at 8.2042 15.0622 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 55.5498 13.081 90)
		(layer "F.SilkS")
	)
	(gr_text "MP6"
		(at 37.8192 35.655 90)
		(layer "F.SilkS")
	)
	(gr_text "5V"
		(at 0.7112 12.4968 0)
		(layer "F.SilkS")
	)
	(gr_text "V+"
		(at 29.8898 35.6616 90)
		(layer "F.SilkS")
	)
	(gr_text "MGP0"
		(at 46.3042 12.4968 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 55.7784 23.2918 90)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 8.0518 22.606 0)
		(layer "F.SilkS")
	)
	(gr_text "MGP5"
		(at 46.3042 25.1968 0)
		(layer "F.SilkS")
	)
	(gr_text "SDA"
		(at 13.0048 35.6362 90)
		(layer "F.SilkS")
	)
	(gr_text "3V"
		(at 8.1026 25.0698 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 20.4724 32.512 0)
		(layer "F.SilkS")
	)
	(gr_text "3V"
		(at 0.7112 17.7038 0)
		(layer "F.SilkS")
	)
	(gr_text "MGP4"
		(at 46.3296 22.5806 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 55.8038 18.2626 90)
		(layer "F.SilkS")
	)
	(gr_text "SCL"
		(at 13.9446 35.5854 90)
		(layer "F.SilkS")
	)
	(gr_text "TXD"
		(at 21.9202 35.6108 90)
		(layer "F.SilkS")
	)
	(gr_text "MGP1"
		(at 46.3296 15.113 0)
		(layer "F.SilkS")
	)
	(gr_text "RXD"
		(at 20.8788 35.687 90)
		(layer "F.SilkS")
	)
	(gr_text "AIN3"
		(at 46.7868 27.7114 0)
		(layer "F.SilkS")
	)
	(gr_text "3V"
		(at 35.8126 35.6296 90)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 10.9488 35.6682 90)
		(layer "F.SilkS")
	)
	(gr_text "UGP1"
		(at -0.127 22.7076 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 42.6988 35.719 90)
		(layer "F.SilkS")
	)
	(gr_text "UGP2"
		(at 26.8686 35.7698 90)
		(layer "F.SilkS")
	)
	(gr_text "TXD"
		(at 8.2804 30.1752 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 34.7458 35.7566 90)
		(layer "F.SilkS")
	)
	(gr_text "AIN2"
		(at 43.6894 35.592 90)
		(layer "F.SilkS")
	)
	(gr_text "UGP0"
		(at -0.1016 20.0152 0)
		(layer "F.SilkS")
	)
	(gr_text "5V"
		(at 0.6858 15.0876 0)
		(layer "F.SilkS")
	)
	(gr_text "AIN2"
		(at 46.8122 30.2768 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 55.7784 15.6464 90)
		(layer "F.SilkS")
	)
	(gr_text "3V"
		(at 19.8882 35.6108 90)
		(layer "F.SilkS")
	)
	(gr_text "SDA"
		(at 8.1534 17.526 0)
		(layer "F.SilkS")
	)
	(gr_text "AIN3"
		(at 45.6946 35.6682 90)
		(layer "F.SilkS")
	)
	(gr_text "MGP2"
		(at 46.3042 17.526 0)
		(layer "F.SilkS")
	)
	(gr_text "SCL"
		(at 8.0772 20.1676 0)
		(layer "F.SilkS")
	)
	(gr_text "3V"
		(at 12.0142 35.56 90)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 55.7784 28.3718 90)
		(layer "F.SilkS")
	)
	(gr_text "AIN0"
		(at 0 25.1206 0)
		(layer "F.SilkS")
	)
	(gr_text "MPG7"
		(at 28.8498 35.7444 90)
		(layer "F.SilkS")
	)
	(gr_text "UGP3"
		(at 36.8554 35.6616 90)
		(layer "F.SilkS")
	)
	(gr_text "5V"
		(at 27.8578 35.7124 90)
		(layer "F.SilkS")
	)
	(gr_text "MGP3"
		(at 46.3042 20.0914 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 55.5498 30.861 90)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 8.128 12.4968 0)
		(layer "F.SilkS")
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 15.9766 7.0866) (xy 21.336 7.0866) (xy 21.3106 8.509) (xy 15.9766 8.509)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.4)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy -0.635 -0.635) (xy 56.515 -0.635) (xy 56.515 42.545) (xy -0.635 42.545)
			)
		)
	)
)
