(kicad_pcb (version 20171130) (host pcbnew "(5.1.4-0)")
  (general
    (thickness 1.6)
    (drawings 13)
    (tracks 136)
    (zones 0)
    (modules 21)
    (nets 20)
  )
  (page A4)
  (title_block
    (date 2019-10-09)
    (rev 1.1)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.254)
    (user_trace_width 0.3048)
    (user_trace_width 0.3556)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.1016)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "manufacturing/"))
  )
  (net 0 "")
  (net 1 "Net-(J2-PadT)")
  (net 2 "Net-(J2-PadS)")
  (net 3 "Net-(J3-PadT)")
  (net 4 "Net-(J3-PadS)")
  (net 5 /POW_A)
  (net 6 /GND)
  (net 7 /DIO_C)
  (net 8 /5VDC)
  (net 9 /POW_B)
  (net 10 "Net-(C5-Pad2)")
  (net 11 "Net-(R1-Pad1)")
  (net 12 "Net-(C6-Pad1)")
  (net 13 "Net-(R2-Pad1)")
  (net 14 "Net-(C3-Pad1)")
  (net 15 "Net-(C4-Pad1)")
  (net 16 "Net-(C3-Pad2)")
  (net 17 "Net-(C4-Pad2)")
  (net 18 /RX)
  (net 19 /TX)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /12VDC)
    (add_net /5VDC)
    (add_net /DIO_C)
    (add_net /GND)
    (add_net /POW_A)
    (add_net /POW_B)
    (add_net /RX)
    (add_net /TX)
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C4-Pad2)")
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(J2-PadS)")
    (add_net "Net-(J2-PadT)")
    (add_net "Net-(J3-PadS)")
    (add_net "Net-(J3-PadT)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(J4-Pad2)")
    (add_net "Net-(J4-Pad3)")
    (add_net "Net-(J4-Pad4)")
    (add_net "Net-(J4-Pad5)")
    (add_net "Net-(J4-Pad6)")
    (add_net "Net-(J4-Pad7)")
    (add_net "Net-(J4-Pad8)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(U1-Pad11)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U1-Pad13)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U1-Pad15)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U1-Pad8)")
    (add_net "Net-(U1-Pad9)")
  )
  (module asl_footprints:RJ45_SMD (layer F.Cu) (tedit 5D49D52B)
    (at 135.128 83.82 180)
    (descr "SMD RJ45")
    (fp_text reference J1 (at 10.16 -1.143) (layer F.SilkS))
    (fp_text value "RJ45 Jack" (at 6.858 -2.413) (layer F.SilkS) hide)
    (pad G2 smd rect (at 7.35 -7.88 180) (size 3.7 2.2) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at 4.445 -18.205 270) (size 6.35 0.76) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at 3.175 -18.205 270) (size 6.35 0.76) (layers F.Cu F.Paste F.Mask)
      (net 9 /POW_B))
    (pad 6 smd rect (at 1.905 -18.205 270) (size 6.35 0.76) (layers F.Cu F.Paste F.Mask)
      (net 8 /5VDC))
    (pad 5 smd rect (at 0.635 -18.205 270) (size 6.35 0.76) (layers F.Cu F.Paste F.Mask)
      (net 7 /DIO_C))
    (pad 1 smd rect (at -4.445 -18.205 270) (size 6.35 0.76) (layers F.Cu F.Paste F.Mask)
      (net 19 /TX))
    (pad 2 smd rect (at -3.175 -18.205 270) (size 6.35 0.76) (layers F.Cu F.Paste F.Mask)
      (net 6 /GND))
    (pad 3 smd rect (at -1.905 -18.205 270) (size 6.35 0.76) (layers F.Cu F.Paste F.Mask)
      (net 5 /POW_A))
    (pad G1 smd rect (at -7.35 -7.88 180) (size 3.7 2.2) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at -0.635 -18.205 270) (size 6.35 0.76) (layers F.Cu F.Paste F.Mask)
      (net 18 /RX))
  )
  (module asl_footprints:8pin_header (layer F.Cu) (tedit 5D9E27D5)
    (at 156.718 116.205)
    (descr ".1\" Screw terminal")
    (tags "8pos, screw, terminal")
    (fp_text reference X2 (at -2.413 0) (layer F.SilkS))
    (fp_text value 8pin_header (at 0.127 11.684) (layer F.Fab))
  )
  (module asl_footprints:8pin_header (layer F.Cu) (tedit 5D9E27D5)
    (at 138.938 116.205)
    (descr ".1\" Screw terminal")
    (tags "8pos, screw, terminal")
    (fp_text reference X1 (at 2.413 0) (layer F.SilkS))
    (fp_text value 8pin_header (at 0.127 11.684) (layer F.Fab))
  )
  (module asl_footprints:MonoJack (layer F.Cu) (tedit 5D49CFC1)
    (at 166.37 92.456)
    (fp_text reference J3 (at -3.81 -7.62) (layer F.SilkS))
    (fp_text value "Mono Audio Jack" (at 0.254 12.446) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 4.5) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 -2.5) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask))
    (pad T smd rect (at -3.7 5.8) (size 2.8 2.8) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J3-PadT)"))
    (pad TN smd rect (at 0.75 9.8) (size 2.8 2.6) (layers F.Cu F.Paste F.Mask))
    (pad S smd rect (at -3.7 -3.6) (size 2.8 2.2) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J3-PadS)"))
  )
  (module asl_footprints:MonoJack (layer F.Cu) (tedit 5D49CFC1)
    (at 154.94 92.456)
    (fp_text reference J2 (at -4.064 -7.62) (layer F.SilkS))
    (fp_text value "Mono Audio Jack" (at 0.254 12.446) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 4.5) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 -2.5) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask))
    (pad T smd rect (at -3.7 5.8) (size 2.8 2.8) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J2-PadT)"))
    (pad TN smd rect (at 0.75 9.8) (size 2.8 2.6) (layers F.Cu F.Paste F.Mask))
    (pad S smd rect (at -3.7 -3.6) (size 2.8 2.2) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J2-PadS)"))
  )
  (module asl_footprints:DIN_Clip (layer F.Cu) (tedit 5D0BF83A)
    (at 147.828 105.41)
    (fp_text reference DRA1 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value DIN_Rail_Adapter (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 12.5) (size 3 3) (drill 3) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 -12.5) (size 3 3) (drill 3) (layers *.Cu *.Mask))
  )
  (module Package_SO:SOIC-8_3.9x4.9mm_P1.27mm (layer F.Cu) (tedit 5C97300E)
    (at 131.318 119.507)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference U2 (at -4.699 -2.032 180) (layer F.SilkS))
    (fp_text value NCS2211 (at 0 3.4) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 8 smd roundrect (at 2.475 -1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(J2-PadS)"))
    (pad 7 smd roundrect (at 2.475 -0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 /GND))
    (pad 6 smd roundrect (at 2.475 0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 /5VDC))
    (pad 5 smd roundrect (at 2.475 1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 "Net-(J2-PadT)"))
    (pad 4 smd roundrect (at -2.475 1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(R1-Pad1)"))
    (pad 3 smd roundrect (at -2.475 0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(C5-Pad2)"))
    (pad 2 smd roundrect (at -2.475 -0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(C5-Pad2)"))
    (pad 1 smd roundrect (at -2.475 -1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /POW_A))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-8_3.9x4.9mm_P1.27mm (layer F.Cu) (tedit 5C97300E)
    (at 164.338 119.253)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference U3 (at -4.699 -1.905 180) (layer F.SilkS))
    (fp_text value NCS2211 (at 0 3.4) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 8 smd roundrect (at 2.475 -1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(J3-PadS)"))
    (pad 7 smd roundrect (at 2.475 -0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 /GND))
    (pad 6 smd roundrect (at 2.475 0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 /5VDC))
    (pad 5 smd roundrect (at 2.475 1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(J3-PadT)"))
    (pad 4 smd roundrect (at -2.475 1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(R2-Pad1)"))
    (pad 3 smd roundrect (at -2.475 0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(C6-Pad1)"))
    (pad 2 smd roundrect (at -2.475 -0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(C6-Pad1)"))
    (pad 1 smd roundrect (at -2.475 -1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 /POW_B))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module asl_footprints:DFPlayer (layer F.Cu) (tedit 5D3B1071)
    (at 147.828 116.205)
    (descr ".1\" Screw terminal")
    (tags "8pos, screw, terminal")
    (fp_text reference U1 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value DFPlayer (at 7.62 11.43) (layer F.Fab))
    (pad 14 thru_hole circle (at 8.89 -3.81) (size 1.524 1.524) (drill 0.95) (layers *.Cu *.Mask))
    (pad 13 thru_hole circle (at 8.89 -1.27) (size 1.524 1.524) (drill 0.95) (layers *.Cu *.Mask))
    (pad 12 thru_hole circle (at 8.89 1.27) (size 1.524 1.524) (drill 0.95) (layers *.Cu *.Mask))
    (pad 11 thru_hole circle (at 8.89 3.81) (size 1.524 1.524) (drill 0.95) (layers *.Cu *.Mask))
    (pad 10 thru_hole circle (at 8.89 6.35) (size 1.524 1.524) (drill 0.95) (layers *.Cu *.Mask)
      (net 6 /GND))
    (pad 9 thru_hole circle (at 8.89 8.89) (size 1.524 1.524) (drill 0.95) (layers *.Cu *.Mask))
    (pad 15 thru_hole circle (at 8.89 -6.35) (size 1.524 1.524) (drill 0.95) (layers *.Cu *.Mask))
    (pad 16 thru_hole circle (at 8.89 -8.89) (size 1.524 1.524) (drill 0.95) (layers *.Cu *.Mask)
      (net 7 /DIO_C))
    (pad 8 thru_hole circle (at -8.89 8.89) (size 1.524 1.524) (drill 0.95) (layers *.Cu *.Mask))
    (pad 7 thru_hole circle (at -8.89 6.35) (size 1.524 1.524) (drill 0.95) (layers *.Cu *.Mask)
      (net 6 /GND))
    (pad 6 thru_hole circle (at -8.89 3.81) (size 1.524 1.524) (drill 0.95) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at -8.89 1.27) (size 1.524 1.524) (drill 0.95) (layers *.Cu *.Mask)
      (net 14 "Net-(C3-Pad1)"))
    (pad 4 thru_hole circle (at -8.89 -1.27) (size 1.524 1.524) (drill 0.95) (layers *.Cu *.Mask)
      (net 15 "Net-(C4-Pad1)"))
    (pad 3 thru_hole circle (at -8.89 -3.81) (size 1.524 1.524) (drill 0.95) (layers *.Cu *.Mask)
      (net 18 /RX))
    (pad 2 thru_hole circle (at -8.89 -6.35) (size 1.524 1.524) (drill 0.95) (layers *.Cu *.Mask)
      (net 19 /TX))
    (pad 1 thru_hole circle (at -8.89 -8.89) (size 1.524 1.524) (drill 0.95) (layers *.Cu *.Mask)
      (net 8 /5VDC))
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 131.953 107.95 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 10µF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 /5VDC))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 /GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 134.366 107.95 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at 0 1.778 90) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 /5VDC))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 /GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 134.493 124.1275 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 1µF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 "Net-(C3-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(C3-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 167.513 123.8735 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 1µF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 "Net-(C4-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 "Net-(C4-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 131.318 113.538 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C5 (at -2.667 -0.127) (layer F.SilkS))
    (fp_text value 1µF (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(C5-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 /GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 164.338 113.284)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C6 (at 2.667 0.127) (layer F.SilkS))
    (fp_text value 1µF (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 /GND))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(C6-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 128.143 124.1275 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 0 1.651 90) (layer F.SilkS))
    (fp_text value 10KΩ (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 "Net-(C3-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(R1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 161.163 123.8735 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at -0.0485 1.651 90) (layer F.SilkS))
    (fp_text value 10KΩ (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 "Net-(C4-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(R2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 131.318 115.697 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at -2.667 0) (layer F.SilkS))
    (fp_text value 10KΩ (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /POW_A))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 /5VDC))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 164.338 115.443 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at -2.667 -0.127) (layer F.SilkS))
    (fp_text value 10KΩ (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 /POW_B))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 /5VDC))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 131.318 123.382)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at 0 1.713) (layer F.SilkS))
    (fp_text value 15KΩ (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 "Net-(J2-PadT)"))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(R1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 164.338 123.128)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R6 (at 0.127 1.713) (layer F.SilkS))
    (fp_text value 15KΩ (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(J3-PadT)"))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(R2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Licensed under the\nTAPR Open Hardware License\n(www.tapr.org/OHL)" (at 166.37 113.03 270) (layer B.SilkS))
  (gr_text "Audio\nPlayer\nv1.1" (at 133.35 90.932) (layer B.SilkS))
  (gr_arc (start 168.783 85.725) (end 170.688 85.725) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 126.873 85.725) (end 126.873 83.82) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 168.783 125.095) (end 168.783 127) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 126.873 125.095) (end 124.968 125.095) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_text Left (at 153.94 102.616) (layer F.SilkS))
  (gr_text Right (at 165.37 102.616) (layer F.SilkS))
  (gr_text "Audio\nPlayer\nv1.1" (at 164.592 108.204) (layer F.SilkS))
  (gr_line (start 124.968 125.095) (end 124.968 85.725) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 168.783 127) (end 126.873 127) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 170.688 85.725) (end 170.688 125.095) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 126.873 83.82) (end 168.783 83.82) (layer Edge.Cuts) (width 0.05))
  (zone (net 6) (net_name /GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 117.983 81.28) (xy 174.498 81.28) (xy 174.498 129.54) (xy 117.983 129.54)
      )
    )
  )
  (zone (net 6) (net_name /GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 117.983 81.28) (xy 174.498 81.28) (xy 174.498 129.54) (xy 117.983 129.54)
      )
    )
  )
)
