<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.2.0">
<drawing>
<board>
<plain>
<wire x1="33.161378125" y1="43.039234375" x2="3.8805875" y2="43.039234375" width="0.3048" layer="46"/>
<wire x1="3.8805875" y1="43.039234375" x2="0" y2="39.158646875" width="0.3048" layer="46" curve="90"/>
<wire x1="0" y1="39.158646875" x2="-0.42280625" y2="12.692175" width="0.3048" layer="46"/>
<wire x1="-0.42280625" y1="12.692175" x2="0.7396" y2="10.08940625" width="0.3048" layer="46" curve="47.885224"/>
<wire x1="0.7396" y1="10.08940625" x2="-0.323765625" y2="7.549446875" width="0.3048" layer="46" curve="46.397031"/>
<wire x1="-0.323765625" y1="7.549446875" x2="-0.35278125" y2="3.175025" width="0.3048" layer="46"/>
<wire x1="-0.35278125" y1="3.175025" x2="3.175025" y2="-0.35278125" width="0.3048" layer="46" curve="90"/>
<wire x1="3.175025" y1="-0.35278125" x2="33.8669375" y2="-0.35278125" width="0.3048" layer="46"/>
<wire x1="33.8669375" y1="-0.35278125" x2="37.0419625" y2="3.175025" width="0.3048" layer="46" curve="90"/>
<wire x1="37.0419625" y1="3.175025" x2="37.08225" y2="8.45658125" width="0.3048" layer="46"/>
<wire x1="37.08225" y1="8.45658125" x2="36.275965625" y2="10.331409375" width="0.3048" layer="46" curve="36.869827"/>
<wire x1="36.275965625" y1="10.331409375" x2="37.142684375" y2="13.12320625" width="0.3048" layer="46" curve="53.130468"/>
<wire x1="37.142684375" y1="13.12320625" x2="36.689184375" y2="38.805865625" width="0.3048" layer="46"/>
<wire x1="36.689184375" y1="38.805865625" x2="33.161378125" y2="43.039234375" width="0.3048" layer="46" curve="90"/>
<text>+</text>
<text>Solder
Pin Here</text>
<text>Living Computers</text>
<text>Living Computers + Labs</text>
<text>Design by Richard Albritton</text>
<text>Bit Badge V2</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="LED5MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
5 mm, round</description>
</package>
<package name="CR2032-SMD">
</package>
<package name="0207/9">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="+" library="adafruit" package="LED5MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BAT" library="adafruit" package="CR2032-SMD" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED2" library="adafruit" package="LED5MM" value="">
<attribute name="VALUE"/>
</element>
<element name="R1" library="adafruit" package="0207/9" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="adafruit" package="0207/9" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="S$1">
</signal>
<signal name="S$2">
</signal>
<signal name="VIN">
<contactref element="R1" pad="1"/>
<contactref element="BAT" pad="+$1"/>
<contactref element="R2" pad="1"/>
<contactref element="BAT" pad="+$2"/>
</signal>
<signal name="GND">
<contactref element="BAT" pad="-"/>
<contactref element="+" pad="K"/>
<contactref element="LED2" pad="K"/>
</signal>
<signal name="S$6">
<contactref element="LED2" pad="A"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="S$7">
<contactref element="+" pad="A"/>
<contactref element="R1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
