(kicad_pcb (version 20171130) (host pcbnew "(5.1.0)-1")
  (general
    (thickness 1.6)
    (drawings 12)
    (tracks 189)
    (zones 0)
    (modules 20)
    (nets 17)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.1778)
    (user_trace_width 0.381)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1778)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.1016)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad1)")
  (net 2 "Net-(J2-Pad1)")
  (net 3 "Net-(J3-Pad1)")
  (net 4 "Net-(J4-Pad1)")
  (net 5 VCC)
  (net 6 "Net-(J6-Pad1)")
  (net 7 "Net-(J7-Pad1)")
  (net 8 "Net-(J8-Pad1)")
  (net 9 "Net-(J9-Pad1)")
  (net 10 "Net-(J10-Pad1)")
  (net 11 "Net-(J11-Pad1)")
  (net 12 GND)
  (net 13 "Net-(J13-Pad1)")
  (net 14 "Net-(J14-Pad1)")
  (net 15 "Net-(J15-Pad1)")
  (net 16 "Net-(J16-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.1778)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J10-Pad1)")
    (add_net "Net-(J11-Pad1)")
    (add_net "Net-(J13-Pad1)")
    (add_net "Net-(J14-Pad1)")
    (add_net "Net-(J15-Pad1)")
    (add_net "Net-(J16-Pad1)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(J6-Pad1)")
    (add_net "Net-(J7-Pad1)")
    (add_net "Net-(J8-Pad1)")
    (add_net "Net-(J9-Pad1)")
    (add_net VCC)
  )
  (module Active:SOP127P620X175-8 (layer F.Cu) (tedit 5FC2DAA4)
    (at 143.51 67.31 90)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U4 (at 0 -3.5 90) (layer F.SilkS) hide)
    (fp_text value LM555 (at 0 3.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 8 smd rect (at 2.5 -1.905 90) (size 2 0.55) (layers F.Cu F.Paste F.Mask)
      (net 5 VCC))
    (pad 7 smd rect (at 2.5 -0.635 90) (size 2 0.55) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(J15-Pad1)"))
    (pad 6 smd rect (at 2.5 0.635 90) (size 2 0.55) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(J15-Pad1)"))
    (pad 5 smd rect (at 2.5 1.905 90) (size 2 0.55) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J4-Pad1)"))
    (pad 4 smd rect (at -2.5 1.905 90) (size 2 0.55) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(J13-Pad1)"))
    (pad 3 smd rect (at -2.5 0.635 90) (size 2 0.55) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(J16-Pad1)"))
    (pad 2 smd rect (at -2.5 -0.635 90) (size 2 0.55) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(J14-Pad1)"))
    (pad 1 smd rect (at -2.5 -1.905 90) (size 2 0.55) (layers F.Cu F.Paste F.Mask)
      (net 12 GND))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Active:SOP127P620X175-8 (layer B.Cu) (tedit 5FC2DAA4)
    (at 143.51 77.47 270)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U3 (at 0 3.5 270) (layer B.SilkS) hide)
    (fp_text value LM555 (at 0 -3.5 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 8 smd rect (at 2.5 1.905 270) (size 2 0.55) (layers B.Cu B.Paste B.Mask)
      (net 5 VCC))
    (pad 7 smd rect (at 2.5 0.635 270) (size 2 0.55) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(J10-Pad1)"))
    (pad 6 smd rect (at 2.5 -0.635 270) (size 2 0.55) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(J10-Pad1)"))
    (pad 5 smd rect (at 2.5 -1.905 270) (size 2 0.55) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(J4-Pad1)"))
    (pad 4 smd rect (at -2.5 -1.905 270) (size 2 0.55) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(J13-Pad1)"))
    (pad 3 smd rect (at -2.5 -0.635 270) (size 2 0.55) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(J9-Pad1)"))
    (pad 2 smd rect (at -2.5 0.635 270) (size 2 0.55) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(J11-Pad1)"))
    (pad 1 smd rect (at -2.5 1.905 270) (size 2 0.55) (layers B.Cu B.Paste B.Mask)
      (net 12 GND))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Active:SOP127P620X175-8 (layer F.Cu) (tedit 5FC2DAA4)
    (at 143.51 77.47 90)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U2 (at 0 -3.5 90) (layer F.SilkS) hide)
    (fp_text value LM555 (at 0 3.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 8 smd rect (at 2.5 -1.905 90) (size 2 0.55) (layers F.Cu F.Paste F.Mask)
      (net 5 VCC))
    (pad 7 smd rect (at 2.5 -0.635 90) (size 2 0.55) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J7-Pad1)"))
    (pad 6 smd rect (at 2.5 0.635 90) (size 2 0.55) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J7-Pad1)"))
    (pad 5 smd rect (at 2.5 1.905 90) (size 2 0.55) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J4-Pad1)"))
    (pad 4 smd rect (at -2.5 1.905 90) (size 2 0.55) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(J13-Pad1)"))
    (pad 3 smd rect (at -2.5 0.635 90) (size 2 0.55) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J8-Pad1)"))
    (pad 2 smd rect (at -2.5 -0.635 90) (size 2 0.55) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J6-Pad1)"))
    (pad 1 smd rect (at -2.5 -1.905 90) (size 2 0.55) (layers F.Cu F.Paste F.Mask)
      (net 12 GND))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Active:SOP127P620X175-8 (layer B.Cu) (tedit 5FC2DAA4)
    (at 143.51 67.31 270)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1 (at 0 3.5 270) (layer B.SilkS) hide)
    (fp_text value LM555 (at 0 -3.5 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 8 smd rect (at 2.5 1.905 270) (size 2 0.55) (layers B.Cu B.Paste B.Mask)
      (net 5 VCC))
    (pad 7 smd rect (at 2.5 0.635 270) (size 2 0.55) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(J2-Pad1)"))
    (pad 6 smd rect (at 2.5 -0.635 270) (size 2 0.55) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(J2-Pad1)"))
    (pad 5 smd rect (at 2.5 -1.905 270) (size 2 0.55) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(J4-Pad1)"))
    (pad 4 smd rect (at -2.5 -1.905 270) (size 2 0.55) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(J13-Pad1)"))
    (pad 3 smd rect (at -2.5 -0.635 270) (size 2 0.55) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 2 smd rect (at -2.5 0.635 270) (size 2 0.55) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(J3-Pad1)"))
    (pad 1 smd rect (at -2.5 1.905 270) (size 2 0.55) (layers B.Cu B.Paste B.Mask)
      (net 12 GND))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Conn:MILL-MAX_0542-0-00-15-00-00-03-0 (layer F.Cu) (tedit 5EEE6BC7)
    (at 147.32 63.5)
    (fp_text reference J16 (at 0 -1.524) (layer F.SilkS) hide)
    (fp_text value OUTD (at 0 1.778) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 16 "Net-(J16-Pad1)"))
    (model :3d:mill_max-0542-0-00-15-00-00-03-0.STEP
      (offset (xyz 0 0 0.35))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Conn:MILL-MAX_0542-0-00-15-00-00-03-0 (layer F.Cu) (tedit 5EEE6BC7)
    (at 147.32 66.04)
    (fp_text reference J15 (at 0 -1.524) (layer F.SilkS) hide)
    (fp_text value TIMD (at 0 1.778) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 15 "Net-(J15-Pad1)"))
    (model :3d:mill_max-0542-0-00-15-00-00-03-0.STEP
      (offset (xyz 0 0 0.35))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Conn:MILL-MAX_0542-0-00-15-00-00-03-0 (layer F.Cu) (tedit 5EEE6BC7)
    (at 147.32 68.58)
    (fp_text reference J14 (at 0 -1.524) (layer F.SilkS) hide)
    (fp_text value TRIGD (at 0 1.778) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 14 "Net-(J14-Pad1)"))
    (model :3d:mill_max-0542-0-00-15-00-00-03-0.STEP
      (offset (xyz 0 0 0.35))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Conn:MILL-MAX_0542-0-00-15-00-00-03-0 (layer F.Cu) (tedit 5EEE6BC7)
    (at 147.32 71.12)
    (fp_text reference J13 (at 0 -1.524) (layer F.SilkS) hide)
    (fp_text value RESET (at 0 1.778) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 13 "Net-(J13-Pad1)"))
    (model :3d:mill_max-0542-0-00-15-00-00-03-0.STEP
      (offset (xyz 0 0 0.35))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Conn:MILL-MAX_0542-0-00-15-00-00-03-0 (layer F.Cu) (tedit 5EEE6BC7)
    (at 147.32 73.66)
    (fp_text reference J12 (at 0 -1.524) (layer F.SilkS) hide)
    (fp_text value GND (at 0 1.778) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 12 GND))
    (model :3d:mill_max-0542-0-00-15-00-00-03-0.STEP
      (offset (xyz 0 0 0.35))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Conn:MILL-MAX_0542-0-00-15-00-00-03-0 (layer F.Cu) (tedit 5EEE6BC7)
    (at 147.32 76.2)
    (fp_text reference J11 (at 0 -1.524) (layer F.SilkS) hide)
    (fp_text value TRIGC (at 0 1.778) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 11 "Net-(J11-Pad1)"))
    (model :3d:mill_max-0542-0-00-15-00-00-03-0.STEP
      (offset (xyz 0 0 0.35))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Conn:MILL-MAX_0542-0-00-15-00-00-03-0 (layer F.Cu) (tedit 5EEE6BC7)
    (at 147.32 78.74)
    (fp_text reference J10 (at 0 -1.524) (layer F.SilkS) hide)
    (fp_text value TIMC (at 0 1.778) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 10 "Net-(J10-Pad1)"))
    (model :3d:mill_max-0542-0-00-15-00-00-03-0.STEP
      (offset (xyz 0 0 0.35))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Conn:MILL-MAX_0542-0-00-15-00-00-03-0 (layer F.Cu) (tedit 5EEE6BC7)
    (at 147.32 81.28)
    (fp_text reference J9 (at 0 -1.524) (layer F.SilkS) hide)
    (fp_text value OUTC (at 0 1.778) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 9 "Net-(J9-Pad1)"))
    (model :3d:mill_max-0542-0-00-15-00-00-03-0.STEP
      (offset (xyz 0 0 0.35))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Conn:MILL-MAX_0542-0-00-15-00-00-03-0 (layer F.Cu) (tedit 5EEE6BC7)
    (at 139.7 81.28)
    (fp_text reference J8 (at 0 -1.524) (layer F.SilkS) hide)
    (fp_text value OUTB (at 0 1.778) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 8 "Net-(J8-Pad1)"))
    (model :3d:mill_max-0542-0-00-15-00-00-03-0.STEP
      (offset (xyz 0 0 0.35))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Conn:MILL-MAX_0542-0-00-15-00-00-03-0 (layer F.Cu) (tedit 5EEE6BC7)
    (at 139.7 78.74)
    (fp_text reference J7 (at 0 -1.524) (layer F.SilkS) hide)
    (fp_text value TIMB (at 0 1.778) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 7 "Net-(J7-Pad1)"))
    (model :3d:mill_max-0542-0-00-15-00-00-03-0.STEP
      (offset (xyz 0 0 0.35))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Conn:MILL-MAX_0542-0-00-15-00-00-03-0 (layer F.Cu) (tedit 5EEE6BC7)
    (at 139.7 76.2)
    (fp_text reference J6 (at 0 -1.524) (layer F.SilkS) hide)
    (fp_text value TRIGB (at 0 1.778) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 6 "Net-(J6-Pad1)"))
    (model :3d:mill_max-0542-0-00-15-00-00-03-0.STEP
      (offset (xyz 0 0 0.35))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Conn:MILL-MAX_0542-0-00-15-00-00-03-0 (layer F.Cu) (tedit 5EEE6BC7)
    (at 139.7 73.66)
    (fp_text reference J5 (at 0 -1.524) (layer F.SilkS) hide)
    (fp_text value VCC (at 0 1.778) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 5 VCC))
    (model :3d:mill_max-0542-0-00-15-00-00-03-0.STEP
      (offset (xyz 0 0 0.35))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Conn:MILL-MAX_0542-0-00-15-00-00-03-0 (layer F.Cu) (tedit 5EEE6BC7)
    (at 139.7 71.12)
    (fp_text reference J4 (at 0 -1.524) (layer F.SilkS) hide)
    (fp_text value CV (at 0 1.778) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 4 "Net-(J4-Pad1)"))
    (model :3d:mill_max-0542-0-00-15-00-00-03-0.STEP
      (offset (xyz 0 0 0.35))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Conn:MILL-MAX_0542-0-00-15-00-00-03-0 (layer F.Cu) (tedit 5EEE6BC7)
    (at 139.7 68.58)
    (fp_text reference J3 (at 0 -1.524) (layer F.SilkS) hide)
    (fp_text value TRIGA (at 0 1.778) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 3 "Net-(J3-Pad1)"))
    (model :3d:mill_max-0542-0-00-15-00-00-03-0.STEP
      (offset (xyz 0 0 0.35))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Conn:MILL-MAX_0542-0-00-15-00-00-03-0 (layer F.Cu) (tedit 5EEE6BC7)
    (at 139.7 66.04)
    (fp_text reference J2 (at 0 -1.524) (layer F.SilkS) hide)
    (fp_text value TIMA (at 0 1.778) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 2 "Net-(J2-Pad1)"))
    (model :3d:mill_max-0542-0-00-15-00-00-03-0.STEP
      (offset (xyz 0 0 0.35))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Conn:MILL-MAX_0542-0-00-15-00-00-03-0 (layer F.Cu) (tedit 5EEE6BC7)
    (at 139.7 63.5)
    (fp_text reference J1 (at 0 -1.524) (layer F.SilkS) hide)
    (fp_text value OUTA (at 0 1.778) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (model :3d:mill_max-0542-0-00-15-00-00-03-0.STEP
      (offset (xyz 0 0 0.35))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (gr_text "NE558-Alike Quad Timer" (at 138.049 73.152 90) (layer F.SilkS))
  (gr_text "©2020 TubeTime" (at 149.098 72.39 90) (layer F.SilkS))
  (dimension 21.59 (width 0.15) (layer Dwgs.User)
    (gr_text "0.8500 in" (at 154.97 72.517 270) (layer Dwgs.User))
    (feature1 (pts (xy 151.13 83.312) (xy 154.256421 83.312)))
    (feature2 (pts (xy 151.13 61.722) (xy 154.256421 61.722)))
    (crossbar (pts (xy 153.67 61.722) (xy 153.67 83.312)))
    (arrow1a (pts (xy 153.67 83.312) (xy 153.083579 82.185496)))
    (arrow1b (pts (xy 153.67 83.312) (xy 154.256421 82.185496)))
    (arrow2a (pts (xy 153.67 61.722) (xy 153.083579 62.848504)))
    (arrow2b (pts (xy 153.67 61.722) (xy 154.256421 62.848504)))
  )
  (dimension 12.7 (width 0.15) (layer Dwgs.User)
    (gr_text "0.5000 in" (at 143.51 54.58) (layer Dwgs.User))
    (feature1 (pts (xy 149.86 59.69) (xy 149.86 55.293579)))
    (feature2 (pts (xy 137.16 59.69) (xy 137.16 55.293579)))
    (crossbar (pts (xy 137.16 55.88) (xy 149.86 55.88)))
    (arrow1a (pts (xy 149.86 55.88) (xy 148.733496 56.466421)))
    (arrow1b (pts (xy 149.86 55.88) (xy 148.733496 55.293579)))
    (arrow2a (pts (xy 137.16 55.88) (xy 138.286504 56.466421)))
    (arrow2b (pts (xy 137.16 55.88) (xy 138.286504 55.293579)))
  )
  (gr_text 1 (at 138.176 63.5) (layer F.SilkS))
  (gr_text 558D (at 143.51 72.39) (layer F.SilkS))
  (gr_line (start 138.43 61.722) (end 137.16 62.992) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 149.86 83.312) (end 149.86 61.722) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 137.16 83.312) (end 149.86 83.312) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 137.16 62.992) (end 137.16 83.312) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 149.86 61.722) (end 138.43 61.722) (layer Edge.Cuts) (width 0.05))
)
