(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 18)
    (no_connects 0)
    (area 134.956499 94.316499 185.083501 144.443501)
    (thickness 1.6002)
    (drawings 2)
    (tracks 107)
    (zones 0)
    (modules 6)
    (nets 21)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.1524)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.8)
    (trace_clearance 0.254)
    (zone_clearance 0.1524)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.127)
    (edge_width 0.127)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.127)
    (pcb_text_size 0.6 0.6)
    (mod_edge_width 0.127)
    (mod_text_size 0.6 0.6)
    (mod_text_width 0.127)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (pad_to_paste_clearance -0.04)
    (aux_axis_origin 0 0)
    (grid_origin 160.02 119.38)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x3ffff_80000001)
      (usegerberextensions true)
      (usegerberattributes true)
      (excludeedgelayer true)
      (linewidth 0.127000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory CAM/))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 GND)
  (net 3 /Anode)
  (net 4 /Din)
  (net 5 "Net-(J1-Pad3)")
  (net 6 /HV6)
  (net 7 /HV5)
  (net 8 /HV10)
  (net 9 /HV4)
  (net 10 /HV9)
  (net 11 /HV3)
  (net 12 /HV8)
  (net 13 /HV2)
  (net 14 /HV7)
  (net 15 /HV1)
  (net 16 "Net-(J1-Pad5)")
  (net 17 "Net-(N1-PadA)")
  (net 18 "Net-(N1-PadA2)")
  (net 19 "Net-(J1-Pad15)")
  (net 20 "Net-(LED1-Pad1-DO)")
  (net_class Default "Imperial - this is the standard class"
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net +5V)
    (add_net /Anode)
    (add_net /Din)
    (add_net /HV1)
    (add_net /HV10)
    (add_net /HV2)
    (add_net /HV3)
    (add_net /HV4)
    (add_net /HV5)
    (add_net /HV6)
    (add_net /HV7)
    (add_net /HV8)
    (add_net /HV9)
    (add_net GND)
    (add_net "Net-(J1-Pad15)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(LED1-Pad1-DO)")
    (add_net "Net-(N1-PadA)")
    (add_net "Net-(N1-PadA2)")
  )
  (net_class 0.2mm ""
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (net_class Minimal ""
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5A3B126B)
    (at 155.67 115.48 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at -2.4 0.05 180) (layer F.SilkS))
    (fp_text value 0.1uF (at -0.4 4.85 90) (layer F.SilkS))
    (fp_text user %R (at 0 -1.25 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x09_Pitch2.54mm (layer F.Cu) (tedit 5A3B14FF)
    (at 170.18 99.38 270)
    (descr "Through hole straight pin header, 2x09, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x09 2.54mm double row")
    (fp_text reference J1 (at 1.27 -2.33 270) (layer F.SilkS) hide)
    (fp_text value Nixie (at 1.27 22.65 270) (layer F.Fab))
    (fp_text user %R (at 1.27 10.16 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /Anode))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /Anode))
    (pad 3 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad3)"))
    (pad 4 thru_hole oval (at 2.54 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /HV6))
    (pad 5 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-Pad5)"))
    (pad 6 thru_hole oval (at 2.54 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /HV5))
    (pad 7 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /HV10))
    (pad 8 thru_hole oval (at 2.54 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /HV4))
    (pad 9 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /HV9))
    (pad 10 thru_hole oval (at 2.54 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /HV3))
    (pad 11 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /HV8))
    (pad 12 thru_hole oval (at 2.54 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /HV2))
    (pad 13 thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /HV7))
    (pad 14 thru_hole oval (at 2.54 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /HV1))
    (pad 15 thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J1-Pad15)"))
    (pad 16 thru_hole oval (at 2.54 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /Din))
    (pad 17 thru_hole oval (at 0 20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 18 thru_hole oval (at 2.54 20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x09_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module adafruit:adafruit-LED3535 (layer F.Cu) (tedit 5A3B14EC)
    (at 160.02 114.18)
    (attr smd)
    (fp_text reference LED1 (at 3.175 -0.254 90) (layer F.SilkS))
    (fp_text value WS2812BSK6812MINI (at 0.127 2.54) (layer F.SilkS) hide)
    (pad 1-DO smd rect (at 1.74752 0.87376 90) (size 0.84836 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(LED1-Pad1-DO)"))
    (pad 2-GN smd rect (at 1.74752 -0.87376 90) (size 0.84836 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3-DI smd rect (at -1.74752 -0.87376 90) (size 0.84836 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 4 /Din))
    (pad 4-VD smd rect (at -1.74752 0.87376 90) (size 0.84836 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
  )
  (module nixies-us:nixies-us-IN-18-DSUB (layer F.Cu) (tedit 5A3B14F4)
    (at 160 119.38 180)
    (descr "MAY BE USED WITH SOCKET: PL31-P")
    (tags "MAY BE USED WITH SOCKET: PL31-P")
    (attr virtual)
    (fp_text reference N1 (at 17.61998 -0.79248 270) (layer F.SilkS))
    (fp_text value IN-18D-SUB (at 0 0 180) (layer F.SilkS) hide)
    (pad 0 thru_hole circle (at 6.28142 6.35508 180) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 8 /HV10))
    (pad 1 thru_hole circle (at -0.64262 8.97128 180) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 15 /HV1))
    (pad 2 thru_hole circle (at -4.32816 7.9375 180) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 13 /HV2))
    (pad 3 thru_hole circle (at -8.75792 -1.86182 180) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 11 /HV3))
    (pad 4 thru_hole circle (at 6.34746 -6.38048 180) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 9 /HV4))
    (pad 5 thru_hole circle (at 3.08864 -8.44804 180) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 7 /HV5))
    (pad 6 thru_hole circle (at -4.29006 -7.90448 180) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 6 /HV6))
    (pad 7 thru_hole circle (at -7.2136 -5.3848 180) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 14 /HV7))
    (pad 8 thru_hole circle (at -7.2263 5.34162 180) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 12 /HV8))
    (pad 9 thru_hole circle (at 8.45566 3.1877 180) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 10 /HV9))
    (pad A thru_hole circle (at -0.65786 -8.97382 180) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 17 "Net-(N1-PadA)"))
    (pad A2 thru_hole circle (at 3.12166 8.39216 180) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 18 "Net-(N1-PadA2)"))
    (pad N/C thru_hole circle (at 8.39216 -3.12166 180) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask))
    (pad N/C2 thru_hole circle (at -8.78078 1.94818 180) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask))
    (pad "" np_thru_hole circle (at 0 0 180) (size 4.99872 4.99872) (drill 4.99872) (layers *.Cu *.Mask))
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5A3B125F)
    (at 171.52 111.58 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 0 -1.45 90) (layer F.SilkS))
    (fp_text value 4k7 (at 0 1.55 90) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(N1-PadA)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 /Anode))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module logos:mermaid_l (layer B.Cu) (tedit 0)
    (at 163.22 137.18 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (gr_text "nixies.us\nIN-18" (at 161.92 137.58) (layer B.Mask))
  (gr_circle (center 160.02 119.38) (end 135.02 119.38) (layer Edge.Cuts) (width 0.127))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer))
    (polygon
      (pts
        (xy 190.02 89.38) (xy 130.02 89.38) (xy 130.02 149.38) (xy 190.02 149.38)
      )
    )
  )
)
