(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "Net-(C1-Pad2)")
	(net 2 "Net-(C1-Pad1)")
	(net 3 "Net-(D1-Pad3)")
	(net 4 "Net-(D1--)")
	(net 5 "Net-(D1-+)")
	(net 6 "Net-(D1-Pad4)")
	(net 7 "Net-(D2-K)")
	(net 8 "Net-(D3-A)")
	(net 9 "Net-(J1-Pad2)")
	(net 10 "Net-(J3-Pin_1)")
	(net 11 "Net-(J4-Pin_1)")
	(net 12 "Net-(J5-Pin_1)")
	(footprint "Capacitor_THT:C_Axial_L3.8mm_D2.6mm_P10.00mm_Horizontal"
		(layer "F.Cu")
		(at 116 137 180)
		(descr "C, Axial series, Axial, Horizontal, pin pitch=10mm, , length*diameter=3.8*2.6mm^2, http://www.vishay.com/docs/45231/arseries.pdf")
		(tags "C Axial series Axial Horizontal pin pitch 10mm  length 3.8mm diameter 2.6mm")
		(property "Reference" "C1"
			(at 5.125 0.15 0)
			(layer "F.SilkS")
		)
		(property "Value" "1uF 400v"
			(at 5 2.42 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_THT:C_Axial_L3.8mm_D2.6mm_P10.00mm_Horizontal"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "Emergency-and-Night-Light.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(C1-Pad1)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "Net-(C1-Pad2)")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Axial_L3.8mm_D2.6mm_P10.00mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:Diode_Bridge_Diotec_ABS"
		(layer "F.Cu")
		(at 116.85 127.5 180)
		(descr "SMD diode bridge ABS (Diotec), see https://diotec.com/tl_files/diotec/files/pdf/datasheets/abs2.pdf")
		(tags "ABS MBLS")
		(property "Reference" "D1"
			(at 3 -0.15 0)
			(layer "F.SilkS")
		)
		(property "Value" "ABS10"
			(at 0 3.7 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Diode_SMD:Diode_Bridge_Diotec_ABS"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Miniature Glass Passivated Single-Phase Surface Mount Bridge Rectifiers, 700V Vrms, 0.8A If, ABS SMD package"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "Emergency-and-Night-Light.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.065 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.975 -2 180)
			(size 1 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "Net-(D1-+)")
			(pinfunction "+")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -2.975 2 180)
			(size 1 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "Net-(D1--)")
			(pinfunction "-")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 2.975 2 180)
			(size 1 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "Net-(D1-Pad3)")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 2.975 -2 180)
			(size 1 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "Net-(D1-Pad4)")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Diode_SMD.3dshapes/Diode_Bridge_Diotec_ABS.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_1206_3216Metric_Pad1.42x1.75mm_HandSolder"
		(layer "F.Cu")
		(at 123.5 136.75 180)
		(descr "LED SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED handsolder")
		(property "Reference" "D2"
			(at 3 -0.25 0)
			(layer "F.SilkS")
		)
		(property "Value" "RED LED"
			(at 0 1.82 0)
			(layer "F.Fab")
		)
		(property "Footprint" "LED_SMD:LED_1206_3216Metric_Pad1.42x1.75mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "Emergency-and-Night-Light.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4875 0 180)
			(size 1.425 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.175439)
			(net 7 "Net-(D2-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4875 0 180)
			(size 1.425 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.175439)
			(net 5 "Net-(D1-+)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/LED_SMD.3dshapes/LED_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_THT:D_DO-41_SOD81_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 130.5 124 -90)
		(descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
		(tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 7.62mm  length 5.2mm diameter 2.7mm")
		(property "Reference" "D3"
			(at 3.81 -2.47 90)
			(layer "F.SilkS")
		)
		(property "Value" "1N4007"
			(at 3.81 2.47 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Diode_THT:D_DO-41_SOD81_P7.62mm_Horizontal"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "1000V 1A General Purpose Rectifier Diode, DO-41"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "Emergency-and-Night-Light.kicad_sch")
		(attr through_hole)
		(fp_text user "K"
			(at 0 -2.1 90)
			(layer "F.SilkS")
		)
		(fp_text user "K"
			(at 0 -2.1 90)
			(layer "F.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 4.2 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 2.2 2.2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(D1--)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 270)
			(size 2.2 2.2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "Net-(D3-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-41_SOD81_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "digikey-footprints:Term_Block_1x2_P5mm"
		(layer "F.Cu")
		(at 109.05 129.45 90)
		(descr "http://www.on-shore.com/wp-content/uploads/2015/09/osttcxx0162.pdf")
		(property "Reference" "J1"
			(at 8.5 -1 180)
			(layer "F.SilkS")
		)
		(property "Value" "OSTTC020162"
			(at 2.05 5.05 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "digikey-footprints:Term_Block_1x2_P5mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "TERM BLK 2POS SIDE ENTRY 5MM PCB"
			(at 109.05 129.45 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Connectors, Interconnects"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK_Datasheet_Link" "http://www.on-shore.com/wp-content/uploads/OSTTCXX0162.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK_Detail_Page" "/product-detail/en/on-shore-technology-inc/OSTTC020162/ED2600-ND/614549"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digi-Key_PN" "ED2600-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Family" "Terminal Blocks - Wire to Board"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "OSTTC020162"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "On Shore Technology Inc."
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Status" "Active"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "Emergency-and-Night-Light.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 2.5 2.5)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "Net-(C1-Pad2)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0 90)
			(size 2.5 2.5)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "Net-(J1-Pad2)")
			(pintype "passive")
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 134.8 133.1 180)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "J2"
			(at 0 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "22-23-2021"
			(at 0 4.87 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CONN HEADER VERT 2POS 2.54MM"
			(at 134.8 133.1 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Connectors, Interconnects"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK_Datasheet_Link" "https://media.digikey.com/pdf/Data%20Sheets/Molex%20PDFs/A-6373-N_Series_Dwg_2010-12-03.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK_Detail_Page" "/product-detail/en/molex/22-23-2021/WM4200-ND/26667"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digi-Key_PN" "WM4200-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Family" "Rectangular Connectors - Headers, Male Pins"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "22-23-2021"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Molex"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Status" "Active"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "Emergency-and-Night-Light.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "Net-(D3-A)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Net-(D2-K)")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_2010_5025Metric_Pad1.40x2.65mm_HandSolder"
		(layer "F.Cu")
		(at 117.7 122.2 180)
		(descr "Resistor SMD 2010 (5025 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R2"
			(at 0 -2 180)
			(layer "F.SilkS")
		)
		(property "Value" "120 1W"
			(at 0 2.28 180)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_2010_5025Metric_Pad1.40x2.65mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Untitled Field" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "Emergency-and-Night-Light.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.4 0 180)
			(size 1.4 2.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.178571)
			(net 3 "Net-(D1-Pad3)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.4 0 180)
			(size 1.4 2.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.178571)
			(net 9 "Net-(J1-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_2010_5025Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_2010_5025Metric_Pad1.40x2.65mm_HandSolder"
		(layer "F.Cu")
		(at 118.2 133.2 180)
		(descr "Resistor SMD 2010 (5025 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R3"
			(at 0 -2.28 180)
			(layer "F.SilkS")
		)
		(property "Value" "120 1W"
			(at 0 2.28 180)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_2010_5025Metric_Pad1.40x2.65mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Untitled Field" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "Emergency-and-Night-Light.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.4 0 180)
			(size 1.4 2.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.178571)
			(net 6 "Net-(D1-Pad4)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.4 0 180)
			(size 1.4 2.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.178571)
			(net 2 "Net-(C1-Pad1)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_2010_5025Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(at 127.5 129 90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R5"
			(at -2.5 -1.5 180)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0.5 1.5 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "Emergency-and-Night-Light.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 90)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 7 "Net-(D2-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 90)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 4 "Net-(D1--)")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(at 133.75 125.5 90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R6"
			(at 2.75 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "1R"
			(at 0 1.82 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "Emergency-and-Night-Light.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -1.55 0 90)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 7 "Net-(D2-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 90)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 11 "Net-(J4-Pin_1)")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(at 136.25 125.5 90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R7"
			(at 2.75 0.5 180)
			(layer "F.SilkS")
		)
		(property "Value" "1R"
			(at 0 1.82 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "Emergency-and-Night-Light.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -1.55 0 90)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 7 "Net-(D2-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 90)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 12 "Net-(J5-Pin_1)")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(at 110.95 134 180)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R1"
			(at -3.5 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "1M"
			(at 0 1.82 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "Emergency-and-Night-Light.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 180)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 2 "Net-(C1-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 180)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 1 "Net-(C1-Pad2)")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_THT:TO-92_Inline"
		(layer "F.Cu")
		(at 126.5 125 90)
		(descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
		(tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
		(property "Reference" "Q1"
			(at 3.5 -2.25 180)
			(layer "F.SilkS")
		)
		(property "Value" "2N3904"
			(at 1.27 2.79 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "0.2A Ic, 40V Vce, Small Signal NPN Transistor, TO-92"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "Emergency-and-Night-Light.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.05 1.5)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "Net-(D3-A)")
			(pinfunction "E")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 1.27 0 90)
			(size 1.05 1.5)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(D1--)")
			(pinfunction "B")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 2.54 0 90)
			(size 1.05 1.5)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "Net-(J3-Pin_1)")
			(pinfunction "C")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:CP_Radial_D5.0mm_P2.50mm"
		(layer "F.Cu")
		(at 123.5 130.5 90)
		(descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
		(tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
		(property "Reference" "C2"
			(at -1.25 -2.25 180)
			(layer "F.SilkS")
		)
		(property "Value" "100uF"
			(at 1.25 3.75 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_THT:CP_Radial_D5.0mm_P2.50mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "Emergency-and-Night-Light.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(D1-+)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.5 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(D1--)")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_THT:D_T-1_P5.08mm_Horizontal"
		(layer "F.Cu")
		(at 129.25 137.25)
		(descr "Diode, T-1 series, Axial, Horizontal, pin pitch=5.08mm, , length*diameter=3.2*2.6mm^2, , http://www.diodes.com/_files/packages/T-1.pdf")
		(tags "Diode T-1 series Axial Horizontal pin pitch 5.08mm  length 3.2mm diameter 2.6mm")
		(property "Reference" "D6"
			(at 7 0.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "5.1v"
			(at 7.5 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Diode_THT:D_T-1_P5.08mm_Horizontal"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "Emergency-and-Night-Light.kicad_sch")
		(attr through_hole)
		(fp_text user "K"
			(at 6.8 -0.475 0)
			(layer "F.SilkS")
		)
		(fp_text user "K"
			(at 0 -2 0)
			(layer "F.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 2.78 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "Net-(D3-A)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 5.08 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Net-(D2-K)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_T-1_P5.08mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(at 126.25 133.5 180)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R4"
			(at 0 -1.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "220"
			(at 0 1.82 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "Emergency-and-Night-Light.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 180)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 7 "Net-(D2-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 180)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 5 "Net-(D1-+)")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Wire:SolderWire-0.1sqmm_1x01_D0.4mm_OD1mm"
		(layer "F.Cu")
		(at 130 121.25)
		(descr "Soldered wire connection, for a single 0.1 mm² wire, basic insulation, conductor diameter 0.4mm, outer diameter 1mm, size source Multi-Contact FLEXI-E 0.1 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
		(tags "connector wire 0.1sqmm")
		(property "Reference" "J3"
			(at 0 -2 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x01_Female"
			(at 0 2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_Wire:SolderWire-0.1sqmm_1x01_D0.4mm_OD1mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "Emergency-and-Night-Light.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15625)
			(net 10 "Net-(J3-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Connector_Wire.3dshapes/SolderWire-0.1sqmm_1x01_D0.4mm_OD1mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Wire:SolderWire-0.1sqmm_1x01_D0.4mm_OD1mm"
		(layer "F.Cu")
		(at 133.25 121.25)
		(descr "Soldered wire connection, for a single 0.1 mm² wire, basic insulation, conductor diameter 0.4mm, outer diameter 1mm, size source Multi-Contact FLEXI-E 0.1 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
		(tags "connector wire 0.1sqmm")
		(property "Reference" "J4"
			(at 0 -2 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x01_Female"
			(at 0 2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_Wire:SolderWire-0.1sqmm_1x01_D0.4mm_OD1mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "Emergency-and-Night-Light.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15625)
			(net 11 "Net-(J4-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Connector_Wire.3dshapes/SolderWire-0.1sqmm_1x01_D0.4mm_OD1mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Wire:SolderWire-0.1sqmm_1x01_D0.4mm_OD1mm"
		(layer "F.Cu")
		(at 136.25 121.25)
		(descr "Soldered wire connection, for a single 0.1 mm² wire, basic insulation, conductor diameter 0.4mm, outer diameter 1mm, size source Multi-Contact FLEXI-E 0.1 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
		(tags "connector wire 0.1sqmm")
		(property "Reference" "J5"
			(at 0 -2 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x01_Female"
			(at 0 2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_Wire:SolderWire-0.1sqmm_1x01_D0.4mm_OD1mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "Emergency-and-Night-Light.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15625)
			(net 12 "Net-(J5-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Connector_Wire.3dshapes/SolderWire-0.1sqmm_1x01_D0.4mm_OD1mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(at 122.5 123 -90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R8"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.82 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "Emergency-and-Night-Light.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 270)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 10 "Net-(J3-Pin_1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 270)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 8 "Net-(D3-A)")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_line
		(start 137.75 120)
		(end 137.75 139)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 104.85 119.95)
		(end 137.75 120)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 137.75 139)
		(end 104.85 139)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 104.85 119.95)
		(end 104.85 139)
		(layer "Edge.Cuts")
	)
	(gr_text "Emergency Back up light v8 PCB\nSherman Stebbins\n20230528"
		(at 118.75 134 0)
		(layer "B.SilkS")
	)
	(gr_text "120"
		(at 120.4 135.25 0)
		(layer "F.SilkS")
	)
	(gr_text "1 Ohm"
		(at 135.75 128.35 0)
		(layer "F.SilkS")
	)
	(gr_text "+"
		(at 135 120.45 0)
		(layer "F.SilkS")
	)
	(gr_text "+"
		(at 118 129.35 0)
		(layer "F.SilkS")
	)
	(gr_text "1m"
		(at 110.95 134 0)
		(layer "F.SilkS")
	)
	(gr_text "-"
		(at 136.5 133 0)
		(layer "F.SilkS")
	)
	(gr_text "Batt"
		(at 136.1 131.65 0)
		(layer "F.SilkS")
	)
	(gr_text "1"
		(at 133.8 125.45 0)
		(layer "F.SilkS")
	)
	(gr_text "LED -"
		(at 127.75 120.5 0)
		(layer "F.SilkS")
	)
	(gr_text "1k"
		(at 125.95 133.4 0)
		(layer "F.SilkS")
	)
	(gr_text "-"
		(at 118 125.4 0)
		(layer "F.SilkS")
	)
	(gr_text "120"
		(at 115.8 124.15 0)
		(layer "F.SilkS")
	)
	(gr_text "-"
		(at 126.45 137.3 0)
		(layer "F.SilkS")
	)
	(gr_text "1k"
		(at 120.95 124.3 0)
		(layer "F.SilkS")
	)
	(gr_text "K"
		(at 126.3 136.75 0)
		(layer "F.SilkS")
	)
	(gr_text "1k"
		(at 127.5 129.05 0)
		(layer "F.SilkS")
	)
	(gr_text "3904"
		(at 124.9 123.75 90)
		(layer "F.SilkS")
	)
	(gr_text "-"
		(at 122.4 126.25 0)
		(layer "F.SilkS")
	)
	(gr_text "4007"
		(at 130.4 128.75 0)
		(layer "F.SilkS")
	)
	(gr_text "5.1v"
		(at 132 137.05 0)
		(layer "F.SilkS")
	)
	(gr_text "+"
		(at 136.5 130.5 0)
		(layer "F.SilkS")
	)
	(gr_text "+"
		(at 131.95 120.45 0)
		(layer "F.SilkS")
	)
	(gr_text "A"
		(at 127.45 138.125 0)
		(layer "F.SilkS")
	)
	(dimension
		(type aligned)
		(layer "F.SilkS")
		(pts
			(xy 143.1 137.35) (xy 143.1 118.35)
		)
		(height 1.5)
		(gr_text "19.0000 mm"
			(at 143.45 127.85 90)
			(layer "F.SilkS")
		)
		(format
			(prefix "")
			(suffix "")
			(units 2)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.12)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(layer "F.SilkS")
		(pts
			(xy 137.75 120) (xy 104 120)
		)
		(height 1.5)
		(gr_text "33.7500 mm"
			(at 120.875 117.35 0)
			(layer "F.SilkS")
		)
		(format
			(prefix "")
			(suffix "")
			(units 2)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.12)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0) keep_text_aligned)
	)
)
