(kicad_pcb (version 20171130) (host pcbnew "(5.1.2-1)-1")
  (general
    (thickness 1.6)
    (drawings 14)
    (tracks 487)
    (zones 0)
    (modules 55)
    (nets 58)
  )
  (page User 190.5 165.1)
  (title_block
    (title "Instrumental Amplifier Board - PCB Layout ")
    (date 2019-06-30)
    (rev 0.0.0)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.381)
    (user_trace_width 0.254)
    (user_trace_width 0.381)
    (user_trace_width 0.508)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 0.762 0.381)
    (user_via 1.016 0.508)
    (user_via 1.27 0.635)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.8796 1.8796)
    (pad_drill 1.016)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (grid_origin 95.25 65.405)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 V_PWR)
  (net 3 /M1-D:PWR_CHK/M1-D:GND)
  (net 4 /CH2)
  (net 5 /CH1)
  (net 6 "Net-(M1-D_PWR:LED_GRN1-PadA)")
  (net 7 "Net-(M1-D_PWR:LED_RED1-PadA)")
  (net 8 "Net-(M1-HB:P1-Pad1)")
  (net 9 /M1-AMP/M1-SG_V:CH1)
  (net 10 "Net-(M1-HB:P1-Pad3)")
  (net 11 "Net-(M1-HB:P2-Pad1)")
  (net 12 /M1-AMP/M1-SG_V:CH2)
  (net 13 "Net-(M1-HB:P2-Pad3)")
  (net 14 VCM)
  (net 15 SG_REF:CH7)
  (net 16 V_REF)
  (net 17 /M2-D:PWR_CHK/M2-D:GND)
  (net 18 /CH4)
  (net 19 /CH3)
  (net 20 "Net-(M2-D_PWR:LED_GRN1-PadA)")
  (net 21 "Net-(M2-D_PWR:LED_RED1-PadA)")
  (net 22 /M2-AMP/M2-IN_AMP:2/M2-G:WIP2)
  (net 23 "Net-(M2-HB:P1-Pad1)")
  (net 24 /M2-AMP/M2-SG_V:CH3)
  (net 25 "Net-(M2-HB:P1-Pad3)")
  (net 26 "Net-(M2-HB:P2-Pad1)")
  (net 27 /M2-AMP/M2-SG_V:CH4)
  (net 28 "Net-(M2-HB:P2-Pad3)")
  (net 29 /M3-D:PWR_CHK/M3-D:GND)
  (net 30 /CH6)
  (net 31 /CH5)
  (net 32 "Net-(M3-D_PWR:LED_GRN1-PadA)")
  (net 33 "Net-(M3-D_PWR:LED_RED1-PadA)")
  (net 34 "Net-(M3-HB:P1-Pad1)")
  (net 35 /M3-AMP/M3-SG_V:CH5)
  (net 36 "Net-(M3-HB:P1-Pad3)")
  (net 37 "Net-(M3-HB:P2-Pad1)")
  (net 38 /M3-AMP/M3-SG_V:CH6)
  (net 39 "Net-(M3-HB:P2-Pad3)")
  (net 40 "Net-(VCM:LED_BLU1-PadA)")
  (net 41 /M1-D:OUT2)
  (net 42 /M1-D:OUT1)
  (net 43 /M2-D:OUT2)
  (net 44 /M2-D:OUT1)
  (net 45 /M3-D:OUT2)
  (net 46 /M3-D:OUT1)
  (net 47 /M1-AMP/M1-IN_AMP:1/M1-G:WIP1)
  (net 48 /M1-AMP/M1-IN_AMP:1/M1-G:V_IN1)
  (net 49 /M1-AMP/M1-IN_AMP:2/M1-G:V_IN2)
  (net 50 /M1-AMP/M1-IN_AMP:2/M1-G:WIP2)
  (net 51 /M2-AMP/M2-IN_AMP:1/M2-G:V_IN1)
  (net 52 /M2-AMP/M2-IN_AMP:1/M2-G:WIP1)
  (net 53 /M2-AMP/M2-IN_AMP:2/M2-G:V_IN2)
  (net 54 /M3-AMP/M3-IN_AMP:1/M3-G:WIP1)
  (net 55 /M3-AMP/M3-IN_AMP:1/M3-G:V_IN1)
  (net 56 /M3-AMP/M3-IN_AMP:2/M3-G:WIP2)
  (net 57 /M3-AMP/M3-IN_AMP:2/M3-G:V_IN2)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /CH1)
    (add_net /CH2)
    (add_net /CH3)
    (add_net /CH4)
    (add_net /CH5)
    (add_net /CH6)
    (add_net /M1-AMP/M1-IN_AMP:1/M1-G:V_IN1)
    (add_net /M1-AMP/M1-IN_AMP:1/M1-G:WIP1)
    (add_net /M1-AMP/M1-IN_AMP:2/M1-G:V_IN2)
    (add_net /M1-AMP/M1-IN_AMP:2/M1-G:WIP2)
    (add_net /M1-AMP/M1-SG_V:CH1)
    (add_net /M1-AMP/M1-SG_V:CH2)
    (add_net /M1-D:OUT1)
    (add_net /M1-D:OUT2)
    (add_net /M1-D:PWR_CHK/M1-D:GND)
    (add_net /M2-AMP/M2-IN_AMP:1/M2-G:V_IN1)
    (add_net /M2-AMP/M2-IN_AMP:1/M2-G:WIP1)
    (add_net /M2-AMP/M2-IN_AMP:2/M2-G:V_IN2)
    (add_net /M2-AMP/M2-IN_AMP:2/M2-G:WIP2)
    (add_net /M2-AMP/M2-SG_V:CH3)
    (add_net /M2-AMP/M2-SG_V:CH4)
    (add_net /M2-D:OUT1)
    (add_net /M2-D:OUT2)
    (add_net /M2-D:PWR_CHK/M2-D:GND)
    (add_net /M3-AMP/M3-IN_AMP:1/M3-G:V_IN1)
    (add_net /M3-AMP/M3-IN_AMP:1/M3-G:WIP1)
    (add_net /M3-AMP/M3-IN_AMP:2/M3-G:V_IN2)
    (add_net /M3-AMP/M3-IN_AMP:2/M3-G:WIP2)
    (add_net /M3-AMP/M3-SG_V:CH5)
    (add_net /M3-AMP/M3-SG_V:CH6)
    (add_net /M3-D:OUT1)
    (add_net /M3-D:OUT2)
    (add_net /M3-D:PWR_CHK/M3-D:GND)
    (add_net GND)
    (add_net "Net-(M1-D_PWR:LED_GRN1-PadA)")
    (add_net "Net-(M1-D_PWR:LED_RED1-PadA)")
    (add_net "Net-(M1-HB:P1-Pad1)")
    (add_net "Net-(M1-HB:P1-Pad3)")
    (add_net "Net-(M1-HB:P2-Pad1)")
    (add_net "Net-(M1-HB:P2-Pad3)")
    (add_net "Net-(M2-D_PWR:LED_GRN1-PadA)")
    (add_net "Net-(M2-D_PWR:LED_RED1-PadA)")
    (add_net "Net-(M2-HB:P1-Pad1)")
    (add_net "Net-(M2-HB:P1-Pad3)")
    (add_net "Net-(M2-HB:P2-Pad1)")
    (add_net "Net-(M2-HB:P2-Pad3)")
    (add_net "Net-(M3-D_PWR:LED_GRN1-PadA)")
    (add_net "Net-(M3-D_PWR:LED_RED1-PadA)")
    (add_net "Net-(M3-HB:P1-Pad1)")
    (add_net "Net-(M3-HB:P1-Pad3)")
    (add_net "Net-(M3-HB:P2-Pad1)")
    (add_net "Net-(M3-HB:P2-Pad3)")
    (add_net "Net-(VCM:LED_BLU1-PadA)")
    (add_net SG_REF:CH7)
    (add_net VCM)
    (add_net V_PWR)
    (add_net V_REF)
  )
  (module Connectors:2X5-SHROUDED_LOCK (layer F.Cu) (tedit 5D199B7E)
    (at 50.8 40.767 270)
    (descr "PLATED THROUGH HOLE - 2X5 SHROUDED HEADER LOCKING FOOTPRINT")
    (tags "PLATED THROUGH HOLE - 2X5 SHROUDED HEADER LOCKING FOOTPRINT")
    (attr virtual)
    (fp_text reference M1-CTRL:CN1 (at -5.842 0 180 unlocked) (layer F.SilkS))
    (fp_text value CONN_05X2SHD_LOCK (at -5.207 0) (layer F.SilkS) hide)
    (pad 10 thru_hole circle (at 1.397 5.08 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 V_PWR) (solder_mask_margin 0.1016))
    (pad 9 thru_hole circle (at -1.397 5.08 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 V_PWR) (solder_mask_margin 0.1016))
    (pad 8 thru_hole circle (at 1.397 2.54 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 7 thru_hole circle (at -1.397 2.54 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 6 thru_hole circle (at 1.397 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 41 /M1-D:OUT2) (solder_mask_margin 0.1016))
    (pad 5 thru_hole circle (at -1.397 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 42 /M1-D:OUT1) (solder_mask_margin 0.1016))
    (pad 4 thru_hole circle (at 1.397 -2.54 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 /M1-D:PWR_CHK/M1-D:GND) (solder_mask_margin 0.1016))
    (pad 3 thru_hole circle (at -1.397 -2.54 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 2 thru_hole circle (at 1.397 -5.08 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 /CH2) (solder_mask_margin 0.1016))
    (pad 1 thru_hole rect (at -1.397 -5.08 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 /CH1) (solder_mask_margin 0.1016))
  )
  (module LED:LED-0603 (layer F.Cu) (tedit 595FF906)
    (at 45.3263 25.4)
    (descr "LED 0603 SMT")
    (tags "LED 0603 SMT")
    (attr smd)
    (fp_text reference M1-D_PWR:LED_GRN1 (at 1.6637 -1.905 180 unlocked) (layer F.SilkS))
    (fp_text value LED-GREEN0603 (at 0 2.54) (layer F.SilkS) hide)
    (pad A smd rect (at -0.8763 0 270) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(M1-D_PWR:LED_GRN1-PadA)") (solder_mask_margin 0.1016))
    (pad C smd rect (at 0.8763 0 270) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 3 /M1-D:PWR_CHK/M1-D:GND) (solder_mask_margin 0.1016))
  )
  (module LED:LED-0603 (layer F.Cu) (tedit 595FF906)
    (at 56.2737 25.4 180)
    (descr "LED 0603 SMT")
    (tags "LED 0603 SMT")
    (attr smd)
    (fp_text reference M1-D_PWR:LED_RED1 (at 1.6637 1.905 180 unlocked) (layer F.SilkS))
    (fp_text value LED-RED0603 (at 0 -2.54) (layer F.SilkS) hide)
    (pad C smd rect (at 0.8763 0 90) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 3 /M1-D:PWR_CHK/M1-D:GND) (solder_mask_margin 0.1016))
    (pad A smd rect (at -0.8763 0 90) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(M1-D_PWR:LED_RED1-PadA)") (solder_mask_margin 0.1016))
  )
  (module ERA-3AEB331V:RESC1608X55N (layer F.Cu) (tedit 0)
    (at 44.45 29.065 90)
    (attr smd)
    (fp_text reference M1-D_PWR:R_GRN1 (at -3.32 0.635 180 unlocked) (layer F.SilkS))
    (fp_text value ERA-3AEB331V (at -2.54 0 180) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.78 0 90) (size 0.87 0.93) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(M1-D_PWR:LED_GRN1-PadA)"))
    (pad 1 smd rect (at -0.78 0 90) (size 0.87 0.93) (layers F.Cu F.Paste F.Mask)
      (net 42 /M1-D:OUT1))
  )
  (module ERA-3AEB331V:RESC1608X55N (layer F.Cu) (tedit 0)
    (at 57.15 29.065 90)
    (attr smd)
    (fp_text reference M1-D_PWR:R_RED1 (at -3.32 -0.635 180 unlocked) (layer F.SilkS))
    (fp_text value ERA-3AEB331V (at -2.54 0 180) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.78 0 90) (size 0.87 0.93) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(M1-D_PWR:LED_RED1-PadA)"))
    (pad 1 smd rect (at -0.78 0 90) (size 0.87 0.93) (layers F.Cu F.Paste F.Mask)
      (net 41 /M1-D:OUT2))
  )
  (module RC0201FR-074K7L:RESC0603X26N (layer F.Cu) (tedit 0)
    (at 32.385 73.025 90)
    (attr smd)
    (fp_text reference M1-HB:R_GND1 (at -3.175 8.255 180 unlocked) (layer F.SilkS))
    (fp_text value RC0201FR-074K7L (at -0.065 0.8 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.28 0 180) (size 0.4 0.38) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.305 0 180) (size 0.4 0.33) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(M1-HB:P1-Pad3)"))
  )
  (module RC0201FR-074K7L:RESC0603X26N (layer F.Cu) (tedit 0)
    (at 69.215 73.025 90)
    (attr smd)
    (fp_text reference M1-HB:R_GND2 (at -3.175 -8.255 180 unlocked) (layer F.SilkS))
    (fp_text value RC0201FR-074K7L (at -0.065 0.8 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.28 0 180) (size 0.4 0.38) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.305 0 180) (size 0.4 0.33) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(M1-HB:P2-Pad3)"))
  )
  (module RC0201FR-074K7L:RESC0603X26N (layer F.Cu) (tedit 0)
    (at 43.815 78.105 180)
    (attr smd)
    (fp_text reference M1-HB:R_VCM1 (at -0.635 -1.905 180 unlocked) (layer F.SilkS))
    (fp_text value RC0201FR-074K7L (at -0.065 0.8) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.305 0 270) (size 0.4 0.33) (layers F.Cu F.Paste F.Mask)
      (net 14 VCM))
    (pad 2 smd rect (at 0.28 0 270) (size 0.4 0.38) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(M1-HB:P1-Pad1)"))
  )
  (module RC0201FR-074K7L:RESC0603X26N (layer F.Cu) (tedit 0)
    (at 57.785 78.105)
    (attr smd)
    (fp_text reference M1-HB:R_VCM2 (at -0.635 1.905 180 unlocked) (layer F.SilkS))
    (fp_text value RC0201FR-074K7L (at -0.065 0.8) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.28 0 90) (size 0.4 0.38) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(M1-HB:P2-Pad1)"))
    (pad 1 smd rect (at -0.305 0 90) (size 0.4 0.33) (layers F.Cu F.Paste F.Mask)
      (net 14 VCM))
  )
  (module Connectors:2X5-SHROUDED_LOCK (layer F.Cu) (tedit 200000)
    (at 95.25 40.64 270)
    (descr "PLATED THROUGH HOLE - 2X5 SHROUDED HEADER LOCKING FOOTPRINT")
    (tags "PLATED THROUGH HOLE - 2X5 SHROUDED HEADER LOCKING FOOTPRINT")
    (attr virtual)
    (fp_text reference M2-CTRL:CN1 (at -5.715 0 180 unlocked) (layer F.SilkS))
    (fp_text value CONN_05X2SHD_LOCK (at -5.08 -5.08) (layer F.SilkS) hide)
    (pad 10 thru_hole circle (at 1.397 5.08 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 V_PWR) (solder_mask_margin 0.1016))
    (pad 9 thru_hole circle (at -1.397 5.08 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 V_PWR) (solder_mask_margin 0.1016))
    (pad 8 thru_hole circle (at 1.397 2.54 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 7 thru_hole circle (at -1.397 2.54 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 6 thru_hole circle (at 1.397 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 43 /M2-D:OUT2) (solder_mask_margin 0.1016))
    (pad 5 thru_hole circle (at -1.397 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 44 /M2-D:OUT1) (solder_mask_margin 0.1016))
    (pad 4 thru_hole circle (at 1.397 -2.54 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 /M2-D:PWR_CHK/M2-D:GND) (solder_mask_margin 0.1016))
    (pad 3 thru_hole circle (at -1.397 -2.54 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 2 thru_hole circle (at 1.397 -5.08 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 /CH4) (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at -1.397 -5.08 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 /CH3) (solder_mask_margin 0.1016))
  )
  (module LED:LED-0603 (layer F.Cu) (tedit 595FF906)
    (at 89.7763 25.4)
    (descr "LED 0603 SMT")
    (tags "LED 0603 SMT")
    (attr smd)
    (fp_text reference M2-D_PWR:LED_GRN1 (at 1.6637 -1.905 180 unlocked) (layer F.SilkS))
    (fp_text value LED-GREEN0603 (at 0 1.016) (layer F.SilkS) hide)
    (pad C smd rect (at 0.8763 0 270) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 17 /M2-D:PWR_CHK/M2-D:GND) (solder_mask_margin 0.1016))
    (pad A smd rect (at -0.8763 0 270) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(M2-D_PWR:LED_GRN1-PadA)") (solder_mask_margin 0.1016))
  )
  (module LED:LED-0603 (layer F.Cu) (tedit 595FF906)
    (at 100.7237 25.4 180)
    (descr "LED 0603 SMT")
    (tags "LED 0603 SMT")
    (attr smd)
    (fp_text reference M2-D_PWR:LED_RED1 (at -0.2413 1.905 180 unlocked) (layer F.SilkS))
    (fp_text value LED-RED0603 (at 0 1.016) (layer F.SilkS) hide)
    (pad A smd rect (at -0.8763 0 90) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(M2-D_PWR:LED_RED1-PadA)") (solder_mask_margin 0.1016))
    (pad C smd rect (at 0.8763 0 90) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 17 /M2-D:PWR_CHK/M2-D:GND) (solder_mask_margin 0.1016))
  )
  (module ERA-3AEB331V:RESC1608X55N (layer F.Cu) (tedit 0)
    (at 88.9 29.21 90)
    (attr smd)
    (fp_text reference M2-D_PWR:R_GRN1 (at -3.175 0.635 180 unlocked) (layer F.SilkS))
    (fp_text value ERA-3AEB331V (at -0.21 1.05 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.78 0 90) (size 0.87 0.93) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(M2-D_PWR:LED_GRN1-PadA)"))
    (pad 1 smd rect (at -0.78 0 90) (size 0.87 0.93) (layers F.Cu F.Paste F.Mask)
      (net 44 /M2-D:OUT1))
  )
  (module ERA-3AEB331V:RESC1608X55N (layer F.Cu) (tedit 0)
    (at 101.6 29.21 90)
    (attr smd)
    (fp_text reference M2-D_PWR:R_RED1 (at -3.175 -0.635 180 unlocked) (layer F.SilkS))
    (fp_text value ERA-3AEB331V (at -0.21 1.05 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.78 0 90) (size 0.87 0.93) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(M2-D_PWR:LED_RED1-PadA)"))
    (pad 1 smd rect (at -0.78 0 90) (size 0.87 0.93) (layers F.Cu F.Paste F.Mask)
      (net 43 /M2-D:OUT2))
  )
  (module RC0201FR-074K7L:RESC0603X26N (layer F.Cu) (tedit 0)
    (at 76.835 73.025 90)
    (attr smd)
    (fp_text reference M2-HB:R_GND1 (at -3.175 8.255 180 unlocked) (layer F.SilkS))
    (fp_text value RC0201FR-074K7L (at -0.065 0.8 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.28 0 180) (size 0.4 0.38) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.305 0 180) (size 0.4 0.33) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(M2-HB:P1-Pad3)"))
  )
  (module RC0201FR-074K7L:RESC0603X26N (layer F.Cu) (tedit 0)
    (at 113.665 72.72 90)
    (attr smd)
    (fp_text reference M2-HB:R_GND2 (at -3.48 -8.255 180 unlocked) (layer F.SilkS))
    (fp_text value RC0201FR-074K7L (at -0.065 0.8 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.28 0 180) (size 0.4 0.38) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.305 0 180) (size 0.4 0.33) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(M2-HB:P2-Pad3)"))
  )
  (module RC0201FR-074K7L:RESC0603X26N (layer F.Cu) (tedit 0)
    (at 88.265 78.105 180)
    (attr smd)
    (fp_text reference M2-HB:R_VCM1 (at -0.635 -1.905 180 unlocked) (layer F.SilkS))
    (fp_text value RC0201FR-074K7L (at -0.065 0.8) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.28 0 270) (size 0.4 0.38) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(M2-HB:P1-Pad1)"))
    (pad 1 smd rect (at -0.305 0 270) (size 0.4 0.33) (layers F.Cu F.Paste F.Mask)
      (net 14 VCM))
  )
  (module RC0201FR-074K7L:RESC0603X26N (layer F.Cu) (tedit 0)
    (at 102.235 78.105)
    (attr smd)
    (fp_text reference M2-HB:R_VCM2 (at -0.635 1.905 180 unlocked) (layer F.SilkS))
    (fp_text value RC0201FR-074K7L (at -0.065 0.8) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.28 0 90) (size 0.4 0.38) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(M2-HB:P2-Pad1)"))
    (pad 1 smd rect (at -0.305 0 90) (size 0.4 0.33) (layers F.Cu F.Paste F.Mask)
      (net 14 VCM))
  )
  (module Connectors:2X5-SHROUDED_LOCK (layer F.Cu) (tedit 200000)
    (at 139.7 40.64 270)
    (descr "PLATED THROUGH HOLE - 2X5 SHROUDED HEADER LOCKING FOOTPRINT")
    (tags "PLATED THROUGH HOLE - 2X5 SHROUDED HEADER LOCKING FOOTPRINT")
    (attr virtual)
    (fp_text reference M3-CTRL:CN1 (at -5.715 0 180 unlocked) (layer F.SilkS))
    (fp_text value CONN_05X2SHD_LOCK (at -5.08 -5.08) (layer F.SilkS) hide)
    (pad 10 thru_hole circle (at 1.397 5.08 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 V_PWR) (solder_mask_margin 0.1016))
    (pad 9 thru_hole circle (at -1.397 5.08 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 V_PWR) (solder_mask_margin 0.1016))
    (pad 8 thru_hole circle (at 1.397 2.54 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 7 thru_hole circle (at -1.397 2.54 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 6 thru_hole circle (at 1.397 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 45 /M3-D:OUT2) (solder_mask_margin 0.1016))
    (pad 5 thru_hole circle (at -1.397 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 46 /M3-D:OUT1) (solder_mask_margin 0.1016))
    (pad 4 thru_hole circle (at 1.397 -2.54 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 29 /M3-D:PWR_CHK/M3-D:GND) (solder_mask_margin 0.1016))
    (pad 3 thru_hole circle (at -1.397 -2.54 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 2 thru_hole circle (at 1.397 -5.08 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 30 /CH6) (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at -1.397 -5.08 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 31 /CH5) (solder_mask_margin 0.1016))
  )
  (module LED:LED-0603 (layer F.Cu) (tedit 595FF906)
    (at 134.2263 25.4)
    (descr "LED 0603 SMT")
    (tags "LED 0603 SMT")
    (attr smd)
    (fp_text reference M3-D_PWR:LED_GRN1 (at 1.6637 -1.905 180 unlocked) (layer F.SilkS))
    (fp_text value LED-GREEN0603 (at 0 1.016) (layer F.SilkS) hide)
    (pad C smd rect (at 0.8763 0 270) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 29 /M3-D:PWR_CHK/M3-D:GND) (solder_mask_margin 0.1016))
    (pad A smd rect (at -0.8763 0 270) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(M3-D_PWR:LED_GRN1-PadA)") (solder_mask_margin 0.1016))
  )
  (module LED:LED-0603 (layer F.Cu) (tedit 595FF906)
    (at 145.1737 25.4 180)
    (descr "LED 0603 SMT")
    (tags "LED 0603 SMT")
    (attr smd)
    (fp_text reference M3-D_PWR:LED_RED1 (at 1.6637 1.905 180 unlocked) (layer F.SilkS))
    (fp_text value LED-RED0603 (at 0 1.016) (layer F.SilkS) hide)
    (pad C smd rect (at 0.8763 0 90) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 29 /M3-D:PWR_CHK/M3-D:GND) (solder_mask_margin 0.1016))
    (pad A smd rect (at -0.8763 0 90) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(M3-D_PWR:LED_RED1-PadA)") (solder_mask_margin 0.1016))
  )
  (module ERA-3AEB331V:RESC1608X55N (layer F.Cu) (tedit 0)
    (at 133.35 29.21 90)
    (attr smd)
    (fp_text reference M3-D_PWR:R_GRN1 (at -3.175 0.635 180 unlocked) (layer F.SilkS))
    (fp_text value ERA-3AEB331V (at -0.21 1.05 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.78 0 90) (size 0.87 0.93) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(M3-D_PWR:LED_GRN1-PadA)"))
    (pad 1 smd rect (at -0.78 0 90) (size 0.87 0.93) (layers F.Cu F.Paste F.Mask)
      (net 46 /M3-D:OUT1))
  )
  (module ERA-3AEB331V:RESC1608X55N (layer F.Cu) (tedit 0)
    (at 146.05 29.21 90)
    (attr smd)
    (fp_text reference M3-D_PWR:R_RED1 (at -3.175 -0.635 180 unlocked) (layer F.SilkS))
    (fp_text value ERA-3AEB331V (at -0.21 1.05 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.78 0 90) (size 0.87 0.93) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(M3-D_PWR:LED_RED1-PadA)"))
    (pad 1 smd rect (at -0.78 0 90) (size 0.87 0.93) (layers F.Cu F.Paste F.Mask)
      (net 45 /M3-D:OUT2))
  )
  (module RC0201FR-074K7L:RESC0603X26N (layer F.Cu) (tedit 0)
    (at 121.285 72.72 90)
    (attr smd)
    (fp_text reference M3-HB:R_GND1 (at -3.48 8.255 180 unlocked) (layer F.SilkS))
    (fp_text value RC0201FR-074K7L (at -0.065 0.8 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.28 0 180) (size 0.4 0.38) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.305 0 180) (size 0.4 0.33) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(M3-HB:P1-Pad3)"))
  )
  (module RC0201FR-074K7L:RESC0603X26N (layer F.Cu) (tedit 0)
    (at 158.115 72.72 90)
    (attr smd)
    (fp_text reference M3-HB:R_GND2 (at -3.48 -7.62 180 unlocked) (layer F.SilkS))
    (fp_text value RC0201FR-074K7L (at -0.065 0.8 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.28 0 180) (size 0.4 0.38) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.305 0 180) (size 0.4 0.33) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(M3-HB:P2-Pad3)"))
  )
  (module RC0201FR-074K7L:RESC0603X26N (layer F.Cu) (tedit 0)
    (at 132.715 78.105 180)
    (attr smd)
    (fp_text reference M3-HB:R_VCM1 (at -0.635 -1.905 180 unlocked) (layer F.SilkS))
    (fp_text value RC0201FR-074K7L (at -0.065 0.8) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.28 0 270) (size 0.4 0.38) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(M3-HB:P1-Pad1)"))
    (pad 1 smd rect (at -0.305 0 270) (size 0.4 0.33) (layers F.Cu F.Paste F.Mask)
      (net 14 VCM))
  )
  (module RC0201FR-074K7L:RESC0603X26N (layer F.Cu) (tedit 0)
    (at 146.685 78.105)
    (attr smd)
    (fp_text reference M3-HB:R_VCM2 (at -0.635 1.905 180 unlocked) (layer F.SilkS))
    (fp_text value RC0201FR-074K7L (at -0.065 0.8) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.28 0 90) (size 0.4 0.38) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(M3-HB:P2-Pad1)"))
    (pad 1 smd rect (at -0.305 0 90) (size 0.4 0.33) (layers F.Cu F.Paste F.Mask)
      (net 14 VCM))
  )
  (module Capacitors:EIA3216 (layer F.Cu) (tedit 200000)
    (at 79.375 40.51046 90)
    (descr "GENERIC EIA 3216 (1206) POLARIZED TANTALUM CAPACITOR")
    (tags "GENERIC EIA 3216 (1206) POLARIZED TANTALUM CAPACITOR")
    (attr smd)
    (fp_text reference PWR_BYP:C1 (at -3.93954 0 180 unlocked) (layer F.SilkS))
    (fp_text value 10UF-POLAR-EIA3216 (at -0.127 1.905 90) (layer F.SilkS) hide)
    (pad - smd rect (at -1.39954 0 180) (size 1.59766 1.39954) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad + smd rect (at 1.39954 0 180) (size 1.59766 1.39954) (layers F.Cu F.Paste F.Mask)
      (net 2 V_PWR) (solder_mask_margin 0.1016))
  )
  (module "S7B-PH-K-S(LF)(SN):SHDR7W50P0X200_1X7_1590X760X480P" (layer F.Cu) (tedit 5D17145E)
    (at 69.85 99.06 180)
    (descr "S7B-PH-K-S(")
    (tags Connector)
    (fp_text reference SG_V:CN1 (at -5.969 -7.62 180 unlocked) (layer F.SilkS))
    (fp_text value "S7B-PH-K-S(LF)(SN)" (at 0 0) (layer F.SilkS) hide)
    (pad 7 thru_hole circle (at -12 0 270) (size 1.35 1.35) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 15 SG_REF:CH7))
    (pad 6 thru_hole circle (at -10 0 270) (size 1.35 1.35) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 38 /M3-AMP/M3-SG_V:CH6))
    (pad 5 thru_hole circle (at -8 0 270) (size 1.35 1.35) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 35 /M3-AMP/M3-SG_V:CH5))
    (pad 4 thru_hole circle (at -6 0 270) (size 1.35 1.35) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 27 /M2-AMP/M2-SG_V:CH4))
    (pad 3 thru_hole circle (at -4 0 270) (size 1.35 1.35) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 24 /M2-AMP/M2-SG_V:CH3))
    (pad 2 thru_hole circle (at -2 0 270) (size 1.35 1.35) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 12 /M1-AMP/M1-SG_V:CH2))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.35 1.35) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 9 /M1-AMP/M1-SG_V:CH1))
  )
  (module Connectors:JST-2-PTH (layer F.Cu) (tedit 200000)
    (at 92.34678 99.06 180)
    (descr "JST 2 PIN RIGHT ANGLE PLATED THROUGH  HOLE")
    (tags "JST 2 PIN RIGHT ANGLE PLATED THROUGH  HOLE")
    (attr virtual)
    (fp_text reference SG_VCM:CN1 (at -0.27178 -7.62 180 unlocked) (layer F.SilkS))
    (fp_text value CONN_02JST-PTH-2 (at 3.556 0 180) (layer F.SilkS) hide)
    (fp_text user + (at 1.23444 -1.3335) (layer Dwgs.User))
    (fp_text user - (at -0.76454 -1.3335) (layer Dwgs.User))
    (pad 1 thru_hole circle (at -0.99822 0 180) (size 1.59766 1.59766) (drill 0.6985) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 2 thru_hole circle (at 0.99822 0 180) (size 1.59766 1.59766) (drill 0.6985) (layers *.Cu *.Mask)
      (net 14 VCM) (solder_mask_margin 0.1016))
  )
  (module LED:LED-0603 (layer F.Cu) (tedit 595FF906)
    (at 107.7087 94.615 180)
    (descr "LED 0603 SMT")
    (tags "LED 0603 SMT")
    (attr smd)
    (fp_text reference VCM:LED_BLU1 (at 0 -2.54 180 unlocked) (layer F.SilkS))
    (fp_text value LED-BLUE0603 (at 0 1.016) (layer F.SilkS) hide)
    (pad C smd rect (at 0.8763 0 90) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad A smd rect (at -0.8763 0 90) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(VCM:LED_BLU1-PadA)") (solder_mask_margin 0.1016))
  )
  (module ERA-3AEB331V:RESC1608X55N (layer F.Cu) (tedit 0)
    (at 120.16 94.615 180)
    (attr smd)
    (fp_text reference VCM:R_GRN1 (at 0.145 -2.54 180 unlocked) (layer F.SilkS))
    (fp_text value ERA-3AEB331V (at -0.21 1.05) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.78 0 180) (size 0.87 0.93) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(VCM:LED_BLU1-PadA)"))
    (pad 1 smd rect (at -0.78 0 180) (size 0.87 0.93) (layers F.Cu F.Paste F.Mask)
      (net 14 VCM))
  )
  (module Capacitors:EIA3216 (layer F.Cu) (tedit 200000)
    (at 139.7 100.965 180)
    (descr "GENERIC EIA 3216 (1206) POLARIZED TANTALUM CAPACITOR")
    (tags "GENERIC EIA 3216 (1206) POLARIZED TANTALUM CAPACITOR")
    (attr smd)
    (fp_text reference VCM_BYP:C1 (at 0 -2.54 180 unlocked) (layer F.SilkS))
    (fp_text value 10UF-POLAR-EIA3216 (at -0.127 1.905) (layer F.SilkS) hide)
    (pad - smd rect (at -1.39954 0 270) (size 1.59766 1.39954) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad + smd rect (at 1.39954 0 270) (size 1.59766 1.39954) (layers F.Cu F.Paste F.Mask)
      (net 14 VCM) (solder_mask_margin 0.1016))
  )
  (module lib_fp:EIA3216 (layer F.Cu) (tedit 200000)
    (at 95.25 66.675)
    (descr "GENERIC EIA 3216 (1206) POLARIZED TANTALUM CAPACITOR")
    (tags "GENERIC EIA 3216 (1206) POLARIZED TANTALUM CAPACITOR")
    (attr smd)
    (fp_text reference BYP_AMP:C1 (at 0 2.54 180 unlocked) (layer F.SilkS))
    (fp_text value 10UF-POLAR-EIA3216 (at -0.127 1.905) (layer F.SilkS) hide)
    (pad + smd rect (at 1.39954 0 90) (size 1.59766 1.39954) (layers F.Cu F.Paste F.Mask)
      (net 2 V_PWR) (solder_mask_margin 0.1016))
    (pad - smd rect (at -1.39954 0 90) (size 1.59766 1.39954) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
  )
  (module POT_3296W:3296W-1-501LF (layer F.Cu) (tedit 5D191657)
    (at 63.5 54.61 270)
    (fp_text reference M1-G:P2 (at 3.81 2.54 180 unlocked) (layer F.SilkS))
    (fp_text value 3296W-1-501LF (at -2.53 4.04 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -5.0546 -0.127 270) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -2.5146 -0.127 270) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 50 /M1-AMP/M1-IN_AMP:2/M1-G:WIP2))
    (pad 3 thru_hole circle (at 0.0254 -0.127 270) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 49 /M1-AMP/M1-IN_AMP:2/M1-G:V_IN2))
  )
  (module POT_3296W:3296W-1-501LF (layer F.Cu) (tedit 5D191657)
    (at 38.1 54.5846 270)
    (fp_text reference M1-G:P1 (at 3.8354 -2.54 180 unlocked) (layer F.SilkS))
    (fp_text value 3296W-1-501LF (at -2.53 4.04 90) (layer F.SilkS) hide)
    (pad 3 thru_hole circle (at 0.0254 -0.127 270) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 48 /M1-AMP/M1-IN_AMP:1/M1-G:V_IN1))
    (pad 2 thru_hole circle (at -2.5146 -0.127 270) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 47 /M1-AMP/M1-IN_AMP:1/M1-G:WIP1))
    (pad 1 thru_hole rect (at -5.0546 -0.127 270) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask))
  )
  (module lib_fp:4_40_Screw_Mounting_Hole (layer F.Cu) (tedit 5D1B7371)
    (at 69.85 39.37)
    (fp_text reference MH1 (at 0 5.08 180 unlocked) (layer F.SilkS))
    (fp_text value MountingHole (at 0 5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3.22 3.22) (drill 3.22) (layers *.Cu *.Mask))
  )
  (module lib_fp:4_40_Screw_Mounting_Hole (layer F.Cu) (tedit 5D1B7371)
    (at 95.25 86.36)
    (fp_text reference MH3 (at 0 5.08 180 unlocked) (layer F.SilkS))
    (fp_text value MountingHole (at 0 5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3.22 3.22) (drill 3.22) (layers *.Cu *.Mask))
  )
  (module lib_fp:4_40_Screw_Mounting_Hole (layer F.Cu) (tedit 5D1B7371)
    (at 120.65 39.37)
    (fp_text reference MH2 (at 0 5.08 180 unlocked) (layer F.SilkS))
    (fp_text value MountingHole (at 0 5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3.22 3.22) (drill 3.22) (layers *.Cu *.Mask))
  )
  (module Package_TO_SOT_SMD:SOT-23-5 (layer F.Cu) (tedit 5A02FF57)
    (at 139.7 96.52 180)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference VCM:VR1 (at 0 3.175 180 unlocked) (layer F.SilkS))
    (fp_text value MIC5205-5.0YM5 (at 0 2.9) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90 unlocked) (layer F.Fab) hide)
    (pad 5 smd rect (at 1.1 -0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 14 VCM))
    (pad 4 smd rect (at 1.1 0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at -1.1 0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 V_PWR))
    (pad 2 smd rect (at -1.1 0 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.1 -0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 V_PWR))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module INA2126:SO16 (layer F.Cu) (tedit 0)
    (at 95.25 59.69 270)
    (descr "<b>PLASTIC SMALL-OUTLINES PACKAGE</b> D (R-PDSO-G16)<p>Source: http://focus.ti.com/lit/ds/symlink/ina2126.pdf")
    (attr smd)
    (fp_text reference M2-INAS1 (at -6.35 0.00001 180 unlocked) (layer F.SilkS))
    (fp_text value INA2126 (at -0.636065 0.000001 90) (layer F.SilkS))
    (pad 16 smd rect (at -4.445 -2.8752 270) (size 0.762 1.524) (layers F.Cu F.Paste F.Mask)
      (net 15 SG_REF:CH7))
    (pad 15 smd rect (at -3.175 -2.8752 270) (size 0.762 1.524) (layers F.Cu F.Paste F.Mask)
      (net 27 /M2-AMP/M2-SG_V:CH4))
    (pad 14 smd rect (at -1.905 -2.8752 270) (size 0.762 1.524) (layers F.Cu F.Paste F.Mask)
      (net 22 /M2-AMP/M2-IN_AMP:2/M2-G:WIP2))
    (pad 13 smd rect (at -0.635 -2.8752 270) (size 0.762 1.524) (layers F.Cu F.Paste F.Mask)
      (net 53 /M2-AMP/M2-IN_AMP:2/M2-G:V_IN2))
    (pad 12 smd rect (at 0.635 -2.8752 270) (size 0.762 1.524) (layers F.Cu F.Paste F.Mask)
      (net 16 V_REF))
    (pad 11 smd rect (at 1.905 -2.8752 270) (size 0.762 1.524) (layers F.Cu F.Paste F.Mask)
      (net 18 /CH4))
    (pad 10 smd rect (at 3.175 -2.8752 270) (size 0.762 1.524) (layers F.Cu F.Paste F.Mask)
      (net 18 /CH4))
    (pad 9 smd rect (at 4.445 -2.8752 270) (size 0.762 1.524) (layers F.Cu F.Paste F.Mask)
      (net 2 V_PWR))
    (pad 8 smd rect (at 4.445 2.8752 270) (size 0.762 1.524) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 7 smd rect (at 3.175 2.8752 270) (size 0.762 1.524) (layers F.Cu F.Paste F.Mask)
      (net 19 /CH3))
    (pad 6 smd rect (at 1.905 2.8752 270) (size 0.762 1.524) (layers F.Cu F.Paste F.Mask)
      (net 19 /CH3))
    (pad 5 smd rect (at 0.635 2.8752 270) (size 0.762 1.524) (layers F.Cu F.Paste F.Mask)
      (net 16 V_REF))
    (pad 4 smd rect (at -0.635 2.8752 270) (size 0.762 1.524) (layers F.Cu F.Paste F.Mask)
      (net 51 /M2-AMP/M2-IN_AMP:1/M2-G:V_IN1))
    (pad 3 smd rect (at -1.905 2.8752 270) (size 0.762 1.524) (layers F.Cu F.Paste F.Mask)
      (net 52 /M2-AMP/M2-IN_AMP:1/M2-G:WIP1))
    (pad 2 smd rect (at -3.175 2.8752 270) (size 0.762 1.524) (layers F.Cu F.Paste F.Mask)
      (net 24 /M2-AMP/M2-SG_V:CH3))
    (pad 1 smd rect (at -4.445 2.8752 270) (size 0.762 1.524) (layers F.Cu F.Paste F.Mask)
      (net 15 SG_REF:CH7))
  )
  (module INA2126:SO16 (layer F.Cu) (tedit 0)
    (at 50.8 59.69 270)
    (descr "<b>PLASTIC SMALL-OUTLINES PACKAGE</b> D (R-PDSO-G16)<p>Source: http://focus.ti.com/lit/ds/symlink/ina2126.pdf")
    (attr smd)
    (fp_text reference M1-INAS1 (at -6.35 0.00001 180 unlocked) (layer F.SilkS))
    (fp_text value INA2126 (at -0.636065 0.000001 270) (layer F.SilkS))
    (pad 1 smd rect (at -4.445 2.8752 270) (size 0.762 1.524) (layers F.Cu F.Paste F.Mask)
      (net 15 SG_REF:CH7))
    (pad 2 smd rect (at -3.175 2.8752 270) (size 0.762 1.524) (layers F.Cu F.Paste F.Mask)
      (net 9 /M1-AMP/M1-SG_V:CH1))
    (pad 3 smd rect (at -1.905 2.8752 270) (size 0.762 1.524) (layers F.Cu F.Paste F.Mask)
      (net 47 /M1-AMP/M1-IN_AMP:1/M1-G:WIP1))
    (pad 4 smd rect (at -0.635 2.8752 270) (size 0.762 1.524) (layers F.Cu F.Paste F.Mask)
      (net 48 /M1-AMP/M1-IN_AMP:1/M1-G:V_IN1))
    (pad 5 smd rect (at 0.635 2.8752 270) (size 0.762 1.524) (layers F.Cu F.Paste F.Mask)
      (net 16 V_REF))
    (pad 6 smd rect (at 1.905 2.8752 270) (size 0.762 1.524) (layers F.Cu F.Paste F.Mask)
      (net 5 /CH1))
    (pad 7 smd rect (at 3.175 2.8752 270) (size 0.762 1.524) (layers F.Cu F.Paste F.Mask)
      (net 5 /CH1))
    (pad 8 smd rect (at 4.445 2.8752 270) (size 0.762 1.524) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at 4.445 -2.8752 270) (size 0.762 1.524) (layers F.Cu F.Paste F.Mask)
      (net 2 V_PWR))
    (pad 10 smd rect (at 3.175 -2.8752 270) (size 0.762 1.524) (layers F.Cu F.Paste F.Mask)
      (net 4 /CH2))
    (pad 11 smd rect (at 1.905 -2.8752 270) (size 0.762 1.524) (layers F.Cu F.Paste F.Mask)
      (net 4 /CH2))
    (pad 12 smd rect (at 0.635 -2.8752 270) (size 0.762 1.524) (layers F.Cu F.Paste F.Mask)
      (net 16 V_REF))
    (pad 13 smd rect (at -0.635 -2.8752 270) (size 0.762 1.524) (layers F.Cu F.Paste F.Mask)
      (net 49 /M1-AMP/M1-IN_AMP:2/M1-G:V_IN2))
    (pad 14 smd rect (at -1.905 -2.8752 270) (size 0.762 1.524) (layers F.Cu F.Paste F.Mask)
      (net 50 /M1-AMP/M1-IN_AMP:2/M1-G:WIP2))
    (pad 15 smd rect (at -3.175 -2.8752 270) (size 0.762 1.524) (layers F.Cu F.Paste F.Mask)
      (net 12 /M1-AMP/M1-SG_V:CH2))
    (pad 16 smd rect (at -4.445 -2.8752 270) (size 0.762 1.524) (layers F.Cu F.Paste F.Mask)
      (net 15 SG_REF:CH7))
  )
  (module INA2126:SO16 (layer F.Cu) (tedit 0)
    (at 139.7 59.69 270)
    (descr "<b>PLASTIC SMALL-OUTLINES PACKAGE</b> D (R-PDSO-G16)<p>Source: http://focus.ti.com/lit/ds/symlink/ina2126.pdf")
    (attr smd)
    (fp_text reference M3-INAS1 (at -6.35 0 180 unlocked) (layer F.SilkS))
    (fp_text value INA2126 (at -0.636065 0.000001 90) (layer F.SilkS))
    (pad 16 smd rect (at -4.445 -2.8752 270) (size 0.762 1.524) (layers F.Cu F.Paste F.Mask)
      (net 15 SG_REF:CH7))
    (pad 15 smd rect (at -3.175 -2.8752 270) (size 0.762 1.524) (layers F.Cu F.Paste F.Mask)
      (net 38 /M3-AMP/M3-SG_V:CH6))
    (pad 14 smd rect (at -1.905 -2.8752 270) (size 0.762 1.524) (layers F.Cu F.Paste F.Mask)
      (net 56 /M3-AMP/M3-IN_AMP:2/M3-G:WIP2))
    (pad 13 smd rect (at -0.635 -2.8752 270) (size 0.762 1.524) (layers F.Cu F.Paste F.Mask)
      (net 57 /M3-AMP/M3-IN_AMP:2/M3-G:V_IN2))
    (pad 12 smd rect (at 0.635 -2.8752 270) (size 0.762 1.524) (layers F.Cu F.Paste F.Mask)
      (net 16 V_REF))
    (pad 11 smd rect (at 1.905 -2.8752 270) (size 0.762 1.524) (layers F.Cu F.Paste F.Mask)
      (net 30 /CH6))
    (pad 10 smd rect (at 3.175 -2.8752 270) (size 0.762 1.524) (layers F.Cu F.Paste F.Mask)
      (net 30 /CH6))
    (pad 9 smd rect (at 4.445 -2.8752 270) (size 0.762 1.524) (layers F.Cu F.Paste F.Mask)
      (net 2 V_PWR))
    (pad 8 smd rect (at 4.445 2.8752 270) (size 0.762 1.524) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 7 smd rect (at 3.175 2.8752 270) (size 0.762 1.524) (layers F.Cu F.Paste F.Mask)
      (net 31 /CH5))
    (pad 6 smd rect (at 1.905 2.8752 270) (size 0.762 1.524) (layers F.Cu F.Paste F.Mask)
      (net 31 /CH5))
    (pad 5 smd rect (at 0.635 2.8752 270) (size 0.762 1.524) (layers F.Cu F.Paste F.Mask)
      (net 16 V_REF))
    (pad 4 smd rect (at -0.635 2.8752 270) (size 0.762 1.524) (layers F.Cu F.Paste F.Mask)
      (net 55 /M3-AMP/M3-IN_AMP:1/M3-G:V_IN1))
    (pad 3 smd rect (at -1.905 2.8752 270) (size 0.762 1.524) (layers F.Cu F.Paste F.Mask)
      (net 54 /M3-AMP/M3-IN_AMP:1/M3-G:WIP1))
    (pad 2 smd rect (at -3.175 2.8752 270) (size 0.762 1.524) (layers F.Cu F.Paste F.Mask)
      (net 35 /M3-AMP/M3-SG_V:CH5))
    (pad 1 smd rect (at -4.445 2.8752 270) (size 0.762 1.524) (layers F.Cu F.Paste F.Mask)
      (net 15 SG_REF:CH7))
  )
  (module POT_3296W:3296W-1-501LF (layer F.Cu) (tedit 5D191657)
    (at 82.55 71.755 270)
    (fp_text reference M2-HB:P1 (at -8.89 -2.54 180 unlocked) (layer F.SilkS))
    (fp_text value 3296W-1-501LF (at -2.53 4.04 90) (layer F.SilkS) hide)
    (pad 3 thru_hole circle (at 0.0254 -0.127 270) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 25 "Net-(M2-HB:P1-Pad3)"))
    (pad 2 thru_hole circle (at -2.5146 -0.127 270) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 24 /M2-AMP/M2-SG_V:CH3))
    (pad 1 thru_hole rect (at -5.0546 -0.127 270) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 23 "Net-(M2-HB:P1-Pad1)"))
  )
  (module POT_3296W:3296W-1-501LF (layer F.Cu) (tedit 5D191657)
    (at 152.4 71.755 270)
    (fp_text reference M3-HB:P2 (at -8.89 2.54 180 unlocked) (layer F.SilkS))
    (fp_text value 3296W-1-501LF (at -2.53 4.04 90) (layer F.SilkS) hide)
    (pad 3 thru_hole circle (at 0.0254 -0.127 270) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 39 "Net-(M3-HB:P2-Pad3)"))
    (pad 2 thru_hole circle (at -2.5146 -0.127 270) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 38 /M3-AMP/M3-SG_V:CH6))
    (pad 1 thru_hole rect (at -5.0546 -0.127 270) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 37 "Net-(M3-HB:P2-Pad1)"))
  )
  (module POT_3296W:3296W-1-501LF (layer F.Cu) (tedit 5D191657)
    (at 127 71.755 270)
    (fp_text reference M3-HB:P1 (at -8.89 -2.54 180 unlocked) (layer F.SilkS))
    (fp_text value 3296W-1-501LF (at -2.53 4.04 90) (layer F.SilkS) hide)
    (pad 3 thru_hole circle (at 0.0254 -0.127 270) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 36 "Net-(M3-HB:P1-Pad3)"))
    (pad 2 thru_hole circle (at -2.5146 -0.127 270) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 35 /M3-AMP/M3-SG_V:CH5))
    (pad 1 thru_hole rect (at -5.0546 -0.127 270) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 34 "Net-(M3-HB:P1-Pad1)"))
  )
  (module POT_3296W:3296W-1-501LF (layer F.Cu) (tedit 5D191657)
    (at 152.4 54.61 270)
    (fp_text reference M3-G:P2 (at 3.81 2.54 180 unlocked) (layer F.SilkS))
    (fp_text value 3296W-1-501LF (at -2.53 4.04 90) (layer F.SilkS) hide)
    (pad 3 thru_hole circle (at 0.0254 -0.127 270) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 57 /M3-AMP/M3-IN_AMP:2/M3-G:V_IN2))
    (pad 2 thru_hole circle (at -2.5146 -0.127 270) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 56 /M3-AMP/M3-IN_AMP:2/M3-G:WIP2))
    (pad 1 thru_hole rect (at -5.0546 -0.127 270) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask))
  )
  (module POT_3296W:3296W-1-501LF (layer F.Cu) (tedit 5D191657)
    (at 127 54.61 270)
    (fp_text reference M3-G:P1 (at 3.81 -2.54 180 unlocked) (layer F.SilkS))
    (fp_text value 3296W-1-501LF (at -2.53 4.04 90) (layer F.SilkS) hide)
    (pad 3 thru_hole circle (at 0.0254 -0.127 270) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 55 /M3-AMP/M3-IN_AMP:1/M3-G:V_IN1))
    (pad 2 thru_hole circle (at -2.5146 -0.127 270) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 54 /M3-AMP/M3-IN_AMP:1/M3-G:WIP1))
    (pad 1 thru_hole rect (at -5.0546 -0.127 270) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask))
  )
  (module POT_3296W:3296W-1-501LF (layer F.Cu) (tedit 5D191657)
    (at 107.95 71.755 270)
    (fp_text reference M2-HB:P2 (at -8.89 2.54 180 unlocked) (layer F.SilkS))
    (fp_text value 3296W-1-501LF (at -2.53 4.04 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -5.0546 -0.127 270) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 26 "Net-(M2-HB:P2-Pad1)"))
    (pad 2 thru_hole circle (at -2.5146 -0.127 270) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 27 /M2-AMP/M2-SG_V:CH4))
    (pad 3 thru_hole circle (at 0.0254 -0.127 270) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 28 "Net-(M2-HB:P2-Pad3)"))
  )
  (module POT_3296W:3296W-1-501LF (layer F.Cu) (tedit 5D191657)
    (at 107.95 54.61 270)
    (fp_text reference M2-G:P2 (at 3.81 2.54 180 unlocked) (layer F.SilkS))
    (fp_text value 3296W-1-501LF (at -2.53 4.04 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -5.0546 -0.127 270) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -2.5146 -0.127 270) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 22 /M2-AMP/M2-IN_AMP:2/M2-G:WIP2))
    (pad 3 thru_hole circle (at 0.0254 -0.127 270) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 53 /M2-AMP/M2-IN_AMP:2/M2-G:V_IN2))
  )
  (module POT_3296W:3296W-1-501LF (layer F.Cu) (tedit 5D191657)
    (at 82.55 54.61 270)
    (fp_text reference M2-G:P1 (at 3.81 -2.54 180 unlocked) (layer F.SilkS))
    (fp_text value 3296W-1-501LF (at -2.53 4.04 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -5.0546 -0.127 270) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -2.5146 -0.127 270) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 52 /M2-AMP/M2-IN_AMP:1/M2-G:WIP1))
    (pad 3 thru_hole circle (at 0.0254 -0.127 270) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 51 /M2-AMP/M2-IN_AMP:1/M2-G:V_IN1))
  )
  (module POT_3296W:3296W-1-501LF (layer F.Cu) (tedit 5D191657)
    (at 63.5 71.7296 270)
    (fp_text reference M1-HB:P2 (at -8.8646 2.54 180 unlocked) (layer F.SilkS))
    (fp_text value 3296W-1-501LF (at -2.53 4.04 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -5.0546 -0.127 270) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 11 "Net-(M1-HB:P2-Pad1)"))
    (pad 2 thru_hole circle (at -2.5146 -0.127 270) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 12 /M1-AMP/M1-SG_V:CH2))
    (pad 3 thru_hole circle (at 0.0254 -0.127 270) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 13 "Net-(M1-HB:P2-Pad3)"))
  )
  (module POT_3296W:3296W-1-501LF (layer F.Cu) (tedit 5D191657)
    (at 37.973 71.7296 270)
    (fp_text reference M1-HB:P1 (at -8.8646 -2.667 180 unlocked) (layer F.SilkS))
    (fp_text value 3296W-1-501LF (at -2.53 4.04 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -5.0546 -0.127 270) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 8 "Net-(M1-HB:P1-Pad1)"))
    (pad 2 thru_hole circle (at -2.5146 -0.127 270) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 9 /M1-AMP/M1-SG_V:CH1))
    (pad 3 thru_hole circle (at 0.0254 -0.127 270) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 10 "Net-(M1-HB:P1-Pad3)"))
  )
  (module Resistors:0603 (layer F.Cu) (tedit 200000)
    (at 133.35 92.075)
    (descr "GENERIC 1608 (0603) PACKAGE")
    (tags "GENERIC 1608 (0603) PACKAGE")
    (attr smd)
    (fp_text reference V_REF:R_VCM1 (at -1.905 0 180 unlocked) (layer F.SilkS))
    (fp_text value RN732BTTD4001B25 (at 0 1.27) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.84836 0) (size 1.09982 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 16 V_REF) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.84836 0) (size 1.09982 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 14 VCM) (solder_mask_margin 0.1016))
  )
  (module Resistors:0603 (layer F.Cu) (tedit 200000)
    (at 146.05 92.075)
    (descr "GENERIC 1608 (0603) PACKAGE")
    (tags "GENERIC 1608 (0603) PACKAGE")
    (attr smd)
    (fp_text reference V_REF:R_GND1 (at 1.905 0 180 unlocked) (layer F.SilkS))
    (fp_text value ERJ-1GNF1001C (at 0 1.27) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.84836 0) (size 1.09982 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.84836 0) (size 1.09982 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 16 V_REF) (solder_mask_margin 0.1016))
  )
  (gr_text REF (at 81.915 93.98 270) (layer F.SilkS))
  (gr_text "GND\n" (at 93.345 95.25 270) (layer F.SilkS))
  (gr_text 5V (at 91.44 95.25 270) (layer F.SilkS))
  (gr_text V6 (at 80.01 94.996 270) (layer F.SilkS))
  (gr_text V5 (at 77.978 94.996 270) (layer F.SilkS))
  (gr_text V4 (at 76.073 94.996 270) (layer F.SilkS))
  (gr_text V3 (at 74.041 94.996 270) (layer F.SilkS))
  (gr_text V2 (at 72.009 94.996 270) (layer F.SilkS))
  (gr_text V1 (at 69.85 94.996 270) (layer F.SilkS))
  (gr_text "UCLA Biomechatronics\n07/01/2019\nv15.0.1" (at 61.595 98.425 180) (layer F.SilkS))
  (gr_line (start 25.4 109.22) (end 165.1 109.22) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 25.4 19.05) (end 25.4 109.22) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 165.1 19.05) (end 165.1 109.22) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 25.4 19.05) (end 165.1 19.05) (layer Edge.Cuts) (width 0.05))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer) (radius 0.635))
    (polygon
      (pts
        (xy 165.1 19.05) (xy 25.4 19.05) (xy 25.4 109.22) (xy 165.1 109.22)
      )
    )
  )
  (zone (net 2) (net_name V_PWR) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer) (radius 0.635))
    (polygon
      (pts
        (xy 25.4 19.05) (xy 165.1 19.05) (xy 165.1 109.22) (xy 25.4 109.22)
      )
    )
  )
)
