(kicad_pcb (version 4) (host pcbnew 4.0.4+e1-6308~48~ubuntu14.04.1-stable)
  (general
    (links 63)
    (no_connects 0)
    (area 134.924999 55.924999 199.075001 139.075001)
    (thickness 1.6)
    (drawings 94)
    (tracks 144)
    (zones 0)
    (modules 39)
    (nets 51)
  )
  (page A4)
  (layers
    (0 F.Cu mixed)
    (31 B.Cu power)
    (33 F.Adhes user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (47 F.CrtYd user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.7)
    (trace_clearance 0.3)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3.2 3.2)
    (pad_drill 3.2)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 135 139)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +12V)
  (net 2 GND)
  (net 3 +5V)
  (net 4 "Net-(C3-Pad1)")
  (net 5 "Net-(C3-Pad2)")
  (net 6 "Net-(P1-Pad2)")
  (net 7 "Net-(P2-Pad2)")
  (net 8 "Net-(P3-Pad2)")
  (net 9 "Net-(Q1-Pad2)")
  (net 10 "Net-(R1-Pad1)")
  (net 11 "Net-(R1-Pad2)")
  (net 12 "Net-(R14-Pad2)")
  (net 13 "Net-(R4-Pad2)")
  (net 14 "Net-(R6-Pad1)")
  (net 15 "Net-(R7-Pad1)")
  (net 16 "Net-(R10-Pad2)")
  (net 17 "Net-(R12-Pad2)")
  (net 18 "Net-(P4-Pad2)")
  (net 19 "Net-(C2-Pad1)")
  (net 20 "Net-(P8-Pad2)")
  (net 21 "Net-(U1-PadSCK)")
  (net 22 "Net-(U1-PadMI)")
  (net 23 "Net-(U1-PadRST)")
  (net 24 "Net-(U1-PadA3)")
  (net 25 "Net-(U1-PadAREF)")
  (net 26 "Net-(U1-Pad3.3V)")
  (net 27 "Net-(U1-Pad13)")
  (net 28 "Net-(U1-PadMO)")
  (net 29 "Net-(U1-PadSS)")
  (net 30 "Net-(U1-PadTX)")
  (net 31 "Net-(U1-PadRX)")
  (net 32 "Net-(U1-Pad2)")
  (net 33 "Net-(U1-PadNC1)")
  (net 34 "Net-(U1-PadNC2)")
  (net 35 "Net-(U1-PadRST2)")
  (net 36 "Net-(U1-PadGND2)")
  (net 37 "Net-(R2-Pad2)")
  (net 38 "Net-(P11-Pad1)")
  (net 39 "Net-(P12-Pad1)")
  (net 40 "Net-(P11-Pad2)")
  (net 41 "Net-(P11-Pad3)")
  (net 42 "Net-(P11-Pad4)")
  (net 43 "Net-(P11-Pad5)")
  (net 44 "Net-(DCDC1-Pad4)")
  (net 45 "Net-(DCDC1-Pad7)")
  (net 46 "Net-(DCDC1-Pad5)")
  (net 47 "Net-(F1-Pad1)")
  (net 48 "Net-(U1-PadA2)")
  (net 49 "Net-(U1-PadA1)")
  (net 50 "Net-(R11-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.3)
    (trace_width 0.7)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(DCDC1-Pad4)")
    (add_net "Net-(DCDC1-Pad5)")
    (add_net "Net-(DCDC1-Pad7)")
    (add_net "Net-(F1-Pad1)")
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(P11-Pad1)")
    (add_net "Net-(P11-Pad2)")
    (add_net "Net-(P11-Pad3)")
    (add_net "Net-(P11-Pad4)")
    (add_net "Net-(P11-Pad5)")
    (add_net "Net-(P12-Pad1)")
    (add_net "Net-(P2-Pad2)")
    (add_net "Net-(P3-Pad2)")
    (add_net "Net-(P4-Pad2)")
    (add_net "Net-(P8-Pad2)")
    (add_net "Net-(Q1-Pad2)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R10-Pad2)")
    (add_net "Net-(R11-Pad1)")
    (add_net "Net-(R12-Pad2)")
    (add_net "Net-(R14-Pad2)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(R4-Pad2)")
    (add_net "Net-(R6-Pad1)")
    (add_net "Net-(R7-Pad1)")
    (add_net "Net-(U1-Pad13)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad3.3V)")
    (add_net "Net-(U1-PadA1)")
    (add_net "Net-(U1-PadA2)")
    (add_net "Net-(U1-PadA3)")
    (add_net "Net-(U1-PadAREF)")
    (add_net "Net-(U1-PadGND2)")
    (add_net "Net-(U1-PadMI)")
    (add_net "Net-(U1-PadMO)")
    (add_net "Net-(U1-PadNC1)")
    (add_net "Net-(U1-PadNC2)")
    (add_net "Net-(U1-PadRST)")
    (add_net "Net-(U1-PadRST2)")
    (add_net "Net-(U1-PadRX)")
    (add_net "Net-(U1-PadSCK)")
    (add_net "Net-(U1-PadSS)")
    (add_net "Net-(U1-PadTX)")
  )
  (net_class 12V ""
    (clearance 0.3)
    (trace_width 0.8)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
  )
  (net_class 5V ""
    (clearance 0.3)
    (trace_width 0.9)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
  )
  (module Capacitors_ThroughHole:C_Disc_D7.5_P5 (layer F.Cu) (tedit 5841F53B)
    (at 195.24 70.13 270)
    (descr "Capacitor 7.5mm Disc, Pitch 5mm")
    (tags Capacitor)
    (fp_text reference C3 (at -2.63 -0.26 360) (layer F.SilkS))
    (fp_text value 100n (at -3.63 -2.26 450) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 "Net-(C3-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D7.5_P5.wrl
      (at (xyz 0.0984252 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module myfootprints:DG306-5.0-02 (layer F.Cu) (tedit 5841CAD5)
    (at 184 131)
    (fp_text reference P7 (at -6.75 4 90) (layer F.SilkS))
    (fp_text value PUSHBUT (at -3 11.5) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 2 thru_hole circle (at -5 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 19 "Net-(C2-Pad1)"))
  )
  (module myfootprints:DG306-5.0-02 (layer F.Cu) (tedit 5841CEEF)
    (at 142 76 270)
    (fp_text reference P6 (at -8.5 1 360) (layer F.SilkS))
    (fp_text value POWER_IN (at -1.5 -5.5 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -5 0 270) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 +12V))
  )
  (module myfootprints:DG306-5.0-02 (layer F.Cu) (tedit 5841CEF5)
    (at 150 63 180)
    (fp_text reference P5 (at 3.5 -1.5 180) (layer F.SilkS))
    (fp_text value "REM 12V OUT" (at -3 9.5 180) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 45 "Net-(DCDC1-Pad7)"))
    (pad 2 thru_hole circle (at -5 0 180) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 47 "Net-(F1-Pad1)"))
  )
  (module myfootprints:DG306-5.0-02 (layer F.Cu) (tedit 5841CBD5)
    (at 182 63 180)
    (fp_text reference P4 (at 4 -0.5 180) (layer F.SilkS))
    (fp_text value "REM 12V IN" (at -3 9 180) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at -5 0 180) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 18 "Net-(P4-Pad2)"))
  )
  (module myfootprints:DG306-5.0-02 (layer F.Cu) (tedit 5841CADF)
    (at 159 131)
    (fp_text reference P2 (at -7 4 90) (layer F.SilkS))
    (fp_text value SSR_R (at -3 11.5) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -5 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 7 "Net-(P2-Pad2)"))
  )
  (module myfootprints:DG306-5.0-02 (layer F.Cu) (tedit 5841CAE4)
    (at 149 131)
    (fp_text reference P1 (at -7 4 90) (layer F.SilkS))
    (fp_text value SSR_L (at -2.5 11) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -5 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 6 "Net-(P1-Pad2)"))
  )
  (module myfootprints:DG306-5.0-03 (layer F.Cu) (tedit 5841CADA)
    (at 174 131)
    (fp_text reference P3 (at -12 4 90) (layer F.SilkS))
    (fp_text value "To WS1812" (at -4.5 11.5) (layer F.Fab) hide)
    (pad 3 thru_hole circle (at -10 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 1 thru_hole rect (at 0 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -5 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 8 "Net-(P3-Pad2)"))
  )
  (module Capacitors_ThroughHole:C_Radial_D12.5_L25_P5 (layer F.Cu) (tedit 5841CF56)
    (at 144.5 86.5 180)
    (descr "Radial Electrolytic Capacitor Diameter 12.5mm x Length 25mm, Pitch 5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C1 (at -3.22 -5.14 180) (layer F.SilkS))
    (fp_text value 220µF/16V (at 2.5 -7.5 180) (layer F.SilkS))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.7 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 +12V))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D12.5_L25_P5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Radial_D12.5_L25_P5 (layer F.Cu) (tedit 5841CF50)
    (at 144.5 105 180)
    (descr "Radial Electrolytic Capacitor Diameter 12.5mm x Length 25mm, Pitch 5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C4 (at -3 6 180) (layer F.SilkS))
    (fp_text value 220µF/16V (at 2.5 8 180) (layer F.SilkS))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.7 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 +5V))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D12.5_L25_P5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D7.5_P5 (layer F.Cu) (tedit 5841CE16)
    (at 165 119 270)
    (descr "Capacitor 7.5mm Disc, Pitch 5mm")
    (tags Capacitor)
    (fp_text reference C2 (at -3 0 270) (layer F.SilkS))
    (fp_text value 100n (at -4 -1.5 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 19 "Net-(C2-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 +5V))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D7.5_P5.wrl
      (at (xyz 0.0984252 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fuse_Holders_and_Fuses:Fuse_TE5_Littlefuse-395Series (layer F.Cu) (tedit 5841E3AE)
    (at 153 69.5)
    (descr "Fuse, TE5, Littlefuse/Wickmann, No. 460, No560,")
    (tags "Fuse, TE5, Littlefuse/Wickmann, No. 460, No560,")
    (fp_text reference F1 (at 0 0) (layer F.SilkS))
    (fp_text value 0.1A (at -5 -0.5 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0) (size 1.50114 1.50114) (drill 1.00076) (layers *.Cu *.Mask)
      (net 47 "Net-(F1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0.01016) (size 1.50114 1.50114) (drill 1.00076) (layers *.Cu *.Mask)
      (net 46 "Net-(DCDC1-Pad5)"))
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 5841CEA1)
    (at 181.61 114.3 270)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R3 (at 5.2 0.11 270) (layer F.SilkS))
    (fp_text value 4k7 (at -3.3 -0.39 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 12 "Net-(R14-Pad2)"))
    (pad 2 thru_hole circle (at 10.16 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 3 +5V))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 5841CC88)
    (at 154 73 270)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R4 (at 5 0 270) (layer F.SilkS))
    (fp_text value 470 (at 5.5 2.5 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 9 "Net-(Q1-Pad2)"))
    (pad 2 thru_hole circle (at 10.16 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 13 "Net-(R4-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 5841CE6B)
    (at 191 70 180)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R5 (at 5 0 180) (layer F.SilkS))
    (fp_text value 680 (at -0.5 2.5 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 18 "Net-(P4-Pad2)"))
    (pad 2 thru_hole circle (at 10.16 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 5 "Net-(C3-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 5841CCCF)
    (at 170.18 114.3 270)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R6 (at 5.2 -0.32 270) (layer F.SilkS))
    (fp_text value 330 (at -3.3 0.18 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 14 "Net-(R6-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 8 "Net-(P3-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 5841CCAD)
    (at 148.59 114.3 270)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R7 (at 5.2 0.09 270) (layer F.SilkS))
    (fp_text value 330 (at -3.3 0.59 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 15 "Net-(R7-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 6 "Net-(P1-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 5841CCB5)
    (at 156.21 114.3 270)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R8 (at 5.2 -0.29 270) (layer F.SilkS))
    (fp_text value 330 (at -3.3 0.21 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 16 "Net-(R10-Pad2)"))
    (pad 2 thru_hole circle (at 10.16 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 7 "Net-(P2-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 5841CCB1)
    (at 152.4 114.3 270)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R9 (at 5.2 -0.1 270) (layer F.SilkS))
    (fp_text value 10k (at -3.3 0.4 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 15 "Net-(R7-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 2 GND))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 5841CCBA)
    (at 160.02 124.46 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R10 (at 4.96 -0.02 90) (layer F.SilkS))
    (fp_text value 10k (at 13.46 -0.02 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 16 "Net-(R10-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 5841E585)
    (at 179 83.7 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R11 (at 5 0 90) (layer F.SilkS))
    (fp_text value 47k (at 4 2.3 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 50 "Net-(R11-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 2 GND))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 5841CCD4)
    (at 173.99 124.46 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R12 (at 5.08 0 90) (layer F.SilkS))
    (fp_text value 330 (at 13.46 0.01 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 19 "Net-(C2-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 17 "Net-(R12-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 5841CCDA)
    (at 177.8 114.3 270)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R13 (at 5.08 0 270) (layer F.SilkS))
    (fp_text value 10k (at -3.3 -0.2 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 17 "Net-(R12-Pad2)"))
    (pad 2 thru_hole circle (at 10.16 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 2 GND))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 5841CCE5)
    (at 185.42 124.46 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R14 (at 5.08 0 90) (layer F.SilkS))
    (fp_text value 330 (at 13.46 -0.42 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 20 "Net-(P8-Pad2)"))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 12 "Net-(R14-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x05 (layer F.Cu) (tedit 5841CCF3)
    (at 193.675 107.315 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P11 (at -0.815 -2.825 270) (layer F.SilkS))
    (fp_text value D8-D12 (at -2.315 4.675 360) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 38 "Net-(P11-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 40 "Net-(P11-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 41 "Net-(P11-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 42 "Net-(P11-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 43 "Net-(P11-Pad5)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x05.wrl
      (at (xyz 0 -0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 5841B328)
    (at 192.5 83.5)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P12 (at -3.81 2.54) (layer F.SilkS) hide)
    (fp_text value A0 (at 2.5 -1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask)
      (net 39 "Net-(P12-Pad1)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module myfootprints:ARDUINO_MICRO_SHIELD (layer F.Cu) (tedit 583CBFCA)
    (at 149.5 104.25)
    (tags "ARDUINO, MICRO")
    (fp_text reference U1 (at 26.67 -10.16) (layer F.SilkS))
    (fp_text value "Arduino Micro" (at 26.67 -7.62) (layer F.SilkS))
    (pad SCK thru_hole circle (at 3.5 -16.746) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(U1-PadSCK)"))
    (pad MI thru_hole circle (at 6.04 -16.746) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(U1-PadMI)"))
    (pad VI thru_hole circle (at 8.58 -16.746) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 +12V))
    (pad GND thru_hole circle (at 11.12 -16.746) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad RST thru_hole circle (at 13.66 -16.746) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(U1-PadRST)"))
    (pad 5V thru_hole circle (at 16.2 -16.746) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 3 +5V))
    (pad NC1 thru_hole circle (at 18.74 -16.746) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 33 "Net-(U1-PadNC1)"))
    (pad NC2 thru_hole circle (at 21.28 -16.746) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 34 "Net-(U1-PadNC2)"))
    (pad A5 thru_hole circle (at 23.82 -16.746) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(R1-Pad2)"))
    (pad A4 thru_hole circle (at 26.36 -16.746) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 50 "Net-(R11-Pad1)"))
    (pad A3 thru_hole circle (at 28.9 -16.746) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(U1-PadA3)"))
    (pad A2 thru_hole circle (at 31.44 -16.746) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 48 "Net-(U1-PadA2)"))
    (pad A1 thru_hole circle (at 33.98 -16.746) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 49 "Net-(U1-PadA1)"))
    (pad A0 thru_hole circle (at 36.52 -16.746) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 39 "Net-(P12-Pad1)"))
    (pad AREF thru_hole circle (at 39.06 -16.746) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(U1-PadAREF)"))
    (pad 3.3V thru_hole circle (at 41.6 -16.746) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(U1-Pad3.3V)"))
    (pad 13 thru_hole circle (at 44.14 -16.746) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(U1-Pad13)"))
    (pad MO thru_hole rect (at 3.5 -1.254) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(U1-PadMO)"))
    (pad SS thru_hole circle (at 6.04 -1.254) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(U1-PadSS)"))
    (pad TX thru_hole circle (at 8.58 -1.254) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(U1-PadTX)"))
    (pad RX thru_hole circle (at 11.12 -1.254) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 31 "Net-(U1-PadRX)"))
    (pad RST2 thru_hole circle (at 13.66 -1.254) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 35 "Net-(U1-PadRST2)"))
    (pad GND2 thru_hole circle (at 16.2 -1.254) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 36 "Net-(U1-PadGND2)"))
    (pad 2 thru_hole circle (at 18.74 -1.254) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 32 "Net-(U1-Pad2)"))
    (pad 3 thru_hole circle (at 21.28 -1.254) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(R7-Pad1)"))
    (pad 4 thru_hole circle (at 23.82 -1.254) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(R10-Pad2)"))
    (pad 5 thru_hole circle (at 26.36 -1.254) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(R6-Pad1)"))
    (pad 6 thru_hole circle (at 28.9 -1.254) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(R12-Pad2)"))
    (pad 7 thru_hole circle (at 31.44 -1.254) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(R14-Pad2)"))
    (pad 8 thru_hole circle (at 33.98 -1.254) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 43 "Net-(P11-Pad5)"))
    (pad 9 thru_hole circle (at 36.52 -1.254) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 42 "Net-(P11-Pad4)"))
    (pad 10 thru_hole circle (at 39.06 -1.254) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 41 "Net-(P11-Pad3)"))
    (pad 11 thru_hole circle (at 41.6 -1.254) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 40 "Net-(P11-Pad2)"))
    (pad 12 thru_hole circle (at 44.14 -1.254) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 38 "Net-(P11-Pad1)"))
  )
  (module myfootprints:RECOM_RN_1212SP (layer F.Cu) (tedit 5841CC64)
    (at 158.5 71)
    (fp_text reference DCDC1 (at 6.3 -5.05) (layer F.SilkS))
    (fp_text value RECOM_RN1212SP (at 7 -11) (layer F.SilkS))
    (pad 1 thru_hole circle (at 2.49 -1.24) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole circle (at 10.11 -1.24) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 44 "Net-(DCDC1-Pad4)"))
    (pad 7 thru_hole circle (at 5.03 -8.86) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 45 "Net-(DCDC1-Pad7)"))
    (pad 5 thru_hole circle (at 10.11 -8.86) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 46 "Net-(DCDC1-Pad5)"))
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 5841CE84)
    (at 175.5 73.5 270)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R15 (at 5 0 270) (layer F.SilkS))
    (fp_text value 10k (at -3.5 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 10.16 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 11 "Net-(R1-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-4_W7.62mm_LongPads (layer F.Cu) (tedit 5841FF1D)
    (at 165 83 180)
    (descr "4-lead dip package, row spacing 7.62 mm (300 mils), longer pads")
    (tags "dil dip 2.54 300")
    (fp_text reference U4 (at -1 4.5 180) (layer F.SilkS))
    (fp_text value SPF620A (at 11 -2.5 180) (layer F.SilkS))
    (pad 1 thru_hole oval (at 0 0 180) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(R1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 7.62 2.54 180) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(R4-Pad2)"))
    (pad 4 thru_hole oval (at 7.62 0 180) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +12V))
    (model Housings_DIP.3dshapes/DIP-4_W7.62mm_LongPads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-4_W7.62mm_LongPads (layer F.Cu) (tedit 5841F549)
    (at 188 74 270)
    (descr "4-lead dip package, row spacing 7.62 mm (300 mils), longer pads")
    (tags "dil dip 2.54 300")
    (fp_text reference U5 (at 2 6 270) (layer F.SilkS))
    (fp_text value SPF620A (at 10 1 360) (layer F.SilkS))
    (pad 1 thru_hole oval (at 0 0 270) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C3-Pad2)"))
    (pad 3 thru_hole oval (at 7.62 2.54 270) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 "Net-(R11-Pad1)"))
    (pad 4 thru_hole oval (at 7.62 0 270) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 "Net-(R2-Pad2)"))
    (model Housings_DIP.3dshapes/DIP-4_W7.62mm_LongPads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 5841CE8D)
    (at 168.5 83.6 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R2 (at 5.1 0 90) (layer F.SilkS))
    (fp_text value 4k7 (at 8.1 -2 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 3 +5V))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 37 "Net-(R2-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 5841CE89)
    (at 172 73.5 270)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R1 (at 5 0 270) (layer F.SilkS))
    (fp_text value 470 (at -3.5 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 10 "Net-(R1-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 11 "Net-(R1-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module myfootprints:DG306-5.0-03 (layer F.Cu) (tedit 5841CF7D)
    (at 192 112 90)
    (fp_text reference P8 (at -14 -3 180) (layer F.SilkS))
    (fp_text value DS18B20x2 (at -3.75 6.75 90) (layer F.Fab) hide)
    (pad 3 thru_hole circle (at -10 0 90) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -5 0 90) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 20 "Net-(P8-Pad2)"))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5841CBD1)
    (at 194 62)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5841CBCC)
    (at 142 62)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5841CABD)
    (at 194 133)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5841CAB7)
    (at 142 120)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module TO_SOT_Packages_THT:TO-92_Inline_Wide (layer F.Cu) (tedit 5841FFE3)
    (at 164.25 75.25 180)
    (descr "TO-92 leads in-line, wide, drill 0.8mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q1 (at -0.5 -1.75 180) (layer F.SilkS))
    (fp_text value PN2222A (at 7 0.5 270) (layer F.SilkS))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(Q1-Pad2)"))
    (pad 3 thru_hole circle (at 5.08 0 270) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 "Net-(DCDC1-Pad4)"))
    (model TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Wide.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (dimension 83 (width 0.3) (layer Eco1.User)
    (gr_text "83,000 mm" (at 117.15 97.5 270) (layer Eco1.User))
    (feature1 (pts (xy 140 139) (xy 115.8 139)))
    (feature2 (pts (xy 140 56) (xy 115.8 56)))
    (crossbar (pts (xy 118.5 56) (xy 118.5 139)))
    (arrow1a (pts (xy 118.5 139) (xy 117.913579 137.873496)))
    (arrow1b (pts (xy 118.5 139) (xy 119.086421 137.873496)))
    (arrow2a (pts (xy 118.5 56) (xy 117.913579 57.126504)))
    (arrow2b (pts (xy 118.5 56) (xy 119.086421 57.126504)))
  )
  (dimension 64 (width 0.3) (layer Eco1.User)
    (gr_text "64,000 mm" (at 167 46.65) (layer Eco1.User))
    (feature1 (pts (xy 199 56.5) (xy 199 45.3)))
    (feature2 (pts (xy 135 56.5) (xy 135 45.3)))
    (crossbar (pts (xy 135 48) (xy 199 48)))
    (arrow1a (pts (xy 199 48) (xy 197.873496 48.586421)))
    (arrow1b (pts (xy 199 48) (xy 197.873496 47.413579)))
    (arrow2a (pts (xy 135 48) (xy 136.126504 48.586421)))
    (arrow2b (pts (xy 135 48) (xy 136.126504 47.413579)))
  )
  (dimension 52 (width 0.3) (layer Eco1.User)
    (gr_text "52,000 mm" (at 168 152.85) (layer Eco1.User))
    (feature1 (pts (xy 142 133) (xy 142 154.2)))
    (feature2 (pts (xy 194 133) (xy 194 154.2)))
    (crossbar (pts (xy 194 151.5) (xy 142 151.5)))
    (arrow1a (pts (xy 142 151.5) (xy 143.126504 150.913579)))
    (arrow1b (pts (xy 142 151.5) (xy 143.126504 152.086421)))
    (arrow2a (pts (xy 194 151.5) (xy 192.873496 150.913579)))
    (arrow2b (pts (xy 194 151.5) (xy 192.873496 152.086421)))
  )
  (dimension 52 (width 0.3) (layer Eco1.User)
    (gr_text "52,000 mm" (at 168 49.65) (layer Eco1.User))
    (feature1 (pts (xy 194 62) (xy 194 48.3)))
    (feature2 (pts (xy 142 62) (xy 142 48.3)))
    (crossbar (pts (xy 142 51) (xy 194 51)))
    (arrow1a (pts (xy 194 51) (xy 192.873496 51.586421)))
    (arrow1b (pts (xy 194 51) (xy 192.873496 50.413579)))
    (arrow2a (pts (xy 142 51) (xy 143.126504 51.586421)))
    (arrow2b (pts (xy 142 51) (xy 143.126504 50.413579)))
  )
  (dimension 71 (width 0.3) (layer Eco1.User)
    (gr_text "71,000 mm" (at 207.35 97.5 270) (layer Eco1.User))
    (feature1 (pts (xy 194 133) (xy 208.7 133)))
    (feature2 (pts (xy 194 62) (xy 208.7 62)))
    (crossbar (pts (xy 206 62) (xy 206 133)))
    (arrow1a (pts (xy 206 133) (xy 205.413579 131.873496)))
    (arrow1b (pts (xy 206 133) (xy 206.586421 131.873496)))
    (arrow2a (pts (xy 206 62) (xy 205.413579 63.126504)))
    (arrow2b (pts (xy 206 62) (xy 206.586421 63.126504)))
  )
  (dimension 58 (width 0.3) (layer Eco1.User)
    (gr_text "58,000 mm" (at 123.15 91 270) (layer Eco1.User))
    (feature1 (pts (xy 142 120) (xy 121.8 120)))
    (feature2 (pts (xy 142 62) (xy 121.8 62)))
    (crossbar (pts (xy 124.5 62) (xy 124.5 120)))
    (arrow1a (pts (xy 124.5 120) (xy 123.913579 118.873496)))
    (arrow1b (pts (xy 124.5 120) (xy 125.086421 118.873496)))
    (arrow2a (pts (xy 124.5 62) (xy 123.913579 63.126504)))
    (arrow2b (pts (xy 124.5 62) (xy 125.086421 63.126504)))
  )
  (gr_text 7 (at 162 64) (layer F.SilkS))
  (gr_text 5 (at 170 64) (layer F.SilkS))
  (gr_text 4 (at 167 69.5) (layer F.SilkS))
  (gr_text 1 (at 163 69.5) (layer F.SilkS))
  (gr_text E (at 164.5 73.25) (layer F.SilkS))
  (gr_text C (at 159 73.25) (layer F.SilkS))
  (gr_text B (at 161.75 72.75) (layer F.SilkS))
  (gr_text 4 (at 188 79) (layer F.SilkS))
  (gr_text 3 (at 185.5 79) (layer F.SilkS))
  (gr_text 2 (at 185.5 76.5) (layer F.SilkS))
  (gr_text 1 (at 188 76.5) (layer F.SilkS))
  (gr_text 4 (at 160 83) (layer F.SilkS))
  (gr_text 3 (at 160 80.5) (layer F.SilkS))
  (gr_text 2 (at 162.5 80.5) (layer F.SilkS))
  (gr_text 1 (at 162.5 83) (layer F.SilkS))
  (gr_text "FirstOne Amplifier Control v0.3\nDesigned by Laurent Monin (zas)\nDecember 2016" (at 175 95) (layer B.SilkS))
  (gr_text "Max. 12V 100mA" (at 167 58 180) (layer F.SilkS))
  (gr_text + (at 144.5 83.5) (layer F.SilkS))
  (gr_text A0 (at 192.5 80.5) (layer F.SilkS))
  (gr_line (start 135 139) (end 135 56) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 199 139) (end 135 139) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 199 56) (end 199 139) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 135 56) (end 199 56) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text + (at 144.5 102) (layer F.SilkS))
  (gr_text "REM 12V IN A4" (at 184.5 57.5 180) (layer F.SilkS))
  (gr_text "POWER IN" (at 136.5 73 270) (layer F.SilkS))
  (gr_text "REM 12V OUT A5" (at 153 57.5 180) (layer F.SilkS))
  (gr_text "_ -- _" (at 182 135) (layer F.SilkS))
  (gr_text DQ (at 196.25 117 90) (layer F.SilkS))
  (gr_text GND (at 196.25 111.75 90) (layer F.SilkS))
  (gr_text GND (at 174 135) (layer F.SilkS))
  (gr_text DI (at 169 135) (layer F.SilkS))
  (gr_text +5V (at 196.5 122 90) (layer F.SilkS))
  (gr_text +5V (at 164 135) (layer F.SilkS))
  (gr_text - (at 159 135) (layer F.SilkS))
  (gr_text - (at 149 135) (layer F.SilkS))
  (gr_text + (at 154 135) (layer F.SilkS))
  (gr_text + (at 144 135) (layer F.SilkS))
  (gr_text "D7 Temp.\nSensors" (at 194.5 127) (layer F.SilkS))
  (gr_text "PushBut D6" (at 182 137) (layer F.SilkS))
  (gr_text "Front LED D5" (at 169.5 137) (layer F.SilkS))
  (gr_text "SSR_R D4" (at 157 137) (layer F.SilkS))
  (gr_text "SSR_L D3" (at 147 137) (layer F.SilkS))
  (gr_text GND (at 138 76 270) (layer F.SilkS))
  (gr_text 12V/1A (at 138 71 270) (layer F.SilkS))
  (gr_text + (at 187 59) (layer F.SilkS))
  (gr_text - (at 182 59) (layer F.SilkS))
  (gr_text - (at 150 59) (layer F.SilkS))
  (gr_text + (at 155 59) (layer F.SilkS))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 198 137) (xy 136 137) (xy 136 68) (xy 147 68) (xy 147 71)
        (xy 159 71) (xy 159 68) (xy 175 68) (xy 179 72) (xy 181.5 72)
        (xy 186 77) (xy 198 77)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 146 124) (xy 138 124) (xy 138 116) (xy 146 116)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 198.5 138) (xy 189.5 138) (xy 189.5 128.5) (xy 198.5 128.5)
      )
    )
  )
)
