(kicad_pcb (version 4) (host pcbnew 4.0.6-e0-6349~53~ubuntu16.04.1)
  (general
    (links 247)
    (no_connects 0)
    (area 53.505713 27 220.814287 140.000001)
    (thickness 1.6)
    (drawings 33)
    (tracks 565)
    (zones 0)
    (modules 21)
    (nets 107)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal hide)
    (32 B.Adhes user hide)
    (33 F.Adhes user)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user hide)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.35)
    (user_trace_width 0.28)
    (user_trace_width 0.35)
    (user_trace_width 0.6)
    (user_trace_width 1)
    (user_trace_width 1.2)
    (user_trace_width 1.8)
    (user_trace_width 3)
    (user_trace_width 5)
    (trace_clearance 0.28)
    (zone_clearance 0.5)
    (zone_45_only no)
    (trace_min 0.28)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 1.2)
    (via_drill 0.6)
    (via_min_size 1.2)
    (via_min_drill 0.6)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.35 0.3)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 AGND)
  (net 2 VDD_5V)
  (net 3 LCD_SCL)
  (net 4 LCD_SDA)
  (net 5 VDD_3V3)
  (net 6 fw_sigout)
  (net 7 track_pulse_a)
  (net 8 track_pulse_b)
  (net 9 SERVO_PWM)
  (net 10 fw_jp3_p1)
  (net 11 fw_jp3_p2)
  (net 12 fw_jp3_p5)
  (net 13 fw_jp3_p6)
  (net 14 fw_jp3_p7)
  (net 15 fw_jp3_p8)
  (net 16 fw_jp3_p10)
  (net 17 fw_jp1_1)
  (net 18 fw_jp1_2)
  (net 19 fw_jp1_3)
  (net 20 fw_jp1_4)
  (net 21 fw_jp1_5)
  (net 22 fw_jp1_6)
  (net 23 fw_jp1_8)
  (net 24 fw_jp1_9)
  (net 25 fw_jp1_10)
  (net 26 fw_jp1_11)
  (net 27 fw_jp1_12)
  (net 28 fw_jp1_14)
  (net 29 fw_jp1_15)
  (net 30 fw_jp1_16)
  (net 31 pt_jp4_p1)
  (net 32 pt_jp4_p2)
  (net 33 pt_jp4_p3)
  (net 34 pt_jp4_p4)
  (net 35 pt_jp4_p5)
  (net 36 pt_jp4_p6)
  (net 37 pt_jp4_p7)
  (net 38 pt_jp4_p10)
  (net 39 pt_jp4_p11)
  (net 40 pt_jp4_p12)
  (net 41 pt_jp1_p1)
  (net 42 pt_jp1_p2)
  (net 43 pt_jp1_p3)
  (net 44 pt_jp1_p4)
  (net 45 pt_jp1_p5)
  (net 46 pt_jp1_p6)
  (net 47 pt_jp1_p7)
  (net 48 pt_jp1_p8)
  (net 49 pt_jp1_p9)
  (net 50 pt_jp1_p10)
  (net 51 j12_1)
  (net 52 j12_3)
  (net 53 j12_5)
  (net 54 j12_7)
  (net 55 j12_9)
  (net 56 j12_11)
  (net 57 j12_13)
  (net 58 j12_15)
  (net 59 j12_17)
  (net 60 j12_19)
  (net 61 j10_3)
  (net 62 j10_2)
  (net 63 j10_4)
  (net 64 j10_6)
  (net 65 j10_7)
  (net 66 j10_8)
  (net 67 j10_9)
  (net 68 j10_10)
  (net 69 j10_11)
  (net 70 j10_12)
  (net 71 j10_13)
  (net 72 j10_14)
  (net 73 j10_15)
  (net 74 j10_16)
  (net 75 j10_17)
  (net 76 j10_18)
  (net 77 j10_19)
  (net 78 j10_20)
  (net 79 j10_21)
  (net 80 j10_22)
  (net 81 j10_23)
  (net 82 j10_24)
  (net 83 j10_25)
  (net 84 j10_26)
  (net 85 j10_27)
  (net 86 j10_28)
  (net 87 j10_30)
  (net 88 j10_34)
  (net 89 j10_35)
  (net 90 j10_36)
  (net 91 j10_37)
  (net 92 j10_38)
  (net 93 j10_39)
  (net 94 j10_40)
  (net 95 U2_4)
  (net 96 U2_5)
  (net 97 U2_6)
  (net 98 U2_7)
  (net 99 U2_8)
  (net 100 U2_11)
  (net 101 RPiN)
  (net 102 U2_13)
  (net 103 U2_15)
  (net 104 Pon3)
  (net 105 Pof3)
  (net 106 U2_18)
  (net_class Default "This is the default net class."
    (clearance 0.28)
    (trace_width 0.35)
    (via_dia 1.2)
    (via_drill 0.6)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net AGND)
    (add_net LCD_SCL)
    (add_net LCD_SDA)
    (add_net Pof3)
    (add_net Pon3)
    (add_net RPiN)
    (add_net SERVO_PWM)
    (add_net U2_11)
    (add_net U2_13)
    (add_net U2_15)
    (add_net U2_18)
    (add_net U2_4)
    (add_net U2_5)
    (add_net U2_6)
    (add_net U2_7)
    (add_net U2_8)
    (add_net VDD_3V3)
    (add_net VDD_5V)
    (add_net fw_jp1_1)
    (add_net fw_jp1_10)
    (add_net fw_jp1_11)
    (add_net fw_jp1_12)
    (add_net fw_jp1_14)
    (add_net fw_jp1_15)
    (add_net fw_jp1_16)
    (add_net fw_jp1_2)
    (add_net fw_jp1_3)
    (add_net fw_jp1_4)
    (add_net fw_jp1_5)
    (add_net fw_jp1_6)
    (add_net fw_jp1_8)
    (add_net fw_jp1_9)
    (add_net fw_jp3_p1)
    (add_net fw_jp3_p10)
    (add_net fw_jp3_p2)
    (add_net fw_jp3_p5)
    (add_net fw_jp3_p6)
    (add_net fw_jp3_p7)
    (add_net fw_jp3_p8)
    (add_net fw_sigout)
    (add_net j10_10)
    (add_net j10_11)
    (add_net j10_12)
    (add_net j10_13)
    (add_net j10_14)
    (add_net j10_15)
    (add_net j10_16)
    (add_net j10_17)
    (add_net j10_18)
    (add_net j10_19)
    (add_net j10_2)
    (add_net j10_20)
    (add_net j10_21)
    (add_net j10_22)
    (add_net j10_23)
    (add_net j10_24)
    (add_net j10_25)
    (add_net j10_26)
    (add_net j10_27)
    (add_net j10_28)
    (add_net j10_3)
    (add_net j10_30)
    (add_net j10_34)
    (add_net j10_35)
    (add_net j10_36)
    (add_net j10_37)
    (add_net j10_38)
    (add_net j10_39)
    (add_net j10_4)
    (add_net j10_40)
    (add_net j10_6)
    (add_net j10_7)
    (add_net j10_8)
    (add_net j10_9)
    (add_net j12_1)
    (add_net j12_11)
    (add_net j12_13)
    (add_net j12_15)
    (add_net j12_17)
    (add_net j12_19)
    (add_net j12_3)
    (add_net j12_5)
    (add_net j12_7)
    (add_net j12_9)
    (add_net pt_jp1_p1)
    (add_net pt_jp1_p10)
    (add_net pt_jp1_p2)
    (add_net pt_jp1_p3)
    (add_net pt_jp1_p4)
    (add_net pt_jp1_p5)
    (add_net pt_jp1_p6)
    (add_net pt_jp1_p7)
    (add_net pt_jp1_p8)
    (add_net pt_jp1_p9)
    (add_net pt_jp4_p1)
    (add_net pt_jp4_p10)
    (add_net pt_jp4_p11)
    (add_net pt_jp4_p12)
    (add_net pt_jp4_p2)
    (add_net pt_jp4_p3)
    (add_net pt_jp4_p4)
    (add_net pt_jp4_p5)
    (add_net pt_jp4_p6)
    (add_net pt_jp4_p7)
    (add_net track_pulse_a)
    (add_net track_pulse_b)
  )
  (module Pin_Headers:Pin_Header_Straight_1x01 (layer B.Cu) (tedit 58CA3420)
    (at 77.845 117.848)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference REF** (at 0 5.1) (layer B.SilkS) hide)
    (fp_text value Pin_Header_Straight_1x01 (at 0 3.1) (layer B.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.318 4.318) (drill 3.556) (layers *.Cu *.Mask B.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01 (layer B.Cu) (tedit 58CA3420)
    (at 202.305 44.188)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference REF** (at 0 5.1) (layer B.SilkS) hide)
    (fp_text value Pin_Header_Straight_1x01 (at 0 3.1) (layer B.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.318 4.318) (drill 3.556) (layers *.Cu *.Mask B.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 58CA3420)
    (at 72.765 42.918)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference REF** (at 0 -5.1) (layer F.SilkS) hide)
    (fp_text value Pin_Header_Straight_1x01 (at 0 -3.1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.318 4.318) (drill 3.556) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x19 (layer F.Cu) (tedit 58CEABF8)
    (at 170.18 88.9)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J8 (at -0.18 48.6 180) (layer F.SilkS))
    (fp_text value Pin_Header_Straight_1x19 (at 0 -3.1) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 AGND))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 VDD_5V))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 fw_sigout))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 95 U2_4))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 96 U2_5))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 97 U2_6))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 98 U2_7))
    (pad 8 thru_hole oval (at 0 17.78) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 99 U2_8))
    (pad 9 thru_hole oval (at 0 20.32) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 track_pulse_a))
    (pad 10 thru_hole oval (at 0 22.86) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 track_pulse_b))
    (pad 11 thru_hole oval (at 0 25.4) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 100 U2_11))
    (pad 12 thru_hole oval (at 0 27.94) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 101 RPiN))
    (pad 13 thru_hole oval (at 0 30.48) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 102 U2_13))
    (pad 14 thru_hole oval (at 0 33.02) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 SERVO_PWM))
    (pad 15 thru_hole oval (at 0 35.56) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 103 U2_15))
    (pad 16 thru_hole oval (at 0 38.1) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 104 Pon3))
    (pad 17 thru_hole oval (at 0 40.64) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 105 Pof3))
    (pad 18 thru_hole oval (at 0 43.18) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 106 U2_18))
    (pad 19 thru_hole oval (at 0 45.72) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 VDD_3V3))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x19.wrl
      (at (xyz 0 -0.9 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x19 (layer F.Cu) (tedit 58CA3123)
    (at 180.34 88.9)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference U2 (at -4.705 23.868 90) (layer F.SilkS))
    (fp_text value Pin_Header_Straight_1x19 (at 0 -3.1) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 AGND))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 VDD_5V))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 fw_sigout))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 95 U2_4))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 96 U2_5))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 97 U2_6))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 98 U2_7))
    (pad 8 thru_hole oval (at 0 17.78) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 99 U2_8))
    (pad 9 thru_hole oval (at 0 20.32) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 track_pulse_a))
    (pad 10 thru_hole oval (at 0 22.86) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 track_pulse_b))
    (pad 11 thru_hole oval (at 0 25.4) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 100 U2_11))
    (pad 12 thru_hole oval (at 0 27.94) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 101 RPiN))
    (pad 13 thru_hole oval (at 0 30.48) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 102 U2_13))
    (pad 14 thru_hole oval (at 0 33.02) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 SERVO_PWM))
    (pad 15 thru_hole oval (at 0 35.56) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 103 U2_15))
    (pad 16 thru_hole oval (at 0 38.1) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 104 Pon3))
    (pad 17 thru_hole oval (at 0 40.64) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 105 Pof3))
    (pad 18 thru_hole oval (at 0 43.18) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 106 U2_18))
    (pad 19 thru_hole oval (at 0 45.72) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 VDD_3V3))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x19.wrl
      (at (xyz 0 -0.9 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x19 (layer F.Cu) (tedit 58CA2F60)
    (at 210.82 88.9)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference U2_R (at 0 -5.1) (layer F.SilkS) hide)
    (fp_text value Pin_Header_Straight_1x19 (at 0 -3.1) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 AGND))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 VDD_5V))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 fw_sigout))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 95 U2_4))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 96 U2_5))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 97 U2_6))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 98 U2_7))
    (pad 8 thru_hole oval (at 0 17.78) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 99 U2_8))
    (pad 9 thru_hole oval (at 0 20.32) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 track_pulse_a))
    (pad 10 thru_hole oval (at 0 22.86) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 track_pulse_b))
    (pad 11 thru_hole oval (at 0 25.4) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 100 U2_11))
    (pad 12 thru_hole oval (at 0 27.94) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 101 RPiN))
    (pad 13 thru_hole oval (at 0 30.48) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 102 U2_13))
    (pad 14 thru_hole oval (at 0 33.02) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 SERVO_PWM))
    (pad 15 thru_hole oval (at 0 35.56) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 103 U2_15))
    (pad 16 thru_hole oval (at 0 38.1) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 104 Pon3))
    (pad 17 thru_hole oval (at 0 40.64) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 105 Pof3))
    (pad 18 thru_hole oval (at 0 43.18) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 106 U2_18))
    (pad 19 thru_hole oval (at 0 45.72) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 VDD_3V3))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x19.wrl
      (at (xyz 0 -0.9 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module footprint:TrinketPro locked (layer F.Cu) (tedit 58CA31F7)
    (at 209.925 65.778)
    (fp_text reference U6 (at -7.62 -33.02) (layer F.SilkS))
    (fp_text value ProTrinket (at -7.62 -15.24) (layer F.SilkS))
    (fp_text user JP4 (at -19.05 -30.48) (layer F.SilkS))
    (fp_text user JP1 (at 3.81 -30.48) (layer F.SilkS))
    (fp_text user D13 (at -21.59 -17.78) (layer F.SilkS))
    (fp_text user A5 (at -21.59 0) (layer F.SilkS))
    (fp_text user A4 (at -21.59 -2.54) (layer F.SilkS))
    (fp_text user A3 (at -21.59 -5.08) (layer F.SilkS))
    (fp_text user A2 (at -21.59 -7.62) (layer F.SilkS))
    (fp_text user A1 (at -21.59 -10.16) (layer F.SilkS))
    (fp_text user A0 (at -21.59 -12.7) (layer F.SilkS))
    (fp_text user AREF (at -21.59 -15.24) (layer F.SilkS))
    (fp_text user D12 (at -21.59 -20.32) (layer F.SilkS))
    (fp_text user D11 (at -21.59 -22.86) (layer F.SilkS))
    (fp_text user D10 (at -21.59 -25.4) (layer F.SilkS))
    (fp_text user D9 (at -21.59 -27.94) (layer F.SilkS))
    (fp_text user RST (at 6.35 0) (layer F.SilkS))
    (fp_text user RXD (at 6.35 -2.54) (layer F.SilkS))
    (fp_text user TXD (at 6.35 -5.08) (layer F.SilkS))
    (fp_text user D3 (at 6.35 -7.62) (layer F.SilkS))
    (fp_text user D4 (at 6.35 -10.16) (layer F.SilkS))
    (fp_text user D5 (at 6.35 -12.7) (layer F.SilkS))
    (fp_text user D6 (at 6.35 -15.24) (layer F.SilkS))
    (fp_text user D8 (at 6.35 -17.78) (layer F.SilkS))
    (fp_text user 5V (at 6.35 -20.32) (layer F.SilkS))
    (fp_text user VBUS (at 6.35 -22.86) (layer F.SilkS))
    (fp_text user GND (at 6.35 -25.4) (layer F.SilkS))
    (fp_text user VBAT (at 6.35 -27.94) (layer F.SilkS))
    (pad 12 thru_hole circle (at -17.78 -27.94) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 40 pt_jp4_p12))
    (pad 11 thru_hole circle (at -17.78 -25.4) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 39 pt_jp4_p11))
    (pad 10 thru_hole circle (at -17.78 -22.86) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 38 pt_jp4_p10))
    (pad 9 thru_hole circle (at -17.78 -20.32) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 7 track_pulse_a))
    (pad 8 thru_hole circle (at -17.78 -17.78) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 8 track_pulse_b))
    (pad 7 thru_hole circle (at -17.78 -15.24) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 37 pt_jp4_p7))
    (pad 6 thru_hole circle (at -17.78 -12.7) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 36 pt_jp4_p6))
    (pad 5 thru_hole circle (at -17.78 -10.16) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 35 pt_jp4_p5))
    (pad 4 thru_hole circle (at -17.78 -7.62) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 34 pt_jp4_p4))
    (pad 3 thru_hole circle (at -17.78 -5.08) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 33 pt_jp4_p3))
    (pad 2 thru_hole circle (at -17.78 -2.54) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 32 pt_jp4_p2))
    (pad 1 thru_hole circle (at -17.78 0) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 31 pt_jp4_p1))
    (pad 12 thru_hole circle (at 2.54 -27.94) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 2 VDD_5V))
    (pad 11 thru_hole circle (at 2.54 -25.4) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 1 AGND))
    (pad 10 thru_hole circle (at 2.54 -22.86) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 50 pt_jp1_p10))
    (pad 9 thru_hole circle (at 2.54 -20.32) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 49 pt_jp1_p9))
    (pad 8 thru_hole circle (at 2.54 -17.78) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 48 pt_jp1_p8))
    (pad 7 thru_hole circle (at 2.54 -15.24) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 47 pt_jp1_p7))
    (pad 6 thru_hole circle (at 2.54 -12.7) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 46 pt_jp1_p6))
    (pad 5 thru_hole circle (at 2.54 -10.16) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 45 pt_jp1_p5))
    (pad 4 thru_hole circle (at 2.54 -7.62) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 44 pt_jp1_p4))
    (pad 3 thru_hole circle (at 2.54 -5.08) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 43 pt_jp1_p3))
    (pad 2 thru_hole circle (at 2.54 -2.54) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 42 pt_jp1_p2))
    (pad 1 thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 41 pt_jp1_p1))
    (pad 12 thru_hole circle (at 0 -27.94) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 2 VDD_5V))
    (pad 11 thru_hole circle (at 0 -25.4) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 1 AGND))
    (pad 10 thru_hole circle (at 0 -22.86) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 50 pt_jp1_p10))
    (pad 9 thru_hole circle (at 0 -20.32) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 49 pt_jp1_p9))
    (pad 8 thru_hole circle (at 0 -17.78) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 48 pt_jp1_p8))
    (pad 7 thru_hole circle (at 0 -15.24) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 47 pt_jp1_p7))
    (pad 6 thru_hole circle (at 0 -12.7) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 46 pt_jp1_p6))
    (pad 5 thru_hole circle (at 0 -10.16) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 45 pt_jp1_p5))
    (pad 4 thru_hole circle (at 0 -7.62) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 44 pt_jp1_p4))
    (pad 3 thru_hole circle (at 0 -5.08) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 43 pt_jp1_p3))
    (pad 2 thru_hole circle (at 0 -2.54) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 42 pt_jp1_p2))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 41 pt_jp1_p1))
    (pad 12 thru_hole circle (at -15.24 -27.94) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 40 pt_jp4_p12))
    (pad 11 thru_hole circle (at -15.24 -25.4) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 39 pt_jp4_p11))
    (pad 10 thru_hole circle (at -15.24 -22.86) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 38 pt_jp4_p10))
    (pad 9 thru_hole circle (at -15.24 -20.32) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 7 track_pulse_a))
    (pad 8 thru_hole circle (at -15.24 -17.78) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 8 track_pulse_b))
    (pad 7 thru_hole circle (at -15.24 -15.24) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 37 pt_jp4_p7))
    (pad 6 thru_hole circle (at -15.24 -12.7) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 36 pt_jp4_p6))
    (pad 5 thru_hole circle (at -15.24 -10.16) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 35 pt_jp4_p5))
    (pad 4 thru_hole circle (at -15.24 -7.62) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 34 pt_jp4_p4))
    (pad 3 thru_hole circle (at -15.24 -5.08) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 33 pt_jp4_p3))
    (pad 2 thru_hole circle (at -15.24 -2.54) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 32 pt_jp4_p2))
    (pad 1 thru_hole circle (at -15.24 0) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 31 pt_jp4_p1))
    (pad 1 thru_hole circle (at -13.97 2.54) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 1 AGND))
    (pad 2 thru_hole circle (at -11.43 2.54) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 1 AGND))
    (pad 3 thru_hole circle (at -8.89 2.54) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at -6.35 2.54) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at -3.81 2.54) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at -1.27 2.54) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -14.605 -29.972) (size 2.286 2.286) (drill 2.286) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -0.635 -29.972) (size 2.286 2.286) (drill 2.286) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -7.62 -4.064) (size 2.286 2.286) (drill 2.286) (layers *.Cu *.Mask))
  )
  (module footprint:mb102 (layer F.Cu) (tedit 58C27C46)
    (at 58.795 81.018 270)
    (fp_text reference MB102 (at 26.67 -34.29 270) (layer F.SilkS) hide)
    (fp_text value mb102 (at 26.67 -16.51 360) (layer F.SilkS))
    (fp_text user + (at 2.54 -33.02 270) (layer F.SilkS))
    (fp_text user - (at 0 -33.02 270) (layer F.SilkS))
    (fp_text user - (at 48.26 -33.02 270) (layer F.SilkS))
    (fp_text user + (at 50.8 -33.02 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 -27.94 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 AGND))
    (pad 2 thru_hole circle (at 2.54 -27.94 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 VDD_5V))
    (pad 3 thru_hole circle (at 0 -22.86 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 AGND))
    (pad 4 thru_hole circle (at 2.54 -22.86 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 VDD_5V))
    (pad 5 thru_hole circle (at 48.26 -27.94 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 AGND))
    (pad 6 thru_hole circle (at 50.8 -27.94 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 5 VDD_3V3))
    (pad 7 thru_hole circle (at 48.26 -22.86 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 AGND))
    (pad 8 thru_hole circle (at 50.8 -22.86 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 5 VDD_3V3))
  )
  (module Discret:C1V8 (layer F.Cu) (tedit 58CE334A)
    (at 96.895 82.288 90)
    (fp_text reference C1 (at 5.5 0 180) (layer F.SilkS))
    (fp_text value 100uFx16V (at -0.212 9.105 180) (layer F.SilkS))
    (fp_text user + (at -3.04546 0 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at -1.27 0 90) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 VDD_5V))
    (pad 2 thru_hole circle (at 1.27 0 90) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 AGND))
    (model Discret.3dshapes/C1V8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Discret:C1V8 (layer F.Cu) (tedit 58CEAE2C)
    (at 96.895 130.548 90)
    (fp_text reference C2 (at 7.048 0.105 180) (layer F.SilkS))
    (fp_text value 100uFx16V (at 5.048 0.105 180) (layer F.SilkS))
    (fp_text user + (at -3.04546 0 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at -1.27 0 90) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 5 VDD_3V3))
    (pad 2 thru_hole circle (at 1.27 0 90) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 AGND))
    (model Discret.3dshapes/C1V8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprint:feather_wiced (layer F.Cu) (tedit 58CA34AE)
    (at 113.405 54.348)
    (fp_text reference U7 (at 12.7 -24.13) (layer F.SilkS))
    (fp_text value feather_wiced (at 0 -0.5) (layer F.SilkS))
    (fp_text user B7/SDA (at 16.51 19.05) (layer F.SilkS))
    (fp_text user B6/SCL (at 16.51 16.51) (layer F.SilkS))
    (fp_text user C5 (at 16.51 13.97) (layer F.SilkS))
    (fp_text user C7 (at 16.51 11.43) (layer F.SilkS))
    (fp_text user JP3 (at 13.97 -12.7) (layer F.SilkS))
    (fp_text user SWCLK/SWDIO (at 19.05 1.27) (layer F.SilkS))
    (fp_text user B4/MISO3 (at 17.78 6.35) (layer F.SilkS))
    (fp_text user A4/CS (at 16.51 3.81) (layer F.SilkS))
    (fp_text user A15 (at 16.51 8.89) (layer F.SilkS))
    (fp_text user B5/MOSI3 (at 17.78 -1.27) (layer F.SilkS))
    (fp_text user VBUS (at 16.51 -3.81) (layer F.SilkS))
    (fp_text user EN (at 16.51 -6.35) (layer F.SilkS))
    (fp_text user VBAT (at 16.51 -8.89) (layer F.SilkS))
    (fp_text user RESET (at -19.05 -19.05) (layer F.SilkS))
    (fp_text user +3.3V (at -19.05 -16.51) (layer F.SilkS))
    (fp_text user VRTC (at -19.05 -13.97) (layer F.SilkS))
    (fp_text user GND (at -19.05 -11.43) (layer F.SilkS))
    (fp_text user A0/WAKEUP (at -19.05 -8.89) (layer F.SilkS))
    (fp_text user C3/ADC13 (at -19.05 -6.35) (layer F.SilkS))
    (fp_text user C2/ADC12 (at -19.05 -3.81) (layer F.SilkS))
    (fp_text user A3/ADC3 (at -19.05 -1.27) (layer F.SilkS))
    (fp_text user A2/ADC2 (at -19.05 1.27) (layer F.SilkS))
    (fp_text user A1/ADC1 (at -19.05 3.81) (layer F.SilkS))
    (fp_text user A5/SCK1 (at -19.05 6.35) (layer F.SilkS))
    (fp_text user A7/MOSI1 (at -19.05 8.89) (layer F.SilkS))
    (fp_text user A6/MISO1 (at -19.05 11.43) (layer F.SilkS))
    (fp_text user A10/RXD> (at -19.05 13.97) (layer F.SilkS))
    (fp_text user "A9/TXD <" (at -19.05 16.51) (layer F.SilkS))
    (fp_text user DFU/SCK3 (at -19.05 19.05) (layer F.SilkS))
    (fp_text user JP1 (at -17.78 -21.59) (layer F.SilkS))
    (pad 1 thru_hole circle (at 12.7 -8.89) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 10 fw_jp3_p1))
    (pad 2 thru_hole circle (at 12.7 -6.35) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 11 fw_jp3_p2))
    (pad 3 thru_hole circle (at 12.7 -3.81) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 2 VDD_5V))
    (pad 4 thru_hole circle (at 12.7 -1.27) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 7 track_pulse_a))
    (pad 5 thru_hole circle (at 12.7 1.27) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 12 fw_jp3_p5))
    (pad 6 thru_hole circle (at 12.7 3.81) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 13 fw_jp3_p6))
    (pad 7 thru_hole circle (at 12.7 6.35) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 14 fw_jp3_p7))
    (pad 8 thru_hole circle (at 12.7 8.89) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 15 fw_jp3_p8))
    (pad 9 thru_hole circle (at 12.7 11.43) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 9 SERVO_PWM))
    (pad 10 thru_hole circle (at 12.7 13.97) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 16 fw_jp3_p10))
    (pad 11 thru_hole circle (at 12.7 16.51) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 3 LCD_SCL))
    (pad 12 thru_hole circle (at 12.7 19.05) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 4 LCD_SDA))
    (pad 16 thru_hole circle (at -12.7 -19.05) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 30 fw_jp1_16))
    (pad 15 thru_hole circle (at -12.7 -16.51) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 29 fw_jp1_15))
    (pad 14 thru_hole circle (at -12.7 -13.97) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 28 fw_jp1_14))
    (pad 13 thru_hole circle (at -12.7 -11.43) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 1 AGND))
    (pad 12 thru_hole circle (at -12.7 -8.89) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 27 fw_jp1_12))
    (pad 11 thru_hole circle (at -12.7 -6.35) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 26 fw_jp1_11))
    (pad 10 thru_hole circle (at -12.7 -3.81) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 25 fw_jp1_10))
    (pad 9 thru_hole circle (at -12.7 -1.27) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 24 fw_jp1_9))
    (pad 8 thru_hole circle (at -12.7 1.27) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 23 fw_jp1_8))
    (pad 7 thru_hole circle (at -12.7 3.81) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 6 fw_sigout))
    (pad 6 thru_hole circle (at -12.7 6.35) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 22 fw_jp1_6))
    (pad 5 thru_hole circle (at -12.7 8.89) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 21 fw_jp1_5))
    (pad 4 thru_hole circle (at -12.7 11.43) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 20 fw_jp1_4))
    (pad 3 thru_hole circle (at -12.7 13.97) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 19 fw_jp1_3))
    (pad 2 thru_hole circle (at -12.7 16.51) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 18 fw_jp1_2))
    (pad 1 thru_hole circle (at -12.7 19.05) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 17 fw_jp1_1))
    (pad 0 thru_hole circle (at -8.89 -22.86) (size 4.572 4.572) (drill 2.54) (layers *.Cu *.Mask)
      (net 1 AGND))
    (pad 0 thru_hole circle (at -8.89 22.86) (size 4.572 4.572) (drill 2.54) (layers *.Cu *.Mask)
      (net 1 AGND))
    (pad 0 thru_hole circle (at 8.89 22.86) (size 4.572 4.572) (drill 2.54) (layers *.Cu *.Mask)
      (net 1 AGND))
    (pad 0 thru_hole circle (at 8.89 -22.86) (size 4.572 4.572) (drill 2.54) (layers *.Cu *.Mask)
      (net 1 AGND))
    (pad 1 thru_hole circle (at -10.16 19.05) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 17 fw_jp1_1))
    (pad 2 thru_hole circle (at -10.16 16.51) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 18 fw_jp1_2))
    (pad 3 thru_hole circle (at -10.16 13.97) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 19 fw_jp1_3))
    (pad 4 thru_hole circle (at -10.16 11.43) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 20 fw_jp1_4))
    (pad 5 thru_hole circle (at -10.16 8.89) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 21 fw_jp1_5))
    (pad 6 thru_hole circle (at -10.16 6.35) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 22 fw_jp1_6))
    (pad 7 thru_hole circle (at -10.16 3.81) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 6 fw_sigout))
    (pad 8 thru_hole circle (at -10.16 1.27) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 23 fw_jp1_8))
    (pad 9 thru_hole circle (at -10.16 -1.27) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 24 fw_jp1_9))
    (pad 10 thru_hole circle (at -10.16 -3.81) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 25 fw_jp1_10))
    (pad 11 thru_hole circle (at -10.16 -6.35) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 26 fw_jp1_11))
    (pad 12 thru_hole circle (at -10.16 -8.89) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 27 fw_jp1_12))
    (pad 13 thru_hole circle (at -10.16 -11.43) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 1 AGND))
    (pad 14 thru_hole circle (at -10.16 -13.97) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 28 fw_jp1_14))
    (pad 15 thru_hole circle (at -10.16 -16.51) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 29 fw_jp1_15))
    (pad 16 thru_hole circle (at -10.16 -19.05) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 30 fw_jp1_16))
    (pad 12 thru_hole circle (at 10.16 19.05) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 4 LCD_SDA))
    (pad 11 thru_hole circle (at 10.16 16.51) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 3 LCD_SCL))
    (pad 10 thru_hole circle (at 10.16 13.97) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 16 fw_jp3_p10))
    (pad 9 thru_hole circle (at 10.16 11.43) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 9 SERVO_PWM))
    (pad 8 thru_hole circle (at 10.16 8.89) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 15 fw_jp3_p8))
    (pad 7 thru_hole circle (at 10.16 6.35) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 14 fw_jp3_p7))
    (pad 6 thru_hole circle (at 10.16 3.81) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 13 fw_jp3_p6))
    (pad 5 thru_hole circle (at 10.16 1.27) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 12 fw_jp3_p5))
    (pad 4 thru_hole circle (at 10.16 -1.27) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 7 track_pulse_a))
    (pad 3 thru_hole circle (at 10.16 -3.81) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 2 VDD_5V))
    (pad 2 thru_hole circle (at 10.16 -6.35) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 11 fw_jp3_p2))
    (pad 1 thru_hole circle (at 10.16 -8.89) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 10 fw_jp3_p1))
    (pad 1 thru_hole circle (at 7.62 1.27) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask))
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 58CA3551)
    (at 96.895 110.228 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J4 (at 0 7.62 360) (layer F.SilkS))
    (fp_text value Pin_Header_Straight_1x03 (at 0 -3.1 180) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 SERVO_PWM))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 VDD_5V))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 AGND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Connect:USB_Micro-B (layer F.Cu) (tedit 58CC16F5)
    (at 71.495 65.778 270)
    (descr "Micro USB Type B Receptacle")
    (tags "USB USB_B USB_micro USB_OTG")
    (attr smd)
    (fp_text reference J7 (at 6.35 0 360) (layer F.SilkS))
    (fp_text value USB_Micro-B (at 0 4.8 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.3009 -1.56254) (size 1.35 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 VDD_5V))
    (pad 2 smd rect (at -0.6509 -1.56254) (size 1.35 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at -0.0009 -1.56254) (size 1.35 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 0.6491 -1.56254) (size 1.35 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 1.2991 -1.56254) (size 1.35 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 AGND))
    (pad 6 thru_hole oval (at -2.5009 -1.56254) (size 0.95 1.25) (drill oval 0.55 0.85) (layers *.Cu *.Mask F.SilkS)
      (net 1 AGND))
    (pad 6 thru_hole oval (at 2.4991 -1.56254) (size 0.95 1.25) (drill oval 0.55 0.85) (layers *.Cu *.Mask F.SilkS)
      (net 1 AGND))
    (pad 6 thru_hole oval (at -3.5009 1.13746) (size 1.55 1) (drill oval 1.15 0.5) (layers *.Cu *.Mask F.SilkS)
      (net 1 AGND))
    (pad 6 thru_hole oval (at 3.4991 1.13746) (size 1.55 1) (drill oval 1.15 0.5) (layers *.Cu *.Mask F.SilkS)
      (net 1 AGND))
  )
  (module Pin_Headers:Pin_Header_Straight_1x19 (layer F.Cu) (tedit 58CC040C)
    (at 157.48 88.9)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference U3_R (at 0 -5.1) (layer F.SilkS) hide)
    (fp_text value Pin_Header_Straight_1x19 (at 0 -3.1) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 AGND))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 VDD_5V))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 fw_sigout))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 95 U2_4))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 96 U2_5))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 97 U2_6))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 98 U2_7))
    (pad 8 thru_hole oval (at 0 17.78) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 99 U2_8))
    (pad 9 thru_hole oval (at 0 20.32) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 track_pulse_a))
    (pad 10 thru_hole oval (at 0 22.86) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 track_pulse_b))
    (pad 11 thru_hole oval (at 0 25.4) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 100 U2_11))
    (pad 12 thru_hole oval (at 0 27.94) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 101 RPiN))
    (pad 13 thru_hole oval (at 0 30.48) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 102 U2_13))
    (pad 14 thru_hole oval (at 0 33.02) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 SERVO_PWM))
    (pad 15 thru_hole oval (at 0 35.56) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 103 U2_15))
    (pad 16 thru_hole oval (at 0 38.1) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 104 Pon3))
    (pad 17 thru_hole oval (at 0 40.64) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 105 Pof3))
    (pad 18 thru_hole oval (at 0 43.18) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 106 U2_18))
    (pad 19 thru_hole oval (at 0 45.72) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 VDD_3V3))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x19.wrl
      (at (xyz 0 -0.9 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x19 (layer F.Cu) (tedit 58CA3179)
    (at 127 88.9)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference U3 (at -4.705 23.868 90) (layer F.SilkS))
    (fp_text value Pin_Header_Straight_1x19 (at 0 -3.1) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 AGND))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 VDD_5V))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 fw_sigout))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 95 U2_4))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 96 U2_5))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 97 U2_6))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 98 U2_7))
    (pad 8 thru_hole oval (at 0 17.78) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 99 U2_8))
    (pad 9 thru_hole oval (at 0 20.32) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 track_pulse_a))
    (pad 10 thru_hole oval (at 0 22.86) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 track_pulse_b))
    (pad 11 thru_hole oval (at 0 25.4) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 100 U2_11))
    (pad 12 thru_hole oval (at 0 27.94) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 101 RPiN))
    (pad 13 thru_hole oval (at 0 30.48) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 102 U2_13))
    (pad 14 thru_hole oval (at 0 33.02) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 SERVO_PWM))
    (pad 15 thru_hole oval (at 0 35.56) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 103 U2_15))
    (pad 16 thru_hole oval (at 0 38.1) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 104 Pon3))
    (pad 17 thru_hole oval (at 0 40.64) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 105 Pof3))
    (pad 18 thru_hole oval (at 0 43.18) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 106 U2_18))
    (pad 19 thru_hole oval (at 0 45.72) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 VDD_3V3))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x19.wrl
      (at (xyz 0 -0.9 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x19 (layer F.Cu) (tedit 58CA30D6)
    (at 116.84 88.9)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J3 (at 0.375 -4.072) (layer F.SilkS))
    (fp_text value Pin_Header_Straight_1x19 (at 0 -3.1) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 AGND))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 VDD_5V))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 fw_sigout))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 95 U2_4))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 96 U2_5))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 97 U2_6))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 98 U2_7))
    (pad 8 thru_hole oval (at 0 17.78) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 99 U2_8))
    (pad 9 thru_hole oval (at 0 20.32) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 track_pulse_a))
    (pad 10 thru_hole oval (at 0 22.86) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 track_pulse_b))
    (pad 11 thru_hole oval (at 0 25.4) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 100 U2_11))
    (pad 12 thru_hole oval (at 0 27.94) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 101 RPiN))
    (pad 13 thru_hole oval (at 0 30.48) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 102 U2_13))
    (pad 14 thru_hole oval (at 0 33.02) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 SERVO_PWM))
    (pad 15 thru_hole oval (at 0 35.56) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 103 U2_15))
    (pad 16 thru_hole oval (at 0 38.1) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 104 Pon3))
    (pad 17 thru_hole oval (at 0 40.64) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 105 Pof3))
    (pad 18 thru_hole oval (at 0 43.18) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 106 U2_18))
    (pad 19 thru_hole oval (at 0 45.72) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 VDD_3V3))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x19.wrl
      (at (xyz 0 -0.9 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x20 locked (layer F.Cu) (tedit 58CA3373)
    (at 135.89 38.1 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J10 (at 5.342 -0.895 180) (layer F.SilkS))
    (fp_text value Pin_Header_Straight_2x20 (at 0 -3.1 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 VDD_5V))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 62 j10_2))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 61 j10_3))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 63 j10_4))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 AGND))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 64 j10_6))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 65 j10_7))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 66 j10_8))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 67 j10_9))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 68 j10_10))
    (pad 11 thru_hole oval (at 0 12.7 90) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 69 j10_11))
    (pad 12 thru_hole oval (at 2.54 12.7 90) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 70 j10_12))
    (pad 13 thru_hole oval (at 0 15.24 90) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 71 j10_13))
    (pad 14 thru_hole oval (at 2.54 15.24 90) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 72 j10_14))
    (pad 15 thru_hole oval (at 0 17.78 90) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 73 j10_15))
    (pad 16 thru_hole oval (at 2.54 17.78 90) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 74 j10_16))
    (pad 17 thru_hole oval (at 0 20.32 90) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 75 j10_17))
    (pad 18 thru_hole oval (at 2.54 20.32 90) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 76 j10_18))
    (pad 19 thru_hole oval (at 0 22.86 90) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 77 j10_19))
    (pad 20 thru_hole oval (at 2.54 22.86 90) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 78 j10_20))
    (pad 21 thru_hole oval (at 0 25.4 90) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 79 j10_21))
    (pad 22 thru_hole oval (at 2.54 25.4 90) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 80 j10_22))
    (pad 23 thru_hole oval (at 0 27.94 90) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 81 j10_23))
    (pad 24 thru_hole oval (at 2.54 27.94 90) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 82 j10_24))
    (pad 25 thru_hole oval (at 0 30.48 90) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 83 j10_25))
    (pad 26 thru_hole oval (at 2.54 30.48 90) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 84 j10_26))
    (pad 27 thru_hole oval (at 0 33.02 90) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 85 j10_27))
    (pad 28 thru_hole oval (at 2.54 33.02 90) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 86 j10_28))
    (pad 29 thru_hole oval (at 0 35.56 90) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 101 RPiN))
    (pad 30 thru_hole oval (at 2.54 35.56 90) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 87 j10_30))
    (pad 31 thru_hole oval (at 0 38.1 90) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 SERVO_PWM))
    (pad 32 thru_hole oval (at 2.54 38.1 90) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 105 Pof3))
    (pad 33 thru_hole oval (at 0 40.64 90) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 104 Pon3))
    (pad 34 thru_hole oval (at 2.54 40.64 90) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 88 j10_34))
    (pad 35 thru_hole oval (at 0 43.18 90) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 89 j10_35))
    (pad 36 thru_hole oval (at 2.54 43.18 90) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 90 j10_36))
    (pad 37 thru_hole oval (at 0 45.72 90) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 91 j10_37))
    (pad 38 thru_hole oval (at 2.54 45.72 90) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 92 j10_38))
    (pad 39 thru_hole oval (at 0 48.26 90) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 93 j10_39))
    (pad 40 thru_hole oval (at 2.54 48.26 90) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 94 j10_40))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x20 locked (layer F.Cu) (tedit 58CE35AC)
    (at 135.89 73.66 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J11 (at 1.16 51.61 180) (layer F.SilkS))
    (fp_text value Pin_Header_Straight_2x20 (at 0 -3.1 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 VDD_5V))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 62 j10_2))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 61 j10_3))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 63 j10_4))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 AGND))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 64 j10_6))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 65 j10_7))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 66 j10_8))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 67 j10_9))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 68 j10_10))
    (pad 11 thru_hole oval (at 0 12.7 90) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 69 j10_11))
    (pad 12 thru_hole oval (at 2.54 12.7 90) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 70 j10_12))
    (pad 13 thru_hole oval (at 0 15.24 90) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 71 j10_13))
    (pad 14 thru_hole oval (at 2.54 15.24 90) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 72 j10_14))
    (pad 15 thru_hole oval (at 0 17.78 90) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 73 j10_15))
    (pad 16 thru_hole oval (at 2.54 17.78 90) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 74 j10_16))
    (pad 17 thru_hole oval (at 0 20.32 90) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 75 j10_17))
    (pad 18 thru_hole oval (at 2.54 20.32 90) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 76 j10_18))
    (pad 19 thru_hole oval (at 0 22.86 90) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 77 j10_19))
    (pad 20 thru_hole oval (at 2.54 22.86 90) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 78 j10_20))
    (pad 21 thru_hole oval (at 0 25.4 90) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 79 j10_21))
    (pad 22 thru_hole oval (at 2.54 25.4 90) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 80 j10_22))
    (pad 23 thru_hole oval (at 0 27.94 90) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 81 j10_23))
    (pad 24 thru_hole oval (at 2.54 27.94 90) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 82 j10_24))
    (pad 25 thru_hole oval (at 0 30.48 90) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 83 j10_25))
    (pad 26 thru_hole oval (at 2.54 30.48 90) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 84 j10_26))
    (pad 27 thru_hole oval (at 0 33.02 90) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 85 j10_27))
    (pad 28 thru_hole oval (at 2.54 33.02 90) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 86 j10_28))
    (pad 29 thru_hole oval (at 0 35.56 90) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 101 RPiN))
    (pad 30 thru_hole oval (at 2.54 35.56 90) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 87 j10_30))
    (pad 31 thru_hole oval (at 0 38.1 90) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 SERVO_PWM))
    (pad 32 thru_hole oval (at 2.54 38.1 90) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 105 Pof3))
    (pad 33 thru_hole oval (at 0 40.64 90) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 104 Pon3))
    (pad 34 thru_hole oval (at 2.54 40.64 90) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 88 j10_34))
    (pad 35 thru_hole oval (at 0 43.18 90) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 89 j10_35))
    (pad 36 thru_hole oval (at 2.54 43.18 90) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 90 j10_36))
    (pad 37 thru_hole oval (at 0 45.72 90) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 91 j10_37))
    (pad 38 thru_hole oval (at 2.54 45.72 90) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 92 j10_38))
    (pad 39 thru_hole oval (at 0 48.26 90) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 93 j10_39))
    (pad 40 thru_hole oval (at 2.54 48.26 90) (size 1.5 1.5) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 94 j10_40))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 58CA3420)
    (at 202.305 82.288)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference REF** (at 0 -5.1) (layer F.SilkS) hide)
    (fp_text value Pin_Header_Straight_1x01 (at 0 -3.1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.318 4.318) (drill 3.556) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x04 (layer F.Cu) (tedit 58CA366A)
    (at 63.5 44.196)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference U5 (at 1.27 -2.54) (layer F.SilkS))
    (fp_text value Pin_Header_Straight_2x04 (at 0 -3.1) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 LCD_SDA))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 LCD_SDA))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 LCD_SCL))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 LCD_SCL))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 AGND))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 AGND))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 VDD_5V))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 VDD_5V))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x04.wrl
      (at (xyz 0.05 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x10 (layer F.Cu) (tedit 58CA366C)
    (at 78.74 36.576)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J12 (at 1.27 -2.54) (layer F.SilkS))
    (fp_text value Pin_Header_Straight_2x10 (at 0 -3.1) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 j12_1))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 j12_1))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 52 j12_3))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 52 j12_3))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 53 j12_5))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 53 j12_5))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 54 j12_7))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 54 j12_7))
    (pad 9 thru_hole oval (at 0 10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 55 j12_9))
    (pad 10 thru_hole oval (at 2.54 10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 55 j12_9))
    (pad 11 thru_hole oval (at 0 12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 56 j12_11))
    (pad 12 thru_hole oval (at 2.54 12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 56 j12_11))
    (pad 13 thru_hole oval (at 0 15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 57 j12_13))
    (pad 14 thru_hole oval (at 2.54 15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 57 j12_13))
    (pad 15 thru_hole oval (at 0 17.78) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 58 j12_15))
    (pad 16 thru_hole oval (at 2.54 17.78) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 58 j12_15))
    (pad 17 thru_hole oval (at 0 20.32) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 59 j12_17))
    (pad 18 thru_hole oval (at 2.54 20.32) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 59 j12_17))
    (pad 19 thru_hole oval (at 0 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 60 j12_19))
    (pad 20 thru_hole oval (at 2.54 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 60 j12_19))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x10.wrl
      (at (xyz 0.05 -0.45 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (gr_text "This project has a specific target\n of providing a low-cost, open \nsource technological kit to allow\n scientists, academics, hackers, \nmakers or OSHW fans to hack their\n way to ultrasound imaging -\n below 500$ - at home, with no \nspecific equipment required. " (at 93.98 96.52) (layer B.SilkS))
  (gr_text "Article at \nhttp://openhardware.metajnl.com/articles/10.5334/joh.2/" (at 158.75 81.28) (layer B.SilkS))
  (gr_text "All source code is available at \nhttps://github.com/kelu124/echomods/\nand the corresponding documentation at \nhttps://www.gitbook.com/book/kelu124/echomods" (at 158.75 59.69) (layer B.SilkS))
  (gr_text "Some room left for two raspberry pi headers\nor even two pi zero" (at 158.75 49.53) (layer B.SilkS))
  (gr_text "This place can \nbe used for the\nTobo, aka the \npulser module. " (at 194.31 106.68) (layer B.SilkS))
  (gr_text "This place\nis used for\nthe Goblin\nanalog\nprocessing \nmodule." (at 142.24 109.22) (layer B.SilkS))
  (gr_text "Motherboard \"Doj\" board" (at 73.66 31.75) (layer F.SilkS))
  (gr_text "Open Hardware\nLicense TAPR\n(c) kelu124, 2017" (at 72.39 95.25) (layer F.SilkS))
  (gr_text "Documentation at https://github.com/kelu124/echomods/" (at 166.37 30.48) (layer F.SilkS))
  (gr_text "GND\n5V\nENV\nRENV\nRSIG\nP6\nGain\nP8\nPon\nPoff\nP11\nRPiN\nP13\nPWM\nP15\nPon3\nPof3\nRaw\n3.3V" (at 196 112) (layer F.SilkS))
  (gr_text "GND\n5V\nENV\nRENV\nRSIG\nP6\nGain\nP8\nPon\nPoff\nP11\nRPiN\nP13\nPWM\nP15\nPon3\nPof3\nRaw\n3.3V" (at 142.5 112) (layer F.SilkS))
  (gr_text "GND\n5V\nENV\nRENV\nRSIG\nP6\nGain\nP8\nPon\nPoff\nP11\nRPiN\nP13\nPWM\nP15\nPon3\nPof3\nRaw\n3.3V" (at 167.5 112) (layer F.SilkS))
  (gr_text "GND\n5V\nENV\nRENV\nRSIG\nP6\nGain\nP8\nPon\nPoff\nP11\nRPiN\nP13\nPWM\nP15\nPon3\nPof3\nRaw\n3.3V" (at 114 112) (layer F.SilkS))
  (gr_text "RPI GPIO HEADER" (at 158.5 47) (layer F.SilkS))
  (gr_text "5v\n5v\nGND\nGPIO14 (TXD0)\nGPIO15 (RXD0)\nGPIO18 (GPIO_GEN1)\nGND\nGPIO23 (GPIO_GEN4)\nGPIO24 (GPIO_GEN5)\nGND\nGPIO25 (GPIO_GEN6)\nGPIO08 (SPI_CE0_N)\nGPIO07 (SPI_CE1_N)\nID_SC (I2C ID EEPROM)\nGND\nGPIO12\nGND\nGPIO16\nGPIO20\nGPIO21" (at 160 68.5 90) (layer F.SilkS))
  (gr_text "3.3v\nGPIO02 (SDA1, I2C)\nGPIO03 (SCL1, I2C)\nGPIO04 (GPIO_GCLK)\nGND\nGPIO17 (GPIO_GEN0)\nGPIO27 (GPIO_GEN2)\nGPIO22 (GPIO_GEN3)\n3.3v\nGPIO10 (SPI_MOSI)\nGPIO09 (SPI_MISO)\nGPIO11 (SPI_CLK)\nGND\nID_SD (I2C ID EEPROM)\nGPIO05\nGPIO06\nGPIO13\nGPIO19\nGPIO26\nGND" (at 160 76 90) (layer F.SilkS))
  (gr_text "+3.3 V" (at 96.5 136.5) (layer F.SilkS))
  (gr_text "+5 V" (at 97 88.5) (layer F.SilkS))
  (gr_line (start 57.525 139.438) (end 57.525 27.678) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 218.815 139.438) (end 57.525 139.438) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 218.815 27.678) (end 218.815 139.438) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 57.525 27.678) (end 218.815 27.678) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "GND\n+5\nPWM" (at 101.975 107.688) (layer F.SilkS))
  (zone (net 1) (net_name AGND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.5)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 57 140) (xy 57 27) (xy 219 27) (xy 219 140)
      )
    )
  )
  (zone (net 1) (net_name AGND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.5)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 57 140) (xy 57 27) (xy 219 27) (xy 219 140)
      )
    )
  )
)
