(kicad_pcb (version 20171130) (host pcbnew "(5.1.7)-1")
  (general
    (thickness 1.6002)
    (drawings 27)
    (tracks 353)
    (zones 0)
    (modules 64)
    (nets 30)
  )
  (page USLetter)
  (title_block
    (rev 1)
  )
  (layers
    (0 Front signal)
    (1 In1.Cu power)
    (2 In2.Cu power)
    (31 Back signal)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.762)
    (user_trace_width 0.254)
    (user_trace_width 0.508)
    (user_trace_width 0.762)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.254)
    (via_size 0.4572)
    (via_drill 0.254)
    (via_min_size 0.4572)
    (via_min_drill 0.254)
    (user_via 0.4572 0.254)
    (user_via 0.889 0.381)
    (uvia_size 0.4572)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (edge_width 0.0381)
    (segment_width 0.254)
    (pcb_text_width 0.3048)
    (pcb_text_size 1.524 1.524)
    (mod_edge_width 0.127)
    (mod_text_size 0.762 0.762)
    (mod_text_width 0.127)
    (pad_size 4.5 4.5)
    (pad_drill 3.7)
    (pad_to_mask_clearance 0.1016)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.152400)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "./gerbers"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(C1-Pad1)")
  (net 3 V-)
  (net 4 V+)
  (net 5 "Net-(D1-Pad2)")
  (net 6 "Net-(D1-Pad1)")
  (net 7 "Net-(D2-Pad1)")
  (net 8 "Net-(R2-Pad1)")
  (net 9 "Net-(R3-Pad1)")
  (net 10 "Net-(R4-Pad2)")
  (net 11 "Net-(R6-Pad2)")
  (net 12 "Net-(R7-Pad2)")
  (net 13 "Net-(RV1-Pad2)")
  (net 14 "Net-(R1-Pad2)")
  (net 15 "Net-(C16-Pad1)")
  (net 16 "Net-(C17-Pad1)")
  (net 17 "Net-(C18-Pad1)")
  (net 18 "Net-(TP8-Pad1)")
  (net 19 "Net-(TP10-Pad1)")
  (net 20 "Net-(TP11-Pad1)")
  (net 21 "Net-(TP12-Pad1)")
  (net 22 "Net-(TP13-Pad1)")
  (net 23 "Net-(TP14-Pad1)")
  (net 24 "Net-(RV2-Pad2)")
  (net 25 "Net-(R5-Pad2)")
  (net 26 "Net-(R5-Pad1)")
  (net 27 "Net-(RV3-Pad2)")
  (net 28 Va+)
  (net 29 "Net-(J1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.4572)
    (via_drill 0.254)
    (uvia_dia 0.4572)
    (uvia_drill 0.254)
    (diff_pair_width 0.254)
    (diff_pair_gap 0.254)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C16-Pad1)")
    (add_net "Net-(C17-Pad1)")
    (add_net "Net-(C18-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R4-Pad2)")
    (add_net "Net-(R5-Pad1)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(R6-Pad2)")
    (add_net "Net-(R7-Pad2)")
    (add_net "Net-(RV1-Pad2)")
    (add_net "Net-(RV2-Pad2)")
    (add_net "Net-(RV3-Pad2)")
    (add_net "Net-(TP10-Pad1)")
    (add_net "Net-(TP11-Pad1)")
    (add_net "Net-(TP12-Pad1)")
    (add_net "Net-(TP13-Pad1)")
    (add_net "Net-(TP14-Pad1)")
    (add_net "Net-(TP8-Pad1)")
    (add_net V+)
    (add_net V-)
    (add_net Va+)
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer Front) (tedit 59FED5CC)
    (at 75.4126 74.83348)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J1 (at 2.50952 2.7686) (layer F.SilkS))
    (fp_text value Conn_01x03_Male (at 0 7.41) (layer F.Fab))
    (fp_text user %R (at 0 2.54 90) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 V+))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 Va+))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Bridge_Pitch2.54mm_Drill1.0mm (layer Front) (tedit 5A0F774F)
    (at 68.0212 83.61934)
    (descr "wire loop as test point, pitch 2.54mm, hole diameter 1.0mm, wire diameter 0.8mm")
    (tags "test point wire loop")
    (fp_text reference TP16 (at 1.07188 1.95834) (layer F.SilkS))
    (fp_text value Vbits (at 1 -1.7) (layer F.SilkS))
    (fp_text user %R (at 1.1 2.1) (layer F.Fab))
    (pad 1 thru_hole circle (at 2.54 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(R5-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(R5-Pad2)"))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Bridge_Pitch2.54mm_Drill1.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometer_THT:Potentiometer_Bourns_3296W_Vertical (layer Front) (tedit 5A3D4994)
    (at 80.75422 83.0453 180)
    (descr "Potentiometer, vertical, Bourns 3296W, https://www.bourns.com/pdfs/3296.pdf")
    (tags "Potentiometer vertical Bourns 3296W")
    (fp_text reference RV3 (at -1.64084 -3.45948) (layer F.SilkS))
    (fp_text value R_POT (at -2.54 3.67) (layer F.Fab))
    (fp_text user %R (at -3.175 0.005) (layer F.Fab))
    (pad 3 thru_hole circle (at -5.08 0 180) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at -2.54 0 180) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(RV3-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 V-))
    (model ${KISYS3DMOD}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_3296W_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer Front) (tedit 5F68FEEE)
    (at 86.59444 87.30488)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R9 (at 2.55956 -0.84836 90) (layer F.SilkS))
    (fp_text value 6.65k (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1 0) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 25 "Net-(R5-Pad2)"))
    (pad 1 smd roundrect (at -1 0) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 28 Va+))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer Front) (tedit 5F68FEEE)
    (at 85.8012 91.02522 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R5 (at -0.15062 1.71704 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1 0 90) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 25 "Net-(R5-Pad2)"))
    (pad 1 smd roundrect (at -1 0 90) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 26 "Net-(R5-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module art:squad (layer Back) (tedit 0)
    (at 89.22766 102.31882 180)
    (fp_text reference G*** (at 0 0) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer B.SilkS) hide)
  )
  (module art:sawtooth (layer Back) (tedit 0)
    (at 76.27366 72.06742 270)
    (fp_text reference G*** (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 270) (layer B.SilkS) hide)
  )
  (module MountingHole:MountingHole_3mm_Pad (layer Front) (tedit 56D1B4CB)
    (at 70.7136 108.966)
    (descr "Mounting Hole 3mm")
    (tags "mounting hole 3mm")
    (attr virtual)
    (fp_text reference REF** (at 0 -4) (layer F.SilkS) hide)
    (fp_text value MountingHole_3mm_Pad (at 0 4) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3mm_Pad (layer Front) (tedit 56D1B4CB)
    (at 118.618 108.966)
    (descr "Mounting Hole 3mm")
    (tags "mounting hole 3mm")
    (attr virtual)
    (fp_text reference REF** (at 0 -4) (layer F.SilkS) hide)
    (fp_text value MountingHole_3mm_Pad (at 0 4) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3mm_Pad (layer Front) (tedit 56D1B4CB)
    (at 118.618 57.404)
    (descr "Mounting Hole 3mm")
    (tags "mounting hole 3mm")
    (attr virtual)
    (fp_text reference REF** (at 0 -4) (layer F.SilkS) hide)
    (fp_text value MountingHole_3mm_Pad (at 0 4) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3mm_Pad (layer Front) (tedit 56D1B4CB)
    (at 70.7136 57.404)
    (descr "Mounting Hole 3mm")
    (tags "mounting hole 3mm")
    (attr virtual)
    (fp_text reference REF** (at 0 -4) (layer F.SilkS) hide)
    (fp_text value MountingHole_3mm_Pad (at 0 4) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Mask))
  )
  (module TestPoint:TestPoint_Bridge_Pitch2.54mm_Drill1.0mm (layer Front) (tedit 5A0F774F)
    (at 79.72552 108.89996 270)
    (descr "wire loop as test point, pitch 2.54mm, hole diameter 1.0mm, wire diameter 0.8mm")
    (tags "test point wire loop")
    (fp_text reference TP4 (at 1.1 2.1 90) (layer F.SilkS))
    (fp_text value V+ (at 1 -1.7 90) (layer F.SilkS))
    (fp_text user %R (at 1.1 2.1 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 2.54 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 4 V+))
    (pad 1 thru_hole circle (at 0 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 4 V+))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Bridge_Pitch2.54mm_Drill1.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder (layer Back) (tedit 5F68FEEF)
    (at 85.93972 76.65212 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference CE3 (at 0 1.68) (layer B.SilkS))
    (fp_text value dnp (at 0 -1.68) (layer B.SilkS))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -1.0375 0 180) (size 1.175 1.45) (layers Back B.Paste B.Mask) (roundrect_rratio 0.2127659574468085)
      (net 17 "Net-(C18-Pad1)"))
    (pad 2 smd roundrect (at 1.0375 0 180) (size 1.175 1.45) (layers Back B.Paste B.Mask) (roundrect_rratio 0.2127659574468085)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder (layer Back) (tedit 5F68FEEF)
    (at 102.09666 76.59624 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference CE2 (at 0 1.68) (layer B.SilkS))
    (fp_text value dnp (at 0 -1.68) (layer B.SilkS))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -1.0375 0 180) (size 1.175 1.45) (layers Back B.Paste B.Mask) (roundrect_rratio 0.2127659574468085)
      (net 16 "Net-(C17-Pad1)"))
    (pad 2 smd roundrect (at 1.0375 0 180) (size 1.175 1.45) (layers Back B.Paste B.Mask) (roundrect_rratio 0.2127659574468085)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder (layer Back) (tedit 5F68FEEF)
    (at 114.45612 76.77404 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference CE1 (at 0 1.68) (layer B.SilkS))
    (fp_text value dnp (at 0 -1.68) (layer B.SilkS))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 1.0375 0 180) (size 1.175 1.45) (layers Back B.Paste B.Mask) (roundrect_rratio 0.2127659574468085)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.0375 0 180) (size 1.175 1.45) (layers Back B.Paste B.Mask) (roundrect_rratio 0.2127659574468085)
      (net 15 "Net-(C16-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometer_THT:Potentiometer_Bourns_3296W_Vertical (layer Front) (tedit 5A3D4994)
    (at 97.05086 83.05038)
    (descr "Potentiometer, vertical, Bourns 3296W, https://www.bourns.com/pdfs/3296.pdf")
    (tags "Potentiometer vertical Bourns 3296W")
    (fp_text reference RV2 (at -2.32918 -3.42138) (layer F.SilkS))
    (fp_text value R_POT (at -3.81 1.81356) (layer F.Fab))
    (fp_text user %R (at -3.175 0.005) (layer F.Fab))
    (pad 3 thru_hole circle (at -5.08 0) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(RV2-Pad2)"))
    (pad 2 thru_hole circle (at -2.54 0) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(RV2-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(R4-Pad2)"))
    (model ${KISYS3DMOD}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_3296W_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Bridge_Pitch2.54mm_Drill1.0mm (layer Front) (tedit 5A0F774F)
    (at 68.64656 69.55802)
    (descr "wire loop as test point, pitch 2.54mm, hole diameter 1.0mm, wire diameter 0.8mm")
    (tags "test point wire loop")
    (fp_text reference TP15 (at 1.1 2.1) (layer F.SilkS))
    (fp_text value Vext (at 1 -1.7) (layer F.SilkS))
    (fp_text user %R (at 1.1 2.1) (layer F.Fab))
    (pad 1 thru_hole circle (at 2.54 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(J1-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Bridge_Pitch2.54mm_Drill1.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D5.0mm_P2.00mm (layer Front) (tedit 5AE50EF0)
    (at 104.69372 82.76082)
    (descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C9 (at 3.68046 -3.91414 90) (layer F.SilkS))
    (fp_text value 10u (at -2.08788 -2.89052) (layer F.SilkS))
    (fp_text user %R (at 1 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 V-))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D5.0mm_P2.00mm (layer Front) (tedit 5AE50EF0)
    (at 119.21744 88.18372)
    (descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C8 (at -1.5494 -3.0226) (layer F.SilkS))
    (fp_text value 10u (at 3.6957 -3.05308) (layer F.SilkS) hide)
    (fp_text user %R (at -2.54 -2.54) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 V+))
    (pad 2 thru_hole circle (at 2 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Bridge_Pitch2.54mm_Drill1.0mm (layer Front) (tedit 5A0F774F)
    (at 98.59264 57.7088 90)
    (descr "wire loop as test point, pitch 2.54mm, hole diameter 1.0mm, wire diameter 0.8mm")
    (tags "test point wire loop")
    (fp_text reference TP12 (at 1.1 2.1 90) (layer F.SilkS))
    (fp_text value Vclock- (at 1 -1.7 90) (layer F.SilkS))
    (fp_text user %R (at 1.1 2.1 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 2.54 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(TP12-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(TP12-Pad1)"))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Bridge_Pitch2.54mm_Drill1.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Rect_L10.3mm_W5.0mm_P7.50mm_MKS4 (layer Front) (tedit 5AE50EF0)
    (at 89.662 76.5048 180)
    (descr "C, Rect series, Radial, pin pitch=7.50mm, , length*width=10.3*5mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf")
    (tags "C Rect series Radial pin pitch 7.50mm  length 10.3mm width 5mm Capacitor")
    (fp_text reference C18 (at -3.0099 1.62306) (layer F.SilkS))
    (fp_text value 0.1u (at -3.37058 0.2921) (layer F.SilkS))
    (fp_text user %R (at 3.75 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 7.5 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(C18-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L10.3mm_W5.0mm_P7.50mm_MKS4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Rect_L10.3mm_W5.0mm_P7.50mm_MKS4 (layer Front) (tedit 5AE50EF0)
    (at 105.918 76.5048 180)
    (descr "C, Rect series, Radial, pin pitch=7.50mm, , length*width=10.3*5mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf")
    (tags "C Rect series Radial pin pitch 7.50mm  length 10.3mm width 5mm Capacitor")
    (fp_text reference C17 (at 4.39166 -4.72948) (layer F.SilkS))
    (fp_text value 0.1u (at -2.286 0.16002 270) (layer F.SilkS))
    (fp_text user %R (at 3.75 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 7.5 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(C17-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L10.3mm_W5.0mm_P7.50mm_MKS4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Rect_L10.3mm_W5.0mm_P7.50mm_MKS4 (layer Front) (tedit 5AE50EF0)
    (at 118.2116 76.7334 180)
    (descr "C, Rect series, Radial, pin pitch=7.50mm, , length*width=10.3*5mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf")
    (tags "C Rect series Radial pin pitch 7.50mm  length 10.3mm width 5mm Capacitor")
    (fp_text reference C16 (at -2.7432 -1.4478 90) (layer F.SilkS))
    (fp_text value 0.1u (at -2.5273 2.1082 90) (layer F.SilkS))
    (fp_text user %R (at 3.75 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 7.5 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(C16-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L10.3mm_W5.0mm_P7.50mm_MKS4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:DIP-8_W7.62mm (layer Front) (tedit 5B86B3A2)
    (at 82.042 63.754)
    (descr http://media.digikey.com/pdf/Data%20Sheets/Lite-On%20PDFs/6N137%20Series.pdf)
    (fp_text reference U6 (at 0.254 -2.3368) (layer F.SilkS))
    (fp_text value LF398_DIP8 (at 3.94 10.33) (layer F.Fab))
    (fp_text user REF** (at 3.94 3.49) (layer F.Fab))
    (pad 8 thru_hole circle (at 7.62 0) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(TP10-Pad1)"))
    (pad 7 thru_hole circle (at 7.62 2.54) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole circle (at 7.62 5.08) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(C18-Pad1)"))
    (pad 5 thru_hole circle (at 7.62 7.62) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(TP14-Pad1)"))
    (pad 4 thru_hole circle (at 0 7.62) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 3 V-))
    (pad 3 thru_hole circle (at 0 5.08) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(TP13-Pad1)"))
    (pad 2 thru_hole circle (at 0 2.54) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 4 V+))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-8_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:DIP-8_W7.62mm (layer Front) (tedit 5B86B3A2)
    (at 98.298 63.5)
    (descr http://media.digikey.com/pdf/Data%20Sheets/Lite-On%20PDFs/6N137%20Series.pdf)
    (fp_text reference U5 (at 0.254 -2.3876) (layer F.SilkS))
    (fp_text value LF398_DIP8 (at 3.94 10.33) (layer F.Fab))
    (fp_text user REF** (at 3.94 3.49) (layer F.Fab))
    (pad 8 thru_hole circle (at 7.62 0) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(TP12-Pad1)"))
    (pad 7 thru_hole circle (at 7.62 2.54) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole circle (at 7.62 5.08) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(C17-Pad1)"))
    (pad 5 thru_hole circle (at 7.62 7.62) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(TP13-Pad1)"))
    (pad 4 thru_hole circle (at 0 7.62) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 3 V-))
    (pad 3 thru_hole circle (at 0 5.08) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(TP11-Pad1)"))
    (pad 2 thru_hole circle (at 0 2.54) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 4 V+))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-8_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:DIP-8_W7.62mm (layer Front) (tedit 5B86B3A2)
    (at 113.1062 63.5254)
    (descr http://media.digikey.com/pdf/Data%20Sheets/Lite-On%20PDFs/6N137%20Series.pdf)
    (fp_text reference U4 (at 0.2794 -2.2606) (layer F.SilkS))
    (fp_text value LF398_DIP8 (at 3.94 10.33) (layer F.Fab))
    (fp_text user REF** (at 3.94 3.49) (layer F.Fab))
    (pad 8 thru_hole circle (at 7.62 0) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(TP10-Pad1)"))
    (pad 7 thru_hole circle (at 7.62 2.54) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole circle (at 7.62 5.08) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(C16-Pad1)"))
    (pad 5 thru_hole circle (at 7.62 7.62) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(TP11-Pad1)"))
    (pad 4 thru_hole circle (at 0 7.62) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 3 V-))
    (pad 3 thru_hole circle (at 0 5.08) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 0 2.54) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 4 V+))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-8_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:DIP-8_W7.62mm (layer Front) (tedit 5B86B3A2)
    (at 116.078 91.9988 270)
    (descr http://media.digikey.com/pdf/Data%20Sheets/Lite-On%20PDFs/6N137%20Series.pdf)
    (fp_text reference U3 (at 0.1016 -2.286 90) (layer F.SilkS))
    (fp_text value TL082IP (at 3.94 10.033 90) (layer F.SilkS))
    (fp_text user REF** (at 3.94 3.49 90) (layer F.Fab))
    (pad 8 thru_hole circle (at 7.62 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 4 V+))
    (pad 7 thru_hole circle (at 7.62 2.54 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(D2-Pad1)"))
    (pad 6 thru_hole circle (at 7.62 5.08 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(D1-Pad1)"))
    (pad 5 thru_hole circle (at 7.62 7.62 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(R6-Pad2)"))
    (pad 4 thru_hole circle (at 0 7.62 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 3 V-))
    (pad 3 thru_hole circle (at 0 5.08 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(R6-Pad2)"))
    (pad 2 thru_hole circle (at 0 2.54 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(D1-Pad1)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-8_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:DIP-8_W7.62mm (layer Front) (tedit 5B86B3A2)
    (at 90.58148 88.4555)
    (descr http://media.digikey.com/pdf/Data%20Sheets/Lite-On%20PDFs/6N137%20Series.pdf)
    (fp_text reference U2 (at 1.46558 -2.01168) (layer F.SilkS))
    (fp_text value TL082IP (at 5.588 10.287) (layer F.SilkS))
    (fp_text user REF** (at 3.94 3.49) (layer F.Fab))
    (pad 8 thru_hole circle (at 7.62 0) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 4 V+))
    (pad 7 thru_hole circle (at 7.62 2.54) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(R2-Pad1)"))
    (pad 6 thru_hole circle (at 7.62 5.08) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(R4-Pad2)"))
    (pad 5 thru_hole circle (at 7.62 7.62) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 4 thru_hole circle (at 0 7.62) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 3 V-))
    (pad 3 thru_hole circle (at 0 5.08) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(RV1-Pad2)"))
    (pad 2 thru_hole circle (at 0 2.54) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(RV2-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(RV2-Pad2)"))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-8_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:DIP-14_W3mm (layer Front) (tedit 596E717A)
    (at 75.20686 89.57564)
    (fp_text reference U1 (at -0.1524 -2.7432) (layer F.SilkS))
    (fp_text value LM339AN (at 0.6223 -4.20624) (layer F.SilkS))
    (fp_text user REF** (at 3.86 7.77) (layer F.Fab))
    (pad 14 thru_hole circle (at 7.62 0) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask))
    (pad 13 thru_hole circle (at 7.62 2.54) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(R5-Pad1)"))
    (pad 12 thru_hole circle (at 7.62 5.08) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 3 V-))
    (pad 11 thru_hole circle (at 7.62 7.62) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(TP11-Pad1)"))
    (pad 10 thru_hole circle (at 7.62 10.16) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(RV3-Pad2)"))
    (pad 9 thru_hole circle (at 7.62 12.7) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 4 V+))
    (pad 8 thru_hole circle (at 7.62 15.24) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole circle (at 0 15.24) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(TP8-Pad1)"))
    (pad 6 thru_hole circle (at 0 12.7) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(R7-Pad2)"))
    (pad 5 thru_hole circle (at 0 10.16) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 4 thru_hole circle (at 0 7.62) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at 0 5.08) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 4 V+))
    (pad 2 thru_hole circle (at 0 2.54) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(R3-Pad1)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(R6-Pad2)"))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-14_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Bridge_Pitch2.54mm_Drill1.0mm (layer Front) (tedit 5A0F774F)
    (at 85.12048 55.1688 270)
    (descr "wire loop as test point, pitch 2.54mm, hole diameter 1.0mm, wire diameter 0.8mm")
    (tags "test point wire loop")
    (fp_text reference TP14 (at 0.9144 -2.10312 90) (layer F.SilkS))
    (fp_text value Vsn (at 1.3208 1.91008 90) (layer F.SilkS))
    (fp_text user %R (at 1.1 2.1 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 2.54 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(TP14-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(TP14-Pad1)"))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Bridge_Pitch2.54mm_Drill1.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Bridge_Pitch2.54mm_Drill1.0mm (layer Front) (tedit 5A0F774F)
    (at 91.85656 57.7088 90)
    (descr "wire loop as test point, pitch 2.54mm, hole diameter 1.0mm, wire diameter 0.8mm")
    (tags "test point wire loop")
    (fp_text reference TP13 (at 1.1 2.1 90) (layer F.SilkS))
    (fp_text value Vsn+1/2 (at 1 -1.7 90) (layer F.SilkS))
    (fp_text user %R (at 1.1 2.1 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 2.54 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(TP13-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(TP13-Pad1)"))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Bridge_Pitch2.54mm_Drill1.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Bridge_Pitch2.54mm_Drill1.0mm (layer Front) (tedit 5A0F774F)
    (at 105.32872 57.7088 90)
    (descr "wire loop as test point, pitch 2.54mm, hole diameter 1.0mm, wire diameter 0.8mm")
    (tags "test point wire loop")
    (fp_text reference TP11 (at 1.1 2.1 90) (layer F.SilkS))
    (fp_text value Vsn+1 (at 1 -1.7 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 2.54 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(TP11-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(TP11-Pad1)"))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Bridge_Pitch2.54mm_Drill1.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Bridge_Pitch2.54mm_Drill1.0mm (layer Front) (tedit 5A0F774F)
    (at 78.3844 57.7088 90)
    (descr "wire loop as test point, pitch 2.54mm, hole diameter 1.0mm, wire diameter 0.8mm")
    (tags "test point wire loop")
    (fp_text reference TP10 (at 1.1 2.1 90) (layer F.SilkS))
    (fp_text value Vclock (at 1 -1.7 90) (layer F.SilkS))
    (fp_text user %R (at 1.1 2.1 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 2.54 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(TP10-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(TP10-Pad1)"))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Bridge_Pitch2.54mm_Drill1.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Bridge_Pitch2.54mm_Drill1.0mm (layer Front) (tedit 5A0F774F)
    (at 67.84594 89.29878)
    (descr "wire loop as test point, pitch 2.54mm, hole diameter 1.0mm, wire diameter 0.8mm")
    (tags "test point wire loop")
    (fp_text reference TP9 (at 0.72898 2.06502) (layer F.SilkS))
    (fp_text value VcompA (at 1.09474 -2.1844) (layer F.SilkS))
    (fp_text user %R (at 1.1 2.1) (layer F.Fab))
    (pad 1 thru_hole circle (at 2.54 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(R6-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(R6-Pad2)"))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Bridge_Pitch2.54mm_Drill1.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Bridge_Pitch2.54mm_Drill1.0mm (layer Front) (tedit 5A0F774F)
    (at 68.8721 103.02748)
    (descr "wire loop as test point, pitch 2.54mm, hole diameter 1.0mm, wire diameter 0.8mm")
    (tags "test point wire loop")
    (fp_text reference TP8 (at -0.9271 2.38252) (layer F.SilkS))
    (fp_text value ana_in (at 1 -1.7) (layer F.SilkS))
    (fp_text user %R (at 1.1 2.1) (layer F.Fab))
    (pad 1 thru_hole circle (at 2.54 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(TP8-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(TP8-Pad1)"))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Bridge_Pitch2.54mm_Drill1.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Bridge_Pitch2.54mm_Drill1.0mm (layer Front) (tedit 5A0F774F)
    (at 100.711 105.0798 90)
    (descr "wire loop as test point, pitch 2.54mm, hole diameter 1.0mm, wire diameter 0.8mm")
    (tags "test point wire loop")
    (fp_text reference TP7 (at 1.1 2.1 90) (layer F.SilkS))
    (fp_text value Vctrl (at 1 -1.7 90) (layer F.SilkS))
    (fp_text user %R (at 1.1 2.1 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 2.54 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(RV1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(RV1-Pad2)"))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Bridge_Pitch2.54mm_Drill1.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Bridge_Pitch2.54mm_Drill1.0mm (layer Front) (tedit 5A0F774F)
    (at 92.71 104.9528 90)
    (descr "wire loop as test point, pitch 2.54mm, hole diameter 1.0mm, wire diameter 0.8mm")
    (tags "test point wire loop")
    (fp_text reference TP6 (at 1.1 2.1 90) (layer F.SilkS))
    (fp_text value Vbuffer (at 1 -1.7 90) (layer F.SilkS))
    (fp_text user %R (at 1.1 2.1 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 2.54 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(RV2-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(RV2-Pad2)"))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Bridge_Pitch2.54mm_Drill1.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Bridge_Pitch2.54mm_Drill1.0mm (layer Front) (tedit 5A0F774F)
    (at 96.20758 108.89996 270)
    (descr "wire loop as test point, pitch 2.54mm, hole diameter 1.0mm, wire diameter 0.8mm")
    (tags "test point wire loop")
    (fp_text reference TP5 (at 1.1 2.1 90) (layer F.SilkS))
    (fp_text value V- (at 0.9017 -2.0701 90) (layer F.SilkS))
    (fp_text user %R (at 1.1 2.1 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 2.54 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 3 V-))
    (pad 1 thru_hole circle (at 0 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 3 V-))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Bridge_Pitch2.54mm_Drill1.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Bridge_Pitch2.54mm_Drill1.0mm (layer Front) (tedit 5A0F774F)
    (at 87.96655 108.89996 270)
    (descr "wire loop as test point, pitch 2.54mm, hole diameter 1.0mm, wire diameter 0.8mm")
    (tags "test point wire loop")
    (fp_text reference TP3 (at 1.1 2.1 90) (layer F.SilkS))
    (fp_text value GND (at 1 -1.7 90) (layer F.SilkS))
    (fp_text user %R (at 1.1 2.1 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 2.54 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Bridge_Pitch2.54mm_Drill1.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Bridge_Pitch2.54mm_Drill1.0mm (layer Front) (tedit 5A0F774F)
    (at 68.51904 63.74892)
    (descr "wire loop as test point, pitch 2.54mm, hole diameter 1.0mm, wire diameter 0.8mm")
    (tags "test point wire loop")
    (fp_text reference TP2 (at 1.1176 2.0828) (layer F.SilkS))
    (fp_text value ana_out (at 1.0287 -2.032) (layer F.SilkS))
    (fp_text user %R (at 1.1 2.1) (layer F.Fab))
    (pad 1 thru_hole circle (at 2.54 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(R1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(R1-Pad2)"))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Bridge_Pitch2.54mm_Drill1.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Bridge_Pitch2.54mm_Drill1.0mm (layer Front) (tedit 5A0F774F)
    (at 112.0648 57.7088 90)
    (descr "wire loop as test point, pitch 2.54mm, hole diameter 1.0mm, wire diameter 0.8mm")
    (tags "test point wire loop")
    (fp_text reference TP1 (at 1.1 2.1 90) (layer F.SilkS))
    (fp_text value Vc (at 1 -1.7 90) (layer F.SilkS))
    (fp_text user %R (at 1.1 2.1 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 2.54 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Bridge_Pitch2.54mm_Drill1.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometer_THT:Potentiometer_Bourns_3296W_Vertical (layer Front) (tedit 5A3D4994)
    (at 105.54716 109.16666 180)
    (descr "Potentiometer, vertical, Bourns 3296W, https://www.bourns.com/pdfs/3296.pdf")
    (tags "Potentiometer vertical Bourns 3296W")
    (fp_text reference RV1 (at -2.4892 -3.4544) (layer F.SilkS))
    (fp_text value R_POT (at -2.54 3.67) (layer F.Fab))
    (fp_text user %R (at -5.715 1.778) (layer F.Fab))
    (pad 3 thru_hole circle (at -5.08 0 180) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at -2.54 0 180) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(RV1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_3296W_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer Front) (tedit 5F68FEEE)
    (at 71.20204 99.51466 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R8 (at 3.25704 -0.18034) (layer F.SilkS))
    (fp_text value 10k (at 3.191 1.08966) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1 0 180) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 1 GND))
    (pad 1 smd roundrect (at -1 0 180) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 12 "Net-(R7-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer Front) (tedit 5F68FEEE)
    (at 72.20204 95.97466 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R7 (at 0 1.524 90) (layer F.SilkS))
    (fp_text value 10k (at -0.143 2.921 90) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1 0 270) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 12 "Net-(R7-Pad2)"))
    (pad 1 smd roundrect (at -1 0 270) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 28 Va+))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer Front) (tedit 5F68FEEE)
    (at 110.998 88.4588 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R6 (at -2.9116 -1.3716 90) (layer F.SilkS))
    (fp_text value 10k (at -0.4732 -1.778 90) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1 0 270) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 11 "Net-(R6-Pad2)"))
    (pad 1 smd roundrect (at -1 0 270) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 4 V+))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer Front) (tedit 5F68FEEE)
    (at 101.23678 92.3069 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R4 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 220 (at 0 1.65 90) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1 0 270) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 10 "Net-(R4-Pad2)"))
    (pad 1 smd roundrect (at -1 0 270) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 8 "Net-(R2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer Front) (tedit 5F68FEEE)
    (at 74.01052 64.74384 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R3 (at -1.82956 1.7018 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1 0 90) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 14 "Net-(R1-Pad2)"))
    (pad 1 smd roundrect (at -1 0 90) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 9 "Net-(R3-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer Front) (tedit 5F68FEEE)
    (at 102.24948 96.5835 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 220 (at 0 1.65) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1 0 180) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 2 "Net-(C1-Pad1)"))
    (pad 1 smd roundrect (at -1 0 180) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 8 "Net-(R2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer Front) (tedit 5F68FEEE)
    (at 77.994 63.754 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at -1.51308 -1.64084) (layer F.SilkS))
    (fp_text value 6.65k (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1 0 180) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 14 "Net-(R1-Pad2)"))
    (pad 1 smd roundrect (at -1 0 180) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 28 Va+))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:Diode_DO-35_P10mm (layer Front) (tedit 5A466F52)
    (at 115.57 103.1748 180)
    (fp_text reference D2 (at 5.1435 -2.0955) (layer F.SilkS))
    (fp_text value 1N4148 (at 6 3.6) (layer F.Fab))
    (fp_text user %R (at 4.83 0.02) (layer F.Fab))
    (pad 2 thru_hole circle (at 10 0 180) (size 2 2) (drill 0.76) (layers *.Cu *.Mask)
      (net 6 "Net-(D1-Pad1)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 2 2) (drill 0.76) (layers *.Cu *.Mask)
      (net 7 "Net-(D2-Pad1)"))
  )
  (module digikey-footprints:Diode_DO-35_P10mm (layer Front) (tedit 5A466F52)
    (at 110.1674 82.1944)
    (fp_text reference D1 (at 8.93828 -1.94056) (layer F.SilkS))
    (fp_text value 1N4148 (at 5.428 2.286) (layer F.Fab))
    (fp_text user %R (at 4.83 0.02) (layer F.Fab))
    (pad 2 thru_hole circle (at 10 0) (size 2 2) (drill 0.76) (layers *.Cu *.Mask)
      (net 5 "Net-(D1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 0.76) (layers *.Cu *.Mask)
      (net 6 "Net-(D1-Pad1)"))
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder (layer Front) (tedit 5F68FEEF)
    (at 107.315 88.6753 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C15 (at -2.9757 -1.397 90) (layer F.SilkS))
    (fp_text value 0.1u (at 0 1.68 90) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.0375 0 270) (size 1.175 1.45) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2127659574468085)
      (net 3 V-))
    (pad 1 smd roundrect (at -1.0375 0 270) (size 1.175 1.45) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2127659574468085)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder (layer Front) (tedit 5F68FEEF)
    (at 79.7091 61.25464)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C14 (at -3.4837 0.0508) (layer F.SilkS))
    (fp_text value 0.1u (at 2.41418 -1.64592) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2127659574468085)
      (net 4 V+))
    (pad 1 smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2127659574468085)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder (layer Front) (tedit 5F68FEEF)
    (at 89.41698 98.7425)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C13 (at 0.12818 1.68148) (layer F.SilkS))
    (fp_text value 0.1u (at -1.45932 -1.63576) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2127659574468085)
      (net 3 V-))
    (pad 1 smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2127659574468085)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder (layer Front) (tedit 5F68FEEF)
    (at 94.7205 63.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C12 (at 0 -1.68) (layer F.SilkS))
    (fp_text value 0.1u (at 0 1.68) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2127659574468085)
      (net 4 V+))
    (pad 1 smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2127659574468085)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder (layer Front) (tedit 5F68FEEF)
    (at 85.34146 95.58392 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C11 (at 0.27042 2.37236 90) (layer F.SilkS))
    (fp_text value 0.1u (at 1.00194 1.7399 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.0375 0 90) (size 1.175 1.45) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2127659574468085)
      (net 3 V-))
    (pad 1 smd roundrect (at -1.0375 0 90) (size 1.175 1.45) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2127659574468085)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder (layer Front) (tedit 5F68FEEF)
    (at 100.8507 87.12826 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C10 (at 0 -1.68 90) (layer F.SilkS))
    (fp_text value 0.1u (at 0 1.68 90) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.0375 0 270) (size 1.175 1.45) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2127659574468085)
      (net 4 V+))
    (pad 1 smd roundrect (at -1.0375 0 270) (size 1.175 1.45) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2127659574468085)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder (layer Front) (tedit 5F68FEEF)
    (at 71.6065 92.7608 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C7 (at 3.11286 -0.37592) (layer F.SilkS))
    (fp_text value 0.1u (at 3.79612 -0.91186) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.0375 0 180) (size 1.175 1.45) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2127659574468085)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.0375 0 180) (size 1.175 1.45) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2127659574468085)
      (net 4 V+))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder (layer Front) (tedit 5F68FEEF)
    (at 78.72866 71.4502 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C6 (at 2.9757 0.0508) (layer F.SilkS))
    (fp_text value 0.1u (at -0.1485 -2.032) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.0375 0 180) (size 1.175 1.45) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2127659574468085)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.0375 0 180) (size 1.175 1.45) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2127659574468085)
      (net 3 V-))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder (layer Front) (tedit 5F68FEEF)
    (at 94.7205 71.12 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C5 (at 0 -1.68) (layer F.SilkS))
    (fp_text value 0.1u (at 0 1.68) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.0375 0 180) (size 1.175 1.45) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2127659574468085)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.0375 0 180) (size 1.175 1.45) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2127659574468085)
      (net 3 V-))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder (layer Front) (tedit 5F68FEEF)
    (at 119.634 100.6563 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C4 (at -3.0265 0.381 90) (layer F.SilkS))
    (fp_text value 0.1u (at 0 1.68 90) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.0375 0 90) (size 1.175 1.45) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2127659574468085)
      (net 4 V+))
    (pad 1 smd roundrect (at -1.0375 0 90) (size 1.175 1.45) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2127659574468085)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder (layer Front) (tedit 5F68FEEF)
    (at 109.3763 63.5 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C3 (at 0 -1.68) (layer F.SilkS))
    (fp_text value 0.1u (at 0 1.68) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.0375 0 180) (size 1.175 1.45) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2127659574468085)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.0375 0 180) (size 1.175 1.45) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2127659574468085)
      (net 4 V+))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder (layer Front) (tedit 5F68FEEF)
    (at 110.4138 69.4475 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C2 (at 3.0441 0.0254 90) (layer F.SilkS))
    (fp_text value 0.1u (at 0 1.68 90) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.0375 0 270) (size 1.175 1.45) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2127659574468085)
      (net 3 V-))
    (pad 1 smd roundrect (at -1.0375 0 270) (size 1.175 1.45) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2127659574468085)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder (layer Front) (tedit 5F68FEEF)
    (at 86.614 102.8153 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C1 (at 2.78774 -0.05588 90) (layer F.SilkS))
    (fp_text value 1u (at 3.14588 0.66548 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.0375 0 270) (size 1.175 1.45) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2127659574468085)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.0375 0 270) (size 1.175 1.45) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2127659574468085)
      (net 2 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Va+ select" (at 69.54012 77.11948) (layer F.SilkS))
  (gr_text V+ (at 70.13448 79.07528) (layer F.SilkS))
  (gr_text Vext (at 69.6468 75.1078) (layer F.SilkS))
  (gr_arc (start 120.141638 56.134) (end 123.698 56.134) (angle -90) (layer Edge.Cuts) (width 0.001))
  (gr_arc (start 69.3928 56.134) (end 69.3928 52.5272) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 69.85 110.1598) (end 65.7098 110.1598) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 119.024401 109.626401) (end 119.126 114.3) (angle -90.3) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 123.698 56.134) (end 123.697416 109.500783) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 69.3928 52.5272) (end 120.141638 52.577638) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 65.7098 110.1598) (end 65.786 56.134) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 119.126 114.3) (end 69.85 114.3) (layer Edge.Cuts) (width 0.1))
  (gr_text "Chaotic Crew\nUAH Senior Design 2020\nTent Map CRNG" (at 109.9693 86.87308) (layer B.SilkS))
  (zone (net 1) (net_name GND) (layer Back) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 137.16 121.92) (xy 60.96 121.92) (xy 60.96 50.8) (xy 137.16 50.8)
      )
    )
  )
  (zone (net 4) (net_name V+) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 137.16 121.92) (xy 60.96 121.92) (xy 60.96 50.8) (xy 137.16 50.8)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 137.16 121.92) (xy 60.96 121.92) (xy 60.96 50.8) (xy 137.16 50.8)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer Front) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 137.7696 130.81) (xy 57.658 129.0828) (xy 53.0352 55.4736) (xy 60.2996 49.1236) (xy 137.3124 48.514)
      )
    )
  )
)
